Program version: 1.6.0, Extraction mode: UEFI
FormSet Guid: 7B59104A-C00D-4158-87FF-F04D6396A915, Title: "Setup", Help: "Setup"
	Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: Class, Class: 0x1
	Guid Guid: 0F0B1735-87A0-4193-B266-538C38AF48CE, ExtendedOpCode: SubClass, SubClass: 0x0
	DefaultStore DefaultId: 0x0, Name: ""
	DefaultStore DefaultId: 0x1, Name: ""
	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x1, Size: 0x10DD, Name: "Setup"
	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x2, Size: 0x2, Name: "PlatformLang"
	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x3, Size: 0x2, Name: "PlatformLangCodes"
	VarStore Guid: E770BB69-BCB4-4D04-9E97-23FF9456FEAC, VarStoreId: 0x4, Size: 0x1, Name: "SystemAccess"
	VarStore Guid: 9CF0F18E-7C7D-49DE-B5AA-BBBAD6B21007, VarStoreId: 0x5, Size: 0x2, Name: "AMICallback"
	VarStore Guid: C811FA38-42C8-4579-A9BB-60E94EDDFB34, VarStoreId: 0x6, Size: 0x51, Name: "AMITSESetup"
	VarStore Guid: B4909CF3-7B93-4751-9BD8-5BA8220B9BB2, VarStoreId: 0x7, Size: 0x2, Name: "BootManager"
	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x8, Size: 0x2, Name: "Timeout"
	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x9, Size: 0x2, Name: "BootOrder"
	VarStore Guid: 19D96D3F-6A6A-47D2-B195-7B2432DA3BE2, VarStoreId: 0xA, Size: 0x11C, Name: "AddBootOption"
	VarStore Guid: F6C73719-F34C-479C-B32F-277FCBBCFE4F, VarStoreId: 0xB, Size: 0x2, Name: "DelBootOption"
	VarStore Guid: A56074DB-65FE-45F7-BD21-2D2BDD8E9652, VarStoreId: 0xC, Size: 0x2, Name: "LegacyDev"
	VarStore Guid: A56074DB-65FE-45F7-BD21-2D2BDD8E9652, VarStoreId: 0xD, Size: 0x2, Name: "LegacyGroup"
	VarStore Guid: A56074DB-65FE-45F7-BD21-2D2BDD8E9652, VarStoreId: 0xE, Size: 0x2, Name: "LegacyDevOrder"
	VarStore Guid: 052E6EB0-F240-42C5-8309-45874545C6B4, VarStoreId: 0xF, Size: 0x2, Name: "BootNowCount"
	VarStore Guid: C57AD6B7-0515-40A8-9D21-551652854E37, VarStoreId: 0x10, Size: 0x2, Name: "Shell"
	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x11, Size: 0x29, Name: "SetupCpuFeatures"
	VarStore Guid: B08F97FF-E6E8-4193-A997-5E9E9B0ADB32, VarStoreId: 0x12, Size: 0xA, Name: "CpuSetupVolatileData"
	VarStore Guid: 90D93E09-4E91-4B3D-8C77-C82FF10E3C81, VarStoreId: 0x13, Size: 0x6, Name: "CpuSmm"
	VarStore Guid: 5432122D-D034-49D2-A6DE-65A829EB4C74, VarStoreId: 0x14, Size: 0xA, Name: "MeSetupStorage"
	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x15, Size: 0x1, Name: "SetupAmtFeatures"
	VarStore Guid: 64192DCA-D034-49D2-A6DE-65A829EB4C74, VarStoreId: 0x16, Size: 0x10, Name: "IccAdvancedSetupDataVar"
	VarStore Guid: B63BF800-F267-4F55-9217-E97FB3B69846, VarStoreId: 0x17, Size: 0x2, Name: "DynamicPageCount"
	VarStore Guid: 0885F288-418C-4BE1-A6AF-8BAD61DA08FE, VarStoreId: 0x18, Size: 0x2, Name: "DriverHlthEnable"
	VarStore Guid: 7459A7D4-6533-4480-BBA7-79E25A4443C9, VarStoreId: 0x19, Size: 0x2, Name: "DriverHealthCount"
	VarStore Guid: 58279C2D-FB19-466E-B42E-CD437016DC25, VarStoreId: 0x1A, Size: 0x2, Name: "DrvHealthCtrlCnt"
	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x1B, Size: 0xA, Name: "SetupPlatformData"
	VarStore Guid: 560BF58A-1E0D-4D7E-953F-2980A261E031, VarStoreId: 0x1C, Size: 0x9, Name: "PNP0400_0_VV"
	VarStore Guid: 560BF58A-1E0D-4D7E-953F-2980A261E031, VarStoreId: 0x1D, Size: 0x3, Name: "PNP0400_0_NV"
	VarStore Guid: 560BF58A-1E0D-4D7E-953F-2980A261E031, VarStoreId: 0x1E, Size: 0x9, Name: "PNP0510_0_VV"
	VarStore Guid: 560BF58A-1E0D-4D7E-953F-2980A261E031, VarStoreId: 0x1F, Size: 0x3, Name: "PNP0510_0_NV"
	VarStore Guid: 560BF58A-1E0D-4D7E-953F-2980A261E031, VarStoreId: 0x20, Size: 0x9, Name: "PNP0501_0_VV"
	VarStore Guid: 560BF58A-1E0D-4D7E-953F-2980A261E031, VarStoreId: 0x21, Size: 0x3, Name: "PNP0501_0_NV"
	VarStore Guid: 560BF58A-1E0D-4D7E-953F-2980A261E031, VarStoreId: 0x22, Size: 0x9, Name: "PNP0501_1_VV"
	VarStore Guid: 560BF58A-1E0D-4D7E-953F-2980A261E031, VarStoreId: 0x23, Size: 0x3, Name: "PNP0501_1_NV"
	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x24, Size: 0x11, Name: "NBPlatformData"
	VarStore Guid: C0B4FB05-15E5-4588-9FE9-B3D39C067715, VarStoreId: 0x25, Size: 0x2, Name: "DriverManager"
	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x26, Size: 0x2, Name: "DriverOrder"
	VarStore Guid: C143929C-BF5D-423B-999B-0F2DD2B61FF7, VarStoreId: 0x27, Size: 0x2, Name: "AmiGopPolicySetupData"
	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x28, Size: 0x2, Name: "NBGopPlatformData"
	VarStore Guid: 69ECC1BE-A981-446D-8EB6-AF0E53D06CE8, VarStoreId: 0x29, Size: 0x1, Name: "NewOptionPolicy"
	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x2A, Size: 0x2, Name: "UsbMassDevNum"
	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x2B, Size: 0x10, Name: "UsbMassDevValid"
	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x2C, Size: 0x4, Name: "UsbControllerNum"
	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x2D, Size: 0x21, Name: "UsbSupport"
	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x2E, Size: 0x4A, Name: "SdioDevConfiguration"
	VarStore Guid: 7B59104A-C00D-4158-87FF-F04D6396A915, VarStoreId: 0x2F, Size: 0x7, Name: "SecureBootSetup"
	VarStore Guid: 7B59104A-C00D-4158-87FF-F04D6396A915, VarStoreId: 0x30, Size: 0x6, Name: "SecureVarPresent"
	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x31, Size: 0x1, Name: "VendorKeys"
	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x32, Size: 0x1, Name: "SetupMode"
	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x33, Size: 0x1, Name: "SecureBoot"
	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x34, Size: 0x1, Name: "AuditMode"
	VarStore Guid: 8BE4DF61-93CA-11D2-AA0D-00E098032B8C, VarStoreId: 0x35, Size: 0x1, Name: "DeployedMode"
	VarStore Guid: EC87D643-EBA4-4BB5-A1E5-3F3E36B20DA9, VarStoreId: 0x36, Size: 0x7D, Name: "SetupVolatileData"
	Form FormId: 0x2710, Title: "Setup"
		Ref Prompt: "Main", Help: "", QuestionFlags: 0x0, QuestionId: 0x1, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2711
		Ref Prompt: "Advanced", Help: "", QuestionFlags: 0x0, QuestionId: 0x2, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2712
		Ref Prompt: "Chipset", Help: "", QuestionFlags: 0x0, QuestionId: 0x3, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2713
		Ref Prompt: "Security", Help: "", QuestionFlags: 0x0, QuestionId: 0x4, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2714
		Ref Prompt: "Boot", Help: "", QuestionFlags: 0x0, QuestionId: 0x5, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2715
		Ref Prompt: "Save & Exit", Help: "", QuestionFlags: 0x0, QuestionId: 0x6, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716
	End 
	Form FormId: 0x2711, Title: "Main"
		Subtitle Prompt: "BIOS Information", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Text Prompt: "BIOS Vendor", Help: "", Text: "N/A"
			Text Prompt: "Core Version", Help: "", Text: "N/A"
			Text Prompt: "Compliancy", Help: "", Text: "N/A"
			Text Prompt: "Project Version", Help: "", Text: "N/A"
		End 
		Text Prompt: "Project Name", Help: "", Text: "N/A"
		Text Prompt: "Release", Help: "", Text: "N/A"
		Text Prompt: "BIOS ID", Help: "", Text: "N/A"
		Text Prompt: "Build Date and Time", Help: "", Text: "N/A"
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
			Text Prompt: "Access Level", Help: "", Text: "User"
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			Text Prompt: "Access Level", Help: "", Text: "Administrator"
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "Board Information", Help: "", Flags: 0x0
			End 
			Text Prompt: "Board ID", Help: "Displays the Board ID.", Text: "N/A"
			Text Prompt: "Fab ID", Help: "Displays the Fab ID", Text: "N/A"
			Text Prompt: "LAN PHY Revision", Help: "Displays LAN PHY Revision.", Text: "N/A"
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "Processor Information", Help: "", Flags: 0x0
			End 
			Text Prompt: "Name", Help: "Displays the Processor Details.", Text: "N/A"
			Text Prompt: "Type", Help: "Displays the Processor Type.", Text: "N/A"
			Text Prompt: "Speed", Help: "Displays the Processor Speed.", Text: "N/A"
			Text Prompt: "ID", Help: "Displays the Processor ID.", Text: "N/A"
			Text Prompt: "Stepping", Help: "Displays the Processor Stepping.", Text: "Unknown"
			Text Prompt: "Package", Help: "Displays the Processor Package.", Text: "N/A"
			Text Prompt: "Number of Processors", Help: "Displays number of CPU cores.", Text: "xCore(s) / yThread(s)"
			Text Prompt: "Microcode Revision", Help: "CPU Microcode Revision", Text: "Not loaded"
			Text Prompt: "GT Info", Help: "Processor GT Info. Only valid if SNB stepping is D0 or above.", Text: "Not Applicable"
			Text Prompt: "eDRAM Size", Help: "eDRAM Size supported by the SKU", Text: "N/A"
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC8C, Value: 0x4
				Text Prompt: "IGFX VBIOS Version", Help: "IGFX VBIOS Version", Text: "N/A"
				Text Prompt: "IGFX GOP Version", Help: "IGFX GOP Version", Text: "N/A"
			End 
			Text Prompt: "Memory RC Version", Help: "Memory RC Version", Text: "N/A"
			Text Prompt: "Total Memory", Help: "Total Memory in the System.", Text: "N/A"
			Text Prompt: "Memory Frequency", Help: "Displays the Frequency of Memory", Text: "N/A"
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH Information", Help: "", Flags: 0x0
			End 
			Text Prompt: "Name", Help: "PCH Name", Text: "UnKnown"
			Text Prompt: "PCH SKU", Help: "PCH SKU", Text: "UnKnown"
			Text Prompt: "Stepping", Help: "PCH Stepping", Text: "UnKnown"
			Text Prompt: "Hsio Revision", Help: "Hsio Revision", Text: "UnKnown"
			Text Prompt: "Package", Help: "PCH Package", Text: "N/A"
			Text Prompt: "TXT Capability of Platform/PCH", Help: "Platform/PCH TXT capability", Text: "Not Supported"
			Text Prompt: "Production Type", Help: "Platform Production Type", Text: "Not Supported"
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Text Prompt: "Dual Output Fast Read support", Help: "Dual Output Fast Read support", Text: "N/A"
			Text Prompt: "Read ID/Status Clock Freq", Help: "Read ID and Read Status Clock Frequency", Text: "N/A"
			Text Prompt: "Write and Erase Clock Freq", Help: "Write and Erase Clock Frequency ", Text: "N/A"
			Text Prompt: "Fast Read Clock Freq", Help: "Fast Read Clock Frequency", Text: "N/A"
			Text Prompt: "Fast Read support", Help: "Fast Read support", Text: "N/A"
			Text Prompt: "Read Clock Freq", Help: "Read Clock Frequency", Text: "N/A"
			Text Prompt: "Number of Components", Help: "Number of Components", Text: "N/A"
			SuppressIf 
				EqIdVal QuestionId: 0xCF6, Value: 0x0
				Text Prompt: "SPI Component 1 Density", Help: "SPI Component 1 Density", Text: "N/A"
			End 
			Text Prompt: "SPI Component 0 Density", Help: "SPI Component 0 Density", Text: "N/A"
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Text Prompt: "EC FW Version", Help: "EC FW Version", Text: "N/A"
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
					Not 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xCF5, Value: 0x0
					Text Prompt: "Base EC FW Version", Help: "Base EC FW Version", Text: "Not Present"
					Text Prompt: "EC Protocol Version", Help: "EC Protocol Version", Text: "Not Present"
					Text Prompt: "Base EC Protocol Version", Help: "Base EC Protocol Version", Text: "Not Present"
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
					Not 
				End 
				Text Prompt: "STM32 FW Version", Help: "STM32 FW Version", Text: "Not Ready"
				SuppressIf 
					True 
					SuppressIf 
						EqIdVal QuestionId: 0xC41, Value: 0xB
						Action Prompt: "STM32 FW Version", Help: "STM32 FW Version", QuestionFlags: 0x4, QuestionId: 0x2911, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, QuestionConfig: ""
						End 
					End 
				End 
			End 
			Text Prompt: "ME FW Version", Help: "ME Firmware Version", Text: "N/A"
			Text Prompt: "ME Firmware SKU", Help: "ME Firmware SKU", Text: "N/A"
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x1
					Not 
					EqIdVal QuestionId: 0xC50, Value: 0x2
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x4
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x14
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0xA
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x1A
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x8
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0xB
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x7
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x13
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x3
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x1B
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0xC
					Not 
					And 
				End 
				Text Prompt: "Sensor Hub FW", Help: "Sensor Hub Firmware Version", Text: "N/A"
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCF4, Value: 0xFFFF
			OneOf Prompt: "System Language", Help: "Choose the system default language", QuestionFlags: 0x0, QuestionId: 0x7, VarStoreId: 0x2, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "" Value: 0
				OneOfOption Option: "" Value: 1
				Default DefaultId: 0x0 Value: 0
				Default DefaultId: 0x1 Value: 0
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Date Prompt: "System Date", Help: "Set the Date. Use Tab to switch between Date elements.", QuestionFlags: 0x0, QuestionId: 0x8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, Flags: 0x10
			Default DefaultId: 0x0 Value: 2014-01-01
		End 
		Time Prompt: "System Time", Help: "Set the Time. Use Tab to switch between Time elements.", QuestionFlags: 0x0, QuestionId: 0x9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, Flags: 0x10
			Default DefaultId: 0x0 Value: 00:00:00
		End 
	End 
	Form FormId: 0x2712, Title: "Advanced"
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "Intel RC ACPI Settings", Help: "System ACPI Parameters.", QuestionFlags: 0x0, QuestionId: 0xA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2717
		End 
		Ref Prompt: "CPU Configuration", Help: "CPU Configuration Parameters", QuestionFlags: 0x0, QuestionId: 0xB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x272A
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "Power & Performance", Help: "Power & Performance Options", QuestionFlags: 0x0, QuestionId: 0xC, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x272C
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "PCH-FW Configuration", Help: "Configure Management Engine Technology Parameters", QuestionFlags: 0x0, QuestionId: 0xD, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2794
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "Thermal Configuration", Help: "Thermal Configuration Parameters", QuestionFlags: 0x0, QuestionId: 0xE, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2798
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "Platform Settings", Help: "Platform related settings", QuestionFlags: 0x0, QuestionId: 0xF, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x279D
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "Realsense 3D Camera Settings", Help: "Realsense 3D Camera related settings", QuestionFlags: 0x0, QuestionId: 0x10, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x279E
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "OverClocking Performance Menu", Help: "Performance Menu for Processor and Memory.", QuestionFlags: 0x0, QuestionId: 0x11, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B4
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "Intel ICC", Help: "Intel ICC", QuestionFlags: 0x0, QuestionId: 0x12, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27CA
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "Thunderbolt(TM) Configuration", Help: "Thunderbolt(TM) Related Configuration", QuestionFlags: 0x0, QuestionId: 0x13, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27DB
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xCF3, Values: [65535]
			Ref Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x14, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2712
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xCF2, Values: [65535]
			Ref Prompt: "Driver Health", Help: "Provides Health Status for the Drivers/Controllers", QuestionFlags: 0x0, QuestionId: 0x15, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27DD
		End 
		SuppressIf 
			Uint64 Value: 0x1
				Uint64 Value: 0x0
				Equal 
			End 
			Ref Prompt: "ACPI Settings", Help: "System ACPI Parameters.", QuestionFlags: 0x0, QuestionId: 0x16, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27E0
		End 
		Ref Prompt: "Miscellaneous Configuration", Help: "Enable\Disable Misc. Features", QuestionFlags: 0x0, QuestionId: 0x17, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27FB
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "SMART Settings", Help: "System SMART Settings", QuestionFlags: 0x0, QuestionId: 0x18, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27FC
		End 
		Ref Prompt: "IT8784 Super IO Configuration", Help: "System Super IO Chip Parameters.", QuestionFlags: 0x0, QuestionId: 0x19, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2805
		Ref Prompt: "Hardware Monitor", Help: "Monitor hardware status", QuestionFlags: 0x0, QuestionId: 0x1A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x280A
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "Intel(R) Bios Guard Technology", Help: "Enable/Disable Intel Bios Guard Support", QuestionFlags: 0x0, QuestionId: 0x1B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x280C
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "Intel TXT Information", Help: "Display Intel TXT information", QuestionFlags: 0x0, QuestionId: 0x1C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2810
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCF1, Value: 0x0
			Ref Prompt: "AMI Graphic Output Protocol Policy", Help: "User Select Monitor Output by Graphic Output Protocol", QuestionFlags: 0x0, QuestionId: 0x1D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2813
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "PCI Subsystem Settings", Help: "PCI, PCI-X and PCI Express Settings.", QuestionFlags: 0x0, QuestionId: 0x1E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x281F
		End 
		Ref Prompt: "USB Configuration", Help: "USB Configuration Parameters", QuestionFlags: 0x0, QuestionId: 0x1F, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2827
		Ref Prompt: "CSM Configuration", Help: "CSM configuration: Enable/Disable, Option ROM execution settings, etc.", QuestionFlags: 0x0, QuestionId: 0x20, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x282A
		Ref Prompt: "NVMe Configuration", Help: "NVMe Device Options Settings", QuestionFlags: 0x0, QuestionId: 0x21, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x1, RefQuestionId: 0x0, FormSetGuid: 5E39CF2E-6712-45AB-84C4-35D3C6A3686D
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "SDIO Configuration", Help: "SDIO Configuration Parameters", QuestionFlags: 0x0, QuestionId: 0x22, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28ED
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "Switchable Graphics", Help: "Switchable Graphics selections", QuestionFlags: 0x0, QuestionId: 0x23, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x290E
		End 
	End 
	Form FormId: 0x2717, Title: "Intel RC ACPI Settings"
		Subtitle Prompt: "Intel RC ACPI Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		CheckBox Prompt: "PTID Support", Help: "PTID Support will be loaded if enabled.", QuestionFlags: 0x10, QuestionId: 0x24, VarStoreId: 0x1, VarOffset: 0x6, Flags: 0x3, Default: Enabled, MfgDefault: Enabled
		End 
		OneOf Prompt: "PECI Access Method", Help: "PECI Access Method is Direct I/O or ACPI", QuestionFlags: 0x10, QuestionId: 0x25, VarStoreId: 0x1, VarOffset: 0x12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Direct I/O" Value: 0, Default, MfgDefault
			OneOfOption Option: "ACPI" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x644, Value: 0x0
			OneOf Prompt: "Native PCIE Enable", Help: "Bit - PCIe Native * control
 0 - ~ Hot Plug
 1 - SHPC Native Hot Plug control
 2 - ~ Power Management Events
 3 - PCIe Advanced Error Reporting control
 4 - PCIe Capability Structure control
 5 - Latency Tolerance Reporting control", QuestionFlags: 0x10, QuestionId: 0x26, VarStoreId: 0x1, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x26, Value: 0x0
			OneOf Prompt: "Native ASPM", Help: "Enabled - OS Controlled ASPM, Disabled - BIOS Controlled ASPM", QuestionFlags: 0x10, QuestionId: 0x27, VarStoreId: 0x1, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Auto" Value: 2
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "ACPI Debug", Help: "Open a memory buffer for storing debug strings. Reenter SETUP after enabling to see the buffer address. Use method ADBG to write strings to buffer.", QuestionFlags: 0x10, QuestionId: 0x28, VarStoreId: 0x1, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x28, Value: 0x0
			Text Prompt: "  Acpi Memory Buffer Address", Help: "Acpi Memory Buffer Address", Text: "N/A"
		End 
		OneOf Prompt: "Low Power S0 Idle Capability", Help: "This variable determines if we enable ACPI Lower Power S0 Idle Capability (Mutually exclusive with Smart connect)", QuestionFlags: 0x10, QuestionId: 0x29, VarStoreId: 0x1, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x29, Value: 0x1
				Not 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x1
					Not 
					EqIdVal QuestionId: 0xC50, Value: 0x2
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x4
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x14
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0xA
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x1A
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x8
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0xB
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x7
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x13
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x3
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x1B
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0xC
					Not 
					And 
					EqIdVal QuestionId: 0x2B, Value: 0x1
					Not 
					And 
				End 
				OneOf Prompt: "10sec Power Button OVR", Help: "Enable/Disable/Auto 10sec Power Button Override feature.  When enabled, Power button must be pressed for 10 seconds to cause an unconditional S5 transition(Power Button Override). Auto enables this feature automatically if BIOS detects supported Board and Fab ID. Note: This feature requires HW support.  Please make sure your HW has a proper rework.", QuestionFlags: 0x10, QuestionId: 0x2A, VarStoreId: 0x1, VarOffset: 0x2C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			OneOf Prompt: "EC Notification", Help: "Sends EC notification of Low Power S0 Idle State", QuestionFlags: 0x10, QuestionId: 0x2B, VarStoreId: 0x1, VarOffset: 0x23, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2B, Value: 0x1
					Not 
				End 
				OneOf Prompt: "EC CS Debug Light", Help: "When EC enters Low Power S0 Idle State, the CAPS LOCK light will be turned on", QuestionFlags: 0x10, QuestionId: 0x2C, VarStoreId: 0x1, VarOffset: 0x24, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				OneOf Prompt: "EC Low Power Mode", Help: "This option controls whether EC will go to Low power mode during Low Power S0 Idle State", QuestionFlags: 0x10, QuestionId: 0x2D, VarStoreId: 0x1, VarOffset: 0x25, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
					Not 
				End 
				OneOf Prompt: "EC Debug LED", Help: "When disabled all LEDs controlled by the EC are turned off to save power in CS", QuestionFlags: 0x10, QuestionId: 0x2E, VarStoreId: 0x1, VarOffset: 0x26, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 1
					OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
				End 
				OneOf Prompt: "EC Base CS Pwr Policy", Help: "While in CS, this policy controls how the system behaves when the Base Battery is depleted.", QuestionFlags: 0x10, QuestionId: 0x2F, VarStoreId: 0x1, VarOffset: 0x27, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Battery Saver" Value: 1
					OneOfOption Option: "Fully Functional" Value: 0, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "Sensor Standby", Help: "Enable/Disable Sensor standby mode", QuestionFlags: 0x10, QuestionId: 0x30, VarStoreId: 0x1, VarOffset: 0x28, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "CS PL1 Limit", Help: "Limit PL1 (Power Limit 1) while in Connected Standby", QuestionFlags: 0x10, QuestionId: 0x31, VarStoreId: 0x1, VarOffset: 0x29, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x31, Value: 0x1
					Not 
				End 
				Numeric Prompt: "CS PL1 Value", Help: "PL1 value is in milliwatts with 125 step value", QuestionFlags: 0x0, QuestionId: 0x32, VarStoreId: 0x1, VarOffset: 0x2A, Flags: 0x11, Size: 16, Min: 0xBB8, Max: 0x4E20, Step: 0x7D
					Default DefaultId: 0x0 Value: 4500
				End 
			End 
			Ref Prompt: "PEP Constraints Configuration", Help: "Control which controllers get included in PEP constraint list", QuestionFlags: 0x0, QuestionId: 0x33, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2718
		End 
		OneOf Prompt: "Lpit Windows RS2 Workaround", Help: "This will enable the workaround to publish 2 LPIT entries which is required for Windows RS2", QuestionFlags: 0x10, QuestionId: 0x34, VarStoreId: 0x1, VarOffset: 0x4E9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x34, Value: 0x1
				Not 
			End 
			OneOf Prompt: "Lpit Recidency Counter", Help: "Select Recidency Counter", QuestionFlags: 0x10, QuestionId: 0x35, VarStoreId: 0x1, VarOffset: 0x2D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "SLP S0" Value: 0, Default, MfgDefault
				OneOfOption Option: "C10" Value: 1
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCF0, Value: 0x0
				EqIdVal QuestionId: 0xC8C, Value: 0x2
				Not 
				EqIdVal QuestionId: 0xC8C, Value: 0x1
				Not 
				And 
				EqIdVal QuestionId: 0xC8C, Value: 0x4
				Not 
				And 
				Or 
			End 
			OneOf Prompt: "Intel Ready Mode Technology", Help: "Enable/Disable Ready Mode support based on Windows Away-mode. Only on DT/AIO. ", QuestionFlags: 0x10, QuestionId: 0x36, VarStoreId: 0x1, VarOffset: 0x2E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x36, Value: 0x0
				OneOf Prompt: "  HW Notification", Help: "Hardware notification enabling status.", QuestionFlags: 0x10, QuestionId: 0x37, VarStoreId: 0x1, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
				OneOf Prompt: "  Intel RMT State", Help: "Intel RMT Enabling Status in BIOS.", QuestionFlags: 0x10, QuestionId: 0x38, VarStoreId: 0x1, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "PCI Delay Optimization", Help: "Experimental ACPI additions for FW latency optimizations", QuestionFlags: 0x10, QuestionId: 0x39, VarStoreId: 0x1, VarOffset: 0xC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "ZpODD Support", Help: "ZpODD SSDT table will be loaded if enabled.", QuestionFlags: 0x10, QuestionId: 0x3A, VarStoreId: 0x1, VarOffset: 0xFED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Type C Support", Help: "Enable/Disable USB Type C Support", QuestionFlags: 0x10, QuestionId: 0x3B, VarStoreId: 0x1, VarOffset: 0x4D0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
	End 
	Form FormId: 0x2718, Title: "PEP Constraints Configuration"
		Subtitle Prompt: "PEP Constraints Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "PEP CPU", Help: "Add CPU in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x3C, VarStoreId: 0x1, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "PEP Graphics", Help: "Add Gfx in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x3D, VarStoreId: 0x1, VarOffset: 0x15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "PEP ISP", Help: "Add ISP in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x3E, VarStoreId: 0x1, VarOffset: 0x50E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PEP SATA Controller", Help: "Enable constraints on all storage controllers", QuestionFlags: 0x10, QuestionId: 0x3F, VarStoreId: 0x1, VarOffset: 0x512, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "PEP RAID VOL0", Help: "Enable constraint on logical RAID VOL0", QuestionFlags: 0x10, QuestionId: 0x40, VarStoreId: 0x1, VarOffset: 0x51C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PEP SATA PORT0", Help: "Enable constraints on SATA PORT0", QuestionFlags: 0x10, QuestionId: 0x41, VarStoreId: 0x1, VarOffset: 0x513, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PEP SATA PORT1", Help: "Enable constraints on SATA PORT1", QuestionFlags: 0x10, QuestionId: 0x42, VarStoreId: 0x1, VarOffset: 0x514, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PEP SATA PORT2", Help: "Enable constraints on SATA PORT2", QuestionFlags: 0x10, QuestionId: 0x43, VarStoreId: 0x1, VarOffset: 0x515, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PEP SATA PORT3", Help: "Enable constraints on SATA PORT3", QuestionFlags: 0x10, QuestionId: 0x44, VarStoreId: 0x1, VarOffset: 0x516, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PEP SATA PORT4", Help: "Enable constraints on SATA PORT4", QuestionFlags: 0x10, QuestionId: 0x45, VarStoreId: 0x1, VarOffset: 0x517, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PEP SATA PORT5", Help: "Enable constraints on SATA PORT5", QuestionFlags: 0x10, QuestionId: 0x46, VarStoreId: 0x1, VarOffset: 0x518, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PEP SATA NVM1", Help: "Enable constraints on SATA NVM1", QuestionFlags: 0x10, QuestionId: 0x47, VarStoreId: 0x1, VarOffset: 0x519, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PEP SATA NVM2", Help: "Enable constraints on SATA NVM2", QuestionFlags: 0x10, QuestionId: 0x48, VarStoreId: 0x1, VarOffset: 0x51A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PEP SATA NVM3", Help: "Enable constraints on SATA NVM3", QuestionFlags: 0x10, QuestionId: 0x49, VarStoreId: 0x1, VarOffset: 0x51B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xCEF, Value: 0x0
				EqIdVal QuestionId: 0xCEE, Value: 0x0
				And 
				EqIdVal QuestionId: 0xCED, Value: 0x0
				And 
			End 
			OneOf Prompt: "PEP UART", Help: "Add UART in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x4A, VarStoreId: 0x1, VarOffset: 0x17, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9EF, Value: 0x0
			OneOf Prompt: "PEP I2C0", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x4B, VarStoreId: 0x1, VarOffset: 0x18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xCEC, Value: 0x0
			OneOf Prompt: "PEP I2C1", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x4C, VarStoreId: 0x1, VarOffset: 0x19, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xCEB, Value: 0x0
			OneOf Prompt: "PEP I2C2", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x4D, VarStoreId: 0x1, VarOffset: 0x1A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xCEA, Value: 0x0
			OneOf Prompt: "PEP I2C3", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x4E, VarStoreId: 0x1, VarOffset: 0x1B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xCE9, Value: 0x0
			OneOf Prompt: "PEP I2C4", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x4F, VarStoreId: 0x1, VarOffset: 0x1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xCE8, Value: 0x0
			OneOf Prompt: "PEP I2C5", Help: "Adds I2C in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x50, VarStoreId: 0x1, VarOffset: 0x1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xCE7, Value: 0x0
				EqIdVal QuestionId: 0xCE6, Value: 0x0
				And 
			End 
			OneOf Prompt: "PEP SPI", Help: "Add SPI in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x51, VarStoreId: 0x1, VarOffset: 0x1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		OneOf Prompt: "PEP XHCI", Help: "Add XHCI in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x52, VarStoreId: 0x1, VarOffset: 0x1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9BC, Value: 0x0
			OneOf Prompt: "PEP Audio", Help: "Add Audio in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x53, VarStoreId: 0x1, VarOffset: 0x20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xA62, Value: 0x0
			OneOf Prompt: "PEP EMMC", Help: "Add EMMC in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x54, VarStoreId: 0x1, VarOffset: 0x21, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xA65, Value: 0x0
			OneOf Prompt: "PEP SDXC", Help: "Add SDXC in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x55, VarStoreId: 0x1, VarOffset: 0x22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		OneOf Prompt: "PEP CSME", Help: "Add CSME in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x56, VarStoreId: 0x1, VarOffset: 0x53C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8D, Value: 0x0
			SuppressIf 
				EqIdVal QuestionId: 0x544, Value: 0x0
				OneOf Prompt: "PEP GBE", Help: "Add GBE in PEP mitigation list", QuestionFlags: 0x10, QuestionId: 0x57, VarStoreId: 0x1, VarOffset: 0x4E8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8C, Value: 0x1
				Not 
			End 
			OneOf Prompt: "PEP WIGIG F1", Help: "Enable / Disable PEP F1 constraints for WiGig device", QuestionFlags: 0x10, QuestionId: 0x58, VarStoreId: 0x1, VarOffset: 0x4D8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
	End 
	Form FormId: 0x272A, Title: "CPU Configuration"
		Subtitle Prompt: "CPU Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "Type", Help: "Displays the Processor Type.", Text: "N/A"
		Text Prompt: "ID", Help: "Displays the Processor ID.", Text: "N/A"
		Text Prompt: "Speed", Help: "Displays the Processor Speed.", Text: "N/A"
		Text Prompt: "Stepping", Help: "Displays the Processor Stepping.", Text: "Unknown"
		Text Prompt: "Number of Processors", Help: "Displays number of CPU cores.", Text: "xCore(s) / yThread(s)"
		Text Prompt: "Microcode Revision", Help: "CPU Microcode Revision", Text: "Not loaded"
		Text Prompt: "GT Info", Help: "Processor GT Info. Only valid if SNB stepping is D0 or above.", Text: "Not Applicable"
		Text Prompt: "L1 Data Cache", Help: "Displays the Processor L1 Data Cache size.", Text: "N/A"
		Text Prompt: "L1 Instruction Cache", Help: "Displays the Processor L1 Instruction Cache size.", Text: "N/A"
		Text Prompt: "L2 Cache", Help: "Displays the Processor L2 Cache size.", Text: "N/A"
		Text Prompt: "L3 Cache", Help: "Displays the Processor L3 Cache size.", Text: "N/A"
		Text Prompt: "L4 Cache", Help: "Displays the Processor L4 eDRAM size.", Text: "N/A"
		Text Prompt: "VMX", Help: "VMX Supported or Not", Text: "N/A"
		Text Prompt: "SMX/TXT", Help: "SMX/TXT Supported or Not", Text: "N/A"
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCE5, Value: 0x0
				OneOf Prompt: "SW Guard Extensions (SGX)", Help: "Enable/Disable Software Guard Extensions (SGX)", QuestionFlags: 0x14, QuestionId: 0x2719, VarStoreId: 0x1, VarOffset: 0x639, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Software Controlled" Value: 2, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
					OneOfOption Option: "Disabled" Value: 0
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2719, Value: 0x0
					OneOf Prompt: "Select Owner EPOCH input type", Help: "There are three Owner EPOCH modes (Each EPOCH is 64bit): no change in owner epoch, change to new random owner epoch and manually entered by user. After generating new epoch via 'Change to New Random Owner EPOCHs', the selection reverts back to 'No Change in Owner Epochs', this is to ensure Epoch stays same, across Sx states. After the user enters epoch values manually, the values will not be visible, for security reasons.", QuestionFlags: 0x14, QuestionId: 0x271A, VarStoreId: 0x1, VarOffset: 0x63A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
						OneOfOption Option: "No Change in Owner EPOCHs" Value: 0, Default, MfgDefault
						OneOfOption Option: "Change to New Random Owner EPOCHs" Value: 1
						OneOfOption Option: "Manual User Defined Owner EPOCHs" Value: 2
					End 
					SuppressIf 
						EqIdVal QuestionId: 0xCE4, Value: 0x2
							EqIdVal QuestionId: 0x271A, Value: 0x2
							Not 
							Or 
						End 
						Numeric Prompt: "Software Guard Extensions Epoch 0", Help: "Software Guard Extensions Epoch 0", QuestionFlags: 0x10, QuestionId: 0x59, VarStoreId: 0x1, VarOffset: 0x640, Flags: 0x23, Size: 64, Min: 0x0, Max: 0xFFFFFFFFFFFFFFFF, Step: 0x1
							Default DefaultId: 0x0 Value: 6142344250440060711
						End 
						Numeric Prompt: "Software Guard Extensions Epoch 1", Help: "Software Guard Extensions Epoch 1", QuestionFlags: 0x14, QuestionId: 0x271B, VarStoreId: 0x1, VarOffset: 0x648, Flags: 0x23, Size: 64, Min: 0x0, Max: 0xFFFFFFFFFFFFFFFF, Step: 0x1
							Default DefaultId: 0x0 Value: 15521488688214965697
						End 
					End 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2719, Value: 0x0
				GrayOutIf 
					EqIdVal QuestionId: 0x2719, Value: 0x2
					OneOf Prompt: "PRMRR Size", Help: "Setting the PRMRR Size", QuestionFlags: 0x10, QuestionId: 0x5A, VarStoreId: 0x1, VarOffset: 0x63C, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x8000000, Step: 0x0
						OneOfOption Option: "INVALID PRMRR" Value: 0, Default, MfgDefault
						OneOfOption Option: "32MB" Value: 33554432
						OneOfOption Option: "64MB" Value: 67108864
						OneOfOption Option: "128MB" Value: 134217728
					End 
				End 
			End 
			OneOf Prompt: "CPU Flex Ratio Override", Help: "Enable/Disable CPU Flex Ratio Programming", QuestionFlags: 0x10, QuestionId: 0x5B, VarStoreId: 0x1, VarOffset: 0x54B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0x5B, Value: 0x0
				Numeric Prompt: "CPU Flex Ratio Settings", Help: "This value must be between Max Efficiency Ratio (LFM) and Maximum non-turbo ratio set by Hardware (HFM).", QuestionFlags: 0x14, QuestionId: 0x271C, VarStoreId: 0x1, VarOffset: 0x549, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x0
					Default DefaultId: 0x0 Value: 20
				End 
			End 
			OneOf Prompt: "Hardware Prefetcher", Help: "To turn on/off the MLC streamer prefetcher.", QuestionFlags: 0x10, QuestionId: 0x5C, VarStoreId: 0x1, VarOffset: 0x61B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "Adjacent Cache Line Prefetch", Help: "To turn on/off prefetching of adjacent cache lines.", QuestionFlags: 0x10, QuestionId: 0x5D, VarStoreId: 0x1, VarOffset: 0x61C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCE3, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "Intel (VMX) Virtualization Technology", Help: "When enabled, a VMM can utilize the additional hardware capabilities provided by Vanderpool Technology.", QuestionFlags: 0x10, QuestionId: 0x5E, VarStoreId: 0x1, VarOffset: 0x615, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			OneOf Prompt: "PECI", Help: "Enable/Disable PECI", QuestionFlags: 0x10, QuestionId: 0x5F, VarStoreId: 0x1, VarOffset: 0x54C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xCD0, Value: 0x1
					EqIdVal QuestionId: 0x6B, Value: 0x1
					Or 
				End 
				OneOf Prompt: "Active Processor Cores", Help: "Number of cores to enable in each processor package.", QuestionFlags: 0x10, QuestionId: 0x60, VarStoreId: 0x1, VarOffset: 0x54E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x8, Step: 0x0
					OneOfOption Option: "All" Value: 0, Default, MfgDefault
					OneOfOption Option: "1" Value: 1
					SuppressIf 
						QuestionRef1 QuestionId: 0xCD0
							Uint8 Value: 0x2
							LessEqual 
						End 
						OneOfOption Option: "2" Value: 2
					End 
					SuppressIf 
						QuestionRef1 QuestionId: 0xCD0
							Uint8 Value: 0x3
							LessEqual 
						End 
						OneOfOption Option: "3" Value: 3
					End 
					SuppressIf 
						QuestionRef1 QuestionId: 0xCD0
							Uint8 Value: 0x4
							LessEqual 
						End 
						OneOfOption Option: "4" Value: 4
					End 
					SuppressIf 
						QuestionRef1 QuestionId: 0xCD0
							Uint8 Value: 0x5
							LessEqual 
						End 
						OneOfOption Option: "5" Value: 5
					End 
					SuppressIf 
						QuestionRef1 QuestionId: 0xCD0
							Uint8 Value: 0x6
							LessEqual 
						End 
						OneOfOption Option: "6" Value: 6
					End 
					SuppressIf 
						QuestionRef1 QuestionId: 0xCD0
							Uint8 Value: 0x7
							LessEqual 
						End 
						OneOfOption Option: "7" Value: 7
					End 
					SuppressIf 
						QuestionRef1 QuestionId: 0xCD0
							Uint8 Value: 0x8
							LessEqual 
						End 
						OneOfOption Option: "8" Value: 8
					End 
				End 
			End 
			SuppressIf 
				True 
				OneOf Prompt: "Execute Disable Bit", Help: "XD can prevent certain classes of malicious buffer overflow attacks when combined with a supporting OS (Windows Server 2003 SP1, Windows XP SP2, SuSE Linux 9.2, RedHat Enterprise 3 Update 3.)", QuestionFlags: 0x10, QuestionId: 0x61, VarStoreId: 0x1, VarOffset: 0x546, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
				OneOf Prompt: "Limit CPUID Maximum", Help: "Disabled for Windows XP", QuestionFlags: 0x10, QuestionId: 0x62, VarStoreId: 0x1, VarOffset: 0x547, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Numeric Prompt: "Set Boot Freq Ratio", Help: "", QuestionFlags: 0x10, QuestionId: 0x63, VarStoreId: 0x1, VarOffset: 0x548, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 20
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCDF, Value: 0x0
				GrayOutIf 
					EqIdVal QuestionId: 0x6B, Value: 0x1
					OneOf Prompt: "Hyper-Threading", Help: "Enabled for Windows XP and Linux (OS optimized for Hyper-Threading Technology) and Disabled for other OS (OS not optimized for Hyper-Threading Technology).", QuestionFlags: 0x10, QuestionId: 0x64, VarStoreId: 0x1, VarOffset: 0x54D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0
						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					End 
				End 
			End 
			OneOf Prompt: "BIST", Help: "Enable/Disable BIST (Built-In Self Test) on reset", QuestionFlags: 0x10, QuestionId: 0x65, VarStoreId: 0x1, VarOffset: 0x54F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC98, Value: 0x6E0
					Not 
				End 
				OneOf Prompt: "JTAG C10 Power", Help: "Enable/Disable Power JTAG in C10 and deeper power states", QuestionFlags: 0x10, QuestionId: 0x66, VarStoreId: 0x1, VarOffset: 0x550, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				End 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0x271D, Value: 0x0
				OneOf Prompt: "AP threads Idle Manner", Help: "AP threads Idle Manner for waiting signal to run", QuestionFlags: 0x10, QuestionId: 0x67, VarStoreId: 0x1, VarOffset: 0x650, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3, Step: 0x0
					OneOfOption Option: "HALT Loop" Value: 1
					OneOfOption Option: "MWAIT Loop" Value: 2, Default, MfgDefault
					OneOfOption Option: "RUN Loop" Value: 3
				End 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0x271D, Value: 0x0
				OneOf Prompt: "AP threads Handoff Manner", Help: "AP threads Handoff to OS Manner from end of POST", QuestionFlags: 0x10, QuestionId: 0x68, VarStoreId: 0x1, VarOffset: 0x651, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x2, Step: 0x0
					OneOfOption Option: "HALT Loop" Value: 1
					OneOfOption Option: "MWAIT Loop" Value: 2, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCE2, Value: 0x0
				GrayOutIf 
					EqIdVal QuestionId: 0xC42, Value: 0x1
					OneOf Prompt: "AES", Help: "Enable/Disable AES (Advanced Encryption Standard)", QuestionFlags: 0x10, QuestionId: 0x69, VarStoreId: 0x1, VarOffset: 0x616, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0
						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					End 
				End 
			End 
			OneOf Prompt: "MachineCheck", Help: "Enable/Disable Machine Check", QuestionFlags: 0x10, QuestionId: 0x6A, VarStoreId: 0x1, VarOffset: 0x617, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "MonitorMWait", Help: "Enable/Disable MonitorMWait", QuestionFlags: 0x14, QuestionId: 0x271D, VarStoreId: 0x1, VarOffset: 0x618, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCE1, Value: 0x0
				GrayOutIf 
					EqIdVal QuestionId: 0x5E, Value: 0x0
						EqIdVal QuestionId: 0x3EA, Value: 0x0
						Or 
						EqIdVal QuestionId: 0x60, Value: 0x0
						Not 
						Or 
						EqIdVal QuestionId: 0x64, Value: 0x0
						EqIdVal QuestionId: 0xCDF, Value: 0x1
						And 
						Or 
					End 
					OneOf Prompt: "Intel Trusted Execution Technology", Help: "Enables utilization of additional hardware capabilities provided by Intel (R) Trusted Execution Technology.

Changes require a full power cycle to take effect.", QuestionFlags: 0x10, QuestionId: 0x6B, VarStoreId: 0x1, VarOffset: 0x61D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCE1, Value: 0x0
				GrayOutIf 
					EqIdVal QuestionId: 0x6B, Value: 0x0
					OneOf Prompt: "Alias Check Request", Help: "Enables Txt Alias Checking capability

Changes require full Txt capability before it will take effect.

 It is a one time only change, next reboot will be reset.", QuestionFlags: 0x10, QuestionId: 0x6C, VarStoreId: 0x1, VarOffset: 0x620, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCE1, Value: 0x0
				GrayOutIf 
					EqIdVal QuestionId: 0xCE0, Value: 0x1
						EqIdVal QuestionId: 0x5E, Value: 0x0
						Or 
						EqIdVal QuestionId: 0x3EA, Value: 0x0
						Or 
						EqIdVal QuestionId: 0x6B, Value: 0x0
						Or 
						EqIdVal QuestionId: 0x60, Value: 0x0
						Not 
						Or 
						EqIdVal QuestionId: 0x64, Value: 0x0
						EqIdVal QuestionId: 0xCDF, Value: 0x1
						And 
						Or 
					End 
					Numeric Prompt: "DPR Memory Size (MB)", Help: "Reserve DPR memory size (0-255) MB", QuestionFlags: 0x0, QuestionId: 0x6D, VarStoreId: 0x1, VarOffset: 0x619, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 4
					End 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCE1, Value: 0x0
				GrayOutIf 
					EqIdVal QuestionId: 0xCE0, Value: 0x1
						EqIdVal QuestionId: 0x5E, Value: 0x0
						Or 
						EqIdVal QuestionId: 0x3EA, Value: 0x0
						Or 
						EqIdVal QuestionId: 0x6B, Value: 0x1
						Or 
						EqIdVal QuestionId: 0x60, Value: 0x0
						Not 
						Or 
						EqIdVal QuestionId: 0x64, Value: 0x0
						EqIdVal QuestionId: 0xCDF, Value: 0x1
						And 
						Or 
					End 
					OneOf Prompt: "Reset AUX Content", Help: "Reset TPM Aux content. Txt may not functional after AUX content gets reseted.", QuestionFlags: 0x10, QuestionId: 0x6E, VarStoreId: 0x1, VarOffset: 0x61F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "yes" Value: 1
						OneOfOption Option: "no" Value: 0, Default, MfgDefault
					End 
				End 
			End 
			OneOf Prompt: "Flash Wear Out Protection", Help: "Configure Flash Wear-Out Protection feature. Options are: DISABLE - Disable Flash Wear Out Protection Feature; ENABLE - Enable Flash Wear Out Protection Feature.", QuestionFlags: 0x10, QuestionId: 0x6F, VarStoreId: 0x1, VarOffset: 0x637, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCDE, Value: 0x0
				Text Prompt: "Current Debug Interface Status", Help: "Current Debug Interface Status", Text: "Disabled"
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCDE, Value: 0x0
				OneOf Prompt: "Debug Interface ", Help: "Enable/Disable Debug Interface Support", QuestionFlags: 0x10, QuestionId: 0x70, VarStoreId: 0x1, VarOffset: 0x634, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCDE, Value: 0x0
				OneOf Prompt: "Debug Interface Lock ", Help: "Enable/Disable Debug Interface Lock", QuestionFlags: 0x10, QuestionId: 0x71, VarStoreId: 0x1, VarOffset: 0x635, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCDD, Value: 0x0
				OneOf Prompt: "Processor trace memory allocation", Help: "Disable or Select Processor trace memory region Size: from 4KB to 2MB. Higher values of Processor Trace memory may not be supported. If unsupported, reduce Processor Trace memory size or disable cores/Hyper-threading.", QuestionFlags: 0x10, QuestionId: 0x72, VarStoreId: 0x1, VarOffset: 0x653, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
					OneOfOption Option: "Disabled" Value: 255, Default, MfgDefault
					OneOfOption Option: "4KB" Value: 0
					OneOfOption Option: "8KB" Value: 1
					OneOfOption Option: "16KB" Value: 2
					OneOfOption Option: "32KB" Value: 3
					OneOfOption Option: "64KB" Value: 4
					OneOfOption Option: "128KB" Value: 5
					OneOfOption Option: "256KB" Value: 6
					OneOfOption Option: "512KB" Value: 7
					OneOfOption Option: "1MB" Value: 8
					OneOfOption Option: "2MB" Value: 9
					OneOfOption Option: "4MB" Value: 10
					OneOfOption Option: "8MB" Value: 11
					OneOfOption Option: "16MB" Value: 12
					OneOfOption Option: "32MB" Value: 13
					OneOfOption Option: "64MB" Value: 14
					OneOfOption Option: "128MB" Value: 15
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCDD, Value: 0x0
					EqIdVal QuestionId: 0x72, Value: 0xFF
					Or 
				End 
				OneOf Prompt: "Processor trace", Help: "Enable/Disable processor trace feature from CPU MSR. Enabling this feature will immediately start trace collection.", QuestionFlags: 0x10, QuestionId: 0x73, VarStoreId: 0x1, VarOffset: 0x654, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				OneOf Prompt: "Processor Trace OutPut Scheme", Help: "Select Single Range Output scheme or ToPA table Output scheme", QuestionFlags: 0x10, QuestionId: 0x74, VarStoreId: 0x1, VarOffset: 0x652, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Single Range Output" Value: 0, Default, MfgDefault
					OneOfOption Option: "ToPA Output" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCDD, Value: 0x0
					EqIdVal QuestionId: 0x72, Value: 0xFF
					Or 
				End 
				OneOf Prompt: "SMM Processor Trace", Help: "Enable/Disable usage of Processor Trace in SMM", QuestionFlags: 0x10, QuestionId: 0x75, VarStoreId: 0x13, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCDC, Value: 0x0
				Ref Prompt: "CPU SMM Enhancement", Help: "CPU SMM Enhancement", QuestionFlags: 0x0, QuestionId: 0x76, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x272B
			End 
			OneOf Prompt: "FCLK Frequency for Early Power On", Help: "FCLK frequency can take values of 400MHz, 800MHz  and 1GHz (1GHz not supported for ULT/ULX SKUs)", QuestionFlags: 0x10, QuestionId: 0x77, VarStoreId: 0x1, VarOffset: 0x656, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [67, 81, 70, 68, 69, 80, 65, 66, 74]
							Uint64 Value: 0x0
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Normal (800Mhz)" Value: 0, Default, MfgDefault
				OneOfOption Option: "1GHz" Value: 1
				OneOfOption Option: "400MHz" Value: 2
			End 
			OneOf Prompt: "Three Strike Counter", Help: "Enable/Disable Three Strike Counter.", QuestionFlags: 0x10, QuestionId: 0x78, VarStoreId: 0x1, VarOffset: 0x73A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 1
				OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "Voltage Optimization", Help: "Auto: This Option will honor the Silicon default values; ENABLE - Mobile SKU's, DISABLE - Rest of all SKUs other than Mobile", QuestionFlags: 0x10, QuestionId: 0x79, VarStoreId: 0x1, VarOffset: 0x70D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
			End 
		End 
	End 
	SuppressIf 
		EqIdVal QuestionId: 0xCDC, Value: 0x0
		Form FormId: 0x272B, Title: "CPU SMM Enhancement"
			Subtitle Prompt: "CPU SMM Enhancement", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCDB, Value: 0x0
				OneOf Prompt: "SMM MSR Save State Enable", Help: "Enable/Disable support for MSR Save State", QuestionFlags: 0x10, QuestionId: 0x7A, VarStoreId: 0x13, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCDA, Value: 0x0
				OneOf Prompt: "SMM Code Access Check", Help: "Enable/Disable support for SMM Code Access feature", QuestionFlags: 0x10, QuestionId: 0x7B, VarStoreId: 0x13, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCD9, Value: 0x0
				OneOf Prompt: "SMM Use Delay Indication", Help: "Enable/Disable usage of SMM_DELAYED MSR for MP sync in SMI", QuestionFlags: 0x10, QuestionId: 0x7C, VarStoreId: 0x13, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "SMM Use Block Indication", Help: "Enable/Disable usage of SMM_BLOCKED MSR for MP sync in SMI", QuestionFlags: 0x10, QuestionId: 0x7D, VarStoreId: 0x13, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCD8, Value: 0x0
				OneOf Prompt: "SMM Use SMM en-US Indication", Help: "Enable/Disable usage of SMM_ENABLE MSR for MP sync in SMI", QuestionFlags: 0x10, QuestionId: 0x7E, VarStoreId: 0x13, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
		End 
	End 
	Form FormId: 0x272C, Title: "Power & Performance"
		Subtitle Prompt: "Power & Performance", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Ref Prompt: "CPU - Power Management Control", Help: "CPU - Power Management Control Options", QuestionFlags: 0x0, QuestionId: 0x7F, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x272D
		Ref Prompt: "GT - Power Management Control", Help: "GT - Power Management Control Options", QuestionFlags: 0x0, QuestionId: 0x80, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x274B
	End 
	Form FormId: 0x272D, Title: "CPU - Power Management Control"
		Subtitle Prompt: "CPU - Power Management Control", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Boot performance mode", Help: "Select the performance state that the BIOS will set starting from reset vector.", QuestionFlags: 0x10, QuestionId: 0x81, VarStoreId: 0x1, VarOffset: 0x554, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Max Non-Turbo Performance" Value: 1, Default, MfgDefault
			OneOfOption Option: "Max Battery" Value: 0
			OneOfOption Option: "Turbo Performance" Value: 2
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCD7, Value: 0x0
			OneOf Prompt: "Intel(R) SpeedStep(tm)", Help: "Allows more than two frequency ranges to be supported.", QuestionFlags: 0x10, QuestionId: 0x82, VarStoreId: 0x1, VarOffset: 0x551, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		OneOf Prompt: "Race To Halt (RTH)", Help: "Enable/Disable Race To Halt feature. RTH will dynamically increase CPU frequency in order to enter pkg C-State faster to reduce overall power. (RTH is controlled through MSR 1FC bit 20)", QuestionFlags: 0x10, QuestionId: 0x83, VarStoreId: 0x1, VarOffset: 0x552, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCD6, Value: 0x0
			OneOf Prompt: "Intel(R) Speed Shift Technology", Help: "Enable/Disable Intel(R) Speed Shift Technology support. Enabling will expose the CPPC v2 interface to allow for hardware controlled P-states.", QuestionFlags: 0x10, QuestionId: 0x84, VarStoreId: 0x1, VarOffset: 0x553, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
		End 
		OneOf Prompt: "HDC Control", Help: "This option allows HDC configuration.
 Disabled: Disable HDC
 Enabled:  Can be enabled by OS if OS native support is available. If native OS support is not available, BIOS will try to enable it using the OOB interface, if the interface is supported", QuestionFlags: 0x10, QuestionId: 0x85, VarStoreId: 0x1, VarOffset: 0x58B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
				EqIdVal QuestionId: 0xCD5, Value: 0x0
				Or 
			End 
			OneOf Prompt: "  Turbo Mode", Help: "Enable/Disable processor Turbo Mode (requires EMTTM enabled too). AUTO means enabled, unless max turbo ratio is bigger than 16 - SKL A0 W/A", QuestionFlags: 0x10, QuestionId: 0x86, VarStoreId: 0x1, VarOffset: 0x557, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
			Ref Prompt: "  View/Configure Turbo Options", Help: "View/Configure Turbo Options", QuestionFlags: 0x0, QuestionId: 0x87, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x272F
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCC1, Value: 0x0
			Ref Prompt: "  Config TDP Configurations", Help: "Config TDP Configurations", QuestionFlags: 0x0, QuestionId: 0x88, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2737
		End 
		Ref Prompt: "CPU VR Settings", Help: "CPU VR Settings", QuestionFlags: 0x0, QuestionId: 0x89, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2730
		OneOf Prompt: "Platform PL1 Enable", Help: "Enable/Disable Platform Power Limit 1 programming. If this option is enabled, it activates the PL1 value to be used by the processor to limit the average power of given time window.", QuestionFlags: 0x10, QuestionId: 0x8A, VarStoreId: 0x1, VarOffset: 0x572, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x8A, Value: 0x0
			Numeric Prompt: "Platform PL1 Power", Help: "Platform Power Limit 1 Power in Milli Watts. BIOS will round to the nearest 1/8W when programming. Any value can be programmed between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). For 12.50W, enter 12500. This setting will act as the new PL1 value for the Package RAPL algortihm.", QuestionFlags: 0x10, QuestionId: 0x8B, VarStoreId: 0x1, VarOffset: 0x573, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "Platform PL1 Time Window", Help: "Platform Power Limit 1 Time Window value in seconds. The value may vary from 0 to 128. 0 = default values. Indicates the time window over which Platform TDP value should be maintained.", QuestionFlags: 0x10, QuestionId: 0x8C, VarStoreId: 0x1, VarOffset: 0x577, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x0
				OneOfOption Option: "0" Value: 0, Default, MfgDefault
				OneOfOption Option: "1" Value: 1
				OneOfOption Option: "2" Value: 2
				OneOfOption Option: "3" Value: 3
				OneOfOption Option: "4" Value: 4
				OneOfOption Option: "5" Value: 5
				OneOfOption Option: "6" Value: 6
				OneOfOption Option: "7" Value: 7
				OneOfOption Option: "8" Value: 8
				OneOfOption Option: "10" Value: 10
				OneOfOption Option: "12" Value: 12
				OneOfOption Option: "14" Value: 14
				OneOfOption Option: "16" Value: 16
				OneOfOption Option: "20" Value: 20
				OneOfOption Option: "24" Value: 24
				OneOfOption Option: "28" Value: 28
				OneOfOption Option: "32" Value: 32
				OneOfOption Option: "40" Value: 40
				OneOfOption Option: "48" Value: 48
				OneOfOption Option: "56" Value: 56
				OneOfOption Option: "64" Value: 64
				OneOfOption Option: "80" Value: 80
				OneOfOption Option: "96" Value: 96
				OneOfOption Option: "112" Value: 112
				OneOfOption Option: "128" Value: 128
			End 
		End 
		OneOf Prompt: "Platform PL2 Enable", Help: "Enable/Disable Platform Power Limit 2 programming. If this option is disabled, BIOS will program the default values for Platform Power Limit 2.", QuestionFlags: 0x10, QuestionId: 0x8D, VarStoreId: 0x1, VarOffset: 0x578, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x8D, Value: 0x0
			Numeric Prompt: "Platform PL2 Power", Help: "Platform Power Limit 2 Power in Milli Watts. BIOS will round to the nearest 1/8W when programming. Any value can be programmed between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). For 12.50W, enter 12500. This setting will act as the new PL2 value for the Package RAPL algortihm.", QuestionFlags: 0x10, QuestionId: 0x8E, VarStoreId: 0x1, VarOffset: 0x579, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		OneOf Prompt: "Power Limit 4 Override", Help: "Enable/Disable Power Limit 4 override. If this option is disabled, BIOS will leave the default values for Power Limit 4.", QuestionFlags: 0x10, QuestionId: 0x8F, VarStoreId: 0x1, VarOffset: 0x56B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x8F, Value: 0x0
			Numeric Prompt: "Power Limit 4", Help: "Power Limit 4 in Milli Watts. BIOS will round to the nearest 1/8W when programming. For 12.50W, enter 12500. If the value is 0, BIOS leaves default value", QuestionFlags: 0x10, QuestionId: 0x90, VarStoreId: 0x1, VarOffset: 0x56C, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x8F, Value: 0x0
			OneOf Prompt: "Power Limit 4 Lock", Help: "Power Limit 4 MSR 601h Lock. When enabled PL4 configurations are locked during OS. When disabled PL4 configuration can be changed during OS.", QuestionFlags: 0x10, QuestionId: 0x91, VarStoreId: 0x1, VarOffset: 0x570, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCD3, Value: 0x0
			OneOf Prompt: "C states", Help: "Enable/Disable CPU Power Management. Allows CPU to go to C states when it's not 100% utilized.", QuestionFlags: 0x10, QuestionId: 0x92, VarStoreId: 0x1, VarOffset: 0x555, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCD3, Value: 0x0
				EqIdVal QuestionId: 0x92, Value: 0x0
				Or 
				EqIdVal QuestionId: 0xCD4, Value: 0x0
				Or 
			End 
			OneOf Prompt: "  Enhanced C-states", Help: "Enable/Disable C1E. When enabled, CPU will switch to minimum speed when all cores enter C-State.", QuestionFlags: 0x10, QuestionId: 0x93, VarStoreId: 0x1, VarOffset: 0x556, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCD3, Value: 0x0
				EqIdVal QuestionId: 0x92, Value: 0x0
				Or 
			End 
			OneOf Prompt: "  C-State Auto Demotion", Help: "Configure C-State Auto Demotion", QuestionFlags: 0x10, QuestionId: 0x94, VarStoreId: 0x1, VarOffset: 0x57F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "C1" Value: 1
				OneOfOption Option: "C3" Value: 2
				OneOfOption Option: "C1 and C3" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "  C-State Un-demotion", Help: "Configure C-State Un-demotion", QuestionFlags: 0x10, QuestionId: 0x95, VarStoreId: 0x1, VarOffset: 0x580, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "C1" Value: 1
				OneOfOption Option: "C3" Value: 2
				OneOfOption Option: "C1 and C3" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "  Package C-State Demotion", Help: "Enable or Disable Package C-State Demotion. 0: Disable; 1: Enable; <b>2: Auto</b> (Auto: Enabled for Skylake; Disabled for Kabylake)", QuestionFlags: 0x10, QuestionId: 0x96, VarStoreId: 0x1, VarOffset: 0x581, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
			End 
			OneOf Prompt: "  Package C-State Un-demotion", Help: "Enable or Disable Package C-State UnDemotion. 0: Disable; 1: Enable; <b>2: Auto</b> (Auto: Enabled for Skylake; Disabled for Kabylake)", QuestionFlags: 0x10, QuestionId: 0x97, VarStoreId: 0x1, VarOffset: 0x582, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
			End 
			OneOf Prompt: "CState Pre-Wake", Help: "Disable - Sets bit 30 of POWER_CTL MSR(0x1FC) to 1 to disable the Cstate Pre-Wake", QuestionFlags: 0x10, QuestionId: 0x98, VarStoreId: 0x1, VarOffset: 0x57E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "IO MWAIT Redirection", Help: "When set, will map IO_read instructions sent to IO registers PMG_IO_BASE_ADDRBASE+offset to MWAIT(offset)", QuestionFlags: 0x10, QuestionId: 0x99, VarStoreId: 0x1, VarOffset: 0x589, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Package C State Limit", Help: "Maximum Package C State Limit Setting. Cpu Default: Leaves to Factory default value.Auto: Initializes to deepest available Package C State Limit.", QuestionFlags: 0x10, QuestionId: 0x9A, VarStoreId: 0x1, VarOffset: 0x58C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
				OneOfOption Option: "Auto" Value: 255, Default, MfgDefault
				OneOfOption Option: "Cpu Default" Value: 254
				OneOfOption Option: "C10" Value: 8
				OneOfOption Option: "C9" Value: 7
				OneOfOption Option: "C8" Value: 6
				OneOfOption Option: "C7S" Value: 5
				OneOfOption Option: "C7" Value: 4
				OneOfOption Option: "C6" Value: 3
				OneOfOption Option: "C3" Value: 2
				OneOfOption Option: "C2" Value: 1
				OneOfOption Option: "C0/C1" Value: 0
			End 
			Subtitle Prompt: "C3 Latency Control(MSR 0x60A)", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "Time Unit", Help: "Unit of measurement for IRTL value - bits [12:10]", QuestionFlags: 0x10, QuestionId: 0x9B, VarStoreId: 0x1, VarOffset: 0x58D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "1 ns" Value: 0
				OneOfOption Option: "32 ns" Value: 1
				OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
				OneOfOption Option: "32768 ns" Value: 3
				OneOfOption Option: "1048576 ns" Value: 4
				OneOfOption Option: "33554432 ns" Value: 5
			End 
			Numeric Prompt: "Latency", Help: "Interrupt Response Time Limit value- bits [9:0], Enter 0-1023", QuestionFlags: 0x10, QuestionId: 0x9C, VarStoreId: 0x1, VarOffset: 0x593, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
				Default DefaultId: 0x0 Value: 78
			End 
			Subtitle Prompt: "C6/C7 Short Latency Control(MSR 0x60B)", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "Time Unit", Help: "Unit of measurement for IRTL value - bits [12:10]", QuestionFlags: 0x10, QuestionId: 0x9D, VarStoreId: 0x1, VarOffset: 0x58E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "1 ns" Value: 0
				OneOfOption Option: "32 ns" Value: 1
				OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
				OneOfOption Option: "32768 ns" Value: 3
				OneOfOption Option: "1048576 ns" Value: 4
				OneOfOption Option: "33554432 ns" Value: 5
			End 
			Numeric Prompt: "Latency", Help: "Interrupt Response Time Limit value- bits [9:0], Enter 0-1023", QuestionFlags: 0x10, QuestionId: 0x9E, VarStoreId: 0x1, VarOffset: 0x595, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
				Default DefaultId: 0x0 Value: 118
			End 
			Subtitle Prompt: "C6/C7 Long Latency Control(MSR 0x60C)", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "Time Unit", Help: "Unit of measurement for IRTL value - bits [12:10]", QuestionFlags: 0x10, QuestionId: 0x9F, VarStoreId: 0x1, VarOffset: 0x58F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "1 ns" Value: 0
				OneOfOption Option: "32 ns" Value: 1
				OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
				OneOfOption Option: "32768 ns" Value: 3
				OneOfOption Option: "1048576 ns" Value: 4
				OneOfOption Option: "33554432 ns" Value: 5
			End 
			Numeric Prompt: "Latency", Help: "Interrupt Response Time Limit value- bits [9:0], Enter 0-1023", QuestionFlags: 0x10, QuestionId: 0xA0, VarStoreId: 0x1, VarOffset: 0x597, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
				Default DefaultId: 0x0 Value: 148
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC51, Value: 0x2
					Not 
				End 
				Subtitle Prompt: "C8 Latency Control(MSR 0x633)", Help: "", Flags: 0x0
				End 
				OneOf Prompt: "Time Unit", Help: "Unit of measurement for IRTL value - bits [12:10]", QuestionFlags: 0x10, QuestionId: 0xA1, VarStoreId: 0x1, VarOffset: 0x590, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
					OneOfOption Option: "1 ns" Value: 0
					OneOfOption Option: "32 ns" Value: 1
					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
					OneOfOption Option: "32768 ns" Value: 3
					OneOfOption Option: "1048576 ns" Value: 4
					OneOfOption Option: "33554432 ns" Value: 5
				End 
				Numeric Prompt: "Latency", Help: "Interrupt Response Time Limit value- bits [9:0], Enter 0-1023", QuestionFlags: 0x10, QuestionId: 0xA2, VarStoreId: 0x1, VarOffset: 0x599, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
					Default DefaultId: 0x0 Value: 250
				End 
				Subtitle Prompt: "C9 Latency Control(MSR 0x634)", Help: "", Flags: 0x0
				End 
				OneOf Prompt: "Time Unit", Help: "Unit of measurement for IRTL value - bits [12:10]", QuestionFlags: 0x10, QuestionId: 0xA3, VarStoreId: 0x1, VarOffset: 0x591, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
					OneOfOption Option: "1 ns" Value: 0
					OneOfOption Option: "32 ns" Value: 1
					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
					OneOfOption Option: "32768 ns" Value: 3
					OneOfOption Option: "1048576 ns" Value: 4
					OneOfOption Option: "33554432 ns" Value: 5
				End 
				Numeric Prompt: "Latency", Help: "Interrupt Response Time Limit value- bits [9:0], Enter 0-1023", QuestionFlags: 0x10, QuestionId: 0xA4, VarStoreId: 0x1, VarOffset: 0x59B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
					Default DefaultId: 0x0 Value: 332
				End 
				Subtitle Prompt: "C10 Latency Control(MSR 0x635)", Help: "", Flags: 0x0
				End 
				OneOf Prompt: "Time Unit", Help: "Unit of measurement for IRTL value - bits [12:10]", QuestionFlags: 0x10, QuestionId: 0xA5, VarStoreId: 0x1, VarOffset: 0x592, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
					OneOfOption Option: "1 ns" Value: 0
					OneOfOption Option: "32 ns" Value: 1
					OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
					OneOfOption Option: "32768 ns" Value: 3
					OneOfOption Option: "1048576 ns" Value: 4
					OneOfOption Option: "33554432 ns" Value: 5
				End 
				Numeric Prompt: "Latency", Help: "Interrupt Response Time Limit value- bits [9:0], Enter 0-1023", QuestionFlags: 0x10, QuestionId: 0xA6, VarStoreId: 0x1, VarOffset: 0x59D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
					Default DefaultId: 0x0 Value: 1010
				End 
			End 
		End 
		OneOf Prompt: "Thermal Monitor ", Help: "Enable/Disable Thermal Monitor", QuestionFlags: 0x10, QuestionId: 0xA7, VarStoreId: 0x1, VarOffset: 0x583, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Interrupt Redirection Mode Selection", Help: "Interrupt Redirection Mode Select for Logical Interrupts ", QuestionFlags: 0x10, QuestionId: 0xA8, VarStoreId: 0x1, VarOffset: 0x58A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
			OneOfOption Option: "Fixed Priority" Value: 0
			OneOfOption Option: "Round robin" Value: 1
			OneOfOption Option: "Hash Vector" Value: 2
			OneOfOption Option: "PAIR with Fixed Priority" Value: 4, Default, MfgDefault
			OneOfOption Option: "PAIR with Round Robin" Value: 5
			OneOfOption Option: "PAIR with Hash Vector" Value: 6
			OneOfOption Option: "No Change" Value: 7
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCD2, Value: 0x0
			OneOf Prompt: "Timed MWAIT ", Help: "Enable/Disable Timed MWAIT Support", QuestionFlags: 0x10, QuestionId: 0xA9, VarStoreId: 0x1, VarOffset: 0x588, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		Ref Prompt: "Custom P-state Table", Help: "Add Custom P-state Table", QuestionFlags: 0x0, QuestionId: 0xAA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x272E
		SuppressIf 
			EqIdVal QuestionId: 0xC8C, Value: 0x1
				Not 
				EqIdVal QuestionId: 0xC8C, Value: 0x5
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0x20
				Or 
				EqIdVal QuestionId: 0x86, Value: 0x0
				Or 
			End 
			OneOf Prompt: "EC Turbo Control Mode", Help: "Enable/Disable EC Turbo Control mode", QuestionFlags: 0x10, QuestionId: 0xAB, VarStoreId: 0x1, VarOffset: 0x623, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xAB, Value: 0x0
			OneOf Prompt: "  AC Brick Capacity", Help: "Specify the AC Brick capacity", QuestionFlags: 0x10, QuestionId: 0xAC, VarStoreId: 0x1, VarOffset: 0x624, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3, Step: 0x0
				OneOfOption Option: "90W AC Brick" Value: 1, Default, MfgDefault
				OneOfOption Option: "65W AC Brick" Value: 2
				OneOfOption Option: "75W AC Brick" Value: 3
			End 
			Numeric Prompt: "  EC Polling Period", Help: "Count 1 to 255 for a range of 10ms to 2.55 seconds (1 count = 10ms)", QuestionFlags: 0x10, QuestionId: 0xAD, VarStoreId: 0x1, VarOffset: 0x625, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 1
			End 
			Numeric Prompt: "  EC Guard Band Value", Help: "Count 1 to 20 for a range of 1 watt to 20 watts", QuestionFlags: 0x10, QuestionId: 0xAE, VarStoreId: 0x1, VarOffset: 0x626, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "  EC Algorithm Selection", Help: "Count 1 to 10 for Algorithm Selection", QuestionFlags: 0x10, QuestionId: 0xAF, VarStoreId: 0x1, VarOffset: 0x627, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 1
			End 
		End 
		OneOf Prompt: "Energy Performance Gain", Help: "Enable/disable Energy Performance Gain.", QuestionFlags: 0x10, QuestionId: 0xB0, VarStoreId: 0x1, VarOffset: 0x871, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xB0, Value: 0x0
			Numeric Prompt: "EPG DIMM Idd3N", Help: "Active standby current (Idd3N) in milliamps from datasheet. Must be calculated on a per DIMM basis.", QuestionFlags: 0x10, QuestionId: 0xB1, VarStoreId: 0x1, VarOffset: 0x872, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1
				Default DefaultId: 0x0 Value: 26
			End 
			Numeric Prompt: "EPG DIMM Idd3P", Help: "Active power-down current (Idd3P) in milliamps from datasheet. Must be calculated on a per DIMM basis.", QuestionFlags: 0x10, QuestionId: 0xB2, VarStoreId: 0x1, VarOffset: 0x874, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1
				Default DefaultId: 0x0 Value: 11
			End 
		End 
		Ref Prompt: "Power Limit 3 Settings", Help: "Power Limit 3 Settings", QuestionFlags: 0x0, QuestionId: 0xB3, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2736
		Ref Prompt: "CPU Lock Configuration", Help: "CPU Lock Configuration", QuestionFlags: 0x0, QuestionId: 0xB4, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2738
	End 
	Form FormId: 0x272E, Title: "Custom P-state Table"
		Subtitle Prompt: "Custom P-state Table", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "Number of P states", Help: "Sets the number of custom P-states. At least 2 states must be present.", QuestionFlags: 0x10, QuestionId: 0xB5, VarStoreId: 0x1, VarOffset: 0x5C4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x28, Step: 0x0
			Default DefaultId: 0x0 Value: 0
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x2
				LessThan 
			End 
			Numeric Prompt: "Max P-State Ratio", Help: "Maximum P-state ratio to use in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xB6, VarStoreId: 0x1, VarOffset: 0x5C5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xB7, VarStoreId: 0x1, VarOffset: 0x5C7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x3
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xB8, VarStoreId: 0x1, VarOffset: 0x5C9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x4
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xB9, VarStoreId: 0x1, VarOffset: 0x5CB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x5
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xBA, VarStoreId: 0x1, VarOffset: 0x5CD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x6
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xBB, VarStoreId: 0x1, VarOffset: 0x5CF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x7
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xBC, VarStoreId: 0x1, VarOffset: 0x5D1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x8
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xBD, VarStoreId: 0x1, VarOffset: 0x5D3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x9
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xBE, VarStoreId: 0x1, VarOffset: 0x5D5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0xA
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xBF, VarStoreId: 0x1, VarOffset: 0x5D7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0xB
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xC0, VarStoreId: 0x1, VarOffset: 0x5D9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0xC
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xC1, VarStoreId: 0x1, VarOffset: 0x5DB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0xD
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xC2, VarStoreId: 0x1, VarOffset: 0x5DD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0xE
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xC3, VarStoreId: 0x1, VarOffset: 0x5DF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0xF
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xC4, VarStoreId: 0x1, VarOffset: 0x5E1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x10
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xC5, VarStoreId: 0x1, VarOffset: 0x5E3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x11
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xC6, VarStoreId: 0x1, VarOffset: 0x5E5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x12
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xC7, VarStoreId: 0x1, VarOffset: 0x5E7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x13
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xC8, VarStoreId: 0x1, VarOffset: 0x5E9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x14
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xC9, VarStoreId: 0x1, VarOffset: 0x5EB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x15
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xCA, VarStoreId: 0x1, VarOffset: 0x5ED, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x16
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xCB, VarStoreId: 0x1, VarOffset: 0x5EF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x17
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xCC, VarStoreId: 0x1, VarOffset: 0x5F1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x18
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xCD, VarStoreId: 0x1, VarOffset: 0x5F3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x19
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xCE, VarStoreId: 0x1, VarOffset: 0x5F5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x1A
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xCF, VarStoreId: 0x1, VarOffset: 0x5F7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x1B
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xD0, VarStoreId: 0x1, VarOffset: 0x5F9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x1C
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xD1, VarStoreId: 0x1, VarOffset: 0x5FB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x1D
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xD2, VarStoreId: 0x1, VarOffset: 0x5FD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x1E
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xD3, VarStoreId: 0x1, VarOffset: 0x5FF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x1F
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xD4, VarStoreId: 0x1, VarOffset: 0x601, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x20
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xD5, VarStoreId: 0x1, VarOffset: 0x603, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x21
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xD6, VarStoreId: 0x1, VarOffset: 0x605, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x22
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xD7, VarStoreId: 0x1, VarOffset: 0x607, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x23
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xD8, VarStoreId: 0x1, VarOffset: 0x609, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x24
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xD9, VarStoreId: 0x1, VarOffset: 0x60B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x25
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xDA, VarStoreId: 0x1, VarOffset: 0x60D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x26
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xDB, VarStoreId: 0x1, VarOffset: 0x60F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x27
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xDC, VarStoreId: 0x1, VarOffset: 0x611, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xB5
				Uint8 Value: 0x28
				LessThan 
			End 
			Numeric Prompt: "P-State Ratio", Help: "P-state ratio for the given state in the custom P-state table.", QuestionFlags: 0x10, QuestionId: 0xDD, VarStoreId: 0x1, VarOffset: 0x613, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
	End 
	Form FormId: 0x272F, Title: "  View/Configure Turbo Options"
		Subtitle Prompt: "Current Turbo Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "Max Turbo Power Limit", Help: "Max Turbo Power Limit", Text: ""
		Text Prompt: "Min Turbo Power Limit", Help: "Min Turbo Power Limit", Text: ""
		Text Prompt: "Package TDP Limit", Help: "Package TDP Limit", Text: ""
		Text Prompt: "Power Limit 1", Help: "Power Limit 1 in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and TDP Limit. If value is 0, BIOS will program TDP value.", Text: ""
		Text Prompt: "Power Limit 2", Help: "Power Limit 2 value in Milli Watts. BIOS will round to the nearest 1/8W when programming. If the value is 0, BIOS will program this value as 1.25*TDP. For 12.50W, enter 12500. Processor applies control policies such that the package power does not exceed this limit.", Text: ""
		Text Prompt: "1-core Turbo Ratio", Help: "1-core Turbo Ratio", Text: ""
		SuppressIf 
			QuestionRef1 QuestionId: 0xCD0
				Uint8 Value: 0x2
				LessThan 
				QuestionRef1 QuestionId: 0x60
				Uint8 Value: 0x2
				LessThan 
				EqIdVal QuestionId: 0x60, Value: 0x0
				Not 
				And 
				Or 
			End 
			Text Prompt: "2-core Turbo Ratio", Help: "2-core Turbo Ratio", Text: ""
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xCD0
				Uint8 Value: 0x3
				LessThan 
				QuestionRef1 QuestionId: 0x60
				Uint8 Value: 0x3
				LessThan 
				EqIdVal QuestionId: 0x60, Value: 0x0
				Not 
				And 
				Or 
			End 
			Text Prompt: "3-core Turbo Ratio", Help: "3-core Turbo Ratio", Text: ""
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xCD0
				Uint8 Value: 0x4
				LessThan 
				QuestionRef1 QuestionId: 0x60
				Uint8 Value: 0x4
				LessThan 
				EqIdVal QuestionId: 0x60, Value: 0x0
				Not 
				And 
				Or 
			End 
			Text Prompt: "4-core Turbo Ratio", Help: "4-core Turbo Ratio", Text: ""
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xCD0
				Uint8 Value: 0x5
				LessThan 
				QuestionRef1 QuestionId: 0x60
				Uint8 Value: 0x5
				LessThan 
				EqIdVal QuestionId: 0x60, Value: 0x0
				Not 
				And 
				Or 
			End 
			Text Prompt: "5-core Turbo Ratio", Help: "5-core Turbo Ratio", Text: ""
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xCD0
				Uint8 Value: 0x6
				LessThan 
				QuestionRef1 QuestionId: 0x60
				Uint8 Value: 0x6
				LessThan 
				EqIdVal QuestionId: 0x60, Value: 0x0
				Not 
				And 
				Or 
			End 
			Text Prompt: "6-core Turbo Ratio", Help: "6-core Turbo Ratio", Text: ""
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xCD0
				Uint8 Value: 0x7
				LessThan 
				QuestionRef1 QuestionId: 0x60
				Uint8 Value: 0x7
				LessThan 
				EqIdVal QuestionId: 0x60, Value: 0x0
				Not 
				And 
				Or 
			End 
			Text Prompt: "7-core Turbo Ratio", Help: "7-core Turbo Ratio", Text: ""
		End 
		SuppressIf 
			QuestionRef1 QuestionId: 0xCD0
				Uint8 Value: 0x8
				LessThan 
				QuestionRef1 QuestionId: 0x60
				Uint8 Value: 0x8
				LessThan 
				EqIdVal QuestionId: 0x60, Value: 0x0
				Not 
				And 
				Or 
			End 
			Text Prompt: "8-core Turbo Ratio", Help: "8-core Turbo Ratio", Text: ""
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
				EqIdVal QuestionId: 0xC8C, Value: 0x4
				Or 
			End 
			OneOf Prompt: "Energy Efficient P-state", Help: "Enable/Disable Energy Efficient P-state feature. When set to 0, will disable access to ENERGY_PERFORMANCE_BIAS MSR and CPUID Function 6 ECX[3] will read 0 indicating no support for Energy Efficient policy setting. When set to 1 will enable access to ENERGY_PERFORMANCE_BIAS MSR 1B0h and CPUID Function 6 ECX[3] will read 1 indicating Energy Efficient policy setting is supported.", QuestionFlags: 0x10, QuestionId: 0xDE, VarStoreId: 0x1, VarOffset: 0x57D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
			OneOf Prompt: "Package Power Limit MSR Lock", Help: "Enable/Disable locking of Package Power Limit settings. When enabled, PACKAGE_POWER_LIMIT MSR will be locked and a reset will be required to unlock the register.", QuestionFlags: 0x10, QuestionId: 0xDF, VarStoreId: 0x1, VarOffset: 0x571, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
				EqIdVal QuestionId: 0xCC1, Value: 0x1
				Or 
			End 
			OneOf Prompt: "Power Limit 1 Override", Help: "Enable/Disable Power Limit 1 override. If this option is disabled, BIOS will program the default values for Power Limit 1 and Power Limit 1 Time Window.", QuestionFlags: 0x10, QuestionId: 0xE0, VarStoreId: 0x1, VarOffset: 0x55C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
				EqIdVal QuestionId: 0xCC1, Value: 0x1
				Or 
				EqIdVal QuestionId: 0xE0, Value: 0x0
				Or 
			End 
			Numeric Prompt: "Power Limit 1", Help: "Power Limit 1 in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and TDP Limit. If value is 0, BIOS will program TDP value.", QuestionFlags: 0x10, QuestionId: 0xE1, VarStoreId: 0x1, VarOffset: 0x558, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
				EqIdVal QuestionId: 0xCC1, Value: 0x1
				Or 
				EqIdVal QuestionId: 0xE0, Value: 0x0
				Or 
			End 
			OneOf Prompt: "Power Limit 1 Time Window", Help: "Power Limit 1 Time Window value in seconds. The value may vary from 0 to 128. 0 = default value (28 sec for Mobile and 8 sec for Desktop). Defines time window which TDP value should be maintained.", QuestionFlags: 0x10, QuestionId: 0xE2, VarStoreId: 0x1, VarOffset: 0x55D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x0
				OneOfOption Option: "0" Value: 0, Default, MfgDefault
				OneOfOption Option: "1" Value: 1
				OneOfOption Option: "2" Value: 2
				OneOfOption Option: "3" Value: 3
				OneOfOption Option: "4" Value: 4
				OneOfOption Option: "5" Value: 5
				OneOfOption Option: "6" Value: 6
				OneOfOption Option: "7" Value: 7
				OneOfOption Option: "8" Value: 8
				OneOfOption Option: "10" Value: 10
				OneOfOption Option: "12" Value: 12
				OneOfOption Option: "14" Value: 14
				OneOfOption Option: "16" Value: 16
				OneOfOption Option: "20" Value: 20
				OneOfOption Option: "24" Value: 24
				OneOfOption Option: "28" Value: 28
				OneOfOption Option: "32" Value: 32
				OneOfOption Option: "40" Value: 40
				OneOfOption Option: "48" Value: 48
				OneOfOption Option: "56" Value: 56
				OneOfOption Option: "64" Value: 64
				OneOfOption Option: "80" Value: 80
				OneOfOption Option: "96" Value: 96
				OneOfOption Option: "112" Value: 112
				OneOfOption Option: "128" Value: 128
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
				EqIdVal QuestionId: 0xCC1, Value: 0x1
				Or 
			End 
			OneOf Prompt: "Power Limit 2 Override", Help: "Enable/Disable Power Limit 2 override. If this option is disabled, BIOS will program the default values for Power Limit 2.", QuestionFlags: 0x10, QuestionId: 0xE3, VarStoreId: 0x1, VarOffset: 0x55E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
				EqIdVal QuestionId: 0xCC1, Value: 0x1
				Or 
				EqIdVal QuestionId: 0xE3, Value: 0x0
				Or 
			End 
			Numeric Prompt: "Power Limit 2", Help: "Power Limit 2 value in Milli Watts. BIOS will round to the nearest 1/8W when programming. If the value is 0, BIOS will program this value as 1.25*TDP. For 12.50W, enter 12500. Processor applies control policies such that the package power does not exceed this limit.", QuestionFlags: 0x10, QuestionId: 0xE4, VarStoreId: 0x1, VarOffset: 0x55F, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCD1, Value: 0x0
				EqIdVal QuestionId: 0x82, Value: 0x0
				Or 
				EqIdVal QuestionId: 0x86, Value: 0x0
				Or 
			End 
			Numeric Prompt: "1-Core Ratio Limit Override", Help: "1-Core Ratio Limit with range of (Max Non-Turbo Ratio - 255). Min = Max Non-Turbo Ratio. Max = fused turbo ratio, or 255 if CPU is unlocked for overclocking. This 1-Core Ratio Limit must be greater than or equal all other ratio values.", QuestionFlags: 0x14, QuestionId: 0x271E, VarStoreId: 0x1, VarOffset: 0x62E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				QuestionRef1 QuestionId: 0xCD0
					Uint8 Value: 0x2
					LessThan 
					QuestionRef1 QuestionId: 0x60
					Uint8 Value: 0x2
					LessThan 
					EqIdVal QuestionId: 0x60, Value: 0x0
					Not 
					And 
					Or 
				End 
				Numeric Prompt: "2-Core Ratio Limit Override", Help: "2-Core Ratio Limit with range of (Max Non-Turbo Ratio - 255). Min = Max Non-Turbo Ratio. Max = fused turbo ratio, or 255 if CPU is unlocked for overclocking. This 2-Core Ratio Limit Must be <= to 1-Core Ratio Limit.", QuestionFlags: 0x14, QuestionId: 0x271F, VarStoreId: 0x1, VarOffset: 0x62F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				QuestionRef1 QuestionId: 0xCD0
					Uint8 Value: 0x3
					LessThan 
					QuestionRef1 QuestionId: 0x60
					Uint8 Value: 0x3
					LessThan 
					EqIdVal QuestionId: 0x60, Value: 0x0
					Not 
					And 
					Or 
				End 
				Numeric Prompt: "3-Core Ratio Limit Override", Help: "3-Core Ratio Limit with range of (Max Non-Turbo Ratio - 255). Min = Max Non-Turbo Ratio. Max = fused turbo ratio, or 255 if CPU is unlocked for overclocking. This 3-Core Ratio Limit Must be <= to 1-Core Ratio Limit.", QuestionFlags: 0x14, QuestionId: 0x2720, VarStoreId: 0x1, VarOffset: 0x630, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				QuestionRef1 QuestionId: 0xCD0
					Uint8 Value: 0x4
					LessThan 
					QuestionRef1 QuestionId: 0x60
					Uint8 Value: 0x4
					LessThan 
					EqIdVal QuestionId: 0x60, Value: 0x0
					Not 
					And 
					Or 
				End 
				Numeric Prompt: "4-Core Ratio Limit Override", Help: "4-Core Ratio Limit with range of (Max Non-Turbo Ratio - 255). Min = Max Non-Turbo Ratio. Max = fused turbo ratio, or 255 if CPU is unlocked for overclocking. This 4-Core Ratio Limit Must be <= to 1-Core Ratio Limit.", QuestionFlags: 0x14, QuestionId: 0x2721, VarStoreId: 0x1, VarOffset: 0x631, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				QuestionRef1 QuestionId: 0xCD0
					Uint8 Value: 0x5
					LessThan 
					QuestionRef1 QuestionId: 0x60
					Uint8 Value: 0x5
					LessThan 
					EqIdVal QuestionId: 0x60, Value: 0x0
					Not 
					And 
					Or 
				End 
				Numeric Prompt: "5-Core Ratio Limit Override", Help: "5-Core Ratio Limit with range of (Max Non-Turbo Ratio - 255). Min = Max Non-Turbo Ratio. Max = fused turbo ratio, or 255 if CPU is unlocked for overclocking. This 5-Core Ratio Limit Must be <= to 1-Core Ratio Limit.", QuestionFlags: 0x14, QuestionId: 0x2722, VarStoreId: 0x1, VarOffset: 0x736, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				QuestionRef1 QuestionId: 0xCD0
					Uint8 Value: 0x6
					LessThan 
					QuestionRef1 QuestionId: 0x60
					Uint8 Value: 0x6
					LessThan 
					EqIdVal QuestionId: 0x60, Value: 0x0
					Not 
					And 
					Or 
				End 
				Numeric Prompt: "6-Core Ratio Limit Override", Help: "6-Core Ratio Limit with range of (Max Non-Turbo Ratio - 255). Min = Max Non-Turbo Ratio. Max = fused turbo ratio, or 255 if CPU is unlocked for overclocking. This 6-Core Ratio Limit Must be <= to 1-Core Ratio Limit.", QuestionFlags: 0x14, QuestionId: 0x2723, VarStoreId: 0x1, VarOffset: 0x737, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				QuestionRef1 QuestionId: 0xCD0
					Uint8 Value: 0x7
					LessThan 
					QuestionRef1 QuestionId: 0x60
					Uint8 Value: 0x7
					LessThan 
					EqIdVal QuestionId: 0x60, Value: 0x0
					Not 
					And 
					Or 
				End 
				Numeric Prompt: "7-Core Ratio Limit Override", Help: "7-Core Ratio Limit with range of (Max Non-Turbo Ratio - 255). Min = Max Non-Turbo Ratio. Max = fused turbo ratio, or 255 if CPU is unlocked for overclocking. This 7-Core Ratio Limit Must be <= to 1-Core Ratio Limit.", QuestionFlags: 0x14, QuestionId: 0x2724, VarStoreId: 0x1, VarOffset: 0x738, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				QuestionRef1 QuestionId: 0xCD0
					Uint8 Value: 0x8
					LessThan 
					QuestionRef1 QuestionId: 0x60
					Uint8 Value: 0x8
					LessThan 
					EqIdVal QuestionId: 0x60, Value: 0x0
					Not 
					And 
					Or 
				End 
				Numeric Prompt: "8-Core Ratio Limit Override", Help: "8-Core Ratio Limit with range of (Max Non-Turbo Ratio - 255). Min = Max Non-Turbo Ratio. Max = fused turbo ratio, or 255 if CPU is unlocked for overclocking. This 8-Core Ratio Limit Must be <= to 1-Core Ratio Limit.", QuestionFlags: 0x14, QuestionId: 0x2725, VarStoreId: 0x1, VarOffset: 0x739, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
		End 
		OneOf Prompt: "Energy Efficient Turbo", Help: "Enable/Disable Energy Efficient Turbo Feature. This feature will opportunistically lower the turbo frequency to increase efficiency. Recommended only to disable in overclocking situations where turbo frequency must remain constant. Otherwise, leave enabled.", QuestionFlags: 0x10, QuestionId: 0xE5, VarStoreId: 0x1, VarOffset: 0x6EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1
			OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
		End 
	End 
	Form FormId: 0x2730, Title: "CPU VR Settings"
		Subtitle Prompt: "CPU VR Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "VR Power Delivery Design", Help: "Specifies the CFL-S board design used for the VR settings override values. By default, BIOS will override the default CFL-S VR settings based on the board design. A value of AUTO(0) will use the board ID to determine the board design. Any other value will override the board id logic to provide a custom VR Power Delivery Design value. This is intended primarily for validation.", QuestionFlags: 0x14, QuestionId: 0x2726, VarStoreId: 0x1, VarOffset: 0x72F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x10, Step: 0x0
			Default DefaultId: 0x1 Value: 0
			OneOfOption Option: "AUTO" Value: 0, Default, MfgDefault
			OneOfOption Option: "CFL_S_35_WATT_2_2" Value: 1
			OneOfOption Option: "CFL_S_54_WATT_2_2" Value: 2
			OneOfOption Option: "CFL_S_58_WATT_2_2" Value: 3
			OneOfOption Option: "CFL_S_35_WATT_4_2" Value: 4
			OneOfOption Option: "CFL_S_62_WATT_4_2" Value: 5
			OneOfOption Option: "CFL_S_65_WATT_4_2" Value: 6
			OneOfOption Option: "CFL_S_95_WATT_4_2" Value: 7
			OneOfOption Option: "CFL_S_35_WATT_6_2" Value: 8
			OneOfOption Option: "CFL_S_65_WATT_6_2" Value: 9
			OneOfOption Option: "CFL_S_95_WATT_6_2" Value: 10
			OneOfOption Option: "CFL_S_35_WATT_8_2" Value: 11
			OneOfOption Option: "CFL_S_65_WATT_8_2" Value: 12
			OneOfOption Option: "CFL_S_95_WATT_8_2" Value: 13
			OneOfOption Option: "CFL_S_71_WATT_4_2" Value: 14
			OneOfOption Option: "CFL_S_80_WATT_6_2" Value: 15
			OneOfOption Option: "CFL_S_80_WATT_8_2" Value: 16
		End 
		Numeric Prompt: "PSYS Slope", Help: "PSYS Slope defined in 1/100 increments. Range is 0-200. For a 1.25 slope, enter 125. 0 = AUTO. Uses BIOS VR mailbox command 0x9."", QuestionFlags: 0x10, QuestionId: 0xE6, VarStoreId: 0x1, VarOffset: 0x657, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC8, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "PSYS Offset", Help: "PSYS Offset defined in 1/4 increments. Range is 0-255. For an offset of 25, enter 100. Uses BIOS VR mailbox command 0x9.", QuestionFlags: 0x10, QuestionId: 0xE7, VarStoreId: 0x1, VarOffset: 0x658, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "PSYS PMax Power", Help: "PSYS PMax power, defined in 1/8 Watt increments. Range 0-8192. For a PMax of 125W, enter 1000. 0 = AUTO. Uses BIOS VR mailbox command 0xB.", QuestionFlags: 0x10, QuestionId: 0xE8, VarStoreId: 0x1, VarOffset: 0x659, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1FFF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Ref Prompt: "Acoustic Noise Settings", Help: "Configure Acoustic Noise Settings for IA, GT and SA domains", QuestionFlags: 0x0, QuestionId: 0xE9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2731
		SuppressIf 
			EqIdVal QuestionId: 0xCCF, Value: 0x1
			Ref Prompt: "System Agent VR Settings", Help: "System Agent VR Settings", QuestionFlags: 0x0, QuestionId: 0xEA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2732
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCCE, Value: 0x1
			Ref Prompt: "Core/IA VR Settings", Help: "Core/IA VR Settings", QuestionFlags: 0x0, QuestionId: 0xEB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2733
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCCD, Value: 0x1
			Ref Prompt: "GT-UnSliced VR Settings", Help: "GT-UnSliced VR Settings", QuestionFlags: 0x0, QuestionId: 0xEC, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2734
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCCC, Value: 0x1
			Ref Prompt: "GT-Sliced VR Settings", Help: "GT-Sliced VR Settings", QuestionFlags: 0x0, QuestionId: 0xED, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2735
		End 
		Numeric Prompt: "VR Mailbox Command options", Help: "VR Mailbox Commands to send, 1: MPS VR Cmd, 2: PS4 Exit VR Cmd, 4: MPS VR Decay Cmd. Can select multiple commands by entering sum of values of each command. Example, to send PS4 Exit and MPS VR decay command enter 6 which is sum of 4 and 2.", QuestionFlags: 0x10, QuestionId: 0xEE, VarStoreId: 0x1, VarOffset: 0x71B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		OneOf Prompt: "Intersil VR Command", Help: "VR Mailbox command to fix Intersil VR C-state issues. Disabled- No Mailbox command sent. Default is Disabled.", QuestionFlags: 0x10, QuestionId: 0xEF, VarStoreId: 0x1, VarOffset: 0x750, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Send for IA/GT rails" Value: 1
			OneOfOption Option: "Send for IA/GT/SA rails" Value: 2
		End 
	End 
	Form FormId: 0x2731, Title: "Acoustic Noise Settings"
		Subtitle Prompt: "Acoustic Noise Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Acoustic Noise Mitigation", Help: "Enabling this option will help mitigate acoustic noise on certain SKUs when the CPU is in deeper C state", QuestionFlags: 0x10, QuestionId: 0xF0, VarStoreId: 0x1, VarOffset: 0x713, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xF0, Value: 0x0
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "IA VR Domain", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "Disable Fast PKG C State Ramp for IA Domain", Help: "This option needs to be configured to reduce acoustic noise during deeper C states. False: Don't disable Fast ramp during deeper C states; True: Disable Fast ramp during deeper C state", QuestionFlags: 0x10, QuestionId: 0xF1, VarStoreId: 0x1, VarOffset: 0x714, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "FALSE" Value: 0, Default, MfgDefault
				OneOfOption Option: "TRUE" Value: 1
			End 
			OneOf Prompt: "Slow Slew Rate for IA Domain", Help: "Set VR IA Slow Slew Rate for Deep Package C State ramp time; Slow slew rate equals to Fast devided by number, the number is 2, 4, 8, 16 to slow down the slew rate to help minimize acoustic noise", QuestionFlags: 0x10, QuestionId: 0xF2, VarStoreId: 0x1, VarOffset: 0x717, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Fast/2" Value: 0, Default, MfgDefault
				OneOfOption Option: "Fast/4" Value: 1
				OneOfOption Option: "Fast/8" Value: 2
				OneOfOption Option: "Fast/16" Value: 3
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "GT VR Domain", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "Disable Fast PKG C State Ramp for GT Domain", Help: "This option needs to be configured to reduce acoustic noise during deeper C states. False: Don't disable Fast ramp during deeper C states; True: Disable Fast ramp during deeper C state", QuestionFlags: 0x10, QuestionId: 0xF3, VarStoreId: 0x1, VarOffset: 0x715, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "FALSE" Value: 0, Default, MfgDefault
				OneOfOption Option: "TRUE" Value: 1
			End 
			OneOf Prompt: "Slow Slew Rate for GT Domain", Help: "Set VR GT Slow Slew Rate for Deep Package C State ramp time; Slow slew rate equals to Fast devided by number, the number is 2, 4, 8, 16 to slow down the slew rate to help minimize acoustic noise", QuestionFlags: 0x10, QuestionId: 0xF4, VarStoreId: 0x1, VarOffset: 0x718, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Fast/2" Value: 0, Default, MfgDefault
				OneOfOption Option: "Fast/4" Value: 1
				OneOfOption Option: "Fast/8" Value: 2
				OneOfOption Option: "Fast/16" Value: 3
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "SA VR Domain", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "Disable Fast PKG C State Ramp for SA Domain", Help: "This option needs to be configured to reduce acoustic noise during deeper C states. False: Don't disable Fast ramp during deeper C states; True: Disable Fast ramp during deeper C state", QuestionFlags: 0x10, QuestionId: 0xF5, VarStoreId: 0x1, VarOffset: 0x716, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "FALSE" Value: 0, Default, MfgDefault
				OneOfOption Option: "TRUE" Value: 1
			End 
			OneOf Prompt: "Slow Slew Rate for SA Domain", Help: "Set VR SA Slow Slew Rate for Deep Package C State ramp time; Slow slew rate equals to Fast devided by number, the number is 2, 4, 8, 16 to slow down the slew rate to help minimize acoustic noise", QuestionFlags: 0x10, QuestionId: 0xF6, VarStoreId: 0x1, VarOffset: 0x719, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Fast/2" Value: 0, Default, MfgDefault
				OneOfOption Option: "Fast/4" Value: 1
				OneOfOption Option: "Fast/8" Value: 2
				OneOfOption Option: "Fast/16" Value: 3
			End 
		End 
	End 
	Form FormId: 0x2732, Title: "System Agent VR Settings"
		Subtitle Prompt: "System Agent VR Domain", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "VR Config Enable", Help: "VR Config Enable", QuestionFlags: 0x10, QuestionId: 0xF7, VarStoreId: 0x1, VarOffset: 0x65B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xF7, Value: 0x0
			Numeric Prompt: "AC Loadline", Help: "AC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0xF8, VarStoreId: 0x1, VarOffset: 0x65F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1869, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "DC Loadline", Help: "DC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0xF9, VarStoreId: 0x1, VarOffset: 0x667, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1869, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "PS Current Threshold1", Help: "PS Current Threshold1, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3. Default value = 80 for 20A", QuestionFlags: 0x10, QuestionId: 0xFA, VarStoreId: 0x1, VarOffset: 0x66F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1
				Default DefaultId: 0x0 Value: 80
			End 
			Numeric Prompt: "PS Current Threshold2", Help: "PS Current Threshold2, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3. Default value = 20 for 5A", QuestionFlags: 0x10, QuestionId: 0xFB, VarStoreId: 0x1, VarOffset: 0x677, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1
				Default DefaultId: 0x0 Value: 20
			End 
			Numeric Prompt: "PS Current Threshold3", Help: "PS Current Threshold3, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3. Default value = 4 for 1A", QuestionFlags: 0x10, QuestionId: 0xFC, VarStoreId: 0x1, VarOffset: 0x67F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1
				Default DefaultId: 0x0 Value: 4
			End 
			OneOf Prompt: "PS3 Enable", Help: "PS3 Enable/Disable. 0 - Disabled, 1 - Enabled.Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0xFD, VarStoreId: 0x1, VarOffset: 0x687, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PS4 Enable", Help: "PS4 Enable/Disable. 0 - Disabled, 1 - Enabled. Uses BIOS VR mailbox command 0x3", QuestionFlags: 0x10, QuestionId: 0xFE, VarStoreId: 0x1, VarOffset: 0x68B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			Numeric Prompt: "IMON Slope", Help: "IMON Slope defined in 1/100 increments. Range is 0-200. For a 1.25 slope, enter 125. 0 = AUTO. Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0xFF, VarStoreId: 0x1, VarOffset: 0x68F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC8, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "IMON Offset", Help: "IMON Offset defined in 1/1000 increments. Range is 0-63999. For an offset of 25.348, enter 25348. IMON Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x100, VarStoreId: 0x1, VarOffset: 0x693, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF9FF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "  IMON Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x101, VarStoreId: 0x1, VarOffset: 0x69B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "+" Value: 0, Default, MfgDefault
				OneOfOption Option: "-" Value: 1
			End 
			Numeric Prompt: "VR Current Limit", Help: "Voltage Regulator Current Limit (Icc Max). This value represents the Maximum instantaneous current allowed at any given time. The value is represented in 1/4 A increments. A value of 400 = 100A. 0 means AUTO. Uses BIOS VR mailbox command 0x6.", QuestionFlags: 0x10, QuestionId: 0x102, VarStoreId: 0x1, VarOffset: 0x69F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "VR Voltage Limit", Help: "VR Voltage Limit, defined in mV. Range is 0-7999mV. For a Voltage Limit of 1.25V, enter 1250. 0 = AUTO. Uses BIOS VR mailbox command 0x6", QuestionFlags: 0x10, QuestionId: 0x103, VarStoreId: 0x1, VarOffset: 0x6A7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1F3F, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "TDC Enable", Help: "TDC Enable. 0- Disable, 1 - Enable", QuestionFlags: 0x10, QuestionId: 0x104, VarStoreId: 0x1, VarOffset: 0x6B7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x104, Value: 0x0
				Numeric Prompt: "TDC Current Limit", Help: "TDC Current Limit, defined in 1/8A increments. Range 0-32767. For a TDC Current Limit of 125A, enter 1000. 0 = Auto/Intel Default. Uses BIOS VR mailbox command 0x1A.", QuestionFlags: 0x10, QuestionId: 0x105, VarStoreId: 0x1, VarOffset: 0x6AF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7FFF, Step: 0x7D
					Default DefaultId: 0x0 Value: 0
				End 
				OneOf Prompt: "TDC Time Window", Help: "TDC Time Window, value in milliseconds. 1ms is default. Range from 1ms to 10ms, except for 9ms. 9ms has no valid encoding in the MSR definition.", QuestionFlags: 0x10, QuestionId: 0x106, VarStoreId: 0x1, VarOffset: 0x6BB, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xA, Step: 0x0
					OneOfOption Option: "1 ms" Value: 1, Default, MfgDefault
					OneOfOption Option: "2 ms" Value: 2
					OneOfOption Option: "3 ms" Value: 3
					OneOfOption Option: "4 ms" Value: 4
					OneOfOption Option: "5 ms" Value: 5
					OneOfOption Option: "6 ms" Value: 6
					OneOfOption Option: "7 ms" Value: 7
					OneOfOption Option: "8 ms" Value: 8
					OneOfOption Option: "10 ms" Value: 10
				End 
			End 
			OneOf Prompt: "TDC Lock", Help: "TDC Lock", QuestionFlags: 0x10, QuestionId: 0x107, VarStoreId: 0x1, VarOffset: 0x6BF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
	End 
	Form FormId: 0x2733, Title: "Core/IA VR Settings"
		Subtitle Prompt: "Core/IA VR Domain", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "VR Config Enable", Help: "VR Config Enable", QuestionFlags: 0x10, QuestionId: 0x108, VarStoreId: 0x1, VarOffset: 0x65C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x108, Value: 0x0
			Numeric Prompt: "AC Loadline", Help: "AC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0x109, VarStoreId: 0x1, VarOffset: 0x661, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF424, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "DC Loadline", Help: "DC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0x10A, VarStoreId: 0x1, VarOffset: 0x669, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF424, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "PS Current Threshold1", Help: "PS Current Threshold1, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3. Default value = 80 for 20A", QuestionFlags: 0x10, QuestionId: 0x10B, VarStoreId: 0x1, VarOffset: 0x671, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1
				Default DefaultId: 0x0 Value: 80
			End 
			Numeric Prompt: "PS Current Threshold2", Help: "PS Current Threshold2, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3. Default value = 20 for 5A", QuestionFlags: 0x10, QuestionId: 0x10C, VarStoreId: 0x1, VarOffset: 0x679, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1
				Default DefaultId: 0x0 Value: 20
			End 
			Numeric Prompt: "PS Current Threshold3", Help: "PS Current Threshold3, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3. Default value = 4 for 1A", QuestionFlags: 0x10, QuestionId: 0x10D, VarStoreId: 0x1, VarOffset: 0x681, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1
				Default DefaultId: 0x0 Value: 4
			End 
			OneOf Prompt: "PS3 Enable", Help: "PS3 Enable/Disable. 0 - Disabled, 1 - Enabled.Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x10E, VarStoreId: 0x1, VarOffset: 0x688, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PS4 Enable", Help: "PS4 Enable/Disable. 0 - Disabled, 1 - Enabled. Uses BIOS VR mailbox command 0x3", QuestionFlags: 0x10, QuestionId: 0x10F, VarStoreId: 0x1, VarOffset: 0x68C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			Numeric Prompt: "IMON Slope", Help: "IMON Slope defined in 1/100 increments. Range is 0-200. For a 1.25 slope, enter 125. 0 = AUTO. Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x110, VarStoreId: 0x1, VarOffset: 0x690, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC8, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "IMON Offset", Help: "IMON Offset defined in 1/1000 increments. Range is 0-63999. For an offset of 25.348, enter 25348. IMON Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x111, VarStoreId: 0x1, VarOffset: 0x695, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF9FF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "  IMON Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x112, VarStoreId: 0x1, VarOffset: 0x69C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "+" Value: 0, Default, MfgDefault
				OneOfOption Option: "-" Value: 1
			End 
			Numeric Prompt: "VR Current Limit", Help: "Voltage Regulator Current Limit (Icc Max). This value represents the Maximum instantaneous current allowed at any given time. The value is represented in 1/4 A increments. A value of 400 = 100A. 0 means AUTO. Uses BIOS VR mailbox command 0x6.", QuestionFlags: 0x10, QuestionId: 0x113, VarStoreId: 0x1, VarOffset: 0x6A1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "VR Voltage Limit", Help: "VR Voltage Limit, defined in mV. Range is 0-7999mV. For a Voltage Limit of 1.25V, enter 1250. 0 = AUTO. Uses BIOS VR mailbox command 0x6", QuestionFlags: 0x10, QuestionId: 0x114, VarStoreId: 0x1, VarOffset: 0x6A9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1F3F, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "TDC Enable", Help: "TDC Enable. 0- Disable, 1 - Enable", QuestionFlags: 0x10, QuestionId: 0x115, VarStoreId: 0x1, VarOffset: 0x6B8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x115, Value: 0x0
				Numeric Prompt: "TDC Current Limit", Help: "TDC Current Limit, defined in 1/8A increments. Range 0-32767. For a TDC Current Limit of 125A, enter 1000. 0 = Auto/Intel Default. Uses BIOS VR mailbox command 0x1A.", QuestionFlags: 0x10, QuestionId: 0x116, VarStoreId: 0x1, VarOffset: 0x6B1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7FFF, Step: 0x7D
					Default DefaultId: 0x0 Value: 0
				End 
				OneOf Prompt: "TDC Time Window", Help: "TDC Time Window, value in milliseconds. 1ms is default. Range from 1ms to 10ms, except for 9ms. 9ms has no valid encoding in the MSR definition.", QuestionFlags: 0x10, QuestionId: 0x117, VarStoreId: 0x1, VarOffset: 0x6BC, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xA, Step: 0x0
					OneOfOption Option: "1 ms" Value: 1, Default, MfgDefault
					OneOfOption Option: "2 ms" Value: 2
					OneOfOption Option: "3 ms" Value: 3
					OneOfOption Option: "4 ms" Value: 4
					OneOfOption Option: "5 ms" Value: 5
					OneOfOption Option: "6 ms" Value: 6
					OneOfOption Option: "7 ms" Value: 7
					OneOfOption Option: "8 ms" Value: 8
					OneOfOption Option: "10 ms" Value: 10
				End 
			End 
			OneOf Prompt: "TDC Lock", Help: "TDC Lock", QuestionFlags: 0x10, QuestionId: 0x118, VarStoreId: 0x1, VarOffset: 0x6C0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
	End 
	Form FormId: 0x2734, Title: "GT-UnSliced VR Settings"
		Subtitle Prompt: "GT-UnSliced Domain", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "VR Config Enable", Help: "VR Config Enable", QuestionFlags: 0x10, QuestionId: 0x119, VarStoreId: 0x1, VarOffset: 0x65D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x119, Value: 0x0
			Numeric Prompt: "AC Loadline", Help: "AC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0x11A, VarStoreId: 0x1, VarOffset: 0x663, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF424, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "DC Loadline", Help: "DC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0x11B, VarStoreId: 0x1, VarOffset: 0x66B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF424, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "PS Current Threshold1", Help: "PS Current Threshold1, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3. Default value = 80 for 20A", QuestionFlags: 0x10, QuestionId: 0x11C, VarStoreId: 0x1, VarOffset: 0x673, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1
				Default DefaultId: 0x0 Value: 80
			End 
			Numeric Prompt: "PS Current Threshold2", Help: "PS Current Threshold2, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3. Default value = 20 for 5A", QuestionFlags: 0x10, QuestionId: 0x11D, VarStoreId: 0x1, VarOffset: 0x67B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1
				Default DefaultId: 0x0 Value: 20
			End 
			Numeric Prompt: "PS Current Threshold3", Help: "PS Current Threshold3, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3. Default value = 4 for 1A", QuestionFlags: 0x10, QuestionId: 0x11E, VarStoreId: 0x1, VarOffset: 0x683, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1
				Default DefaultId: 0x0 Value: 4
			End 
			OneOf Prompt: "PS3 Enable", Help: "PS3 Enable/Disable. 0 - Disabled, 1 - Enabled.Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x11F, VarStoreId: 0x1, VarOffset: 0x689, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PS4 Enable", Help: "PS4 Enable/Disable. 0 - Disabled, 1 - Enabled. Uses BIOS VR mailbox command 0x3", QuestionFlags: 0x10, QuestionId: 0x120, VarStoreId: 0x1, VarOffset: 0x68D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			Numeric Prompt: "IMON Slope", Help: "IMON Slope defined in 1/100 increments. Range is 0-200. For a 1.25 slope, enter 125. 0 = AUTO. Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x121, VarStoreId: 0x1, VarOffset: 0x691, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC8, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "IMON Offset", Help: "IMON Offset defined in 1/1000 increments. Range is 0-63999. For an offset of 25.348, enter 25348. IMON Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x122, VarStoreId: 0x1, VarOffset: 0x697, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF9FF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "  IMON Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x123, VarStoreId: 0x1, VarOffset: 0x69D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "+" Value: 0, Default, MfgDefault
				OneOfOption Option: "-" Value: 1
			End 
			Numeric Prompt: "VR Current Limit", Help: "Voltage Regulator Current Limit (Icc Max). This value represents the Maximum instantaneous current allowed at any given time. The value is represented in 1/4 A increments. A value of 400 = 100A. 0 means AUTO. Uses BIOS VR mailbox command 0x6.", QuestionFlags: 0x10, QuestionId: 0x124, VarStoreId: 0x1, VarOffset: 0x6A3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "VR Voltage Limit", Help: "VR Voltage Limit, defined in mV. Range is 0-7999mV. For a Voltage Limit of 1.25V, enter 1250. 0 = AUTO. Uses BIOS VR mailbox command 0x6", QuestionFlags: 0x10, QuestionId: 0x125, VarStoreId: 0x1, VarOffset: 0x6AB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1F3F, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "TDC Enable", Help: "TDC Enable. 0- Disable, 1 - Enable", QuestionFlags: 0x10, QuestionId: 0x126, VarStoreId: 0x1, VarOffset: 0x6B9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x126, Value: 0x0
				Numeric Prompt: "TDC Current Limit", Help: "TDC Current Limit, defined in 1/8A increments. Range 0-32767. For a TDC Current Limit of 125A, enter 1000. 0 = Auto/Intel Default. Uses BIOS VR mailbox command 0x1A.", QuestionFlags: 0x10, QuestionId: 0x127, VarStoreId: 0x1, VarOffset: 0x6B3, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7FFF, Step: 0x7D
					Default DefaultId: 0x0 Value: 0
				End 
				OneOf Prompt: "TDC Time Window", Help: "TDC Time Window, value in milliseconds. 1ms is default. Range from 1ms to 10ms, except for 9ms. 9ms has no valid encoding in the MSR definition.", QuestionFlags: 0x10, QuestionId: 0x128, VarStoreId: 0x1, VarOffset: 0x6BD, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xA, Step: 0x0
					OneOfOption Option: "1 ms" Value: 1, Default, MfgDefault
					OneOfOption Option: "2 ms" Value: 2
					OneOfOption Option: "3 ms" Value: 3
					OneOfOption Option: "4 ms" Value: 4
					OneOfOption Option: "5 ms" Value: 5
					OneOfOption Option: "6 ms" Value: 6
					OneOfOption Option: "7 ms" Value: 7
					OneOfOption Option: "8 ms" Value: 8
					OneOfOption Option: "10 ms" Value: 10
				End 
			End 
			OneOf Prompt: "TDC Lock", Help: "TDC Lock", QuestionFlags: 0x10, QuestionId: 0x129, VarStoreId: 0x1, VarOffset: 0x6C1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
	End 
	Form FormId: 0x2735, Title: "GT-Sliced VR Settings"
		Subtitle Prompt: "GT-Sliced Domain", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "VR Config Enable", Help: "VR Config Enable", QuestionFlags: 0x10, QuestionId: 0x12A, VarStoreId: 0x1, VarOffset: 0x65E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x12A, Value: 0x0
			Numeric Prompt: "AC Loadline", Help: "AC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0x12B, VarStoreId: 0x1, VarOffset: 0x665, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF424, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "DC Loadline", Help: "DC Loadline defined in 1/100 mOhms. A value of 100 = 1.00 mOhm, and 1255 = 12.55 mOhm. Range is 0-6249 (0-62.49 mOhms). 0 = AUTO/HW default. Uses BIOS mailbox command 0x2.", QuestionFlags: 0x10, QuestionId: 0x12C, VarStoreId: 0x1, VarOffset: 0x66D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF424, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "PS Current Threshold1", Help: "PS Current Threshold1, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3. Default value = 80 for 20A", QuestionFlags: 0x10, QuestionId: 0x12D, VarStoreId: 0x1, VarOffset: 0x675, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1
				Default DefaultId: 0x0 Value: 80
			End 
			Numeric Prompt: "PS Current Threshold2", Help: "PS Current Threshold2, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3. Default value = 20 for 5A", QuestionFlags: 0x10, QuestionId: 0x12E, VarStoreId: 0x1, VarOffset: 0x67D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1
				Default DefaultId: 0x0 Value: 20
			End 
			Numeric Prompt: "PS Current Threshold3", Help: "PS Current Threshold3, defined in 1/4 A increments. A value of 400 = 100A. Range 0-512, which translates to 0-128A. 0 = AUTO. Uses BIOS VR mailbox command 0x3. Default value = 4 for 1A", QuestionFlags: 0x10, QuestionId: 0x12F, VarStoreId: 0x1, VarOffset: 0x685, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x200, Step: 0x1
				Default DefaultId: 0x0 Value: 4
			End 
			OneOf Prompt: "PS3 Enable", Help: "PS3 Enable/Disable. 0 - Disabled, 1 - Enabled.Uses BIOS VR mailbox command 0x3.", QuestionFlags: 0x10, QuestionId: 0x130, VarStoreId: 0x1, VarOffset: 0x68A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PS4 Enable", Help: "PS4 Enable/Disable. 0 - Disabled, 1 - Enabled. Uses BIOS VR mailbox command 0x3", QuestionFlags: 0x10, QuestionId: 0x131, VarStoreId: 0x1, VarOffset: 0x68E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			Numeric Prompt: "IMON Slope", Help: "IMON Slope defined in 1/100 increments. Range is 0-200. For a 1.25 slope, enter 125. 0 = AUTO. Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x132, VarStoreId: 0x1, VarOffset: 0x692, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC8, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "IMON Offset", Help: "IMON Offset defined in 1/1000 increments. Range is 0-63999. For an offset of 25.348, enter 25348. IMON Uses BIOS VR mailbox command 0x4.", QuestionFlags: 0x10, QuestionId: 0x133, VarStoreId: 0x1, VarOffset: 0x699, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xF9FF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "  IMON Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x134, VarStoreId: 0x1, VarOffset: 0x69E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "+" Value: 0, Default, MfgDefault
				OneOfOption Option: "-" Value: 1
			End 
			Numeric Prompt: "VR Current Limit", Help: "Voltage Regulator Current Limit (Icc Max). This value represents the Maximum instantaneous current allowed at any given time. The value is represented in 1/4 A increments. A value of 400 = 100A. 0 means AUTO. Uses BIOS VR mailbox command 0x6.", QuestionFlags: 0x10, QuestionId: 0x135, VarStoreId: 0x1, VarOffset: 0x6A5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "VR Voltage Limit", Help: "VR Voltage Limit, defined in mV. Range is 0-7999mV. For a Voltage Limit of 1.25V, enter 1250. 0 = AUTO. Uses BIOS VR mailbox command 0x6", QuestionFlags: 0x10, QuestionId: 0x136, VarStoreId: 0x1, VarOffset: 0x6AD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1F3F, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "TDC Enable", Help: "TDC Enable. 0- Disable, 1 - Enable", QuestionFlags: 0x10, QuestionId: 0x137, VarStoreId: 0x1, VarOffset: 0x6BA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x137, Value: 0x0
				Numeric Prompt: "TDC Current Limit", Help: "TDC Current Limit, defined in 1/8A increments. Range 0-32767. For a TDC Current Limit of 125A, enter 1000. 0 = Auto/Intel Default. Uses BIOS VR mailbox command 0x1A.", QuestionFlags: 0x10, QuestionId: 0x138, VarStoreId: 0x1, VarOffset: 0x6B5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7FFF, Step: 0x7D
					Default DefaultId: 0x0 Value: 0
				End 
				OneOf Prompt: "TDC Time Window", Help: "TDC Time Window, value in milliseconds. 1ms is default. Range from 1ms to 10ms, except for 9ms. 9ms has no valid encoding in the MSR definition.", QuestionFlags: 0x10, QuestionId: 0x139, VarStoreId: 0x1, VarOffset: 0x6BE, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xA, Step: 0x0
					OneOfOption Option: "1 ms" Value: 1, Default, MfgDefault
					OneOfOption Option: "2 ms" Value: 2
					OneOfOption Option: "3 ms" Value: 3
					OneOfOption Option: "4 ms" Value: 4
					OneOfOption Option: "5 ms" Value: 5
					OneOfOption Option: "6 ms" Value: 6
					OneOfOption Option: "7 ms" Value: 7
					OneOfOption Option: "8 ms" Value: 8
					OneOfOption Option: "10 ms" Value: 10
				End 
			End 
			OneOf Prompt: "TDC Lock", Help: "TDC Lock", QuestionFlags: 0x10, QuestionId: 0x13A, VarStoreId: 0x1, VarOffset: 0x6C2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
	End 
	Form FormId: 0x2736, Title: "Power Limit 3 Settings"
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
			OneOf Prompt: "Power Limit 3 Override ", Help: "Enable/DisablePower Limit 3 override. If this option is disabled, BIOS will leave the default values for Power Limit 3 and Power Limit 3 Time Window.", QuestionFlags: 0x10, QuestionId: 0x13B, VarStoreId: 0x1, VarOffset: 0x563, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
				EqIdVal QuestionId: 0x13B, Value: 0x0
				Or 
			End 
			Numeric Prompt: "Power Limit 3", Help: "Power Limit 3 in Milli Watts. BIOS will round to the nearest 1/8W when programming. For 12.50W, enter 12500. XE SKU: Any value can be programmed. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and TDP Limit.If the value is 0, BIOS leaves default value", QuestionFlags: 0x10, QuestionId: 0x13C, VarStoreId: 0x1, VarOffset: 0x564, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
				EqIdVal QuestionId: 0x13B, Value: 0x0
				Or 
			End 
			OneOf Prompt: "Power Limit 3 Time Window", Help: "Power Limit 3 Time Window value in Milli seconds. The value may vary from 3 to 64(max).Indicates the time window over which Power Limit 3 value should be maintained. If the value is 0, BIOS leaves default value", QuestionFlags: 0x10, QuestionId: 0x13D, VarStoreId: 0x1, VarOffset: 0x568, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x40, Step: 0x0
				OneOfOption Option: "0" Value: 0, Default, MfgDefault
				OneOfOption Option: "3" Value: 3
				OneOfOption Option: "4" Value: 4
				OneOfOption Option: "5" Value: 5
				OneOfOption Option: "6" Value: 6
				OneOfOption Option: "7" Value: 7
				OneOfOption Option: "8" Value: 8
				OneOfOption Option: "10" Value: 10
				OneOfOption Option: "12" Value: 12
				OneOfOption Option: "14" Value: 14
				OneOfOption Option: "16" Value: 16
				OneOfOption Option: "20" Value: 20
				OneOfOption Option: "24" Value: 24
				OneOfOption Option: "28" Value: 28
				OneOfOption Option: "32" Value: 32
				OneOfOption Option: "40" Value: 40
				OneOfOption Option: "48" Value: 48
				OneOfOption Option: "55" Value: 55
				OneOfOption Option: "56" Value: 56
				OneOfOption Option: "64" Value: 64
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
				EqIdVal QuestionId: 0x13B, Value: 0x0
				Or 
			End 
			Numeric Prompt: "Powet Limit 3 Duty Cycle", Help: "Specify the duty cycle in percentage that the CPU is required to maintain over the configured time window", QuestionFlags: 0x10, QuestionId: 0x13E, VarStoreId: 0x1, VarOffset: 0x569, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x82, Value: 0x0
				EqIdVal QuestionId: 0x13B, Value: 0x0
				Or 
			End 
			OneOf Prompt: "Power Limit 3 Lock", Help: "Power Limit 3 MSR 615h Lock. When enabled PL3 configurations are locked during OS. When disabled PL3 configuration can be changed during OS.", QuestionFlags: 0x10, QuestionId: 0x13F, VarStoreId: 0x1, VarOffset: 0x56A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
		End 
	End 
	Form FormId: 0x2737, Title: "  Config TDP Configurations"
		Subtitle Prompt: "Config TDP Configurations", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Configurable TDP Boot Mode", Help: "Configurable TDP Mode as Nominal/Up/Down/Deactivate TDP selection. Deactivate option will set MSR to Nominal and MMIO to Zero.", QuestionFlags: 0x10, QuestionId: 0x140, VarStoreId: 0x1, VarOffset: 0x585, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			OneOfOption Option: "Nominal" Value: 0, Default, MfgDefault
			OneOfOption Option: "Down" Value: 1
			SuppressIf 
				EqIdVal QuestionId: 0xCCB, Value: 0x0
					EqIdVal QuestionId: 0xCCA, Value: 0x0
					Or 
				End 
				OneOfOption Option: "Up" Value: 2
			End 
			OneOfOption Option: "Deactivate" Value: 255
		End 
		OneOf Prompt: "Configurable TDP Lock", Help: "Configurable TDP Mode Lock sets the Lock bits on TURBO_ACTIVATION_RATIO and CONFIG_TDP_CONTROL.                 Note: When CTDP Lock is enabled Custom ConfigTDP Count will be forced to 1 and Custom ConfigTDP Boot Index will be forced to 0.", QuestionFlags: 0x10, QuestionId: 0x141, VarStoreId: 0x1, VarOffset: 0x586, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Enabled" Value: 1
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x141, Value: 0x1
				EqIdVal QuestionId: 0x192, Value: 0x1
				Or 
			End 
			OneOf Prompt: "CTDP BIOS control", Help: "Enables CTDP control via runtime ACPI BIOS methods. This "BIOS only" feature does not require EC or driver support.", QuestionFlags: 0x10, QuestionId: 0x142, VarStoreId: 0x1, VarOffset: 0x587, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
		End 
		Text Prompt: "ConfigTDP Levels", Help: "ConfigTDP Levels Supported from MSR", Text: ""
		Text Prompt: "ConfigTDP Turbo Activation Ratio", Help: "ConfigTDP Turbo Activation Ratio values from MSR", Text: "N/A"
		Text Prompt: "Power Limit 1", Help: "Power Limit 1 values from MMIO", Text: "N/A"
		Text Prompt: "Power Limit 2", Help: "Power Limit 2 values from MMIO", Text: "N/A"
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "Custom Settings Nominal", Help: "", Flags: 0x0
		End 
		Text Prompt: "ConfigTDP Nominal", Help: "ConfigTDP Nominal Ratio and TDP from MSR", Text: "N/A"
		GrayOutIf 
			EqIdVal QuestionId: 0x141, Value: 0x1
			Numeric Prompt: "Power Limit 1", Help: "Power Limit 1 in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and TDP Limit.", QuestionFlags: 0x10, QuestionId: 0x143, VarStoreId: 0x1, VarOffset: 0x59F, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "Power Limit 2", Help: "Power Limit 2 value in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Processor applies control policies such that the package power does not exceed this limit.", QuestionFlags: 0x10, QuestionId: 0x144, VarStoreId: 0x1, VarOffset: 0x5A3, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "Power Limit 1 Time Window", Help: "Power Limit 1 Time Window value in seconds. The value may vary from 0 to 128. 0 = default value (28 sec for Mobile and 8 sec for Desktop). Defines time window which TDP value should be maintained.", QuestionFlags: 0x10, QuestionId: 0x145, VarStoreId: 0x1, VarOffset: 0x5A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x0
				Default DefaultId: 0x0 Value: 0
				OneOfOption Option: "0" Value: 0
				OneOfOption Option: "1" Value: 1
				OneOfOption Option: "2" Value: 2
				OneOfOption Option: "3" Value: 3
				OneOfOption Option: "4" Value: 4
				OneOfOption Option: "5" Value: 5
				OneOfOption Option: "6" Value: 6
				OneOfOption Option: "7" Value: 7
				OneOfOption Option: "8" Value: 8
				OneOfOption Option: "10" Value: 10
				OneOfOption Option: "12" Value: 12
				OneOfOption Option: "14" Value: 14
				OneOfOption Option: "16" Value: 16
				OneOfOption Option: "20" Value: 20
				OneOfOption Option: "24" Value: 24
				OneOfOption Option: "28" Value: 28
				OneOfOption Option: "32" Value: 32
				OneOfOption Option: "40" Value: 40
				OneOfOption Option: "48" Value: 48
				OneOfOption Option: "56" Value: 56
				OneOfOption Option: "64" Value: 64
				OneOfOption Option: "80" Value: 80
				OneOfOption Option: "96" Value: 96
				OneOfOption Option: "112" Value: 112
				OneOfOption Option: "128" Value: 128
			End 
			Numeric Prompt: "ConfigTDP Turbo Activation Ratio", Help: "Custom value for Turbo Activation Ratio. Needs to be configured with valid values from LFM to Max Turbo. 0 means don't use custom value.", QuestionFlags: 0x10, QuestionId: 0x146, VarStoreId: 0x1, VarOffset: 0x5A8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCCB, Value: 0x0
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "Custom Settings Down", Help: "", Flags: 0x0
			End 
			Text Prompt: "ConfigTDP Level1", Help: "ConfigTDP Level1 Ratio and TDP from MSR", Text: "N/A"
			GrayOutIf 
				EqIdVal QuestionId: 0x141, Value: 0x1
				Numeric Prompt: "Power Limit 1", Help: "Power Limit 1 in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and TDP Limit.", QuestionFlags: 0x10, QuestionId: 0x147, VarStoreId: 0x1, VarOffset: 0x5A9, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Power Limit 2", Help: "Power Limit 2 value in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Processor applies control policies such that the package power does not exceed this limit.", QuestionFlags: 0x10, QuestionId: 0x148, VarStoreId: 0x1, VarOffset: 0x5AD, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D
					Default DefaultId: 0x0 Value: 0
				End 
				OneOf Prompt: "Power Limit 1 Time Window", Help: "Power Limit 1 Time Window value in seconds. The value may vary from 0 to 128. 0 = default value (28 sec for Mobile and 8 sec for Desktop). Defines time window which TDP value should be maintained.", QuestionFlags: 0x10, QuestionId: 0x149, VarStoreId: 0x1, VarOffset: 0x5B1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x0
					Default DefaultId: 0x0 Value: 0
					OneOfOption Option: "0" Value: 0
					OneOfOption Option: "1" Value: 1
					OneOfOption Option: "2" Value: 2
					OneOfOption Option: "3" Value: 3
					OneOfOption Option: "4" Value: 4
					OneOfOption Option: "5" Value: 5
					OneOfOption Option: "6" Value: 6
					OneOfOption Option: "7" Value: 7
					OneOfOption Option: "8" Value: 8
					OneOfOption Option: "10" Value: 10
					OneOfOption Option: "12" Value: 12
					OneOfOption Option: "14" Value: 14
					OneOfOption Option: "16" Value: 16
					OneOfOption Option: "20" Value: 20
					OneOfOption Option: "24" Value: 24
					OneOfOption Option: "28" Value: 28
					OneOfOption Option: "32" Value: 32
					OneOfOption Option: "40" Value: 40
					OneOfOption Option: "48" Value: 48
					OneOfOption Option: "56" Value: 56
					OneOfOption Option: "64" Value: 64
					OneOfOption Option: "80" Value: 80
					OneOfOption Option: "96" Value: 96
					OneOfOption Option: "112" Value: 112
					OneOfOption Option: "128" Value: 128
				End 
				Numeric Prompt: "ConfigTDP Turbo Activation Ratio", Help: "Custom value for Turbo Activation Ratio. Needs to be configured with valid values from LFM to Max Turbo. 0 means don't use custom value.", QuestionFlags: 0x10, QuestionId: 0x14A, VarStoreId: 0x1, VarOffset: 0x5B2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCCA, Value: 0x0
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "Custom Settings Up", Help: "", Flags: 0x0
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0x141, Value: 0x1
				Text Prompt: "ConfigTDP Level2", Help: "ConfigTDP Level2 Ratio and TDP from MSR", Text: "N/A"
				Numeric Prompt: "Power Limit 1", Help: "Power Limit 1 in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and TDP Limit.", QuestionFlags: 0x10, QuestionId: 0x14B, VarStoreId: 0x1, VarOffset: 0x5B3, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Power Limit 2", Help: "Power Limit 2 value in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Processor applies control policies such that the package power does not exceed this limit.", QuestionFlags: 0x10, QuestionId: 0x14C, VarStoreId: 0x1, VarOffset: 0x5B7, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x3E7F83, Step: 0x7D
					Default DefaultId: 0x0 Value: 0
				End 
				OneOf Prompt: "Power Limit 1 Time Window", Help: "Power Limit 1 Time Window value in seconds. The value may vary from 0 to 128. 0 = default value (28 sec for Mobile and 8 sec for Desktop). Defines time window which TDP value should be maintained.", QuestionFlags: 0x10, QuestionId: 0x14D, VarStoreId: 0x1, VarOffset: 0x5BB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x0
					Default DefaultId: 0x0 Value: 0
					OneOfOption Option: "0" Value: 0
					OneOfOption Option: "1" Value: 1
					OneOfOption Option: "2" Value: 2
					OneOfOption Option: "3" Value: 3
					OneOfOption Option: "4" Value: 4
					OneOfOption Option: "5" Value: 5
					OneOfOption Option: "6" Value: 6
					OneOfOption Option: "7" Value: 7
					OneOfOption Option: "8" Value: 8
					OneOfOption Option: "10" Value: 10
					OneOfOption Option: "12" Value: 12
					OneOfOption Option: "14" Value: 14
					OneOfOption Option: "16" Value: 16
					OneOfOption Option: "20" Value: 20
					OneOfOption Option: "24" Value: 24
					OneOfOption Option: "28" Value: 28
					OneOfOption Option: "32" Value: 32
					OneOfOption Option: "40" Value: 40
					OneOfOption Option: "48" Value: 48
					OneOfOption Option: "56" Value: 56
					OneOfOption Option: "64" Value: 64
					OneOfOption Option: "80" Value: 80
					OneOfOption Option: "96" Value: 96
					OneOfOption Option: "112" Value: 112
					OneOfOption Option: "128" Value: 128
				End 
				Numeric Prompt: "ConfigTDP Turbo Activation Ratio", Help: "Custom value for Turbo Activation Ratio. Needs to be configured with valid values from LFM to Max Turbo. 0 means don't use custom value.", QuestionFlags: 0x10, QuestionId: 0x14E, VarStoreId: 0x1, VarOffset: 0x5BC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
		End 
	End 
	Form FormId: 0x2738, Title: "  View/Configure CPU Lock Options"
		OneOf Prompt: "CFG Lock", Help: "Confgire MSR 0xE2[15], CFG Lock bit", QuestionFlags: 0x10, QuestionId: 0x14F, VarStoreId: 0x1, VarOffset: 0x584, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Overclocking Lock", Help: "Enable/Disable Overclocking Lock (BIT 20) in FLEX_RATIO(194) MSR ", QuestionFlags: 0x10, QuestionId: 0x150, VarStoreId: 0x1, VarOffset: 0x633, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
	End 
	Form FormId: 0x2794, Title: "PCH-FW Configuration"
		Text Prompt: "ME Firmware Version", Help: "ME Firmware Version", Text: "N/A"
		SuppressIf 
			EqIdVal QuestionId: 0xCC9, Value: 0xFF
				Not 
			End 
			Text Prompt: "ME Firmware Mode", Help: "", Text: "Normal Mode"
			Text Prompt: "ME Firmware Mode", Help: "", Text: "ME ALT Disabled"
			Text Prompt: "ME Firmware Mode", Help: "", Text: "ME Temporarily Disabled"
			Text Prompt: "ME Firmware Mode", Help: "", Text: "Secovr Jmpr/Heci MSG"
			Text Prompt: "ME Firmware Mode", Help: "", Text: "ME Failed"
		End 
		Text Prompt: "ME Firmware Mode", Help: "ME Firmware Mode", Text: "N/A"
		Text Prompt: "ME Firmware SKU", Help: "ME Firmware SKU", Text: "N/A"
		Text Prompt: "ME File System Integrity Value", Help: "ME File System Integrity Value", Text: "N/A"
		Text Prompt: "ME Firmware Status 1", Help: "ME Firmware Status 1", Text: "N/A"
		Text Prompt: "ME Firmware Status 2", Help: "ME Firmware Status 2", Text: "N/A"
		Text Prompt: "NFC Support", Help: "Enables support for NFC.", Text: "N/A"
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xCC8, Value: 0x1
				EqIdVal QuestionId: 0xCC2, Value: 0x1
				Or 
			End 
			OneOf Prompt: "ME State", Help: "When Disabled ME will be put into ME Temporarily Disabled Mode.", QuestionFlags: 0x10, QuestionId: 0x151, VarStoreId: 0x14, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x151, Value: 0x0
			SuppressIf 
				EqIdVal QuestionId: 0xCC3, Value: 0x4
					Not 
					EqIdVal QuestionId: 0xCC9, Value: 0x0
					Not 
					Or 
				End 
				GrayOutIf 
					EqIdVal QuestionId: 0xCC8, Value: 0x1
					GrayOutIf 
						EqIdVal QuestionId: 0xCC2, Value: 0x1
						OneOf Prompt: "Manageability Features State", Help: "Enable/Disable Intel(R) Manageability features.

NOTE:
This option disables/enables Manageability Features support in FW.
To disable support platform must be in an unprovisioned state first.", QuestionFlags: 0x14, QuestionId: 0x2791, VarStoreId: 0x14, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
							OneOfOption Option: "Disabled" Value: 0
							OneOfOption Option: "Enabled" Value: 1, Default
						End 
					End 
					SuppressIf 
						EqIdVal QuestionId: 0x2791, Value: 0x0
						GrayOutIf 
							EqIdVal QuestionId: 0xCC2, Value: 0x1
							OneOf Prompt: "AMT BIOS Features", Help: "When disabled AMT BIOS Features are no longer supported and user is no longer able to access MEBx Setup.

Note:
This option does not disable Manageability Features in FW.", QuestionFlags: 0x10, QuestionId: 0x152, VarStoreId: 0x1, VarOffset: 0x76D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
								OneOfOption Option: "Disabled" Value: 0
								OneOfOption Option: "Enabled" Value: 1, Default
							End 
						End 
						GrayOutIf 
							EqIdVal QuestionId: 0x152, Value: 0x0
							Ref Prompt: "AMT Configuration", Help: "Configure Intel(R) Active Management Technology Parameters", QuestionFlags: 0x0, QuestionId: 0x153, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27BE
						End 
					End 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCC7, Value: 0x1
					Not 
				End 
				OneOf Prompt: "ME Unconfig on RTC Clear", Help: "When Disabled ME will not be unconfigured on RTC Clear", QuestionFlags: 0x10, QuestionId: 0x154, VarStoreId: 0x1, VarOffset: 0x781, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCC6, Value: 0x0
				OneOf Prompt: "NFC Feature State", Help: "Enable/Disable NFC Feature", QuestionFlags: 0x14, QuestionId: 0x2792, VarStoreId: 0x14, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "Comms Hub Support", Help: "Enables/Disables support for Comms Hub.", QuestionFlags: 0x10, QuestionId: 0x155, VarStoreId: 0x1, VarOffset: 0x75B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "JHI Support", Help: "Enable/Disable Intel(R) DAL Host Interface Service (JHI)", QuestionFlags: 0x10, QuestionId: 0x156, VarStoreId: 0x1, VarOffset: 0x76C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Core Bios Done Message", Help: "Enable/Disable Core Bios Done message sent to ME", QuestionFlags: 0x10, QuestionId: 0x157, VarStoreId: 0x1, VarOffset: 0x769, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Firmware Update Configuration", Help: "Configure Management Engine Technology Parameters", QuestionFlags: 0x0, QuestionId: 0x158, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2796
			Ref Prompt: "PTT Configuration", Help: "Configure PTT", QuestionFlags: 0x0, QuestionId: 0x159, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2795
			Ref Prompt: "ME Debug Configuration", Help: "Configure ME debug options

NOTE:
This menu is provided for testing purposes. It is recommended to leave the options in their default states", QuestionFlags: 0x0, QuestionId: 0x15A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2797
		End 
	End 
	Form FormId: 0x2795, Title: "PTT Configuration"
		Text Prompt: "PTT Capability / State", Help: "Platform Trust Technology Capability / Enablement State", Text: "N/A"
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "TPM Device Selection", Help: "Selects TPM device: PTT or dTPM. PTT - Enables PTT in SkuMgr dTPM 1.2 - Disables PTT in SkuMgr Warning !  PTT/dTPM will be disabled and all data saved on it will be lost.", QuestionFlags: 0x10, QuestionId: 0x15B, VarStoreId: 0x1, VarOffset: 0x755, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "dTPM" Value: 0, Default, MfgDefault
			OneOfOption Option: "PTT" Value: 1
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xCC2, Value: 0x1
			OneOf Prompt: "PTP aware OS", Help: "Select whether or not the OS you will boot to will be PTP aware", QuestionFlags: 0x10, QuestionId: 0x15C, VarStoreId: 0x1, VarOffset: 0x780, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "PTP Aware" Value: 1, Default, MfgDefault
				OneOfOption Option: "Not PTP Aware" Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCC5, Value: 0x0
					EqIdVal QuestionId: 0xCC4, Value: 0x0
					Or 
				End 
				OneOf Prompt: "TPM 1.2 Deactivate", Help: "Enabling this option will invoke the TPM 1.2 De-activate flow", QuestionFlags: 0x10, QuestionId: 0x15D, VarStoreId: 0x14, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
		End 
	End 
	Form FormId: 0x2796, Title: "Firmware Update Configuration"
		OneOf Prompt: "Me FW Image Re-Flash", Help: "Enable/Disable Me FW Image Re-Flash function.", QuestionFlags: 0x10, QuestionId: 0x15E, VarStoreId: 0x1, VarOffset: 0x758, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCC3, Value: 0x3
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xCC2, Value: 0x1
				OneOf Prompt: "Local FW Update", Help: "Options for Local FW Update function.", QuestionFlags: 0x10, QuestionId: 0x15F, VarStoreId: 0x14, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
		End 
	End 
	Form FormId: 0x2797, Title: "ME Debug Configuration"
		CheckBox Prompt: "HECI Timeouts", Help: "Enable/Disable HECI Send/Receive Timeouts.", QuestionFlags: 0x10, QuestionId: 0x160, VarStoreId: 0x1, VarOffset: 0x75C, Flags: 0x1, Default: Enabled, MfgDefault: Disabled
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Force ME DID Init Status", Help: "Forces the DID Initialization Status value.", QuestionFlags: 0x10, QuestionId: 0x161, VarStoreId: 0x1, VarOffset: 0x75D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "0 - Success" Value: 1
			OneOfOption Option: "1 - No Memory in Channels" Value: 2
			OneOfOption Option: "2 - Memory Init Error" Value: 3
			OneOfOption Option: "3 - Memory not preserved across reset" Value: 4
		End 
		OneOf Prompt: "CPU Replaced Polling Disable", Help: "Setting this option disables CPU replacement polling loop", QuestionFlags: 0x10, QuestionId: 0x162, VarStoreId: 0x1, VarOffset: 0x75E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "ME DID Message", Help: "Enable/Disable ME DID Message (disable will prevent the DID message from being sent).", QuestionFlags: 0x10, QuestionId: 0x163, VarStoreId: 0x1, VarOffset: 0x75F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default
		End 
		OneOf Prompt: "HECI Retry Disable", Help: "Setting this option disables retry mechanism for all HECI APIs", QuestionFlags: 0x10, QuestionId: 0x164, VarStoreId: 0x1, VarOffset: 0x760, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "HECI Message check Disable", Help: "Setting this option disables message check for Bios Boot Path when sending", QuestionFlags: 0x10, QuestionId: 0x165, VarStoreId: 0x1, VarOffset: 0x761, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "MBP HOB Skip", Help: "Setting this option will skip MBP HOB", QuestionFlags: 0x10, QuestionId: 0x166, VarStoreId: 0x1, VarOffset: 0x762, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		CheckBox Prompt: "HECI2 Interface Communication", Help: "Adds and Removes HECI2 Device from PCI space.", QuestionFlags: 0x10, QuestionId: 0x167, VarStoreId: 0x1, VarOffset: 0x763, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: "KT Device", Help: "Enable/Disable KT Device", QuestionFlags: 0x10, QuestionId: 0x168, VarStoreId: 0x1, VarOffset: 0x764, Flags: 0x1, Default: Enabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: "IDER Device", Help: "Enable/Disable IDER Device", QuestionFlags: 0x10, QuestionId: 0x169, VarStoreId: 0x1, VarOffset: 0x765, Flags: 0x1, Default: Enabled, MfgDefault: Disabled
		End 
		OneOf Prompt: "End Of Post Message", Help: "Enable/Disable End of Post message sent to ME", QuestionFlags: 0x10, QuestionId: 0x16A, VarStoreId: 0x1, VarOffset: 0x76A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Send in DXE" Value: 2, Default
		End 
		OneOf Prompt: "D0I3 Setting for HECI Disable", Help: "Setting this option disables setting D0I3 bit for all HECI devices", QuestionFlags: 0x10, QuestionId: 0x16B, VarStoreId: 0x1, VarOffset: 0x766, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
	End 
	Form FormId: 0x2798, Title: "Thermal Configuration"
		Subtitle Prompt: "Thermal Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Ref Prompt: "CPU Thermal Configuration", Help: "CPU Thermal Configuration options", QuestionFlags: 0x0, QuestionId: 0x16C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2799
		Ref Prompt: "Platform Thermal Configuration", Help: "Platform Thermal Configuration options", QuestionFlags: 0x0, QuestionId: 0x16D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x279A
		Ref Prompt: "DPTF Configuration", Help: "DPTF Configuration options", QuestionFlags: 0x0, QuestionId: 0x16E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x279B
	End 
	Form FormId: 0x2799, Title: "Cpu Thermal Configuration"
		Subtitle Prompt: "Cpu Thermal Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "DTS SMM", Help: "Disabled: ACPI thermal management uses EC reported temperature values.
Enabled: ACPI thermal management uses DTS SMM mechanism to obtain CPU temperature values.
Out of Spec: ACPI Thermal Management uses EC reported temperature values and DTS SMM is used to handle Out of Spec condition.", QuestionFlags: 0x10, QuestionId: 0x16F, VarStoreId: 0x1, VarOffset: 0x6F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
			OneOfOption Option: "Critical Temp Reporting (Out Of spec)" Value: 2
		End 
		Numeric Prompt: "Tcc Activation Offset", Help: "Offset from factory set Tcc activation temprature at which the Thermal Control Circuit must be activated. Tcc will be activated at: Tcc Activation Temp - Tcc Activation Offset. Tcc Activation Offset range is 0 to 63.", QuestionFlags: 0x10, QuestionId: 0x170, VarStoreId: 0x1, VarOffset: 0x5C3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x0
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [32, 4, 20, 33, 35, 97]
						Uint64 Value: 0x0
						Uint64 Value: 0xA
						Conditional 
					End 
				End 
			End 
		End 
		OneOf Prompt: "Tcc Offset Time Window", Help: "Tcc Offset Time Window for Running Average Temperature Limit(RATL) feature. The Tcc offset time window can range from 5ms to 448s. For SKL Y SKU the recommended default is 5 Sec, and all other SKUs the recommended default are disabled.", QuestionFlags: 0x10, QuestionId: 0x171, VarStoreId: 0x1, VarOffset: 0x6C3, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x6D600, Step: 0x0
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [32, 4, 20, 33, 35, 97]
						Uint64 Value: 0x0
						Uint64 Value: 0x1388
						Conditional 
					End 
				End 
			End 
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "5 ms" Value: 5
			OneOfOption Option: "10 ms" Value: 10
			OneOfOption Option: "55 ms" Value: 55
			OneOfOption Option: "156 ms" Value: 156
			OneOfOption Option: "375 ms" Value: 375
			OneOfOption Option: "500 ms" Value: 500
			OneOfOption Option: "750 ms" Value: 750
			OneOfOption Option: "1 sec" Value: 1000
			OneOfOption Option: "2 sec" Value: 2000
			OneOfOption Option: "3 sec" Value: 3000
			OneOfOption Option: "4 sec" Value: 4000
			OneOfOption Option: "5 sec" Value: 5000
			OneOfOption Option: "6 sec" Value: 6000
			OneOfOption Option: "7 sec" Value: 7000
			OneOfOption Option: "8 sec" Value: 8000
			OneOfOption Option: "10 sec" Value: 10000
			OneOfOption Option: "12 sec" Value: 12000
			OneOfOption Option: "14 sec" Value: 14000
			OneOfOption Option: "16 sec" Value: 16000
			OneOfOption Option: "20 sec" Value: 20000
			OneOfOption Option: "24 sec" Value: 24000
			OneOfOption Option: "28 sec" Value: 28000
			OneOfOption Option: "32 sec" Value: 32000
			OneOfOption Option: "40 sec" Value: 40000
			OneOfOption Option: "48 sec" Value: 48000
			OneOfOption Option: "56 sec" Value: 56000
			OneOfOption Option: "64 sec" Value: 64000
			OneOfOption Option: "80 sec" Value: 80000
			OneOfOption Option: "96 sec" Value: 96000
			OneOfOption Option: "112 sec" Value: 112000
			OneOfOption Option: "128 sec" Value: 128000
			OneOfOption Option: "160 sec" Value: 160000
			OneOfOption Option: "192 sec" Value: 192000
			OneOfOption Option: "224 sec" Value: 224000
			OneOfOption Option: "256 sec" Value: 256000
			OneOfOption Option: "320 sec" Value: 320000
			OneOfOption Option: "384 sec" Value: 384000
			OneOfOption Option: "448 sec" Value: 448000
		End 
		OneOf Prompt: "Tcc Offset Clamp Enable", Help: "Tcc Offset Clamp bit Enable for Running Average Temperature Limit(RATL) feature to allow CPU to throttle below P1.", QuestionFlags: 0x10, QuestionId: 0x172, VarStoreId: 0x1, VarOffset: 0x6C7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [32, 4, 20, 33, 35, 97]
						Uint64 Value: 0x0
						Uint64 Value: 0x1
						Conditional 
					End 
				End 
			End 
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Tcc Offset Lock Enable", Help: "Lock Enable for Running Average Temperature Limit(RATL) feature to lock Temperature Target MSR.", QuestionFlags: 0x10, QuestionId: 0x173, VarStoreId: 0x1, VarOffset: 0x6C8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Bi-directional PROCHOT#", Help: "When a processor thermal sensor trips (either core), the PROCHOT# will be driven.
If bi-direction is enabled, external agents can drive PROCHOT# to throttle the processor.", QuestionFlags: 0x10, QuestionId: 0x174, VarStoreId: 0x1, VarOffset: 0x5BE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x174, Value: 0x0
			OneOf Prompt: "Disable PROCHOT# Output", Help: "Enable/Disable PROCHOT# Output", QuestionFlags: 0x10, QuestionId: 0x175, VarStoreId: 0x1, VarOffset: 0x5BF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		OneOf Prompt: "Disable VR Thermal Alert", Help: "Enable/Disable VR Thermal Alert", QuestionFlags: 0x10, QuestionId: 0x176, VarStoreId: 0x1, VarOffset: 0x5C0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PROCHOT Response", Help: "Enable/Disable PROCHOT Response", QuestionFlags: 0x10, QuestionId: 0x177, VarStoreId: 0x1, VarOffset: 0x5C2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PROCHOT Lock ", Help: "Enable/Disable PROCHOT Lock", QuestionFlags: 0x10, QuestionId: 0x178, VarStoreId: 0x1, VarOffset: 0x5C1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		CheckBox Prompt: "ACPI T-States", Help: "Enable/Disable ACPI T-States.", QuestionFlags: 0x10, QuestionId: 0x179, VarStoreId: 0x1, VarOffset: 0x5BD, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		OneOf Prompt: "PECI Reset", Help: "Enable/Disable PECI Reset during Sx. Enabling will trigger a PECI Reset during boot to resolve rare Sx PECI issue. Via pcode mailbox command 0x36. Default is disabled.", QuestionFlags: 0x10, QuestionId: 0x17A, VarStoreId: 0x1, VarOffset: 0x71D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PECI C10 Reset", Help: "Enable/Disable PECI C10 Reset command. Enables a mailbox command to resolve rare PECI related C10 issues. Via pcode mailbox command 0x24. Default is disabled/ no command sent.", QuestionFlags: 0x10, QuestionId: 0x17B, VarStoreId: 0x1, VarOffset: 0x71C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
	End 
	Form FormId: 0x279A, Title: "Platform Thermal Configuration"
		Subtitle Prompt: "Platform Thermal Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Automatic Thermal Reporting", Help: "Configure _CRT, _PSV and _AC0 automatically based on values recommended in BWG's Thermal Reporting for Thermal Management settings. Set to Disabled for manual configuration.", QuestionFlags: 0x10, QuestionId: 0x17C, VarStoreId: 0x1, VarOffset: 0x710, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x17C, Value: 0x1
			OneOf Prompt: "Critical Trip Point", Help: "This value controls the temperature of the ACPI Critical Trip Point - the point in which the OS will shut the system off.

NOTE:  119C is the Plan Of Record (POR) for all Intel mobile processors.", QuestionFlags: 0x10, QuestionId: 0x17D, VarStoreId: 0x1, VarOffset: 0x2B2, Flags: 0x10, Size: 8, Min: 0xF, Max: 0x7F, Step: 0x0
				OneOfOption Option: "127 C" Value: 127
				OneOfOption Option: "119 C (POR)" Value: 119, Default, MfgDefault
				OneOfOption Option: "111 C" Value: 111
				OneOfOption Option: "103 C" Value: 103
				OneOfOption Option: "100 C" Value: 100
				OneOfOption Option: "95 C" Value: 95
				OneOfOption Option: "87 C" Value: 87
				OneOfOption Option: "79 C" Value: 79
				OneOfOption Option: "71 C" Value: 71
				OneOfOption Option: "63 C" Value: 63
				OneOfOption Option: "55 C" Value: 55
				OneOfOption Option: "47 C" Value: 47
				OneOfOption Option: "39 C" Value: 39
				OneOfOption Option: "31 C" Value: 31
				OneOfOption Option: "23 C" Value: 23
				OneOfOption Option: "15 C" Value: 15
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x17C, Value: 0x1
			OneOf Prompt: "Active Trip Point 0", Help: "This value controls the temperature of the ACPI Active Trip Point 0 - the point in which the OS will turn the processor fan on Active Trip Point 0 Fan Speed.", QuestionFlags: 0x10, QuestionId: 0x17E, VarStoreId: 0x1, VarOffset: 0x2AE, Flags: 0x10, Size: 8, Min: 0xF, Max: 0x7F, Step: 0x0
				OneOfOption Option: "Disabled" Value: 127
				OneOfOption Option: "15 C" Value: 15
				OneOfOption Option: "23 C" Value: 23
				OneOfOption Option: "31 C" Value: 31
				OneOfOption Option: "39 C" Value: 39
				OneOfOption Option: "47 C" Value: 47
				OneOfOption Option: "55 C" Value: 55
				OneOfOption Option: "63 C" Value: 63
				OneOfOption Option: "71 C" Value: 71, Default, MfgDefault
				OneOfOption Option: "79 C" Value: 79
				OneOfOption Option: "87 C" Value: 87
				OneOfOption Option: "95 C" Value: 95
				OneOfOption Option: "103 C" Value: 103
				OneOfOption Option: "111 C" Value: 111
				OneOfOption Option: "119 C (POR)" Value: 119
			End 
		End 
		Numeric Prompt: "Active Trip Point 0 Fan Speed", Help: "Active Trip Point 0 Fan Speed in percentage. Value must be between 0 (Fan off) - 100 (Max fan speed). This is the speed at which fan will run when Active Trip Point 0 is crossed.", QuestionFlags: 0x0, QuestionId: 0x17F, VarStoreId: 0x1, VarOffset: 0x2B0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
			Default DefaultId: 0x0 Value: 100
		End 
		OneOf Prompt: "Active Trip Point 1", Help: "This value controls the temperature of the ACPI Active Trip Point 1 - the point in which the OS will turn the processor fan on Active Trip Point 1 Fan Speed.", QuestionFlags: 0x10, QuestionId: 0x180, VarStoreId: 0x1, VarOffset: 0x2AD, Flags: 0x10, Size: 8, Min: 0xF, Max: 0x7F, Step: 0x0
			OneOfOption Option: "Disabled" Value: 127
			OneOfOption Option: "15 C" Value: 15
			OneOfOption Option: "23 C" Value: 23
			OneOfOption Option: "31 C" Value: 31
			OneOfOption Option: "39 C" Value: 39
			OneOfOption Option: "47 C" Value: 47
			OneOfOption Option: "55 C" Value: 55, Default, MfgDefault
			OneOfOption Option: "63 C" Value: 63
			OneOfOption Option: "71 C" Value: 71
			OneOfOption Option: "79 C" Value: 79
			OneOfOption Option: "87 C" Value: 87
			OneOfOption Option: "95 C" Value: 95
			OneOfOption Option: "103 C" Value: 103
			OneOfOption Option: "111 C" Value: 111
			OneOfOption Option: "119 C (POR)" Value: 119
		End 
		Numeric Prompt: "Active Trip Point 1 Fan Speed", Help: "Active Trip Point 1 Fan Speed in percentage. Value must be between 0 (Fan off) - 100 (Max fan speed). This value must be less than Active Trip Point 0 Fan speed. This is the speed at which fan will run when Active Trip 1 is crossed.", QuestionFlags: 0x0, QuestionId: 0x181, VarStoreId: 0x1, VarOffset: 0x2AF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
			Default DefaultId: 0x0 Value: 75
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x17C, Value: 0x1
			OneOf Prompt: "Passive Trip Point", Help: "This value controls the temperature of the ACPI Passive Trip Point - the point in which the OS will begin throttling the processor.", QuestionFlags: 0x10, QuestionId: 0x182, VarStoreId: 0x1, VarOffset: 0x2B1, Flags: 0x10, Size: 8, Min: 0xF, Max: 0x7F, Step: 0x0
				OneOfOption Option: "119 C (POR)" Value: 119
				OneOfOption Option: "111 C" Value: 111
				OneOfOption Option: "103 C" Value: 103
				OneOfOption Option: "95 C" Value: 95, Default, MfgDefault
				OneOfOption Option: "87 C" Value: 87
				OneOfOption Option: "79 C" Value: 79
				OneOfOption Option: "71 C" Value: 71
				OneOfOption Option: "63 C" Value: 63
				OneOfOption Option: "55 C" Value: 55
				OneOfOption Option: "47 C" Value: 47
				OneOfOption Option: "39 C" Value: 39
				OneOfOption Option: "31 C" Value: 31
				OneOfOption Option: "23 C" Value: 23
				OneOfOption Option: "15 C" Value: 15
				OneOfOption Option: "Disabled" Value: 127
			End 
		End 
		Numeric Prompt: "  Passive TC1 Value", Help: "This value sets the TC1 value for the ACPI Passive Cooling Formula. Range 1 - 16", QuestionFlags: 0x0, QuestionId: 0x183, VarStoreId: 0x1, VarOffset: 0x2B3, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x10, Step: 0x1
			Default DefaultId: 0x0 Value: 1
		End 
		Numeric Prompt: "  Passive TC2 Value", Help: "This value sets the TC2 value for the ACPI Passive Cooling Formula. Range 1 - 16", QuestionFlags: 0x0, QuestionId: 0x184, VarStoreId: 0x1, VarOffset: 0x2B4, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x10, Step: 0x1
			Default DefaultId: 0x0 Value: 5
		End 
		Numeric Prompt: "  Passive TSP Value", Help: "This item sets the TSP value for the ACPI Passive Cooling Formula.  It represents in tenths of a second how often the OS will read the temperature when passive cooling is enabled. Range 2 - 32", QuestionFlags: 0x0, QuestionId: 0x185, VarStoreId: 0x1, VarOffset: 0x2B5, Flags: 0x10, Size: 8, Min: 0x2, Max: 0x20, Step: 0x2
			Default DefaultId: 0x0 Value: 10
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Active Trip Points", Help: "Disable Active Trip Points", QuestionFlags: 0x10, QuestionId: 0x186, VarStoreId: 0x1, VarOffset: 0x2B6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Passive Trip Points", Help: "Disable Passive Trip Points", QuestionFlags: 0x10, QuestionId: 0x187, VarStoreId: 0x1, VarOffset: 0x2B7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Critical Trip Points", Help: "Disable Critical Trip Points", QuestionFlags: 0x10, QuestionId: 0x188, VarStoreId: 0x1, VarOffset: 0x2B8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "PCH Thermal Device", Help: "Enable/Disable PCH Thermal Device(D20:F2)", QuestionFlags: 0x10, QuestionId: 0x189, VarStoreId: 0x1, VarOffset: 0x2BC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled in PCI mode" Value: 1, Default, MfgDefault
			OneOfOption Option: "Enabled in ACPI mode" Value: 2
		End 
		CheckBox Prompt: "PCH Temp Read", Help: "PCH Temperature Read Enable", QuestionFlags: 0x10, QuestionId: 0x18A, VarStoreId: 0x1, VarOffset: 0x2BF, Flags: 0x1, Default: Enabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: "CPU Energy Read", Help: "CPU Energy Read Enable", QuestionFlags: 0x10, QuestionId: 0x18B, VarStoreId: 0x1, VarOffset: 0x2BE, Flags: 0x1, Default: Enabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: "CPU Temp Read", Help: "CPU Temperature Read Enable", QuestionFlags: 0x10, QuestionId: 0x18C, VarStoreId: 0x1, VarOffset: 0x2BD, Flags: 0x1, Default: Enabled, MfgDefault: Disabled
		End 
		OneOf Prompt: "Alert Enable Lock", Help: "Lock all Alert Enable settings", QuestionFlags: 0x10, QuestionId: 0x18D, VarStoreId: 0x1, VarOffset: 0x2C0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x18D, Value: 0x0
			OneOf Prompt: " PCH Alert", Help: "PCH Alert pin enable", QuestionFlags: 0x10, QuestionId: 0x18E, VarStoreId: 0x1, VarOffset: 0x2C1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: " DIMM Alert", Help: "DIMM Alert pin enable", QuestionFlags: 0x10, QuestionId: 0x18F, VarStoreId: 0x1, VarOffset: 0x2C2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		Numeric Prompt: "CPU Temp", Help: "Fail Safe temp that EC will use if OS is hung", QuestionFlags: 0x0, QuestionId: 0x190, VarStoreId: 0x1, VarOffset: 0x2C3, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x6E, Step: 0x1
			Default DefaultId: 0x0 Value: Other
				Value 
					Uint64 Value: 0x48
				End 
			End 
		End 
		Numeric Prompt: "CPU Fan Speed", Help: "Fan speed that EC will use if OS is hung", QuestionFlags: 0x0, QuestionId: 0x191, VarStoreId: 0x1, VarOffset: 0x2C4, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x64, Step: 0x1
			Default DefaultId: 0x0 Value: 65
		End 
	End 
	Form FormId: 0x279B, Title: "DPTF Configuration"
		Subtitle Prompt: "DPTF Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC50, Value: 0x44
				Not 
				EqIdVal QuestionId: 0xC50, Value: 0x4A
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0x50
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0x45
				Not 
				And 
				EqIdVal QuestionId: 0xC8C, Value: 0x1
				Not 
				And 
			End 
			OneOf Prompt: "DPTF", Help: "Enable/Disable Intel Dynamic Platform Thermal Framework", QuestionFlags: 0x10, QuestionId: 0x192, VarStoreId: 0x1, VarOffset: 0x2C5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x192, Value: 0x0
			Numeric Prompt: "DPTF Configuration", Help: "An Integer containing the DPTF Configuration bitmap:   BIT0[Generic UI Access Control](0=enable,1=disable) BIT1[Restricted UI Access Control](0=enable,1=disable) BIT2[shell Access Control](0=enable,1=disable) BIT3[Environment Monitoring Report Control](0=report,1=silent) BIT4[Thermal Mitigation Report Control](0=silent,1=report)  BIT5[Thermal Policy Report Control](0=silent,1=report)", QuestionFlags: 0x10, QuestionId: 0x193, VarStoreId: 0x1, VarOffset: 0x2C6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x192, Value: 0x0
			OneOf Prompt: "Processor Thermal Device", Help: "Enable/Disable Processor Thermal Device.", QuestionFlags: 0x10, QuestionId: 0x194, VarStoreId: 0x1, VarOffset: 0x2C7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "SA Thermal Device" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x194, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x195, VarStoreId: 0x1, VarOffset: 0x2C8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 86
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x196, VarStoreId: 0x1, VarOffset: 0x2C9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 89
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x197, VarStoreId: 0x1, VarOffset: 0x2CA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x198, VarStoreId: 0x1, VarOffset: 0x2CB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 95
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x199, VarStoreId: 0x1, VarOffset: 0x2CC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 97
				End 
				Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x10, QuestionId: 0x19A, VarStoreId: 0x1, VarOffset: 0x2CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				OneOf Prompt: " PPCC Step Size", Help: "Step size for Turbo power limit (RAPL) control", QuestionFlags: 0x10, QuestionId: 0x19B, VarStoreId: 0x1, VarOffset: 0x2CE, Flags: 0x12, Size: 32, Min: 0x1F4, Max: 0x7D0, Step: 0x0
					OneOfOption Option: "0.5 Watts" Value: 500, Default, MfgDefault
					OneOfOption Option: "1.0 Watts" Value: 1000
					OneOfOption Option: "1.5 Watts" Value: 1500
					OneOfOption Option: "2.0 Watts" Value: 2000
				End 
				Text Prompt: " Minimum Power Limit Default", Help: "Power Limit 1 in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and TDP Limit. If value is 0, BIOS will program TDP value.", Text: ""
				Numeric Prompt: " Minimum Power Limit 0", Help: "This value provides the minimum power limit in the PPCC object for this platform.  Enter the value in milliwatts with 125mw granularity.", QuestionFlags: 0x0, QuestionId: 0x19C, VarStoreId: 0x1, VarOffset: 0x2D7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7530, Step: 0x7D
					Default DefaultId: 0x0 Value: 125
				End 
				Numeric Prompt: " Minimum Power Limit 1", Help: "This value provides the minimum power limit in the PPCC object for this platform.  Enter the value in milliwatts with 125mw granularity.", QuestionFlags: 0x0, QuestionId: 0x19D, VarStoreId: 0x1, VarOffset: 0x2D9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7530, Step: 0x7D
					Default DefaultId: 0x0 Value: 125
				End 
				Numeric Prompt: " Minimum Power Limit 2", Help: "This value provides the minimum power limit in the PPCC object for this platform.  Enter the value in milliwatts with 125mw granularity.", QuestionFlags: 0x0, QuestionId: 0x19E, VarStoreId: 0x1, VarOffset: 0x2DB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7530, Step: 0x7D
					Default DefaultId: 0x0 Value: 125
				End 
				OneOf Prompt: " CLPO Enable", Help: "Instructs the policy to use Active Cores if they are available.", QuestionFlags: 0x10, QuestionId: 0x19F, VarStoreId: 0x1, VarOffset: 0x2D2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
				Numeric Prompt: " CLPO Start PState", Help: "Instructs the policy when to initiate Active Core control if enabled.       Note: 16=LFM", QuestionFlags: 0x10, QuestionId: 0x1A0, VarStoreId: 0x1, VarOffset: 0x2D3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x10, Step: 0x1
					Default DefaultId: 0x0 Value: 16
				End 
				Numeric Prompt: " CLPO Step Size", Help: "Instructs the policy to take away logical processors in the specified percentage steps.", QuestionFlags: 0x10, QuestionId: 0x1A1, VarStoreId: 0x1, VarOffset: 0x2D4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 50
				End 
				OneOf Prompt: " CLPO Power Control", Help: "Instructs the policy whether to use Core offlining or SMT offlining if Active core control is enabled to be used in P0 or when power control is applied.", QuestionFlags: 0x10, QuestionId: 0x1A2, VarStoreId: 0x1, VarOffset: 0x2D5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "SMT Off lining" Value: 1, Default, MfgDefault
					OneOfOption Option: "Core Off lining" Value: 2
				End 
				OneOf Prompt: " CLPO Performance Control", Help: "Instructs the policy whether to use Core offlining or SMT offlining if Active core control is enabled to be used in P1 or when performance control is applied.", QuestionFlags: 0x10, QuestionId: 0x1A3, VarStoreId: 0x1, VarOffset: 0x2D6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "SMT Off lining" Value: 1
					OneOfOption Option: "Core Off lining" Value: 2, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x194, Value: 0x0
					EqIdVal QuestionId: 0xCC1, Value: 0x0
					Or 
				End 
				OneOf Prompt: " ConfigTDP", Help: "Enable/Disable Intel Configurable TDP", QuestionFlags: 0x10, QuestionId: 0x1A4, VarStoreId: 0x1, VarOffset: 0x2DD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC82, Value: 0x7
				SuppressIf 
					EqIdVal QuestionId: 0x194, Value: 0x0
						EqIdVal QuestionId: 0xCC0, Value: 0x0
						Or 
					End 
					OneOf Prompt: " LPM", Help: "Enable/Disable Intel Low Power Mode", QuestionFlags: 0x10, QuestionId: 0x1A5, VarStoreId: 0x1, VarOffset: 0x2DE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x1 Value: Other
							Value 
								EqIdValList QuestionId: 0xC50, Values: [7, 19, 74]
									Uint64 Value: 0x1
									Uint64 Value: 0x0
									Conditional 
								End 
							End 
						End 
						OneOfOption Option: "Disabled" Value: 0
						OneOfOption Option: "Enabled" Value: 1
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x194, Value: 0x0
						EqIdVal QuestionId: 0xCC0, Value: 0x0
						Or 
						EqIdVal QuestionId: 0x1A5, Value: 0x0
						Or 
					End 
					OneOf Prompt: " CLPM", Help: "Current Low Power Mode Setting", QuestionFlags: 0x10, QuestionId: 0x1A6, VarStoreId: 0x1, VarOffset: 0x2DF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
						OneOfOption Option: "Disable LPM" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enable LPM" Value: 1
						OneOfOption Option: "Application Specific LPM" Value: 2
						OneOfOption Option: "Use the LPM setting as requested by the OS" Value: 3
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x194, Value: 0x0
						EqIdVal QuestionId: 0xCC0, Value: 0x0
						Or 
						EqIdVal QuestionId: 0x1A5, Value: 0x0
						Or 
					End 
					OneOf Prompt: " CEUC", Help: "Enable/Disable Current Execution Unit Configuration", QuestionFlags: 0x10, QuestionId: 0x1A7, VarStoreId: 0x1, VarOffset: 0x2E0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0
						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					End 
					Numeric Prompt: " Graphics Freq", Help: "Graphics Frequency for CEUC", QuestionFlags: 0x0, QuestionId: 0x1A8, VarStoreId: 0x1, VarOffset: 0x2E1, Flags: 0x11, Size: 16, Min: 0x190, Max: 0x320, Step: 0x1
						Default DefaultId: 0x0 Value: 400
					End 
				End 
			End 
			OneOf Prompt: "FAN1 Device", Help: "Enable the Fan1 device.", QuestionFlags: 0x10, QuestionId: 0x1A9, VarStoreId: 0x1, VarOffset: 0x2EA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [74]
							Uint64 Value: 0x1
							Uint64 Value: 0x0
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Enabled" Value: 1, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
			OneOf Prompt: "FAN2 Device", Help: "Enable the Fan2 device.", QuestionFlags: 0x10, QuestionId: 0x1AA, VarStoreId: 0x1, VarOffset: 0x2EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
			OneOf Prompt: "Display participant", Help: "Enable/Disable the Display participant.", QuestionFlags: 0x10, QuestionId: 0x1AB, VarStoreId: 0x1, VarOffset: 0x2EC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [74]
							Uint64 Value: 0x0
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Disabled" Value: 0, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1AB, Value: 0x0
				Numeric Prompt: " Display Low Limit", Help: " Display Low Limit", QuestionFlags: 0x10, QuestionId: 0x1AC, VarStoreId: 0x1, VarOffset: 0x2EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 30
				End 
				Numeric Prompt: " Display High Limit", Help: "Display High Limit - Between 0% to 100%", QuestionFlags: 0x10, QuestionId: 0x1AD, VarStoreId: 0x1, VarOffset: 0x2ED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 80
				End 
			End 
			OneOf Prompt: "Wireless Participant", Help: "Enable/Disable the Wireless participant.", QuestionFlags: 0x10, QuestionId: 0x1AE, VarStoreId: 0x1, VarOffset: 0x2EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1AE, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1AF, VarStoreId: 0x1, VarOffset: 0x2F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 63
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1B0, VarStoreId: 0x1, VarOffset: 0x2F1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 71
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1B1, VarStoreId: 0x1, VarOffset: 0x2F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 103
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1B2, VarStoreId: 0x1, VarOffset: 0x2F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1B3, VarStoreId: 0x1, VarOffset: 0x2F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 95
				End 
				Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x10, QuestionId: 0x1B4, VarStoreId: 0x1, VarOffset: 0x4E4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			OneOf Prompt: "WWAN participant", Help: "Enable/Disable the WWAN participant.", QuestionFlags: 0x10, QuestionId: 0x1B5, VarStoreId: 0x1, VarOffset: 0x2F5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1B5, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1B6, VarStoreId: 0x1, VarOffset: 0x2F6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 63
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1B7, VarStoreId: 0x1, VarOffset: 0x2F7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 71
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1B8, VarStoreId: 0x1, VarOffset: 0x2F8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 103
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1B9, VarStoreId: 0x1, VarOffset: 0x2F9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1BA, VarStoreId: 0x1, VarOffset: 0x2FA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 95
				End 
			End 
			OneOf Prompt: "Charger participant", Help: "Enable/Disable Charger device", QuestionFlags: 0x10, QuestionId: 0x1BB, VarStoreId: 0x1, VarOffset: 0x301, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [74]
							Uint64 Value: 0x0
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Disabled" Value: 0, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Power participant", Help: "Enable/Disable the Power participant.", QuestionFlags: 0x10, QuestionId: 0x1BC, VarStoreId: 0x1, VarOffset: 0x302, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [74]
							Uint64 Value: 0x0
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Disabled" Value: 0, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1BC, Value: 0x0
				Numeric Prompt: "DPTF Power Sampling Period", Help: "This power sampling period for the Power Participant Object.", QuestionFlags: 0x10, QuestionId: 0x1BD, VarStoreId: 0x1, VarOffset: 0x303, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			OneOf Prompt: "PerC participant", Help: "Enable/Disable the Perceptual Computing Camera Participant.", QuestionFlags: 0x10, QuestionId: 0x1BE, VarStoreId: 0x1, VarOffset: 0x306, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1BE, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1BF, VarStoreId: 0x1, VarOffset: 0x307, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 63
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1C0, VarStoreId: 0x1, VarOffset: 0x308, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 71
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1C1, VarStoreId: 0x1, VarOffset: 0x309, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 103
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1C2, VarStoreId: 0x1, VarOffset: 0x30A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 97
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1C3, VarStoreId: 0x1, VarOffset: 0x30B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
			End 
			OneOf Prompt: "IVCAM participant", Help: "Enable/Disable Intel (R) RealSense(TM) 3D Camera(SR300).", QuestionFlags: 0x10, QuestionId: 0x1C4, VarStoreId: 0x1, VarOffset: 0x30C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1C4, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1C5, VarStoreId: 0x1, VarOffset: 0x30D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 63
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1C6, VarStoreId: 0x1, VarOffset: 0x30E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 71
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1C7, VarStoreId: 0x1, VarOffset: 0x30F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 103
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1C8, VarStoreId: 0x1, VarOffset: 0x310, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 97
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1C9, VarStoreId: 0x1, VarOffset: 0x311, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
			End 
			OneOf Prompt: "Storage participant", Help: "Enable/Disable Storage device", QuestionFlags: 0x10, QuestionId: 0x1CA, VarStoreId: 0x1, VarOffset: 0x312, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1CA, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1CB, VarStoreId: 0x1, VarOffset: 0x313, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 63
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1CC, VarStoreId: 0x1, VarOffset: 0x314, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 71
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1CD, VarStoreId: 0x1, VarOffset: 0x315, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 103
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1CE, VarStoreId: 0x1, VarOffset: 0x316, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1CF, VarStoreId: 0x1, VarOffset: 0x317, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 95
				End 
			End 
			OneOf Prompt: "Virtual Sensor participant 1", Help: "Enable/Disable Virtual Sensor device", QuestionFlags: 0x10, QuestionId: 0x1D0, VarStoreId: 0x1, VarOffset: 0x318, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [74]
							Uint64 Value: 0x0
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Disabled" Value: 0, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1D0, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1D1, VarStoreId: 0x1, VarOffset: 0x319, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 80
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1D2, VarStoreId: 0x1, VarOffset: 0x31A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 55
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1D3, VarStoreId: 0x1, VarOffset: 0x31B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1D4, VarStoreId: 0x1, VarOffset: 0x31D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 97
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1D5, VarStoreId: 0x1, VarOffset: 0x31C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 95
				End 
			End 
			OneOf Prompt: "Virtual Sensor participant 2", Help: "Enable/Disable Virtual Sensor device", QuestionFlags: 0x10, QuestionId: 0x1D6, VarStoreId: 0x1, VarOffset: 0x31E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1D6, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1D7, VarStoreId: 0x1, VarOffset: 0x31F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 80
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1D8, VarStoreId: 0x1, VarOffset: 0x320, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 55
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1D9, VarStoreId: 0x1, VarOffset: 0x321, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1DA, VarStoreId: 0x1, VarOffset: 0x323, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 97
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1DB, VarStoreId: 0x1, VarOffset: 0x322, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 95
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "Sensor Device 1", Help: "Enable/Disable Memory Thermal Device", QuestionFlags: 0x10, QuestionId: 0x1DC, VarStoreId: 0x1, VarOffset: 0x324, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1DC, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1DD, VarStoreId: 0x1, VarOffset: 0x325, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 63
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1DE, VarStoreId: 0x1, VarOffset: 0x326, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 71
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1DF, VarStoreId: 0x1, VarOffset: 0x327, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 103
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1E0, VarStoreId: 0x1, VarOffset: 0x328, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1E1, VarStoreId: 0x1, VarOffset: 0x329, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x0, QuestionId: 0x1E2, VarStoreId: 0x1, VarOffset: 0x32A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			OneOf Prompt: "Sensor Device 2", Help: "Enable/Disable VR Hotspot Q50 sensor", QuestionFlags: 0x10, QuestionId: 0x1E3, VarStoreId: 0x1, VarOffset: 0x32B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1E3, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1E4, VarStoreId: 0x1, VarOffset: 0x32C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 63
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1E5, VarStoreId: 0x1, VarOffset: 0x32D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 71
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1E6, VarStoreId: 0x1, VarOffset: 0x32E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 103
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1E7, VarStoreId: 0x1, VarOffset: 0x32F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1E8, VarStoreId: 0x1, VarOffset: 0x330, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x0, QuestionId: 0x1E9, VarStoreId: 0x1, VarOffset: 0x331, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			OneOf Prompt: "Sensor Device 3", Help: "Enable/Disable Skin Hotspot U50 sensor", QuestionFlags: 0x10, QuestionId: 0x1EA, VarStoreId: 0x1, VarOffset: 0x332, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1EA, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1EB, VarStoreId: 0x1, VarOffset: 0x333, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 63
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1EC, VarStoreId: 0x1, VarOffset: 0x334, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 71
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1ED, VarStoreId: 0x1, VarOffset: 0x335, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 103
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1EE, VarStoreId: 0x1, VarOffset: 0x336, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x10, QuestionId: 0x1EF, VarStoreId: 0x1, VarOffset: 0x337, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x0, QuestionId: 0x1F0, VarStoreId: 0x1, VarOffset: 0x338, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			OneOf Prompt: "Sensor Device 4", Help: "Enable/Disable PMIC-MCP Hotspot Q16 sensor", QuestionFlags: 0x10, QuestionId: 0x1F1, VarStoreId: 0x1, VarOffset: 0x339, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1F1, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1F2, VarStoreId: 0x1, VarOffset: 0x33A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 63
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1F3, VarStoreId: 0x1, VarOffset: 0x33B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 71
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1F4, VarStoreId: 0x1, VarOffset: 0x33C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 103
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1F5, VarStoreId: 0x1, VarOffset: 0x33D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1F6, VarStoreId: 0x1, VarOffset: 0x33E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 95
				End 
				Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x0, QuestionId: 0x1F7, VarStoreId: 0x1, VarOffset: 0x33F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
					EqIdVal QuestionId: 0xC50, Value: 0x21
					Or 
					EqIdVal QuestionId: 0xC50, Value: 0x9
					Or 
					EqIdVal QuestionId: 0xC50, Value: 0x61
					Or 
				End 
				OneOf Prompt: "Sensor Device 5", Help: "Enable/Disable C-Skin Chassis U50 IR sensor", QuestionFlags: 0x10, QuestionId: 0x1F8, VarStoreId: 0x1, VarOffset: 0x340, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [74]
								Uint64 Value: 0x0
								Uint64 Value: 0x1
								Conditional 
							End 
						End 
					End 
					OneOfOption Option: "Disabled" Value: 0, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1F8, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1F9, VarStoreId: 0x1, VarOffset: 0x341, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 110
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1FA, VarStoreId: 0x1, VarOffset: 0x342, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 115
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1FB, VarStoreId: 0x1, VarOffset: 0x343, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 127
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1FC, VarStoreId: 0x1, VarOffset: 0x344, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 124
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x1FD, VarStoreId: 0x1, VarOffset: 0x345, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 121
				End 
				Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x0, QuestionId: 0x1FE, VarStoreId: 0x1, VarOffset: 0x346, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "Generic Device 1", Help: "Enable/Disable Thermistor 1 device", QuestionFlags: 0x10, QuestionId: 0x1FF, VarStoreId: 0x1, VarOffset: 0x35C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x1FF, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x200, VarStoreId: 0x1, VarOffset: 0x35D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 63
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x201, VarStoreId: 0x1, VarOffset: 0x35E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 71
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x202, VarStoreId: 0x1, VarOffset: 0x35F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 103
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x203, VarStoreId: 0x1, VarOffset: 0x360, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x204, VarStoreId: 0x1, VarOffset: 0x361, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 95
				End 
				Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x0, QuestionId: 0x205, VarStoreId: 0x1, VarOffset: 0x362, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 50
				End 
			End 
			OneOf Prompt: "Generic Device 2", Help: "Enable/Disable Thermistor 2 device", QuestionFlags: 0x10, QuestionId: 0x206, VarStoreId: 0x1, VarOffset: 0x363, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x206, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x207, VarStoreId: 0x1, VarOffset: 0x364, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 63
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x208, VarStoreId: 0x1, VarOffset: 0x365, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 71
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x209, VarStoreId: 0x1, VarOffset: 0x366, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 103
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x20A, VarStoreId: 0x1, VarOffset: 0x367, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x20B, VarStoreId: 0x1, VarOffset: 0x368, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 95
				End 
				Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x0, QuestionId: 0x20C, VarStoreId: 0x1, VarOffset: 0x369, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 50
				End 
			End 
			OneOf Prompt: "Generic Device 3", Help: "Enable/Disable Thermistor 3 device", QuestionFlags: 0x10, QuestionId: 0x20D, VarStoreId: 0x1, VarOffset: 0x36A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x20D, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x20E, VarStoreId: 0x1, VarOffset: 0x36B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 63
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x20F, VarStoreId: 0x1, VarOffset: 0x36C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 71
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x210, VarStoreId: 0x1, VarOffset: 0x36D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 103
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x211, VarStoreId: 0x1, VarOffset: 0x36E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x212, VarStoreId: 0x1, VarOffset: 0x36F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 95
				End 
				Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x0, QuestionId: 0x213, VarStoreId: 0x1, VarOffset: 0x370, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 50
				End 
			End 
			OneOf Prompt: "Generic Device 4", Help: "Enable/Disable Thermistor 4 device", QuestionFlags: 0x10, QuestionId: 0x214, VarStoreId: 0x1, VarOffset: 0x371, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x214, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x215, VarStoreId: 0x1, VarOffset: 0x372, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 63
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x216, VarStoreId: 0x1, VarOffset: 0x373, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 71
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x217, VarStoreId: 0x1, VarOffset: 0x374, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 103
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x218, VarStoreId: 0x1, VarOffset: 0x375, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x219, VarStoreId: 0x1, VarOffset: 0x376, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 95
				End 
				Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x0, QuestionId: 0x21A, VarStoreId: 0x1, VarOffset: 0x377, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 50
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
					Not 
				End 
				OneOf Prompt: "Generic Device 5", Help: "Enable/Disable Thermistor 5 device", QuestionFlags: 0x10, QuestionId: 0x21B, VarStoreId: 0x1, VarOffset: 0x378, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x21B, Value: 0x0
				Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x21C, VarStoreId: 0x1, VarOffset: 0x379, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 43
				End 
				Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x21D, VarStoreId: 0x1, VarOffset: 0x37A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 42
				End 
				Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x21E, VarStoreId: 0x1, VarOffset: 0x37B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x21F, VarStoreId: 0x1, VarOffset: 0x37C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x220, VarStoreId: 0x1, VarOffset: 0x37D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x0, QuestionId: 0x221, VarStoreId: 0x1, VarOffset: 0x37E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 50
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x4A
					Not 
				End 
				OneOf Prompt: "Discrete Gfx Core Participant", Help: "Enable/Disable Discrete Gfx Core Participant", QuestionFlags: 0x10, QuestionId: 0x222, VarStoreId: 0x1, VarOffset: 0x37F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [74]
								Uint64 Value: 0x0
								Uint64 Value: 0x1
								Conditional 
							End 
						End 
					End 
					OneOfOption Option: "Disabled" Value: 0, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x222, Value: 0x0
					Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x223, VarStoreId: 0x1, VarOffset: 0x380, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
						Default DefaultId: 0x0 Value: 63
					End 
					Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x224, VarStoreId: 0x1, VarOffset: 0x381, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
						Default DefaultId: 0x0 Value: 89
					End 
					Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x225, VarStoreId: 0x1, VarOffset: 0x382, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
						Default DefaultId: 0x0 Value: 103
					End 
					Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x226, VarStoreId: 0x1, VarOffset: 0x383, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
						Default DefaultId: 0x0 Value: 100
					End 
					Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x227, VarStoreId: 0x1, VarOffset: 0x384, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
						Default DefaultId: 0x0 Value: 95
					End 
					Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x0, QuestionId: 0x228, VarStoreId: 0x1, VarOffset: 0x385, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
						Default DefaultId: 0x0 Value: 50
					End 
					OneOf Prompt: " PPCC Step Size", Help: "Step size for Turbo power limit (RAPL) control", QuestionFlags: 0x10, QuestionId: 0x229, VarStoreId: 0x1, VarOffset: 0x386, Flags: 0x12, Size: 32, Min: 0x1F4, Max: 0x7D0, Step: 0x0
						OneOfOption Option: "0.5 Watts" Value: 500, Default, MfgDefault
						OneOfOption Option: "1.0 Watts" Value: 1000
						OneOfOption Option: "1.5 Watts" Value: 1500
						OneOfOption Option: "2.0 Watts" Value: 2000
					End 
					Text Prompt: " Minimum Power Limit Default", Help: "Power Limit 1 in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and TDP Limit. If value is 0, BIOS will program TDP value.", Text: ""
					Numeric Prompt: " Minimum Power Limit 0", Help: "This value provides the minimum power limit in the PPCC object for this platform.  Enter the value in milliwatts with 125mw granularity.", QuestionFlags: 0x0, QuestionId: 0x22A, VarStoreId: 0x1, VarOffset: 0x38A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xD6D8, Step: 0x7D
						Default DefaultId: 0x0 Value: 125
					End 
				End 
				Subtitle Prompt: "", Help: "", Flags: 0x0
				End 
				OneOf Prompt: "Discrete Gfx Memory Participant", Help: "Enable/Disable Discrete Gfx Memory Participant", QuestionFlags: 0x10, QuestionId: 0x22B, VarStoreId: 0x1, VarOffset: 0x38C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [74]
								Uint64 Value: 0x0
								Uint64 Value: 0x1
								Conditional 
							End 
						End 
					End 
					OneOfOption Option: "Disabled" Value: 0, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x22B, Value: 0x0
					Numeric Prompt: " Active Thermal Trip Point", Help: "This value controls the temperature of the ACPI Active Thermal Trip Point.      NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x22C, VarStoreId: 0x1, VarOffset: 0x38D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
						Default DefaultId: 0x0 Value: 63
					End 
					Numeric Prompt: " Passive Thermal Trip Point", Help: "This value controls the temperature of the ACPI Passive Thermal Trip Point.     NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x22D, VarStoreId: 0x1, VarOffset: 0x38E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
						Default DefaultId: 0x0 Value: 89
					End 
					Numeric Prompt: " Critical Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point.    NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x22E, VarStoreId: 0x1, VarOffset: 0x38F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
						Default DefaultId: 0x0 Value: 103
					End 
					Numeric Prompt: " S3/CS Thermal Trip Point", Help: "This value controls the temperature of the ACPI Critical Thermal Trip Point for entering S3 or CS.         NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x22F, VarStoreId: 0x1, VarOffset: 0x390, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
						Default DefaultId: 0x0 Value: 100
					End 
					Numeric Prompt: " Hot Thermal Trip Point", Help: "This value controls the temperature of the ACPI Hot Thermal Trip Point.            NOTE: a value of zero will cause the DPTF driver to disable the trip point.", QuestionFlags: 0x0, QuestionId: 0x230, VarStoreId: 0x1, VarOffset: 0x391, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
						Default DefaultId: 0x0 Value: 95
					End 
					Numeric Prompt: " Thermal Sampling Period", Help: "The polling interval in 10ths of seconds. A value of 0 tells the driver to use interrupts.                  NOTE: The granularity of the sampling period is 0.1 seconds. For example, if the sampling period is 30 seconds, then _TSP needs to report 300; if the sampling period is 0.5 seconds, then choose 5.", QuestionFlags: 0x0, QuestionId: 0x231, VarStoreId: 0x1, VarOffset: 0x392, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
						Default DefaultId: 0x0 Value: 50
					End 
				End 
				Subtitle Prompt: "", Help: "", Flags: 0x0
				End 
				OneOf Prompt: "Multi Chip Pkg Participant", Help: "Enable/Disable Multi Chip Pkg Participant", QuestionFlags: 0x10, QuestionId: 0x232, VarStoreId: 0x1, VarOffset: 0x393, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [74]
								Uint64 Value: 0x0
								Uint64 Value: 0x1
								Conditional 
							End 
						End 
					End 
					OneOfOption Option: "Disabled" Value: 0, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x232, Value: 0x0
					OneOf Prompt: " PPCC Step Size", Help: "Step size for Turbo power limit (RAPL) control", QuestionFlags: 0x10, QuestionId: 0x233, VarStoreId: 0x1, VarOffset: 0x394, Flags: 0x12, Size: 32, Min: 0x1F4, Max: 0x7D0, Step: 0x0
						OneOfOption Option: "0.5 Watts" Value: 500, Default, MfgDefault
						OneOfOption Option: "1.0 Watts" Value: 1000
						OneOfOption Option: "1.5 Watts" Value: 1500
						OneOfOption Option: "2.0 Watts" Value: 2000
					End 
					Text Prompt: " Minimum Power Limit Default", Help: "Power Limit 1 in Milli Watts. BIOS will round to the nearest 1/8W when programming. 0 = no custom override. For 12.50W, enter 12500. Overclocking SKU: Value must be between Max and Min Power Limits (specified by PACKAGE_POWER_SKU_MSR). Other SKUs: This value must be between Min Power Limit and TDP Limit. If value is 0, BIOS will program TDP value.", Text: ""
					Numeric Prompt: " Minimum Power Limit 0", Help: "This value provides the minimum power limit in the PPCC object for this platform.  Enter the value in milliwatts with 125mw granularity.", QuestionFlags: 0x0, QuestionId: 0x234, VarStoreId: 0x1, VarOffset: 0x398, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x14C08, Step: 0x7D
						Default DefaultId: 0x0 Value: 125
					End 
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x192, Value: 0x0
			Ref Prompt: "Policy Configuration", Help: "Policy Configuration options", QuestionFlags: 0x0, QuestionId: 0x235, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x279C
		End 
	End 
	Form FormId: 0x279C, Title: "Policy Configuration"
		Subtitle Prompt: "Policy Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Active Policy", Help: "Enable/Disable Active Policy 1.0 or 2.0.", QuestionFlags: 0x10, QuestionId: 0x236, VarStoreId: 0x1, VarOffset: 0x3B1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Active Policy 1.0" Value: 1, Default, MfgDefault
			OneOfOption Option: "Active Policy 2.0" Value: 2
		End 
		OneOf Prompt: "Passive Policy", Help: "Enable/Disable Passive Policy 1.0 or 2.0.", QuestionFlags: 0x10, QuestionId: 0x237, VarStoreId: 0x1, VarOffset: 0x3B2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Passive Policy 1.0" Value: 1, Default, MfgDefault
			OneOfOption Option: "Passive Policy 2.0" Value: 2
			OneOfOption Option: "Disabled" Value: 0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x237, Value: 0x0
			OneOf Prompt: " TRT Revision", Help: "Select the TRT influence.", QuestionFlags: 0x10, QuestionId: 0x238, VarStoreId: 0x1, VarOffset: 0x3B3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Traditional" Value: 0
				OneOfOption Option: "Priority" Value: 1, Default, MfgDefault
			End 
		End 
		OneOf Prompt: "Critical Policy", Help: "Enable/Disable Critical Policy.", QuestionFlags: 0x10, QuestionId: 0x239, VarStoreId: 0x1, VarOffset: 0x3B4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			OneOfOption Option: "Disabled" Value: 0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC82, Value: 0x7
			OneOf Prompt: "Cooling Mode Policy", Help: "Enable/Disable Cooling Mode Policy.", QuestionFlags: 0x10, QuestionId: 0x23A, VarStoreId: 0x1, VarOffset: 0x3B5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [7, 19, 74]
							Uint64 Value: 0x1
							Uint64 Value: 0x0
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0
			End 
		End 
		OneOf Prompt: "Platform Noise Mitigation", Help: "Platform Noise Mitigation Solution.", QuestionFlags: 0x10, QuestionId: 0x23B, VarStoreId: 0x1, VarOffset: 0x3B6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Power Boss", Help: "Power Boss Policy.", QuestionFlags: 0x10, QuestionId: 0x23C, VarStoreId: 0x1, VarOffset: 0x305, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x0
						Uint64 Value: 0x1
						Conditional 
					End 
				End 
			End 
			OneOfOption Option: "Disabled" Value: 0, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Hardware Duty Cycling", Help: "Hardware Duty Cycling Policy.", QuestionFlags: 0x10, QuestionId: 0x23D, VarStoreId: 0x1, VarOffset: 0x3B7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Adaptive Performance", Help: "Adaptive Performance Policy.", QuestionFlags: 0x10, QuestionId: 0x23E, VarStoreId: 0x1, VarOffset: 0x3B8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Virtual Sensor", Help: "Virtual Sensor Policy.", QuestionFlags: 0x10, QuestionId: 0x23F, VarStoreId: 0x1, VarOffset: 0x3B9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x0
						Uint64 Value: 0x1
						Conditional 
					End 
				End 
			End 
			OneOfOption Option: "Disabled" Value: 0, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PID Policy ", Help: "Enable /Disable PID Policy.", QuestionFlags: 0x10, QuestionId: 0x240, VarStoreId: 0x1, VarOffset: 0x4E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC50, Value: 0x4A
				Not 
			End 
			OneOf Prompt: "Power Share", Help: "Power Share Policy.", QuestionFlags: 0x10, QuestionId: 0x241, VarStoreId: 0x1, VarOffset: 0x4E7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [74]
							Uint64 Value: 0x0
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "Design Variable 0", Help: "OEM Design Variable: an integer between 0-255. This allows OEM's to customize DPTF behavior based on platform changes.", QuestionFlags: 0x0, QuestionId: 0x242, VarStoreId: 0x1, VarOffset: 0x3C7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Design Variable 1", Help: "OEM Design Variable: an integer between 0-255. This allows OEM's to customize DPTF behavior based on platform changes.", QuestionFlags: 0x0, QuestionId: 0x243, VarStoreId: 0x1, VarOffset: 0x3C8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Design Variable 2", Help: "OEM Design Variable: an integer between 0-255. This allows OEM's to customize DPTF behavior based on platform changes.", QuestionFlags: 0x0, QuestionId: 0x244, VarStoreId: 0x1, VarOffset: 0x3C9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Design Variable 3", Help: "OEM Design Variable: an integer between 0-255. This allows OEM's to customize DPTF behavior based on platform changes.", QuestionFlags: 0x0, QuestionId: 0x245, VarStoreId: 0x1, VarOffset: 0x3CA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Design Variable 4", Help: "OEM Design Variable: an integer between 0-255. This allows OEM's to customize DPTF behavior based on platform changes.", QuestionFlags: 0x0, QuestionId: 0x246, VarStoreId: 0x1, VarOffset: 0x3CB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Design Variable 5", Help: "OEM Design Variable: an integer between 0-255. This allows OEM's to customize DPTF behavior based on platform changes.", QuestionFlags: 0x0, QuestionId: 0x247, VarStoreId: 0x1, VarOffset: 0x3CC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "PPCC Object", Help: "Enable/Disable PPCC object for validation.", QuestionFlags: 0x10, QuestionId: 0x248, VarStoreId: 0x1, VarOffset: 0x3BA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 1
			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
		End 
		OneOf Prompt: "PDRT Object", Help: "Enable/Disable PDRT object for validation.", QuestionFlags: 0x10, QuestionId: 0x249, VarStoreId: 0x1, VarOffset: 0x3BB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 1
			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
		End 
		OneOf Prompt: "ARTG Object", Help: "Enable/Disable ARTG object for validation.", QuestionFlags: 0x10, QuestionId: 0x24A, VarStoreId: 0x1, VarOffset: 0x3BC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 1
			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
		End 
		OneOf Prompt: "PMAX Object", Help: "Enable/Disable PMAX object for validation.", QuestionFlags: 0x10, QuestionId: 0x24B, VarStoreId: 0x1, VarOffset: 0x3BD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 1
			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC50, Value: 0x20
			Text Prompt: "Processor Thermal Device", Help: "DPTF Configuration options", Text: ""
		End 
		OneOf Prompt: "_TMP 1 Object", Help: "Enable/Disable _TMP 1 object for validation.", QuestionFlags: 0x10, QuestionId: 0x24C, VarStoreId: 0x1, VarOffset: 0x3BE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 1, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 0
		End 
		SuppressIf 
			True 
			OneOf Prompt: "_TMP 2 Object", Help: "Enable/Disable _TMP 2 object for validation.", QuestionFlags: 0x10, QuestionId: 0x24D, VarStoreId: 0x1, VarOffset: 0x3BF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 0
			End 
			OneOf Prompt: "_TMP 3 Object", Help: "Enable/Disable _TMP 3 object for validation.", QuestionFlags: 0x10, QuestionId: 0x24E, VarStoreId: 0x1, VarOffset: 0x3C0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 1
				OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "_TMP 4 Object", Help: "Enable/Disable _TMP 4 object for validation.", QuestionFlags: 0x10, QuestionId: 0x24F, VarStoreId: 0x1, VarOffset: 0x3C1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 1
				OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "_TMP 5 Object", Help: "Enable/Disable _TMP 5 object for validation.", QuestionFlags: 0x10, QuestionId: 0x250, VarStoreId: 0x1, VarOffset: 0x3C2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 1
				OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "_TMP 6 Object", Help: "Enable/Disable _TMP 6 object for validation.", QuestionFlags: 0x10, QuestionId: 0x251, VarStoreId: 0x1, VarOffset: 0x3C3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 1
				OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "_TMP 7 Object", Help: "Enable/Disable _TMP 7 object for validation.", QuestionFlags: 0x10, QuestionId: 0x252, VarStoreId: 0x1, VarOffset: 0x3C4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 1
				OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "_TMP 8 Object", Help: "Enable/Disable _TMP 8 object for validation.", QuestionFlags: 0x10, QuestionId: 0x253, VarStoreId: 0x1, VarOffset: 0x3C5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 1
				OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "Optional Objects", Help: "Enable/Disable PIPR/PAPR for processor participant.", QuestionFlags: 0x10, QuestionId: 0x254, VarStoreId: 0x1, VarOffset: 0x3C6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 0
			End 
		End 
	End 
	Form FormId: 0x279D, Title: "Platform Settings"
		Subtitle Prompt: "Platform Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "UCSI Retry Workaround", Help: "Enable: As needed BIOS will retry to write parameters before EC goes out of burst mode, applicable only to DT platforms", QuestionFlags: 0x10, QuestionId: 0x255, VarStoreId: 0x1, VarOffset: 0x539, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdVal QuestionId: 0xC50, Value: 0x42
						Uint64 Value: 0x0
						Uint64 Value: 0x1
						Conditional 
					End 
				End 
			End 
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Firmware Configuration", Help: "Firmware Configuration options.
NOTE:Ignore Policy Update(STR_FW_CONFIG_DEFAULT_VALUE) is to skip policy update and will ONLY WORK ON A PLATFORM.", QuestionFlags: 0x10, QuestionId: 0x256, VarStoreId: 0x1, VarOffset: 0x34, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Ignore Policy Update" Value: 0
			OneOfOption Option: "Production" Value: 1
			OneOfOption Option: "Test" Value: 2, Default
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "PS2 Keyboard and Mouse", Help: "Enables/Disables PS2 Keyboard and Mouse", QuestionFlags: 0x10, QuestionId: 0x257, VarStoreId: 0x1, VarOffset: 0x2A9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			Default DefaultId: 0x0 Value: 1
			OneOfOption Option: "Enabled" Value: 1, MfgDefault
			OneOfOption Option: "Disabled" Value: 0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8C, Value: 0x1
				Not 
				EqIdVal QuestionId: 0xC8C, Value: 0x5
				Not 
				And 
			End 
			OneOf Prompt: "Pmic Vcc IO Level", Help: "Select the Pmic Vcc IO Voltage Level", QuestionFlags: 0x10, QuestionId: 0x258, VarStoreId: 0x1, VarOffset: 0x2B9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
				OneOfOption Option: "Disabled" Value: 7, Default, MfgDefault
				OneOfOption Option: "1.05V" Value: 0
				OneOfOption Option: "1.071V" Value: 1
				OneOfOption Option: "1.023V" Value: 2
				OneOfOption Option: "0.997V" Value: 3
				OneOfOption Option: "0.850V" Value: 4
				OneOfOption Option: "0.900V" Value: 5
				OneOfOption Option: "0.950V" Value: 6
			End 
			OneOf Prompt: "Pmic Vddq Level", Help: "Select the Pmic Vddq Voltage Level", QuestionFlags: 0x10, QuestionId: 0x259, VarStoreId: 0x1, VarOffset: 0x2BA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x8, Step: 0x0
				OneOfOption Option: "Disabled" Value: 8, Default, MfgDefault
				OneOfOption Option: "0" Value: 0
				OneOfOption Option: "1" Value: 1
				OneOfOption Option: "2" Value: 2
				OneOfOption Option: "3" Value: 3
				OneOfOption Option: "4" Value: 4
				OneOfOption Option: "5" Value: 5
				OneOfOption Option: "6" Value: 6
				OneOfOption Option: "7" Value: 7
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
					Not 
					EqIdVal QuestionId: 0xC50, Value: 0xB
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x7
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x13
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x3
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x4
					Not 
					And 
				End 
				Numeric Prompt: "HEBC value", Help: "HEBC value 32bit ", QuestionFlags: 0x10, QuestionId: 0x25A, VarStoreId: 0x1, VarOffset: 0x4D1, Flags: 0x12, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1
					Default DefaultId: 0x0 Value: 144371
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCBF, Value: 0x0
				OneOf Prompt: "SLP_S0# VM", Help: "SLP_S0# Voltage Margining using Premium PMIC or discrete VR with GPIO control", QuestionFlags: 0x10, QuestionId: 0x25B, VarStoreId: 0x1, VarOffset: 0x4CF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdVal QuestionId: 0xC50, Value: 0x4
								Uint64 Value: 0x0
								Uint64 Value: 0x1
								Conditional 
							End 
						End 
					End 
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x48
					Not 
				End 
				OneOf Prompt: "Audio Connector", Help: "Select the Audio Connector Type", QuestionFlags: 0x10, QuestionId: 0x25C, VarStoreId: 0x1, VarOffset: 0x45E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Type C" Value: 0, Default, MfgDefault
					OneOfOption Option: "Stacked Jack" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x4
					Not 
					EqIdVal QuestionId: 0xC50, Value: 0x14
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0xB
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x7
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x13
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x3
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x1B
					Not 
					And 
				End 
				OneOf Prompt: "Enable EInk DFU device", Help: "Enables or Disables EInk DFU device.", QuestionFlags: 0x10, QuestionId: 0x25D, VarStoreId: 0x1, VarOffset: 0x461, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			OneOf Prompt: "Power Sharing Manager", Help: "Configure the PSM ACPI objects.", QuestionFlags: 0x10, QuestionId: 0x25E, VarStoreId: 0x1, VarOffset: 0x3F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x25E, Value: 0x0
				Numeric Prompt: " Domain Type SPLC 1", Help: "09h: Module(M.2); 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x25F, VarStoreId: 0x1, VarOffset: 0x3F4, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1
					Default DefaultId: 0x0 Value: 9
				End 
				Numeric Prompt: " Default Power Limit 1 SPLC", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x260, VarStoreId: 0x1, VarOffset: 0x3F5, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 4000
				End 
				Numeric Prompt: " Default Time Window 1 SPLC", Help: "Time Window in milli seconds", QuestionFlags: 0x0, QuestionId: 0x261, VarStoreId: 0x1, VarOffset: 0x3F9, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x186A0, Step: 0x1
					Default DefaultId: 0x0 Value: 30000
				End 
				Subtitle Prompt: "", Help: "", Flags: 0x0
				End 
				Numeric Prompt: " Domain Type SPLC 2", Help: "09h: Module(M.2); 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x262, VarStoreId: 0x1, VarOffset: 0x3FD, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1
					Default DefaultId: 0x0 Value: 20
				End 
				Numeric Prompt: " Default Power Limit 2 SPLC", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x263, VarStoreId: 0x1, VarOffset: 0x3FE, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 4000
				End 
				Numeric Prompt: " Default Time Window 2 SPLC", Help: "Time Window in milli seconds", QuestionFlags: 0x0, QuestionId: 0x264, VarStoreId: 0x1, VarOffset: 0x402, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x186A0, Step: 0x1
					Default DefaultId: 0x0 Value: 30000
				End 
				Subtitle Prompt: "", Help: "", Flags: 0x0
				End 
				Numeric Prompt: " Domain Type DPLC 1", Help: "09h: Module(M.2); 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x265, VarStoreId: 0x1, VarOffset: 0x406, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1
					Default DefaultId: 0x0 Value: 9
				End 
				Numeric Prompt: " Domain Preference DPLC 1", Help: "09h: Module(M.2); 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x266, VarStoreId: 0x1, VarOffset: 0x407, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1
					Default DefaultId: 0x0 Value: 9
				End 
				Numeric Prompt: " Power Limit Index 1 DPLC", Help: "Index of the specific power limit range information", QuestionFlags: 0x0, QuestionId: 0x267, VarStoreId: 0x1, VarOffset: 0x408, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xA, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: " Default Power Limit 1 DPLC", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x268, VarStoreId: 0x1, VarOffset: 0x40A, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 1200
				End 
				Numeric Prompt: " Default Time Window 1 DPLC", Help: "Time Window in milli seconds", QuestionFlags: 0x0, QuestionId: 0x269, VarStoreId: 0x1, VarOffset: 0x40C, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x186A0, Step: 0x1
					Default DefaultId: 0x0 Value: 30000
				End 
				Numeric Prompt: " Minimum Power Limit 1 DPLC", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x26A, VarStoreId: 0x1, VarOffset: 0x410, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 1200
				End 
				Numeric Prompt: " Maximum Power Limit 1 DPLC", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x26B, VarStoreId: 0x1, VarOffset: 0x412, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 1200
				End 
				Numeric Prompt: " Maximum Time Window 1 DPLC", Help: "Time Window in milli seconds", QuestionFlags: 0x0, QuestionId: 0x26C, VarStoreId: 0x1, VarOffset: 0x414, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 1000
				End 
				Subtitle Prompt: "", Help: "", Flags: 0x0
				End 
				Numeric Prompt: " Domain Type DPLC 2", Help: "09h: Module(M.2); 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x26D, VarStoreId: 0x1, VarOffset: 0x416, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1
					Default DefaultId: 0x0 Value: 20
				End 
				Numeric Prompt: " Domain Preference DPLC 2", Help: "09h: Module(M.2); 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x26E, VarStoreId: 0x1, VarOffset: 0x417, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x32, Step: 0x1
					Default DefaultId: 0x0 Value: 20
				End 
				Numeric Prompt: " Power Limit Index 2 DPLC", Help: "Index of the specific power limit range information", QuestionFlags: 0x0, QuestionId: 0x26F, VarStoreId: 0x1, VarOffset: 0x418, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xA, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: " Default Power Limit 2 DPLC", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x270, VarStoreId: 0x1, VarOffset: 0x41A, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 1200
				End 
				Numeric Prompt: " Default Time Window 2 DPLC", Help: "Time Window in milli seconds", QuestionFlags: 0x0, QuestionId: 0x271, VarStoreId: 0x1, VarOffset: 0x41C, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x186A0, Step: 0x1
					Default DefaultId: 0x0 Value: 30000
				End 
				Numeric Prompt: " Minimum Power Limit 2 DPLC", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x272, VarStoreId: 0x1, VarOffset: 0x420, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 1200
				End 
				Numeric Prompt: " Maximum Power Limit 2 DPLC", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x273, VarStoreId: 0x1, VarOffset: 0x422, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 1200
				End 
				Numeric Prompt: " Default Time Window 2 SPLC", Help: "Time Window in milli seconds", QuestionFlags: 0x0, QuestionId: 0x274, VarStoreId: 0x1, VarOffset: 0x424, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 1000
				End 
				Subtitle Prompt: "", Help: "", Flags: 0x0
				End 
			End 
			OneOf Prompt: "Wireless device", Help: "Configure ACPI objects for wireless devices.", QuestionFlags: 0x10, QuestionId: 0x275, VarStoreId: 0x1, VarOffset: 0x426, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x275, Value: 0x0
				Numeric Prompt: " Domain Type SPLC 1", Help: "09h: Module(M.2); 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x276, VarStoreId: 0x1, VarOffset: 0x427, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 7
				End 
				Numeric Prompt: " Default Power Limit", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x277, VarStoreId: 0x1, VarOffset: 0x428, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 1600
				End 
				Numeric Prompt: " Default Time Window", Help: "Time Window in milli seconds", QuestionFlags: 0x0, QuestionId: 0x278, VarStoreId: 0x1, VarOffset: 0x42A, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x186A0, Step: 0x1
					Default DefaultId: 0x0 Value: 30000
				End 
				Numeric Prompt: " Domain Type SPLC 2", Help: "09h: Module(M.2); 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x279, VarStoreId: 0x1, VarOffset: 0x42E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 16
				End 
				Numeric Prompt: " Default Power Limit", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x27A, VarStoreId: 0x1, VarOffset: 0x42F, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 1600
				End 
				Numeric Prompt: " Default Time Window", Help: "Time Window in milli seconds", QuestionFlags: 0x0, QuestionId: 0x27B, VarStoreId: 0x1, VarOffset: 0x431, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x186A0, Step: 0x1
					Default DefaultId: 0x0 Value: 30000
				End 
				Numeric Prompt: " Domain Type SPLC 3", Help: "09h: Module(M.2); 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x27C, VarStoreId: 0x1, VarOffset: 0x435, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 20
				End 
				Numeric Prompt: " Default Power Limit", Help: "Power Limit in milli watts", QuestionFlags: 0x0, QuestionId: 0x27D, VarStoreId: 0x1, VarOffset: 0x436, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 1050
				End 
				Numeric Prompt: " Default Time Window", Help: "Time Window in milli seconds", QuestionFlags: 0x0, QuestionId: 0x27E, VarStoreId: 0x1, VarOffset: 0x438, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x186A0, Step: 0x1
					Default DefaultId: 0x0 Value: 30000
				End 
				Numeric Prompt: " TRxDelay_A", Help: "Antenna A delay possible values: 1-100 in 10ths of nano seconds resolution", QuestionFlags: 0x0, QuestionId: 0x27F, VarStoreId: 0x1, VarOffset: 0x43C, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 50
				End 
				Numeric Prompt: " TRxCableLength_A", Help: "Antenna A cable length possible values: 1-100cm in 1cm resolution", QuestionFlags: 0x0, QuestionId: 0x280, VarStoreId: 0x1, VarOffset: 0x43D, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 50
				End 
				Numeric Prompt: " TRxDelay_B", Help: "Antenna B delay possible values: 1-100 in 10ths of nano seconds resolution", QuestionFlags: 0x0, QuestionId: 0x281, VarStoreId: 0x1, VarOffset: 0x43E, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 50
				End 
				Numeric Prompt: " TRxCableLength_B", Help: "Antenna B cable length possible values: 1-100cm in 1cm resolution", QuestionFlags: 0x0, QuestionId: 0x282, VarStoreId: 0x1, VarOffset: 0x43F, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 50
				End 
				Text Prompt: "WRDD Package 1", Help: "WRDD Package 1", Text: ""
				Numeric Prompt: " Domain Type", Help: "09h: Module; 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x283, VarStoreId: 0x1, VarOffset: 0x440, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 7
				End 
				Numeric Prompt: " Country Identifier", Help: "Country identifier as defined in ISO/IEC 3166-1 Alpha 2 code", QuestionFlags: 0x0, QuestionId: 0x284, VarStoreId: 0x1, VarOffset: 0x441, Flags: 0x11, Size: 16, Min: 0x1, Max: 0xFFFF, Step: 0x1
					Default DefaultId: 0x0 Value: 16720
				End 
				Text Prompt: "WRDD Package 2", Help: "WRDD Package 2", Text: ""
				Numeric Prompt: " Domain Type", Help: "09h: Module; 07h: WiFi/WLAN; 0Fh: WWAN; 10h WiGig; 14h: RFEM", QuestionFlags: 0x0, QuestionId: 0x285, VarStoreId: 0x1, VarOffset: 0x443, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x64, Step: 0x1
					Default DefaultId: 0x0 Value: 16
				End 
				Numeric Prompt: " Country Identifier", Help: "Country identifier as defined in ISO/IEC 3166-1 Alpha 2 code", QuestionFlags: 0x0, QuestionId: 0x286, VarStoreId: 0x1, VarOffset: 0x444, Flags: 0x11, Size: 16, Min: 0x1, Max: 0xFFFF, Step: 0x1
					Default DefaultId: 0x0 Value: 16720
				End 
				Text Prompt: "WRDS Package", Help: "WRDS Package", Text: ""
				OneOf Prompt: " WiFi SAR", Help: "Enable/Disable WiFi SAR Tx Power Limit; DISABLE - Device ignores WiFi SAR Configuration Table; ENABLE - Device uses WiFi SAR Configuration Table", QuestionFlags: 0x10, QuestionId: 0x287, VarStoreId: 0x1, VarOffset: 0x446, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x287, Value: 0x0
					Numeric Prompt: " SAR 2400 MHz Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x288, VarStoreId: 0x1, VarOffset: 0x447, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
					Numeric Prompt: " SAR 5150-5350 MHz Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x289, VarStoreId: 0x1, VarOffset: 0x448, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
					Numeric Prompt: " SAR 5350-5470 MHz Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x28A, VarStoreId: 0x1, VarOffset: 0x449, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
					Numeric Prompt: " SAR 5470-5725 MHz Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x28B, VarStoreId: 0x1, VarOffset: 0x44A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
					Numeric Prompt: " SAR 5725-5950 MHz Chain A", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x28C, VarStoreId: 0x1, VarOffset: 0x44B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
					Numeric Prompt: " SAR 2400 MHz Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x28D, VarStoreId: 0x1, VarOffset: 0x44C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
					Numeric Prompt: " SAR 5150-5350 MHz Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x28E, VarStoreId: 0x1, VarOffset: 0x44D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
					Numeric Prompt: " SAR 5350-5470 MHz Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x28F, VarStoreId: 0x1, VarOffset: 0x44E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
					Numeric Prompt: " SAR 5470-5725 MHz Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x290, VarStoreId: 0x1, VarOffset: 0x44F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
					Numeric Prompt: " SAR 5725-5950 MHz Chain B", Help: "Defines the WiFi SAR Tx Power Limit - 8bit unsigned with 5bit integer and 3bit fractional. 0x00 = 0b00000000 = 0.125dB; 0xFF = 0b11111111 = 31.875dB. Each step is equivalent to 0.125dB", QuestionFlags: 0x0, QuestionId: 0x291, VarStoreId: 0x1, VarOffset: 0x450, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
				End 
				OneOf Prompt: " Wigig RFE", Help: "Define the mode of RFE control to be used.

Disabled - Tx power shall be mandated by device OTP RFE Class

Enabled - Tx power shall be the minimum between BIOS RFE table and OTP RFE Class", QuestionFlags: 0x10, QuestionId: 0x292, VarStoreId: 0x1, VarOffset: 0x4DA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [32]
								Uint64 Value: 0x0
								Uint64 Value: 0x1
								Conditional 
							End 
						End 
					End 
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x292, Value: 0x0
					Numeric Prompt: " RFE WiGig Ch1", Help: "Defines the RFE power restriction for the relevant distance in 58.32Ghz central frequency channel", QuestionFlags: 0x0, QuestionId: 0x293, VarStoreId: 0x1, VarOffset: 0x4DB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
					Numeric Prompt: " RFE WiGig Ch2", Help: "Defines the RFE power restriction for the relevant distance in 60.48Ghz central frequency channel", QuestionFlags: 0x0, QuestionId: 0x294, VarStoreId: 0x1, VarOffset: 0x4DC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
					Numeric Prompt: " RFE WiGig Ch3", Help: "Defines the RFE power restriction for the relevant distance in 62.64Ghz central frequency channel", QuestionFlags: 0x0, QuestionId: 0x295, VarStoreId: 0x1, VarOffset: 0x4DD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
					Numeric Prompt: " RFE WiGig Ch4", Help: "Defines the RFE power restriction for the relevant distance in 64.80Ghz central frequency channel", QuestionFlags: 0x0, QuestionId: 0x296, VarStoreId: 0x1, VarOffset: 0x4DE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 0
					End 
				End 
				Numeric Prompt: " AWV Class Index", Help: "Used by WiGig driver to optimize its beamforming scheme accordingly", QuestionFlags: 0x0, QuestionId: 0x297, VarStoreId: 0x1, VarOffset: 0x4DF, Flags: 0x12, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				OneOf Prompt: "Wake On WiGig", Help: "Enable/Disable S3-S4 Wake on WiGig Docking Support", QuestionFlags: 0x10, QuestionId: 0x298, VarStoreId: 0x1, VarOffset: 0x4E5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "Enable Wireless Charge Support", Help: "Enable/Disable Wireless Charge Support.", QuestionFlags: 0x10, QuestionId: 0x299, VarStoreId: 0x1, VarOffset: 0x45F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Enable FFU Support", Help: "Enable/Disable FFU Support.", QuestionFlags: 0x10, QuestionId: 0x29A, VarStoreId: 0x1, VarOffset: 0x460, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "HID Event Filter Driver", Help: "Enables/Disables HID Event Filter Driver interface to OS.", QuestionFlags: 0x10, QuestionId: 0x29B, VarStoreId: 0x1, VarOffset: 0x4CC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [32, 4, 20, 11, 7, 19, 3, 27, 97, 98]
							Uint64 Value: 0x0
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC84, Value: 0x0
				OneOf Prompt: "SSIC_7160_7260_INIT", Help: "SSIC_7160_7260_INIT", QuestionFlags: 0x10, QuestionId: 0x29C, VarStoreId: 0x1, VarOffset: 0x4CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
					Not 
					EqIdVal QuestionId: 0xC50, Value: 0x4
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x7
					Not 
					And 
				End 
				OneOf Prompt: "Enable WWAN", Help: "Enables/Disables M.2 WWAN module. When disabled, BIOS will turn off the power to WWAN module. This will also disable GNSS", QuestionFlags: 0x10, QuestionId: 0x29D, VarStoreId: 0x1, VarOffset: 0x4D6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x7
					Not 
				End 
				OneOf Prompt: "WWAN _DSM L3 Enable/Disable", Help: "Enable/Disable _DSM L3 variable for WWAN", QuestionFlags: 0x10, QuestionId: 0x29E, VarStoreId: 0x1, VarOffset: 0x543, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x4
					Not 
					EqIdVal QuestionId: 0x29D, Value: 0x0
					Or 
				End 
				OneOf Prompt: "WWAN INTERFACE", Help: "KBL-Y RVP3 can support only PCIe or SSIC WWAN at the same time.", QuestionFlags: 0x10, QuestionId: 0x29F, VarStoreId: 0x1, VarOffset: 0x53D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [4]
								Uint64 Value: 0x0
								Uint64 Value: 0x2
								Conditional 
							End 
						End 
					End 
					SuppressIf 
						EqIdVal QuestionId: 0xC50, Value: 0x4
						OneOfOption Option: "PCIe and SSIC" Value: 0
					End 
					OneOfOption Option: "PCIe" Value: 1
					OneOfOption Option: "SSIC" Value: 2
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
					Not 
					EqIdVal QuestionId: 0x29D, Value: 0x0
					Or 
				End 
				Numeric Prompt: "Delay to wait for WWAN device to be ready before SAR reset.", Help: "Value between 0-255 seconds. Default is 8. Will result in Responsiveness impact.", QuestionFlags: 0x0, QuestionId: 0x2A0, VarStoreId: 0x1, VarOffset: 0x4D5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 8
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
					Not 
					EqIdVal QuestionId: 0xC50, Value: 0x4
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x7
					Not 
					And 
					EqIdVal QuestionId: 0x29D, Value: 0x0
					Or 
				End 
				Numeric Prompt: "Delay after Modem reset(GPP_A12)", Help: "Value between 0-10 seconds. Default is 400 ms. Will result in Responsiveness impact.", QuestionFlags: 0x10, QuestionId: 0x2A1, VarStoreId: 0x1, VarOffset: 0x51D, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 400
				End 
				Numeric Prompt: "Delay after PERST de-assert", Help: "Value between 0-10 seconds. Default is 200 ms. Will result in Responsiveness impact.", QuestionFlags: 0x10, QuestionId: 0x2A2, VarStoreId: 0x1, VarOffset: 0x521, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x2710, Step: 0x1
					Default DefaultId: 0x0 Value: 200
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x53F, Value: 0x0
				OneOf Prompt: "Type-C BSSB Mode", Help: "Mode 0: Send debug status to EC.
Mode 1: Do not send debug status to EC.", QuestionFlags: 0x10, QuestionId: 0x2A3, VarStoreId: 0x1, VarOffset: 0x4D7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Mode 0" Value: 0
					OneOfOption Option: "Mode 1" Value: 1, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC29, Value: 0x1
				Numeric Prompt: "Alternate Mode Synch Delay", Help: "Add delay to make sure display alternate mode negotiation completed. Step size for 0.1 sec, Max value 50 to 5 sec.", QuestionFlags: 0x0, QuestionId: 0x2A4, VarStoreId: 0x1, VarOffset: 0x4D9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x32, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
		End 
	End 
	Form FormId: 0x279E, Title: "Realsense 3D Camera Settings"
		Subtitle Prompt: "Realsense 3D Camera Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC50, Value: 0x1
				Not 
				EqIdVal QuestionId: 0xC50, Value: 0x2
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0x4
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0x14
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0xA
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0x1A
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0x8
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0xB
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0x7
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0x13
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0x3
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0x1B
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0x64
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0xC
				Not 
				And 
				EqIdVal QuestionId: 0xC50, Value: 0x20
				Not 
				And 
			End 
			OneOf Prompt: "RTD3 Camera Support", Help: "This option enables runtime power management support for camera", QuestionFlags: 0x10, QuestionId: 0x2A5, VarStoreId: 0x1, VarOffset: 0x3E1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC50, Value: 0x20
			OneOf Prompt: "Select Camera", Help: "Choose the camera connected to the system", QuestionFlags: 0x10, QuestionId: 0x2A6, VarStoreId: 0x1, VarOffset: 0x451, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x2, Step: 0x0
				OneOfOption Option: "Ivcam" Value: 1
				OneOfOption Option: "Double Springs" Value: 2, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2A6, Value: 0x1
				Not 
			End 
			Numeric Prompt: "Delay needed for Ivcam power on", Help: "Delay in milli seconds needed for camera power on", QuestionFlags: 0x10, QuestionId: 0x2A7, VarStoreId: 0x1, VarOffset: 0x454, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1388, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "Delay needed for Ivcam power off", Help: "Delay in milli seconds needed for camera power off", QuestionFlags: 0x10, QuestionId: 0x2A8, VarStoreId: 0x1, VarOffset: 0x456, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1388, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "Rotation", Help: "Rotation in degrees", QuestionFlags: 0x10, QuestionId: 0x2A9, VarStoreId: 0x1, VarOffset: 0x458, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
				OneOfOption Option: "0" Value: 0, Default, MfgDefault
				OneOfOption Option: "90" Value: 2
				OneOfOption Option: "180" Value: 4
				OneOfOption Option: "270" Value: 6
			End 
			OneOf Prompt: "DFU support", Help: "Enables or Disables 3D Imaging Camera DFU device.", QuestionFlags: 0x10, QuestionId: 0x2AA, VarStoreId: 0x1, VarOffset: 0x452, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Wake support", Help: "Enables or Disables 3D Imaging Camera as wake capable.", QuestionFlags: 0x10, QuestionId: 0x2AB, VarStoreId: 0x1, VarOffset: 0x453, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2A6, Value: 0x2
				Not 
			End 
			Numeric Prompt: "Delay needed for DS camera power on", Help: "Delay in milli seconds needed for camera power on", QuestionFlags: 0x10, QuestionId: 0x2AC, VarStoreId: 0x1, VarOffset: 0x459, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1388, Step: 0x0
				Default DefaultId: 0x0 Value: 250
			End 
			Numeric Prompt: "Delay needed for DS camera power off", Help: "Delay in milli seconds needed for camera power off", QuestionFlags: 0x10, QuestionId: 0x2AD, VarStoreId: 0x1, VarOffset: 0x45B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1388, Step: 0x0
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "Rotation", Help: "Rotation in degrees", QuestionFlags: 0x10, QuestionId: 0x2AE, VarStoreId: 0x1, VarOffset: 0x45D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
				OneOfOption Option: "0" Value: 0, Default, MfgDefault
				OneOfOption Option: "90" Value: 2
				OneOfOption Option: "180" Value: 4
				OneOfOption Option: "270" Value: 6
			End 
		End 
	End 
	Form FormId: 0x27B4, Title: "OverClocking Performance Menu"
		Subtitle Prompt: "OverClocking Performance Menu", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "OverClocking Feature", Help: "Performance Menu for Processor and Memory.", QuestionFlags: 0x14, QuestionId: 0x27A0, VarStoreId: 0x1, VarOffset: 0x6F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "WDT Enable", Help: "Enable/Disable WatchDog Timer. Note: This option is ignored on debug BIOS.", QuestionFlags: 0x10, QuestionId: 0x2AF, VarStoreId: 0x1, VarOffset: 0x9A9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x27A0, Value: 0x0
			SuppressIf 
				EqIdVal QuestionId: 0xC51, Value: 0x1
					Not 
				End 
				Text Prompt: "BCLK Frequency (pcode)", Help: "", Text: "100.00 MHz"
			End 
			OneOf Prompt: "XTU Interface", Help: "Enable/Disable XTU Interface. BIOS will only expose XTU interface when enabled.", QuestionFlags: 0x10, QuestionId: 0x2B0, VarStoreId: 0x1, VarOffset: 0x6F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "BCLK Aware Adaptive Voltage", Help: "BCLK Aware Adaptive Voltage enable/disable. When enabled, pcode will be aware of the BCLK frequency when calculating the CPU V/F curves. This is ideal for BCLK OC to avoid high voltage overrides. Uses OC Mailbox command 0x15.", QuestionFlags: 0x10, QuestionId: 0x2B1, VarStoreId: 0x1, VarOffset: 0x71A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x27A0, Value: 0x0
			Ref Prompt: "Processor", Help: "Processor Bus Ratio Override and Bus Speed Override.", QuestionFlags: 0x0, QuestionId: 0x2B2, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B5
			Ref Prompt: "Memory", Help: "Memory Overclocking Menu", QuestionFlags: 0x0, QuestionId: 0x2B3, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27BA
			Ref Prompt: "GT", Help: "GT Ratio Override and Delta voltage programming", QuestionFlags: 0x0, QuestionId: 0x2B4, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B7
			Ref Prompt: "Uncore", Help: "Uncore Overclocking Menu", QuestionFlags: 0x0, QuestionId: 0x2B5, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B8
			Ref Prompt: "Voltage PLL Trim Controls", Help: "Voltage PLL Trim Controls Menu", QuestionFlags: 0x0, QuestionId: 0x2B6, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27BC
			Ref Prompt: "Platform Voltage Overrides", Help: "Platform Voltages related Overclocking Menu", QuestionFlags: 0x0, QuestionId: 0x2B7, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27B9
		End 
	End 
	Form FormId: 0x27B5, Title: "Processor"
		Subtitle Prompt: "Processor", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "Core/Ring", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "  Max OC Ratio", Help: "Sets the maximum OC Ratio for the CPU Core and Ring. Uses Mailbox MSR 0x150, cmd 0x10, 0x11. Range 8-255. 0 is AUTO.", QuestionFlags: 0x14, QuestionId: 0x27A1, VarStoreId: 0x1, VarOffset: 0x6F5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		OneOf Prompt: "  Voltage Mode", Help: "Selects between Adaptive and Override Voltage modes. In Override Mode the voltage selected will be applied over all operating frequencies. In Adaptive Mode the voltage is interpolated only in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11.", QuestionFlags: 0x10, QuestionId: 0x2B8, VarStoreId: 0x1, VarOffset: 0x6F6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Adaptive" Value: 0, Default, MfgDefault
			OneOfOption Option: "Override" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2B8, Value: 0x0
			Numeric Prompt: "  Voltage Override", Help: "Specifies the Override Voltage applied to the IA Core domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range 0-2000 mV.", QuestionFlags: 0x10, QuestionId: 0x2B9, VarStoreId: 0x1, VarOffset: 0x6F7, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2B8, Value: 0x1
			Numeric Prompt: "  Extra Turbo Voltage", Help: "Specifies the extra turbo voltage applied while IA Core is operating in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11. Range 0-2000 mV", QuestionFlags: 0x10, QuestionId: 0x2BA, VarStoreId: 0x1, VarOffset: 0x6FC, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		Numeric Prompt: "  Voltage Offset", Help: "Specifies the Offset Voltage applied to the IA Core domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -500 to 500 mV", QuestionFlags: 0x10, QuestionId: 0x2BB, VarStoreId: 0x1, VarOffset: 0x6F9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [20]
						EqIdValList QuestionId: 0xC50, Values: [26, 27]
						Uint64 Value: 0x0
						Uint64 Value: 0x19
						Conditional 
						Uint64 Value: 0xA
						Conditional 
					End 
				End 
			End 
			Default DefaultId: 0x0 Value: 0
		End 
		OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x2BC, VarStoreId: 0x1, VarOffset: 0x6FB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "+" Value: 0, Default, MfgDefault
			OneOfOption Option: "-" Value: 1
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "Ring Domain", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "  Ring Down Bin", Help: "Enable/Disable Ring Downbin feature. Enabled - CPU will down bin the ring ratio, which means the requested max ring ratio may not be observed. Disable - CPU will not down bin the ring ratio and the requested ring ratio limit will be observed. Default is Enabled. Please use caution when disabling this feature as it may result in overvoltaging of the CPU. Uses OC mailbox command 0x19.", QuestionFlags: 0x10, QuestionId: 0x2BD, VarStoreId: 0x1, VarOffset: 0x727, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		Numeric Prompt: "  Ring Max Ratio", Help: "This sets the maximum ratio for the RING Domain. Uses Mailbox MSR 0x150, cmd 0x11.", QuestionFlags: 0x14, QuestionId: 0x27A2, VarStoreId: 0x1, VarOffset: 0x6FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "  Ring Min Ratio", Help: "This sets the minimum ratio for the RING Domain.", QuestionFlags: 0x14, QuestionId: 0x27A3, VarStoreId: 0x1, VarOffset: 0x70E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "AVX2 Ratio Offset", Help: "AVX2 Ratio Offset. Specifies number of bins to decrease AVX ratio vs. Core Ratio. AVX is a more stressful workload, it is helpful to lower the AVX ratio to ensure maximum possible ratio for SSE workloads. Uses Mailbox MSR 0x150, cmd 0x1B. Range 0 - 31. 0 = No offset.", QuestionFlags: 0x10, QuestionId: 0x2BE, VarStoreId: 0x1, VarOffset: 0x6FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "TjMax Offset", Help: "TjMax Offset. Specified value here is clipped by pCode (125 - TjMax Offset) to support TjMax in the range of 62 to 115 deg Celsius. Uses Mailbox MSR 0x37, command 0x01. Range 10 - 63. 0 = No offset. Only valid on CFL-S 8+2.", QuestionFlags: 0x10, QuestionId: 0x2BF, VarStoreId: 0x1, VarOffset: 0x730, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Subtitle Prompt: "Thermal Velocity Boost (TVB)", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "TVB Ratio Clipping", Help: "This service controls Core frequency reduction caused by high package temperatures for processors that implement the Intel Thermal Velocity Boost (TVB) feature. It is required to be disabled for supporting overclocking at frequencies higher than the default max turbo frequency. Default is disabled. Uses Overclocking Mailbox command 0x18/0x19.", QuestionFlags: 0x10, QuestionId: 0x2C0, VarStoreId: 0x1, VarOffset: 0x72D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "TVB Voltage Optimizations", Help: "This service controls thermal based voltage optimizations for processors that implement the Intel Thermal Velocity Boost (TVB) feature. Default is enabled. Uses Overclocking Mailbox command 0x18/0x19.", QuestionFlags: 0x10, QuestionId: 0x2C1, VarStoreId: 0x1, VarOffset: 0x72E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCBE, Value: 0x0
				EqIdVal QuestionId: 0xCBD, Value: 0x0
				Or 
			End 
			Text Prompt: "Expected CPU Freq", Help: "Expected Processor frequency calculated using Bus ratio and Bus speed.", Text: ""
			SuppressIf 
				True 
				SuppressIf 
					EqIdVal QuestionId: 0xC41, Value: 0xB
					Action Prompt: "Expected CPU Freq", Help: "Expected Processor frequency calculated using Bus ratio and Bus speed.", QuestionFlags: 0x4, QuestionId: 0x27B6, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, QuestionConfig: ""
					End 
				End 
			End 
		End 
	End 
	Form FormId: 0x27B7, Title: "GT"
		Subtitle Prompt: "GT Slice Domain", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "GT OverClocking Frequency", Help: "Overclocked RP0 Frequency (MLC Clk) in multiples of 50 MHz. Range 0-255.", QuestionFlags: 0x10, QuestionId: 0x2C2, VarStoreId: 0x1, VarOffset: 0x950, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		OneOf Prompt: "  GT Voltage Mode", Help: "Selects between Adaptive and Override Voltage modes. In Override Mode the voltage selected will be applied over all operating frequencies. In Adaptive Mode the voltage is interpolated only in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11.", QuestionFlags: 0x10, QuestionId: 0x2C3, VarStoreId: 0x1, VarOffset: 0x951, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Adaptive" Value: 0, Default, MfgDefault
			OneOfOption Option: "Override" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2C3, Value: 0x0
			Numeric Prompt: "  GT Voltage Override", Help: "Specifies the Override Voltage applied to the GT domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range 0-2000 mV", QuestionFlags: 0x10, QuestionId: 0x2C4, VarStoreId: 0x1, VarOffset: 0x955, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2C3, Value: 0x1
			Numeric Prompt: "  GT Extra Turbo Voltage", Help: "Specifies the extra turbo voltage applied while GT is operating in turbo mode. Unit is in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range 0-2000 mV", QuestionFlags: 0x10, QuestionId: 0x2C5, VarStoreId: 0x1, VarOffset: 0x957, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		Numeric Prompt: "  GT Voltage Offset", Help: "Specifies the Offset Voltage applied to the GT domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -1000 to 1000 mV", QuestionFlags: 0x10, QuestionId: 0x2C6, VarStoreId: 0x1, VarOffset: 0x952, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [20]
						EqIdValList QuestionId: 0xC50, Values: [26, 27]
						Uint64 Value: 0x0
						Uint64 Value: 0x19
						Conditional 
						Uint64 Value: 0xA
						Conditional 
					End 
				End 
			End 
			Default DefaultId: 0x0 Value: 0
		End 
		OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x2C7, VarStoreId: 0x1, VarOffset: 0x954, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "+" Value: 0, Default, MfgDefault
			OneOfOption Option: "-" Value: 1
		End 
		Subtitle Prompt: "GT Unslice Domain", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "GT OverClocking Frequency", Help: "Overclocked RP0 Frequency (MLC Clk) in multiples of 50 MHz. Range 0-255.", QuestionFlags: 0x10, QuestionId: 0x2C8, VarStoreId: 0x1, VarOffset: 0x959, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		OneOf Prompt: "  GT Voltage Mode", Help: "Selects between Adaptive and Override Voltage modes. In Override Mode the voltage selected will be applied over all operating frequencies. In Adaptive Mode the voltage is interpolated only in turbo mode. Uses Mailbox MSR 0x150, cmd 0x10, 0x11.", QuestionFlags: 0x10, QuestionId: 0x2C9, VarStoreId: 0x1, VarOffset: 0x95A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Adaptive" Value: 0, Default, MfgDefault
			OneOfOption Option: "Override" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2C9, Value: 0x0
			Numeric Prompt: "  GT Voltage Override", Help: "Specifies the Override Voltage applied to the GT domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range 0-2000 mV", QuestionFlags: 0x10, QuestionId: 0x2CA, VarStoreId: 0x1, VarOffset: 0x95E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2C9, Value: 0x1
			Numeric Prompt: "  GT Extra Turbo Voltage", Help: "Specifies the extra turbo voltage applied while GT is operating in turbo mode. Unit is in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range 0-2000 mV", QuestionFlags: 0x10, QuestionId: 0x2CB, VarStoreId: 0x1, VarOffset: 0x960, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x7D0, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		Numeric Prompt: "  GTU Voltage Offset", Help: "Specifies the Offset Voltage applied to the GT domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -1000 to 1000 mV", QuestionFlags: 0x10, QuestionId: 0x2CC, VarStoreId: 0x1, VarOffset: 0x95B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [20]
						EqIdValList QuestionId: 0xC50, Values: [26, 27]
						Uint64 Value: 0x0
						Uint64 Value: 0x19
						Conditional 
						Uint64 Value: 0xA
						Conditional 
					End 
				End 
			End 
			Default DefaultId: 0x0 Value: 0
		End 
		OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x2CD, VarStoreId: 0x1, VarOffset: 0x95D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "+" Value: 0, Default, MfgDefault
			OneOfOption Option: "-" Value: 1
		End 
	End 
	Form FormId: 0x27B8, Title: "Uncore"
		Subtitle Prompt: "Uncore", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "Uncore Voltage Offset", Help: "Specifies the Offset Voltage applied to the Uncore domain. This voltage is specified in millivolts. Uses Mailbox MSR 0x150, cmd 0x11. Range -1000 to 1000 mV", QuestionFlags: 0x10, QuestionId: 0x2CE, VarStoreId: 0x1, VarOffset: 0x94A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		OneOf Prompt: "  Offset Prefix", Help: "Sets the offset value as positive or negative.", QuestionFlags: 0x10, QuestionId: 0x2CF, VarStoreId: 0x1, VarOffset: 0x94C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "+" Value: 0, Default, MfgDefault
			OneOfOption Option: "-" Value: 1
		End 
	End 
	Form FormId: 0x27B9, Title: "Platform Voltage Overrides"
		Subtitle Prompt: "Platform Voltage Overrides", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "VccCore Override Enable", Help: "Overrides the VccCore voltage using SMBUS/PMBUS interface of VRM. Use the next option for exact voltage configuration", QuestionFlags: 0x10, QuestionId: 0x2D0, VarStoreId: 0x1, VarOffset: 0x73B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2D0, Value: 0x0
			Numeric Prompt: "  VccCore", Help: "Range of VccCore voltage - Up to 2550 mV. Default is 1300 mV", QuestionFlags: 0x10, QuestionId: 0x2D1, VarStoreId: 0x1, VarOffset: 0x73C, Flags: 0x11, Size: 16, Min: 0x320, Max: 0x9F6, Step: 0xA
				Default DefaultId: 0x0 Value: 1300
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "VccST Override Enable", Help: "Overrides the VccST voltage using SMBUS/PMBUS interface of VRM. Use the next option for exact voltage configuration", QuestionFlags: 0x10, QuestionId: 0x2D2, VarStoreId: 0x1, VarOffset: 0x73E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2D2, Value: 0x0
			Numeric Prompt: "  VccST", Help: "Range of VccST voltage - 250 mV to 1500 mV. Default is 1020 mV", QuestionFlags: 0x10, QuestionId: 0x2D3, VarStoreId: 0x1, VarOffset: 0x73F, Flags: 0x11, Size: 16, Min: 0xFA, Max: 0x5DC, Step: 0xA
				Default DefaultId: 0x0 Value: 1020
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "VccSA Override Enable", Help: "Overrides the VccSA voltage using SMBUS/PMBUS interface of VRM. Use the next option for exact voltage configuration", QuestionFlags: 0x10, QuestionId: 0x2D4, VarStoreId: 0x1, VarOffset: 0x742, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2D4, Value: 0x0
			Numeric Prompt: "  VccSA", Help: "Range of VccSA voltage - Up to 1500 mV. Default is 1050 mV", QuestionFlags: 0x10, QuestionId: 0x2D5, VarStoreId: 0x1, VarOffset: 0x743, Flags: 0x11, Size: 16, Min: 0xFA, Max: 0x5F0, Step: 0xA
				Default DefaultId: 0x0 Value: 1050
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "VccSFR_OC Override Enable", Help: "Overrides the VccSFR_OC voltage using SMBUS/PMBUS interface of VRM. Use the next option for exact voltage configuration", QuestionFlags: 0x10, QuestionId: 0x2D6, VarStoreId: 0x1, VarOffset: 0x745, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2D6, Value: 0x0
			Numeric Prompt: "  VccSFR_OC", Help: "Range of VccSFR_OC voltage range - 1000mV to 2520mV. Default is 1250mV", QuestionFlags: 0x10, QuestionId: 0x2D7, VarStoreId: 0x1, VarOffset: 0x746, Flags: 0x11, Size: 16, Min: 0x3E8, Max: 0x9D8, Step: 0xA
				Default DefaultId: 0x0 Value: 1250
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "VccSFR Override Enable", Help: "Overrides the VccSFR voltage using SMBUS/PMBUS interface of VRM. Use the next option for exact voltage configuration", QuestionFlags: 0x10, QuestionId: 0x2D8, VarStoreId: 0x1, VarOffset: 0x749, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2D8, Value: 0x0
			Numeric Prompt: "  VccSFR", Help: "Range of VccSFR voltage - 690mV to 2050mV. Default is 1020mV", QuestionFlags: 0x10, QuestionId: 0x2D9, VarStoreId: 0x1, VarOffset: 0x74A, Flags: 0x11, Size: 16, Min: 0x2B2, Max: 0x802, Step: 0xA
				Default DefaultId: 0x0 Value: 1020
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "VccIO Override Enable", Help: "Overrides the VccIO voltage using SMBUS/PMBUS interface of VRM. Use the next option for exact voltage configuration", QuestionFlags: 0x10, QuestionId: 0x2DA, VarStoreId: 0x1, VarOffset: 0x74D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x2DA, Value: 0x0
			Numeric Prompt: "  VccIO", Help: "Range of VccIO voltage - 900 mV to 1520 mV. Default is 950 mV", QuestionFlags: 0x10, QuestionId: 0x2DB, VarStoreId: 0x1, VarOffset: 0x74E, Flags: 0x11, Size: 16, Min: 0x384, Max: 0x5F0, Step: 0x5
				Default DefaultId: 0x0 Value: 950
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Core VR Loadline Override", Help: "Overrides the Core VR DC Loadline. Use the next option for exact voltage configuration", QuestionFlags: 0x10, QuestionId: 0x2DC, VarStoreId: 0x1, VarOffset: 0x751, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x2DC, Value: 0x0
			OneOf Prompt: "  DC Loadline value", Help: "DC Loadline value as 2100 then override matches to 0xC produces the same value as without override (2.1mOhm).", QuestionFlags: 0x10, QuestionId: 0x2DD, VarStoreId: 0x1, VarOffset: 0x752, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: " -100 uOhm" Value: 0
				OneOfOption Option: "    0 uOhm" Value: 1
				OneOfOption Option: "  100 uOhm" Value: 2
				OneOfOption Option: "  700 uOhm" Value: 3
				OneOfOption Option: "  900 uOhm" Value: 4
				OneOfOption Option: " 1000 uOhm" Value: 5
				OneOfOption Option: " 1200 uOhm" Value: 6
				OneOfOption Option: " 1300 uOhm" Value: 7
				OneOfOption Option: " 1400 uOhm" Value: 8
				OneOfOption Option: " 1500 uOhm" Value: 9
				OneOfOption Option: " 1700 uOhm" Value: 10
				OneOfOption Option: " 1800 uOhm" Value: 11
				OneOfOption Option: " 2100 uOhm" Value: 12, Default, MfgDefault
			End 
		End 
	End 
	Form FormId: 0x27BA, Title: "Memory Overclocking Menu"
		SuppressIf 
			EqIdVal QuestionId: 0xC8C, Value: 0x4
			Text Prompt: "Memory Profile:", Help: "", Text: "Default  Custom    XMP1    XMP2"
			Text Prompt: "  tCK [MHz]", Help: "", Text: "0000000 0000000 0000000 0000000"
			Text Prompt: "  tCL", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  tRCD/tRP", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  tRAS", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  tCWL", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  tFAW", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  tREFI", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  tRFC", Help: "", Text: "  00000   00000   00000   00000"
			SuppressIf 
				EqIdVal QuestionId: 0xCBB, Value: 0x0
				Text Prompt: "  tRRD", Help: "", Text: "  00000   00000   00000   00000"
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCBB, Value: 0x0
					Not 
				End 
				Text Prompt: "  tRRD_L", Help: "", Text: "  00000   00000   00000   00000"
				Text Prompt: "  tRRD_S", Help: "", Text: "  00000   00000   00000   00000"
			End 
			Text Prompt: "  tRTP", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  tWR", Help: "", Text: "  00000   00000   00000   00000"
			SuppressIf 
				EqIdVal QuestionId: 0xCBB, Value: 0x0
				Text Prompt: "  tWTR", Help: "", Text: "  00000   00000   00000   00000"
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCBB, Value: 0x0
					Not 
				End 
				Text Prompt: "  tWTR_L", Help: "", Text: "  00000   00000   00000   00000"
				Text Prompt: "  tWTR_S", Help: "", Text: "  00000   00000   00000   00000"
			End 
			Text Prompt: "  NMode", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  VDD [mV]", Help: "", Text: "  00000   00000   00000   00000"
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "Realtime Memory Timing", Help: "Enable/Disable realtime memory timings. When enabled, the system will allow performing realtime memory timing changes after MRC_DONE.", QuestionFlags: 0x10, QuestionId: 0x2DE, VarStoreId: 0x1, VarOffset: 0x975, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Memory profile", Help: "Select DIMM timing profile. The below values start with the currently running values and don't auto populate.", QuestionFlags: 0x14, QuestionId: 0x27A4, VarStoreId: 0x1, VarOffset: 0x8AE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Default profile" Value: 0, Default, MfgDefault
				OneOfOption Option: "Custom profile" Value: 1
				SuppressIf 
					EqIdVal QuestionId: 0xCBC, Value: 0x1
						EqIdVal QuestionId: 0xCBC, Value: 0x3
						Or 
						Not 
					End 
					OneOfOption Option: "XMP profile 1" Value: 2
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xCBC, Value: 0x2
						EqIdVal QuestionId: 0xCBC, Value: 0x3
						Or 
						Not 
					End 
					OneOfOption Option: "XMP profile 2" Value: 3
				End 
			End 
		End 
		Ref Prompt: "Turn Around Timing", Help: "Knobs to override default timings.  0 is no override.", QuestionFlags: 0x0, QuestionId: 0x2DF, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27BB
		GrayOutIf 
			EqIdVal QuestionId: 0x27A4, Value: 0x1
				Not 
			End 
			OneOf Prompt: "Memory Reference Clock", Help: "Automatic, 100MHz, 133MHz.", QuestionFlags: 0x10, QuestionId: 0x2E0, VarStoreId: 0x1, VarOffset: 0x7A0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Auto" Value: 0
				OneOfOption Option: "133" Value: 1, Default, MfgDefault
				OneOfOption Option: "100" Value: 2
			End 
			OneOf Prompt: "Memory Ratio", Help: "Automatic or the frequency will equal ratio times reference clock. Set to Auto to recalculate memory timings listed below.", QuestionFlags: 0x10, QuestionId: 0x2E1, VarStoreId: 0x1, VarOffset: 0x7A2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "3" Value: 3
				OneOfOption Option: "4" Value: 4
				OneOfOption Option: "5" Value: 5
				OneOfOption Option: "6" Value: 6
				OneOfOption Option: "7" Value: 7
				OneOfOption Option: "8" Value: 8
				OneOfOption Option: "9" Value: 9
				OneOfOption Option: "10" Value: 10
				OneOfOption Option: "11" Value: 11
				OneOfOption Option: "12" Value: 12
				OneOfOption Option: "13" Value: 13
				OneOfOption Option: "14" Value: 14
				OneOfOption Option: "15" Value: 15
				OneOfOption Option: "16" Value: 16
				OneOfOption Option: "17" Value: 17
				OneOfOption Option: "18" Value: 18
				OneOfOption Option: "19" Value: 19
				OneOfOption Option: "20" Value: 20
				OneOfOption Option: "21" Value: 21
				OneOfOption Option: "22" Value: 22
				OneOfOption Option: "23" Value: 23
				OneOfOption Option: "24" Value: 24
				OneOfOption Option: "25" Value: 25
				OneOfOption Option: "26" Value: 26
				OneOfOption Option: "27" Value: 27
				OneOfOption Option: "28" Value: 28
				OneOfOption Option: "29" Value: 29
				OneOfOption Option: "30" Value: 30
				OneOfOption Option: "31" Value: 31
			End 
			OneOf Prompt: "QCLK Odd Ratio", Help: "Adds 133 or 100 MHz to QCLK frequency, depending on RefClk", QuestionFlags: 0x10, QuestionId: 0x2E2, VarStoreId: 0x1, VarOffset: 0x7A3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "  tCL", Help: "CAS Latency, 0: AUTO, max: 31", QuestionFlags: 0x14, QuestionId: 0x27A5, VarStoreId: 0x1, VarOffset: 0x7A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "  tRCD/tRP", Help: "RAS to CAS delay time and Row Precharge delay time, 0: AUTO, max: 63", QuestionFlags: 0x14, QuestionId: 0x27A6, VarStoreId: 0x1, VarOffset: 0x7AA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "  tRAS", Help: "RAS Active Time, 0: AUTO, max: 64", QuestionFlags: 0x14, QuestionId: 0x27A7, VarStoreId: 0x1, VarOffset: 0x7A8, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x40, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "  tCWL", Help: "Min CAS Write Latency Delay Time, 0: AUTO, max: 20", QuestionFlags: 0x14, QuestionId: 0x27A8, VarStoreId: 0x1, VarOffset: 0x7A5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "  tFAW", Help: "Min Four Activate Window Delay Time, 0: AUTO, max: 63", QuestionFlags: 0x14, QuestionId: 0x27A9, VarStoreId: 0x1, VarOffset: 0x7A6, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "  tREFI", Help: "Refresh Interval, 0: AUTO, max: 65535", QuestionFlags: 0x14, QuestionId: 0x27AA, VarStoreId: 0x1, VarOffset: 0x7AB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "  tRFC", Help: "Min Refresh Recovery Delay Time, 0: AUTO, max: 1023", QuestionFlags: 0x14, QuestionId: 0x27AB, VarStoreId: 0x1, VarOffset: 0x7AD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCBB, Value: 0x0
				Numeric Prompt: "  tRRD", Help: "Min Row Active to Row Active Delay Time, 0: AUTO, max: 31", QuestionFlags: 0x14, QuestionId: 0x27AC, VarStoreId: 0x1, VarOffset: 0x7AF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCBB, Value: 0x0
					Not 
				End 
				Numeric Prompt: "  tRRD_L", Help: "Min Row Active to Row Active Delay Time for Same Bank Group, 0: AUTO, max: 31", QuestionFlags: 0x14, QuestionId: 0x27AD, VarStoreId: 0x1, VarOffset: 0x78C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "  tRRD_S", Help: "Min Row Active to Row Active Delay Time for Different Bank Group, 0: AUTO, max: 31", QuestionFlags: 0x14, QuestionId: 0x27AE, VarStoreId: 0x1, VarOffset: 0x78D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Numeric Prompt: "  tRTP", Help: "Min Internal Read to Precharge Command Delay Time. Shall be set to half of tWR value, 0: AUTO, max: 15. DDR4 legal values: 5, 6, 7, 8, 9, 10, 12", QuestionFlags: 0x14, QuestionId: 0x27AF, VarStoreId: 0x1, VarOffset: 0x7B0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "  tWR", Help: "Min Write Recovery Time, 0: AUTO, legal values: 5, 6, 7, 8, 10, 12, 14, 16, 18, 20, 24", QuestionFlags: 0x10, QuestionId: 0x2E3, VarStoreId: 0x1, VarOffset: 0x7B1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x18, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "5" Value: 5
				OneOfOption Option: "6" Value: 6
				OneOfOption Option: "7" Value: 7
				OneOfOption Option: "8" Value: 8
				OneOfOption Option: "10" Value: 10
				OneOfOption Option: "12" Value: 12
				OneOfOption Option: "14" Value: 14
				OneOfOption Option: "16" Value: 16
				OneOfOption Option: "18" Value: 18
				OneOfOption Option: "20" Value: 20
				OneOfOption Option: "24" Value: 24
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCBB, Value: 0x0
				Numeric Prompt: "  tWTR", Help: "Min Internal Write to Read Command Delay Time, 0: AUTO, max: 28", QuestionFlags: 0x14, QuestionId: 0x27B0, VarStoreId: 0x1, VarOffset: 0x7B2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1C, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xCBB, Value: 0x0
					Not 
				End 
				Numeric Prompt: "  tWTR_L", Help: "Min Internal Write to Read Command Delay Time for Same Bank Group, 0: AUTO, max: 60", QuestionFlags: 0x14, QuestionId: 0x27B1, VarStoreId: 0x1, VarOffset: 0x78E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3C, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "  tWTR_S", Help: "Min Internal Write to Read Command Delay Time for Different Bank Group, 0: AUTO, max: 28", QuestionFlags: 0x14, QuestionId: 0x27B2, VarStoreId: 0x1, VarOffset: 0x78F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1C, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			OneOf Prompt: "Memory Voltage", Help: "Memory Voltage Override (Vddq). Default = no override", QuestionFlags: 0x10, QuestionId: 0x2E4, VarStoreId: 0x1, VarOffset: 0x797, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x672, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "1.10 Volts" Value: 1100
				OneOfOption Option: "1.15 Volts" Value: 1150
				OneOfOption Option: "1.20 Volts" Value: 1200
				OneOfOption Option: "1.25 Volts" Value: 1250
				OneOfOption Option: "1.30 Volts" Value: 1300
				OneOfOption Option: "1.35 Volts" Value: 1350
				OneOfOption Option: "1.40 Volts" Value: 1400
				OneOfOption Option: "1.45 Volts" Value: 1450
				OneOfOption Option: "1.50 Volts" Value: 1500
				OneOfOption Option: "1.55 Volts" Value: 1550
				OneOfOption Option: "1.60 Volts" Value: 1600
				OneOfOption Option: "1.65 Volts" Value: 1650
			End 
		End 
		Numeric Prompt: "NMode", Help: "System command rate, range 0-2, 0 means AUTO, 1 = 1N, 2 = 2N", QuestionFlags: 0x14, QuestionId: 0x27B3, VarStoreId: 0x1, VarOffset: 0x7B3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x27B3, Value: 0x1
				Not 
			End 
			OneOf Prompt: "Command Rate Support", Help: "CMD Rate and Limit Support Option. NOTE: ONLY supported in 1N Mode", QuestionFlags: 0x10, QuestionId: 0x2E5, VarStoreId: 0x1, VarOffset: 0x794, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "1 CMD" Value: 1
				OneOfOption Option: "2 CMDs" Value: 2
				OneOfOption Option: "3 CMDs" Value: 3, Default, MfgDefault
				OneOfOption Option: "4 CMDs" Value: 4
				OneOfOption Option: "5 CMDs" Value: 5
				OneOfOption Option: "6 CMDs" Value: 6
				OneOfOption Option: "7 CMDs" Value: 7
			End 
		End 
		Numeric Prompt: "DllBwEn[0]", Help: "DllBwEn[0], for 1067 (0..7)", QuestionFlags: 0x0, QuestionId: 0x2E6, VarStoreId: 0x1, VarOffset: 0x79B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "DllBwEn[1]", Help: "DllBwEn[1], for 1333 (0..7)", QuestionFlags: 0x0, QuestionId: 0x2E7, VarStoreId: 0x1, VarOffset: 0x79C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
			Default DefaultId: 0x0 Value: 1
		End 
		Numeric Prompt: "DllBwEn[2]", Help: "DllBwEn[2], for 1600 (0..7)", QuestionFlags: 0x0, QuestionId: 0x2E8, VarStoreId: 0x1, VarOffset: 0x79D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "DllBwEn[3]", Help: "DllBwEn[3], for 1867 and up (0..7)", QuestionFlags: 0x0, QuestionId: 0x2E9, VarStoreId: 0x1, VarOffset: 0x79E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Text Prompt: "VDD", Help: "", Text: "N/A"
	End 
	Form FormId: 0x27BB, Title: "Turn Around Timing"
		Text Prompt: "Current Turn Around Times", Help: "", Text: "     SG      DG      DR      DD"
		SuppressIf 
			EqIdVal QuestionId: 0xC9C, Value: 0x0
				EqIdVal QuestionId: 0xC9B, Value: 0x0
				And 
			End 
			Text Prompt: "Channel 0", Help: "", Text: ""
			Text Prompt: "  Read-to-Read  ", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  Read-to-Write ", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  Write-to-Read ", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  Write-to-Write", Help: "", Text: "  00000   00000   00000   00000"
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC9A, Value: 0x0
				EqIdVal QuestionId: 0xC99, Value: 0x0
				And 
			End 
			Text Prompt: "Channel 1", Help: "", Text: ""
			Text Prompt: "  Read-to-Read  ", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  Read-to-Write ", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  Write-to-Read ", Help: "", Text: "  00000   00000   00000   00000"
			Text Prompt: "  Write-to-Write", Help: "", Text: "  00000   00000   00000   00000"
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "tRd2RdSG", Help: "Delay between Read-to-Read commands in the same Bank Group. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2EA, VarStoreId: 0x1, VarOffset: 0x978, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "tRd2RdDG", Help: "Delay between Read-to-Read commands in different Bank Group for DDR4. All other DDR technologies should set this equal to SG. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2EB, VarStoreId: 0x1, VarOffset: 0x979, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "tRd2RdDR", Help: "Delay between Read-to-Read commands in different Ranks. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2EC, VarStoreId: 0x1, VarOffset: 0x97A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "tRd2RdDD", Help: "Delay between Read-to-Read commands in different DIMMs. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2ED, VarStoreId: 0x1, VarOffset: 0x97B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "tRd2WrSG", Help: "Delay between Read-to-Write commands in the same Bank Group. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2EE, VarStoreId: 0x1, VarOffset: 0x984, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "tRd2WrDG", Help: "Delay between Read-to-Write commands in different Bank Group for DDR4. All other DDR technologies should set this equal to SG. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2EF, VarStoreId: 0x1, VarOffset: 0x985, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "tRd2WrDR", Help: "Delay between Read-to-Write commands in different Ranks. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2F0, VarStoreId: 0x1, VarOffset: 0x986, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "tRd2WrDD", Help: "Delay between Read-to-Write commands in different DIMMs. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2F1, VarStoreId: 0x1, VarOffset: 0x987, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "tWr2RdSG", Help: "Delay between Write-to-Read commands in the same Bank Group. 0-Auto, Range 4-86.", QuestionFlags: 0x10, QuestionId: 0x2F2, VarStoreId: 0x1, VarOffset: 0x97C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x56, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "tWr2RdDG", Help: "Delay between Write-to-Read commands in different Bank Group for DDR4. All other DDR technologies should set this equal to SG. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2F3, VarStoreId: 0x1, VarOffset: 0x97D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "tWr2RdDR", Help: "Delay between Write-to-Read commands in different Ranks. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2F4, VarStoreId: 0x1, VarOffset: 0x97E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "tWr2RdDD", Help: "Delay between Write-to-Read commands in different DIMMs. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2F5, VarStoreId: 0x1, VarOffset: 0x97F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "tWr2WrSG", Help: "Delay between Write-to-Write commands in the same Bank Group. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2F6, VarStoreId: 0x1, VarOffset: 0x980, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "tWr2WrDG", Help: "Delay between Write-to-Write commands in different Bank Group for DDR4. All other DDR technologies should set this equal to SG. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2F7, VarStoreId: 0x1, VarOffset: 0x981, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "tWr2WrDR", Help: "Delay between Write-to-Write commands in different Ranks. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2F8, VarStoreId: 0x1, VarOffset: 0x982, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "tWr2WrDD", Help: "Delay between Write-to-Write commands in different DIMMs. 0-Auto, Range 4-54.", QuestionFlags: 0x10, QuestionId: 0x2F9, VarStoreId: 0x1, VarOffset: 0x983, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x36, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
	End 
	Form FormId: 0x27BC, Title: "Voltage PLL Trim Controls"
		Subtitle Prompt: "Voltage PLL Trim Controls", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "Core PLL Voltage Offset", Help: "PLL Voltage Offset, Range 0-63. Units are in 17.5mV. Default is 0. This control can be used to increase the range of this domain frequency in extreme overclocking conditions.", QuestionFlags: 0x10, QuestionId: 0x2FA, VarStoreId: 0x1, VarOffset: 0x711, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "GT PLL Voltage Offset", Help: "PLL Voltage Offset, Range 0-63. Units are in 17.5mV. Default is 0. This control can be used to increase the range of this domain frequency in extreme overclocking conditions.", QuestionFlags: 0x10, QuestionId: 0x2FB, VarStoreId: 0x1, VarOffset: 0x729, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Ring PLL Voltage Offset", Help: "PLL Voltage Offset, Range 0-63. Units are in 17.5mV. Default is 0. This control can be used to increase the range of this domain frequency in extreme overclocking conditions.", QuestionFlags: 0x10, QuestionId: 0x2FC, VarStoreId: 0x1, VarOffset: 0x72A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "System Agent PLL Voltage Offset", Help: "PLL Voltage Offset, Range 0-63. Units are in 17.5mV. Default is 0. This control can be used to increase the range of this domain frequency in extreme overclocking conditions.", QuestionFlags: 0x10, QuestionId: 0x2FD, VarStoreId: 0x1, VarOffset: 0x72B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Memory Controller PLL Voltage Offset", Help: "PLL Voltage Offset, Range 0-63. Units are in 17.5mV. Default is 0. This control can be used to increase the range of this domain frequency in extreme overclocking conditions.", QuestionFlags: 0x10, QuestionId: 0x2FE, VarStoreId: 0x1, VarOffset: 0x72C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
	End 
	Form FormId: 0x27BE, Title: "AMT Configuration"
		OneOf Prompt: "ASF support", Help: "Enable/Disable Alert Standard Format support.", QuestionFlags: 0x10, QuestionId: 0x2FF, VarStoreId: 0x1, VarOffset: 0x777, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "USB Provisioning of AMT", Help: "Enable/Disable of AMT USB Provisioning.", QuestionFlags: 0x10, QuestionId: 0x300, VarStoreId: 0x1, VarOffset: 0x775, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		Ref Prompt: "CIRA Configuration", Help: "Configure Remote Assistance Process parameters.", QuestionFlags: 0x0, QuestionId: 0x301, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27BF
		GrayOutIf 
			EqIdVal QuestionId: 0x2FF, Value: 0x0
			Ref Prompt: "ASF Configuration", Help: "Configure Alert Standard Format parameters.", QuestionFlags: 0x0, QuestionId: 0x302, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27C0
			Ref Prompt: "Secure Erase Configuration", Help: "Secure Erase configuration menu", QuestionFlags: 0x0, QuestionId: 0x303, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27C1
		End 
		Ref Prompt: "OEM Flags Settings", Help: "Configure OEM Flags", QuestionFlags: 0x0, QuestionId: 0x304, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27C2
		Ref Prompt: "MEBx Resolution Settings", Help: "Resolution settings for MEBx display modes", QuestionFlags: 0x0, QuestionId: 0x305, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27C3
	End 
	Form FormId: 0x27BF, Title: "CIRA Configuration"
		CheckBox Prompt: "Activate Remote Assistance Process", Help: "Trigger CIRA boot

Note:
Network Access must be activated first from MEBx Setup.", QuestionFlags: 0x10, QuestionId: 0x306, VarStoreId: 0x1, VarOffset: 0x773, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x306, Value: 0x0
			Numeric Prompt: "CIRA Timeout", Help: "OEM defined timeout for MPS connection to be established.
  0 - use the default timeout value of 60 seconds. 
  255 - MEBx waits until the connection succeeds", QuestionFlags: 0x10, QuestionId: 0x307, VarStoreId: 0x1, VarOffset: 0x774, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
	End 
	Form FormId: 0x27C0, Title: "ASF Configuration"
		OneOf Prompt: "PET Progress", Help: "Enable/Disable PET Events Progress to receive PET Events.", QuestionFlags: 0x10, QuestionId: 0x308, VarStoreId: 0x1, VarOffset: 0x776, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "WatchDog", Help: "Enable/Disable WatchDog Timer.", QuestionFlags: 0x10, QuestionId: 0x309, VarStoreId: 0x1, VarOffset: 0x778, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x309, Value: 0x0
			Numeric Prompt: "OS Timer", Help: "Set OS watchdog timer.", QuestionFlags: 0x0, QuestionId: 0x30A, VarStoreId: 0x1, VarOffset: 0x779, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "BIOS Timer", Help: "Set BIOS watchdog timer.", QuestionFlags: 0x0, QuestionId: 0x30B, VarStoreId: 0x1, VarOffset: 0x77B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
	End 
	Form FormId: 0x27C1, Title: "Secure Erase Configuration"
		OneOf Prompt: "Secure Erase mode", Help: "Change Secure Erase module behavior:
Simulated: Performs SE flow without erasing SSD
Real: Erase SSD.", QuestionFlags: 0x0, QuestionId: 0x30C, VarStoreId: 0x1, VarOffset: 0x4CA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Simulated" Value: 0, Default
			OneOfOption Option: "Real" Value: 1
		End 
		OneOf Prompt: "Force Secure Erase", Help: "Force Secure Erase on next boot", QuestionFlags: 0x10, QuestionId: 0x30D, VarStoreId: 0x1, VarOffset: 0x4CB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
	End 
	Form FormId: 0x27C2, Title: "OEM Flags Settings"
		CheckBox Prompt: "MEBx hotkey Pressed", Help: "OEMFLag Bit 1:
Enable automatic MEBx hotkey press.", QuestionFlags: 0x10, QuestionId: 0x30E, VarStoreId: 0x1, VarOffset: 0x76E, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: "MEBx Selection Screen", Help: "OEMFLag Bit 2:
Enable MEBx selection screen with 2 options:
Press 1 to enter ME Configuration Screens
Press 2 to initiate a remote connection
Note:

Network Access must be activated from MEBx Setup for this screen to be displayed.", QuestionFlags: 0x10, QuestionId: 0x30F, VarStoreId: 0x1, VarOffset: 0x76F, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: "Hide Unconfigure ME Confirmation Prompt", Help: "OEMFlag Bit 6:
Hide Unconfigure ME confirmation prompt when attempting ME unconfiguration.", QuestionFlags: 0x10, QuestionId: 0x310, VarStoreId: 0x1, VarOffset: 0x770, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: "MEBx OEM Debug Menu Enable", Help: "OEMFlag Bit 14:
Enable OEM debug menu in MEBx.", QuestionFlags: 0x0, QuestionId: 0x311, VarStoreId: 0x1, VarOffset: 0x771, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: "Unconfigure ME", Help: "OEMFlag Bit 15:
Unconfigure ME with resetting MEBx password to default.", QuestionFlags: 0x10, QuestionId: 0x312, VarStoreId: 0x1, VarOffset: 0x772, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
	End 
	Form FormId: 0x27C3, Title: "MEBx Resolution Settings"
		OneOf Prompt: "Non-UI Mode Resolution", Help: "Resolution for non-UI text mode.", QuestionFlags: 0x0, QuestionId: 0x313, VarStoreId: 0x1, VarOffset: 0x77D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
			OneOfOption Option: "80x25" Value: 1
			OneOfOption Option: "100x31" Value: 2
		End 
		OneOf Prompt: "UI Mode Resolution", Help: "Resolution for UI text mode.", QuestionFlags: 0x0, QuestionId: 0x314, VarStoreId: 0x1, VarOffset: 0x77E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
			OneOfOption Option: "80x25" Value: 1
			OneOfOption Option: "100x31" Value: 2
		End 
		OneOf Prompt: "Graphics Mode Resolution", Help: "Resolution for graphics mode.", QuestionFlags: 0x0, QuestionId: 0x315, VarStoreId: 0x1, VarOffset: 0x77F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
			OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
			OneOfOption Option: "640x480" Value: 1
			OneOfOption Option: "800x600" Value: 2
			OneOfOption Option: "1024x768" Value: 3
		End 
	End 
	Form FormId: 0x27CA, Title: "Intel ICC"
		OneOf Prompt: "ICC/OC Watchdog Timer", Help: "When enabled, the ICC/OC watchdog timer is exposed to OS as an ACPI device. WDT HW is always used by BIOS when clock settings are changed.", QuestionFlags: 0x10, QuestionId: 0x316, VarStoreId: 0x1, VarOffset: 0x4BF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x322, Value: 0x0
			OneOf Prompt: "ICC Locks after EOP", Help: "Specifies the ICC registers that can be written after end-of-post. Default - Dynamic registers for runtime clock adjustments are left writeable. All Locked - No clock register adjustments allowed after EOP. All Unlocked - All ICC registers can be written after EOP.", QuestionFlags: 0x10, QuestionId: 0x317, VarStoreId: 0x16, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default
				OneOfOption Option: "All Locked" Value: 1
				OneOfOption Option: "All Unlocked" Value: 2
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x321, Value: 0x0
			Numeric Prompt: "ICC Profile", Help: "Select clock profile that corresponds to the platform configuration. Profiles are defined by the OEM and platform capabilites. Tpically, profile 0 has failsafe settings. Other profiles correspond to WiMax, 3G, or Overclocking settings.", QuestionFlags: 0x14, QuestionId: 0x27C4, VarStoreId: 0x16, VarOffset: 0xD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC51, Value: 0x2
				Not 
			End 
			OneOf Prompt: "ICC PLL Shutdown", Help: "This option controls the programming of the ICC PLL shutdown flow. When enabled, this ICC PM register will be programmed on every non-Sx boot.", QuestionFlags: 0x10, QuestionId: 0x318, VarStoreId: 0x1, VarOffset: 0x4C4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x322, Value: 0x0
				EqIdVal QuestionId: 0x31B, Value: 0x0
				Or 
			End 
			Subtitle Prompt: "DMI CLOCK placeholder for clock 2 title", Help: "", Flags: 0x0
			End 
			Text Prompt: "    Default Clock Settings", Help: "", Text: "100.00MHz 0.50% Downspread"
			Text Prompt: "    Frequency Range Limits", Help: "", Text: "uninitialized MHz"
			Text Prompt: "    Maximum Spread %", Help: "", Text: "uninitialized %"
			Text Prompt: "    Spread Mode Adjustments", Help: "", Text: "Uninitialized"
			SuppressIf 
				EqIdVal QuestionId: 0x31D, Value: 0x0
				Numeric Prompt: "    Clock Frequency", Help: "Frequency in 10kHz increments. Specifies new BCLK frequency to be applied. Frequency is rounded to nearest valid value. Allowed range is limited by the Max/Min supported frequencies. Changes are not applied until settings are saved and platform resets. Example: For 125.70MHz, enter 12570.", QuestionFlags: 0x14, QuestionId: 0x27C5, VarStoreId: 0x16, VarOffset: 0x2, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				OneOf Prompt: "    Bclk Change Permanent", Help: "Changes how the BCLK frequency changes are applied permanent with warm reset. 0 - Disabled. 1 - Enabled.", QuestionFlags: 0x10, QuestionId: 0x319, VarStoreId: 0x1, VarOffset: 0x976, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1, Default
					OneOfOption Option: "Disabled" Value: 0
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x319, Value: 0x1
					OneOf Prompt: "    Bclk Change w/o Reset", Help: "Changes how the BCLK frequency changes are applied. 0 - Realtime. 1 - Permanent, without warm reset. NOTE: Realtime changes will be applied when 'F4' hotkey is pressed. Uses MEI SET_CLOCK_SETTINGS command 0x1B.", QuestionFlags: 0x0, QuestionId: 0x31A, VarStoreId: 0x1, VarOffset: 0x977, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Real Time change" Value: 0, Default
						OneOfOption Option: "Permanent, no warm reset" Value: 1
					End 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x31B, Value: 0x0
				Numeric Prompt: "    Spread %", Help: "Specifies the amount of spread spectrum clocking to be applied to the base clock frequency in 0.01% increments. Allowed range is limited by Maximum Spread % and supported Spread mode Adjustements. If Changes Allowed, a value between 0 and Max Spread % can be specified. Value is adjusted to settings supported by HW. If only Halt Allowed, only 0% and default spread % can be specified. Changes are not applied until settings are saved and platform resets.", QuestionFlags: 0x14, QuestionId: 0x27C6, VarStoreId: 0x16, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x322, Value: 0x0
				EqIdVal QuestionId: 0x31C, Value: 0x0
				Or 
			End 
			Subtitle Prompt: "PCI CLOCK placeholder for clock 3 title", Help: "", Flags: 0x0
			End 
			Text Prompt: "    Default Clock Settings", Help: "", Text: "100.00MHz 0.50% Downspread"
			Text Prompt: "    Frequency Range Limits", Help: "", Text: "uninitialized MHz"
			Text Prompt: "    Maximum Spread %", Help: "", Text: "uninitialized %"
			Text Prompt: "    Spread Mode Adjustments", Help: "", Text: "Uninitialized"
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x322, Value: 0x0
				EqIdVal QuestionId: 0x31C, Value: 0x0
				Or 
				EqIdVal QuestionId: 0x31E, Value: 0x0
				Or 
			End 
			Numeric Prompt: "    Clock Frequency", Help: "Frequency in 10kHz increments. Specifies new BCLK frequency to be applied. Frequency is rounded to nearest valid value. Allowed range is limited by the Max/Min supported frequencies. Changes are not applied until settings are saved and platform resets. Example: For 125.70MHz, enter 12570.", QuestionFlags: 0x4, QuestionId: 0x27C7, VarStoreId: 0x16, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x322, Value: 0x0
				EqIdVal QuestionId: 0x320, Value: 0x0
				Or 
				EqIdVal QuestionId: 0x31C, Value: 0x0
				Or 
			End 
			Numeric Prompt: "    Spread %", Help: "Specifies the amount of spread spectrum clocking to be applied to the base clock frequency in 0.01% increments. Allowed range is limited by Maximum Spread % and supported Spread mode Adjustements. If Changes Allowed, a value between 0 and Max Spread % can be specified. Value is adjusted to settings supported by HW. If only Halt Allowed, only 0% and default spread % can be specified. Changes are not applied until settings are saved and platform resets.", QuestionFlags: 0x4, QuestionId: 0x27C8, VarStoreId: 0x16, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		SuppressIf 
			True 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x31B, VarStoreId: 0x16, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x31C, VarStoreId: 0x16, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x31D, VarStoreId: 0x16, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x31E, VarStoreId: 0x16, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x31F, VarStoreId: 0x16, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x320, VarStoreId: 0x16, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x321, VarStoreId: 0x16, VarOffset: 0xC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0x322, VarStoreId: 0x16, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			End 
		End 
	End 
	Form FormId: 0x27DB, Title: "Thunderbolt(TM) Configuration"
		OneOf Prompt: "Thunderbolt(TM) Support", Help: "Enable or Disable Thunderbolt(TM) Support.", QuestionFlags: 0x14, QuestionId: 0x27CB, VarStoreId: 0x1, VarOffset: 0x465, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			Default DefaultId: 0x0 Value: 2
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1
			OneOfOption Option: "Fully Disabled" Value: 2
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x27CB, Value: 0x1
				EqIdVal QuestionId: 0x27CB, Value: 0x2
				Or 
			End 
			OneOf Prompt: "Thunderbolt(TM) PCIe Support", Help: "Enable or Disable Thunderbolt(TM) Support as regular PCIe device.", QuestionFlags: 0x10, QuestionId: 0x323, VarStoreId: 0x1, VarOffset: 0x46C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x27CB, Value: 0x0
				EqIdVal QuestionId: 0x27CB, Value: 0x2
				Or 
			End 
			OneOf Prompt: "Thunderbolt Usb Support", Help: "Enabled allows boot from Usb devices which is present behind Thunderbolt", QuestionFlags: 0x14, QuestionId: 0x27CC, VarStoreId: 0x1, VarOffset: 0x46E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x0 Value: Other
					Value 
						Uint64 Value: 0x0
					End 
				End 
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "TBT Vt-d base security", Help: "TBT Vt-d base security", QuestionFlags: 0x14, QuestionId: 0x27CD, VarStoreId: 0x1, VarOffset: 0x46F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x1 Value: 0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Thunderbolt Boot Support", Help: "Enabled allows boot from Bootable devices which is present behind Thunderbolt", QuestionFlags: 0x14, QuestionId: 0x27CE, VarStoreId: 0x1, VarOffset: 0x470, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				Default DefaultId: 0x0 Value: Other
					Value 
						Uint64 Value: 0x0
					End 
				End 
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Boot once" Value: 1
				OneOfOption Option: "Pre-Boot ACL" Value: 2
			End 
			OneOf Prompt: "Titan Ridge Workaround for OSUP", Help: "Enable or Disable Titan Ridge Workaround for OSUP", QuestionFlags: 0x14, QuestionId: 0x324, VarStoreId: 0x1, VarOffset: 0x511, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			CheckBox Prompt: "Wake From Thunderbolt(TM) Devices", Help: "Enable or disable system wake from Thunderbolt(TM) devices.", QuestionFlags: 0x10, QuestionId: 0x325, VarStoreId: 0x1, VarOffset: 0x466, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			OneOf Prompt: "Thunderbolt(TM) PCIe Cache-line Size", Help: "Cache-line size value to be configured on Thunderbolt(TM) PCIe subtree.", QuestionFlags: 0x14, QuestionId: 0x326, VarStoreId: 0x1, VarOffset: 0x473, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x0
				OneOfOption Option: "0" Value: 0
				OneOfOption Option: "1" Value: 1
				OneOfOption Option: "2" Value: 2
				OneOfOption Option: "4" Value: 4
				OneOfOption Option: "8" Value: 8
				OneOfOption Option: "16" Value: 16
				OneOfOption Option: "32" Value: 32, Default, MfgDefault
				OneOfOption Option: "64" Value: 64
				OneOfOption Option: "128" Value: 128
			End 
			CheckBox Prompt: "GPIO3 Force Pwr", Help: "Set GPIO3 to 1/0", QuestionFlags: 0x10, QuestionId: 0x327, VarStoreId: 0x1, VarOffset: 0x474, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			Numeric Prompt: "Wait time in ms after applying Force Pwr", Help: "After Force Pwr is asserted the wait time (in milli seconds) before access the TBT controller", QuestionFlags: 0x14, QuestionId: 0x328, VarStoreId: 0x1, VarOffset: 0x475, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x1388, Step: 0x0
				Default DefaultId: 0x0 Value: 200
			End 
			OneOf Prompt: "Skip PCI enumeration", Help: "Enable or Disable Boot time PCI enumeration for Thunderbolt(TM) devices", QuestionFlags: 0x10, QuestionId: 0x329, VarStoreId: 0x1, VarOffset: 0x4A3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "Skip PCI OptionRom", Help: "Enable or Disable PCI OptionRom loading for Thunderbolt(TM) devices", QuestionFlags: 0x10, QuestionId: 0x32A, VarStoreId: 0x1, VarOffset: 0x4A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x0 Value: 0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, MfgDefault
			End 
			OneOf Prompt: "Skip PCI Interrupt Assignment", Help: "Enable or Disable Boot time PCI interrupt assignment for Thunderbolt(TM) devices", QuestionFlags: 0x10, QuestionId: 0x32B, VarStoreId: 0x1, VarOffset: 0x4A5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "ACPI Removal Object Suppport", Help: "Enable or Disable ACPI method _RMV support for Thunderbolt(TM) devices", QuestionFlags: 0x10, QuestionId: 0x32C, VarStoreId: 0x1, VarOffset: 0x4A6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Security Level", Help: "Security level selection.", QuestionFlags: 0x14, QuestionId: 0x27D1, VarStoreId: 0x1, VarOffset: 0x477, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				Default DefaultId: 0x0 Value: Other
					Value 
						Uint64 Value: 0x1
					End 
				End 
				OneOfOption Option: "No Security" Value: 0
				OneOfOption Option: "User Authorization" Value: 1
				OneOfOption Option: "Secure Connect" Value: 2
				OneOfOption Option: "Display Port only" Value: 3
				OneOfOption Option: "USB Docking Only" Value: 4
			End 
			OneOf Prompt: "Call pre boot Smi handler", Help: "Call TBT Smi Handler before boot to OS bit 0 - TBT, bit 1 - Clean Tree", QuestionFlags: 0x10, QuestionId: 0x32D, VarStoreId: 0x1, VarOffset: 0x478, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Reset Host router" Value: 1
				OneOfOption Option: "Enumerate Host router" Value: 2
				OneOfOption Option: "Reset and Enumerate Host router" Value: 3, Default, MfgDefault
			End 
			Numeric Prompt: "Reserve mem per phy slot", Help: "If PCIe device consume < ~ MB of memory BIOS will reserve ~ per physical slot", QuestionFlags: 0x10, QuestionId: 0x32E, VarStoreId: 0x1, VarOffset: 0x486, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
				Default DefaultId: 0x0 Value: 32
			End 
			Numeric Prompt: "Reserve P mem per phy slot", Help: "If PCIe device consume < ~ MB of P memory BIOS will reserve ~ per physical slot", QuestionFlags: 0x10, QuestionId: 0x32F, VarStoreId: 0x1, VarOffset: 0x488, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
				Default DefaultId: 0x0 Value: 32
			End 
			Numeric Prompt: "Reserve IO per phy slot", Help: "If PCIe device consume < ~ KB of IO space BIOS will reserve ~ per physical slot", QuestionFlags: 0x10, QuestionId: 0x330, VarStoreId: 0x1, VarOffset: 0x48A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x40, Step: 0x4
				Default DefaultId: 0x0 Value: 4
			End 
			OneOf Prompt: "    SW SMI on TBT hot-plug", Help: "When enabled, BIOS generates software SMI to assign resource to TBT devices", QuestionFlags: 0x10, QuestionId: 0x331, VarStoreId: 0x1, VarOffset: 0x48F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "GPIO filter", Help: "GPIO filter is needed to avoid electrical noise on PCH GPIOs during hotplug of 12V USB devices", QuestionFlags: 0x10, QuestionId: 0x332, VarStoreId: 0x1, VarOffset: 0x490, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "    ACPI Notify on TBT Hot-plug", Help: "When enabled, BIOS generates ACPI Notify", QuestionFlags: 0x10, QuestionId: 0x333, VarStoreId: 0x1, VarOffset: 0x491, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "MSI enabled in FADT", Help: "When disabled, MSI support is disabled in FADT", QuestionFlags: 0x10, QuestionId: 0x334, VarStoreId: 0x1, VarOffset: 0x492, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "Enable CLK REQ", Help: "Enable clock request (CLKREQ#) for all upstream ports", QuestionFlags: 0x10, QuestionId: 0x335, VarStoreId: 0x1, VarOffset: 0x494, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Enable ASPM", Help: "Enable ASPM support for all the downstreams ports and endpoints devices", QuestionFlags: 0x10, QuestionId: 0x336, VarStoreId: 0x1, VarOffset: 0x495, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
			End 
			OneOf Prompt: "Enable LTR", Help: "Enable Latency Tolerance Reporting support for all the Thunderbolt(TM) devices", QuestionFlags: 0x10, QuestionId: 0x337, VarStoreId: 0x1, VarOffset: 0x496, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
				Numeric Prompt: "AIC Location", Help: "Thunderbolt AIC Location", QuestionFlags: 0x10, QuestionId: 0x338, VarStoreId: 0x1, VarOffset: 0x493, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 9
					OneOfOption Option: "Thunderbolt AIC Location" Value: 9, MfgDefault
				End 
			End 
			OneOf Prompt: "AIC Location Group", Help: "Thunderbolt AIC Location Group", QuestionFlags: 0x14, QuestionId: 0x27D6, VarStoreId: 0x1, VarOffset: 0x498, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x0 Value: 0
				OneOfOption Option: "CPU0 NB PCIE Slot" Value: 1
				OneOfOption Option: "SB PCIE Slot" Value: 0, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27D6, Value: 0x0
					Not 
				End 
				OneOf Prompt: "AIC Location", Help: "Thunderbolt AIC Location", QuestionFlags: 0x14, QuestionId: 0x27D7, VarStoreId: 0x1, VarOffset: 0x49A, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x18, Step: 0x0
					Default DefaultId: 0x0 Value: 9
					OneOfOption Option: "SB PCIE D28F0" Value: 1, MfgDefault
					OneOfOption Option: "SB PCIE D28F1" Value: 2
					OneOfOption Option: "SB PCIE D28F2" Value: 3
					OneOfOption Option: "SB PCIE D28F3" Value: 4
					OneOfOption Option: "SB PCIE D28F4" Value: 5
					OneOfOption Option: "SB PCIE D28F5" Value: 6
					OneOfOption Option: "SB PCIE D28F6" Value: 7
					OneOfOption Option: "SB PCIE D28F7" Value: 8
					OneOfOption Option: "SB PCIE D29F0" Value: 9
					OneOfOption Option: "SB PCIE D29F1" Value: 10
					OneOfOption Option: "SB PCIE D29F2" Value: 11
					OneOfOption Option: "SB PCIE D29F3" Value: 12
					SuppressIf 
						EqIdVal QuestionId: 0xC51, Value: 0x2
						OneOfOption Option: "SB PCIE D29F4" Value: 13
						OneOfOption Option: "SB PCIE D29F5" Value: 14
						OneOfOption Option: "SB PCIE D29F6" Value: 15
						OneOfOption Option: "SB PCIE D29F7" Value: 16
						OneOfOption Option: "SB PCIE D27F0" Value: 17
						OneOfOption Option: "SB PCIE D27F1" Value: 18
						OneOfOption Option: "SB PCIE D27F2" Value: 19
						OneOfOption Option: "SB PCIE D27F3" Value: 20
						OneOfOption Option: "SB PCIE D27F4" Value: 21
						OneOfOption Option: "SB PCIE D27F5" Value: 22
						OneOfOption Option: "SB PCIE D27F6" Value: 23
						OneOfOption Option: "SB PCIE D27F7" Value: 24
					End 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27D6, Value: 0x1
					Not 
				End 
				OneOf Prompt: "AIC Location", Help: "Thunderbolt AIC Location", QuestionFlags: 0x14, QuestionId: 0x27D8, VarStoreId: 0x1, VarOffset: 0x499, Flags: 0x10, Size: 8, Min: 0x19, Max: 0x1B, Step: 0x0
					Default DefaultId: 0x0 Value: 25
					OneOfOption Option: "NB PCIE D01F0" Value: 25, MfgDefault
					OneOfOption Option: "NB PCIE D01F1" Value: 26
					OneOfOption Option: "NB PCIE D01F2" Value: 27
				End 
			End 
			OneOf Prompt: "TBT Host Router", Help: "Enable the host router based on ports available.", QuestionFlags: 0x14, QuestionId: 0x27D9, VarStoreId: 0x1, VarOffset: 0x497, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x2, Step: 0x0
				Default DefaultId: 0x0 Value: 2
				OneOfOption Option: "One port" Value: 1, MfgDefault
				OneOfOption Option: "Two port" Value: 2
			End 
			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved 56-One port Host,106-Two port Host.", QuestionFlags: 0x14, QuestionId: 0x339, VarStoreId: 0x1, VarOffset: 0x49B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 106
			End 
			Numeric Prompt: "Reseved Memory", Help: "Reserved Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x14, QuestionId: 0x33A, VarStoreId: 0x1, VarOffset: 0x49C, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x1000, Step: 0x1
				Default DefaultId: 0x0 Value: 737
			End 
			Numeric Prompt: "Memory Alignment", Help: "Memory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x33B, VarStoreId: 0x1, VarOffset: 0x49F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 26
			End 
			Numeric Prompt: "Reserved PMemory", Help: "Reserved Prefetchable Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x14, QuestionId: 0x33C, VarStoreId: 0x1, VarOffset: 0x4A0, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x1000, Step: 0x1
				Default DefaultId: 0x0 Value: 1184
			End 
			Numeric Prompt: "PMemory Alignment", Help: "PMemory Alignment (0-31 bits)", QuestionFlags: 0x14, QuestionId: 0x33D, VarStoreId: 0x1, VarOffset: 0x4A2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 28
			End 
			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x14, QuestionId: 0x33E, VarStoreId: 0x1, VarOffset: 0x49E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x34, Step: 0x4
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "Alpine Ridge Workaround Select", Help: "Intel Technical Advisory #563778: Using Non-LTR Capable PCIe Devices with Alpine Ridge", QuestionFlags: 0x14, QuestionId: 0x33F, VarStoreId: 0x1, VarOffset: 0x4A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "WA Rev 1" Value: 1
				OneOfOption Option: "WA Rev 2-New WA" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x33F, Value: 0x0
					EqIdVal QuestionId: 0x33F, Value: 0x1
					Or 
				End 
				OneOf Prompt: "AR XHCI Host Pre-wake", Help: "Alpine Ridge XHCI Pre-wake Enabled or Disabled.", QuestionFlags: 0x14, QuestionId: 0x340, VarStoreId: 0x1, VarOffset: 0x4A8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
				Numeric Prompt: "AR XHCI Host Active LTR", Help: "Alpine Ridge XHCI Active LTR allow 1~1023 ms.", QuestionFlags: 0x14, QuestionId: 0x341, VarStoreId: 0x1, VarOffset: 0x4A9, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x3FF, Step: 0x1
					Default DefaultId: 0x0 Value: 20
				End 
				Numeric Prompt: "AR XHCI Host High LTR", Help: "Alpine Ridge XHCI High LTR allow 3~124 ms.", QuestionFlags: 0x14, QuestionId: 0x342, VarStoreId: 0x1, VarOffset: 0x4AD, Flags: 0x12, Size: 32, Min: 0x3, Max: 0x7C, Step: 0x1
					Default DefaultId: 0x0 Value: 80
				End 
				Numeric Prompt: "AR XHCI Host Medium LTR", Help: "Alpine Ridge XHCI Medium LTR allow 2~123 ms.", QuestionFlags: 0x14, QuestionId: 0x343, VarStoreId: 0x1, VarOffset: 0x4B1, Flags: 0x12, Size: 32, Min: 0x2, Max: 0x7B, Step: 0x1
					Default DefaultId: 0x0 Value: 40
				End 
				Numeric Prompt: "AR XHCI Host Low LTR", Help: "Alpine Ridge XHCI Low LTR allow 1~122 ms.", QuestionFlags: 0x14, QuestionId: 0x344, VarStoreId: 0x1, VarOffset: 0x4B5, Flags: 0x12, Size: 32, Min: 0x1, Max: 0x7A, Step: 0x1
					Default DefaultId: 0x0 Value: 30
				End 
			End 
			Numeric Prompt: "Thunderbolt delay before BOOT_ON Command in PEI phase", Help: "Delay allow 0 ~ 65535 ms.", QuestionFlags: 0x14, QuestionId: 0x345, VarStoreId: 0x1, VarOffset: 0x4B9, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "Thunderbolt delay before USB_ON Command in PEI phase", Help: "Delay allow 0 ~ 65535 ms.", QuestionFlags: 0x14, QuestionId: 0x346, VarStoreId: 0x1, VarOffset: 0x4BB, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "Thunderbolt delay before SX_EXIT Command in PEI phase", Help: "Delay allow 0 ~ 65535 ms.", QuestionFlags: 0x14, QuestionId: 0x347, VarStoreId: 0x1, VarOffset: 0x4BD, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 500
			End 
			Ref Prompt: "Thunderbolt(TM) Enumeration Mode", Help: "Thunderbolt(TM) Enumeration Related Configuration", QuestionFlags: 0x0, QuestionId: 0x348, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27DC
		End 
	End 
	Form FormId: 0x27DC, Title: "Thunderbolt(TM) Enumeration Mode"
		OneOf Prompt: "Thunderbolt(TM) Enumeration Mode", Help: "Specify Thunderbolt(TM) Enumeration Mode.

Legacy: BIOS enumerates Thunderbolt(TM) devices.

Native: OS enumerates Thunderbolt(TM) devices.

Native with low power support: OS enumerates Thunderbolt(TM) devices. Requires HW support for RTD3.", QuestionFlags: 0x14, QuestionId: 0x27DA, VarStoreId: 0x1, VarOffset: 0x50F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Native with low power support" Value: 2
			OneOfOption Option: "Native" Value: 1
			OneOfOption Option: "Legacy" Value: 0, Default, MfgDefault
		End 
	End 
	Form FormId: 0x27DD, Title: "Driver Health"
		SuppressIf 
			EqIdValList QuestionId: 0xCBA, Values: [65535]
			Ref Prompt: "", Help: "Provides Health Status for the Drivers/Controllers", QuestionFlags: 0x0, QuestionId: 0x349, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27DE
		End 
	End 
	Form FormId: 0x27DE, Title: "Driver Health"
		SuppressIf 
			EqIdValList QuestionId: 0xCB9, Values: [65535]
			Ref Prompt: "", Help: "Provides Health Status for the Drivers/Controllers", QuestionFlags: 0x0, QuestionId: 0x34A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27DE
		End 
	End 
	Form FormId: 0x27E0, Title: "ACPI Settings"
		Subtitle Prompt: "ACPI Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			CheckBox Prompt: "Enable ACPI Auto Configuration", Help: "Enables or Disables BIOS ACPI Auto Configuration.", QuestionFlags: 0x0, QuestionId: 0x34B, VarStoreId: 0x1, VarOffset: 0xFF5, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
				Default DefaultId: 0x0 Value: 0
				Default DefaultId: 0x1 Value: 0
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x34B, Value: 0x1
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				CheckBox Prompt: "Enable Hibernation", Help: "Enables or Disables System ability to Hibernate (OS/S4 Sleep State). This option may not be effective with some operating systems.", QuestionFlags: 0x0, QuestionId: 0x34C, VarStoreId: 0x1, VarOffset: 0xFF9, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
					Default DefaultId: 0x0 Value: 1
					Default DefaultId: 0x1 Value: 1
				End 
				OneOf Prompt: "ACPI Sleep State", Help: "Select the highest ACPI sleep state the system will enter when the SUSPEND button is pressed.", QuestionFlags: 0x10, QuestionId: 0x34D, VarStoreId: 0x1, VarOffset: 0xFF6, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Suspend Disabled" Value: 0
					OneOfOption Option: "S3 (Suspend to RAM)" Value: 2
					Default DefaultId: 0x0 Value: 2
					Default DefaultId: 0x1 Value: 2
				End 
				CheckBox Prompt: "Lock Legacy Resources", Help: "Enables or Disables Lock of Legacy Resources", QuestionFlags: 0x10, QuestionId: 0x34E, VarStoreId: 0x1, VarOffset: 0xFF8, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
					Default DefaultId: 0x0 Value: 0
					Default DefaultId: 0x1 Value: 0
				End 
				OneOf Prompt: "S3 Video Repost", Help: "Enable or Disable S3 Video Repost", QuestionFlags: 0x10, QuestionId: 0x34F, VarStoreId: 0x1, VarOffset: 0xFFA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1
					Default DefaultId: 0x0 Value: 0
					Default DefaultId: 0x1 Value: 0
				End 
			End 
		End 
	End 
	Form FormId: 0x27FB, Title: "Miscellaneous Configuration"
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			CheckBox Prompt: "Resume On RTC Alarm", Help: "RTC Alarm setting", QuestionFlags: 0x0, QuestionId: 0x350, VarStoreId: 0x1, VarOffset: 0x1074, Flags: 0x2, Default: Disabled, MfgDefault: Enabled
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x350, Value: 0x0
				Numeric Prompt: "  RTC Alarm Date (Days)", Help: "RTC Alarm setting", QuestionFlags: 0x0, QuestionId: 0x351, VarStoreId: 0x1, VarOffset: 0x1075, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "  RTC Alarm Time(Hours)", Help: "RTC Alarm Time Setting", QuestionFlags: 0x0, QuestionId: 0x352, VarStoreId: 0x1, VarOffset: 0x1076, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 15
				End 
				Numeric Prompt: "  RTC Alarm Time(Minutes)", Help: "RTC Alarm Time Setting", QuestionFlags: 0x0, QuestionId: 0x353, VarStoreId: 0x1, VarOffset: 0x1077, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3B, Step: 0x1
					Default DefaultId: 0x0 Value: 15
				End 
				Numeric Prompt: "  RTC Alarm Time(Seconds)", Help: "RTC Alarm Time Setting", QuestionFlags: 0x0, QuestionId: 0x354, VarStoreId: 0x1, VarOffset: 0x1078, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3B, Step: 0x1
					Default DefaultId: 0x0 Value: 15
				End 
			End 
			OneOf Prompt: "Restore AC Power Loss", Help: "Select AC power state when power is re-applied after a power failure.", QuestionFlags: 0x10, QuestionId: 0x355, VarStoreId: 0x1, VarOffset: 0x1079, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				Default DefaultId: 0x0 Value: 0
				OneOfOption Option: "Power Off" Value: 0, MfgDefault
				OneOfOption Option: "Power On" Value: 1
				OneOfOption Option: "Last State" Value: 2
			End 
			OneOf Prompt: "Watch dog Controller", Help: "Allow select second or minute unit", QuestionFlags: 0x10, QuestionId: 0x356, VarStoreId: 0x1, VarOffset: 0x107B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Second mode" Value: 1
				OneOfOption Option: "Minute mode" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x356, Value: 0x0
				Numeric Prompt: "Watch dog timer value input", Help: "Directly Input any value of 1-255", QuestionFlags: 0x0, QuestionId: 0x357, VarStoreId: 0x1, VarOffset: 0x107A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 120
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC42, Value: 0x0
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Or 
				End 
				Subtitle Prompt: "", Help: "", Flags: 0x0
				End 
				Subtitle Prompt: "GPIO1 Modules Settings", Help: "", Flags: 0x0
				End 
				OneOf Prompt: "GPIO 1 Controller", Help: "Allow select Input Mode or Output Mode for control gpio mode", QuestionFlags: 0x10, QuestionId: 0x358, VarStoreId: 0x1, VarOffset: 0x107C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 0
					OneOfOption Option: "Input Mode" Value: 0, MfgDefault
					OneOfOption Option: "Output Mode" Value: 1
				End 
				OneOf Prompt: "GPIO 2 Controller", Help: "Allow select Input Mode or Output Mode for control gpio mode", QuestionFlags: 0x10, QuestionId: 0x359, VarStoreId: 0x1, VarOffset: 0x107D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 1
					OneOfOption Option: "Input Mode" Value: 0
					OneOfOption Option: "Output Mode" Value: 1, MfgDefault
				End 
				OneOf Prompt: "GPIO 3 Controller", Help: "Allow select Input Mode or Output Mode for control gpio mode", QuestionFlags: 0x10, QuestionId: 0x35A, VarStoreId: 0x1, VarOffset: 0x107E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 0
					OneOfOption Option: "Input Mode" Value: 0, MfgDefault
					OneOfOption Option: "Output Mode" Value: 1
				End 
				OneOf Prompt: "GPIO 4 Controller", Help: "Allow select Input Mode or Output Mode for control gpio mode", QuestionFlags: 0x10, QuestionId: 0x35B, VarStoreId: 0x1, VarOffset: 0x107F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 1
					OneOfOption Option: "Input Mode" Value: 0
					OneOfOption Option: "Output Mode" Value: 1, MfgDefault
				End 
				OneOf Prompt: "GPIO 5 Controller", Help: "Allow select Input Mode or Output Mode for control gpio mode", QuestionFlags: 0x10, QuestionId: 0x35C, VarStoreId: 0x1, VarOffset: 0x1080, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 0
					OneOfOption Option: "Input Mode" Value: 0, MfgDefault
					OneOfOption Option: "Output Mode" Value: 1
				End 
				OneOf Prompt: "GPIO 6 Controller", Help: "Allow select Input Mode or Output Mode for control gpio mode", QuestionFlags: 0x10, QuestionId: 0x35D, VarStoreId: 0x1, VarOffset: 0x1081, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 1
					OneOfOption Option: "Input Mode" Value: 0
					OneOfOption Option: "Output Mode" Value: 1, MfgDefault
				End 
				OneOf Prompt: "GPIO 7 Controller", Help: "Allow select Input Mode or Output Mode for control gpio mode", QuestionFlags: 0x10, QuestionId: 0x35E, VarStoreId: 0x1, VarOffset: 0x1082, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 0
					OneOfOption Option: "Input Mode" Value: 0, MfgDefault
					OneOfOption Option: "Output Mode" Value: 1
				End 
				OneOf Prompt: "GPIO 8 Controller", Help: "Allow select Input Mode or Output Mode for control gpio mode", QuestionFlags: 0x10, QuestionId: 0x35F, VarStoreId: 0x1, VarOffset: 0x1083, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 1
					OneOfOption Option: "Input Mode" Value: 0
					OneOfOption Option: "Output Mode" Value: 1, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x358, Value: 0x0
					OneOf Prompt: "GPIO 1 Controller", Help: "Allow select high or low for control gpio status", QuestionFlags: 0x10, QuestionId: 0x360, VarStoreId: 0x1, VarOffset: 0x1084, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "Low" Value: 0, MfgDefault
						OneOfOption Option: "High" Value: 1
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x359, Value: 0x0
					OneOf Prompt: "GPIO 2 Controller", Help: "Allow select high or low for control gpio status", QuestionFlags: 0x10, QuestionId: 0x361, VarStoreId: 0x1, VarOffset: 0x1085, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "Low" Value: 0, MfgDefault
						OneOfOption Option: "High" Value: 1
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x35A, Value: 0x0
					OneOf Prompt: "GPIO 3 Controller", Help: "Allow select high or low for control gpio status", QuestionFlags: 0x10, QuestionId: 0x362, VarStoreId: 0x1, VarOffset: 0x1086, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "Low" Value: 0, MfgDefault
						OneOfOption Option: "High" Value: 1
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x35B, Value: 0x0
					OneOf Prompt: "GPIO 4 Controller", Help: "Allow select high or low for control gpio status", QuestionFlags: 0x10, QuestionId: 0x363, VarStoreId: 0x1, VarOffset: 0x1087, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "Low" Value: 0, MfgDefault
						OneOfOption Option: "High" Value: 1
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x35C, Value: 0x0
					OneOf Prompt: "GPIO 5 Controller", Help: "Allow select high or low for control gpio status", QuestionFlags: 0x10, QuestionId: 0x364, VarStoreId: 0x1, VarOffset: 0x1088, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "Low" Value: 0, MfgDefault
						OneOfOption Option: "High" Value: 1
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x35D, Value: 0x0
					OneOf Prompt: "GPIO 6 Controller", Help: "Allow select high or low for control gpio status", QuestionFlags: 0x10, QuestionId: 0x365, VarStoreId: 0x1, VarOffset: 0x1089, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "Low" Value: 0, MfgDefault
						OneOfOption Option: "High" Value: 1
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x35E, Value: 0x0
					OneOf Prompt: "GPIO 7 Controller", Help: "Allow select high or low for control gpio status", QuestionFlags: 0x10, QuestionId: 0x366, VarStoreId: 0x1, VarOffset: 0x108A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "Low" Value: 0, MfgDefault
						OneOfOption Option: "High" Value: 1
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x35F, Value: 0x0
					OneOf Prompt: "GPIO 8 Controller", Help: "Allow select high or low for control gpio status", QuestionFlags: 0x10, QuestionId: 0x367, VarStoreId: 0x1, VarOffset: 0x108B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "Low" Value: 0, MfgDefault
						OneOfOption Option: "High" Value: 1
					End 
				End 
			End 
		End 
	End 
	Form FormId: 0x27FC, Title: "SMART Settings"
		Subtitle Prompt: "SMART Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			CheckBox Prompt: "SMART Self Test", Help: "Run SMART Self Test on all HDDs during POST.", QuestionFlags: 0x10, QuestionId: 0x368, VarStoreId: 0x1, VarOffset: 0x108C, Flags: 0x2, Default: Disabled, MfgDefault: Enabled
				Default DefaultId: 0x0 Value: Other
					Value 
						Uint64 Value: 0x0
					End 
				End 
			End 
		End 
	End 
	Form FormId: 0x2805, Title: "IT8784 Super IO Configuration"
		Subtitle Prompt: "IT8784 Super IO Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "Super IO Chip", Help: "System Super IO Chip Parameters.", Text: "IT8784"
		SuppressIf 
			EqIdVal QuestionId: 0xCB8, Value: 0x0
			Ref Prompt: "Serial Port 1 Configuration", Help: "Set Parameters of Serial Port 1 (COMA)", QuestionFlags: 0x0, QuestionId: 0x369, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2806
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCB7, Value: 0x0
			Ref Prompt: "Serial Port 2 Configuration", Help: "Set Parameters of Serial Port 2 (COMB)", QuestionFlags: 0x0, QuestionId: 0x36A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2807
		End 
	End 
	Form FormId: 0x2806, Title: "Serial Port 1 Configuration"
		Subtitle Prompt: "Serial Port 1 Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		CheckBox Prompt: "Serial Port", Help: "Enable or Disable Serial Port (COM)", QuestionFlags: 0x10, QuestionId: 0x36B, VarStoreId: 0x21, VarOffset: 0x0, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			Default DefaultId: 0x0 Value: 1
			Default DefaultId: 0x1 Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x36B, Value: 0x0
			Text Prompt: "Device Settings", Help: "Set Parameters of Serial Port 1 (COMA)", Text: "Reset Required"
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x36B, Value: 0x0
			OneOf Prompt: "Change Settings", Help: "Select an optimal settings for Super IO Device", QuestionFlags: 0x10, QuestionId: 0x36C, VarStoreId: 0x21, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "Auto" Value: 0
				OneOfOption Option: "IO=3F8h; IRQ=4;" Value: 1
				OneOfOption Option: "IO=3F8h; IRQ=3,4,5,6,7,9,10,11,12;" Value: 2
				OneOfOption Option: "IO=2F8h; IRQ=3,4,5,6,7,9,10,11,12;" Value: 3
				OneOfOption Option: "IO=3E8h; IRQ=3,4,5,6,7,9,10,11,12;" Value: 4
				OneOfOption Option: "IO=2E8h; IRQ=3,4,5,6,7,9,10,11,12;" Value: 5
				Default DefaultId: 0x0 Value: 0
				Default DefaultId: 0x1 Value: 0
			End 
		End 
	End 
	Form FormId: 0x2807, Title: "Serial Port 2 Configuration"
		Subtitle Prompt: "Serial Port 2 Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		CheckBox Prompt: "Serial Port", Help: "Enable or Disable Serial Port (COM)", QuestionFlags: 0x10, QuestionId: 0x36D, VarStoreId: 0x23, VarOffset: 0x0, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			Default DefaultId: 0x0 Value: 1
			Default DefaultId: 0x1 Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x36D, Value: 0x0
			Text Prompt: "Device Settings", Help: "Set Parameters of Serial Port 2 (COMB)", Text: "Reset Required"
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x36D, Value: 0x0
			OneOf Prompt: "Change Settings", Help: "Select an optimal settings for Super IO Device", QuestionFlags: 0x10, QuestionId: 0x36E, VarStoreId: 0x23, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "Auto" Value: 0
				OneOfOption Option: "IO=2F8h; IRQ=3;" Value: 1
				OneOfOption Option: "IO=3F8h; IRQ=3,4,5,6,7,9,10,11,12;" Value: 2
				OneOfOption Option: "IO=2F8h; IRQ=3,4,5,6,7,9,10,11,12;" Value: 3
				OneOfOption Option: "IO=3E8h; IRQ=3,4,5,6,7,9,10,11,12;" Value: 4
				OneOfOption Option: "IO=2E8h; IRQ=3,4,5,6,7,9,10,11,12;" Value: 5
				Default DefaultId: 0x0 Value: 0
				Default DefaultId: 0x1 Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x36D, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "Serial Port mode Select", Help: "Serial Port mode RS232 RS422 RS485 Selection,when board supported", QuestionFlags: 0x10, QuestionId: 0x36F, VarStoreId: 0x1, VarOffset: 0x108D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "RS-485" Value: 0
					SuppressIf 
						Uint64 Value: 0x1
						OneOfOption Option: "RS-422" Value: 1
					End 
					OneOfOption Option: "RS-232" Value: 2, Default, MfgDefault
				End 
			End 
		End 
	End 
	Form FormId: 0x280A, Title: "Hardware Monitor"
		Subtitle Prompt: "Pc Health Status", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Text Prompt: "System temperature1", Help: "", Text: "N/A"
			SuppressIf 
				True 
				SuppressIf 
					EqIdVal QuestionId: 0xC41, Value: 0xB
					Action Prompt: "System temperature1", Help: "", QuestionFlags: 0x4, QuestionId: 0x280B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, QuestionConfig: ""
					End 
				End 
			End 
		End 
		Text Prompt: "System temperature", Help: "", Text: "N/A"
		Text Prompt: "CPU temperature", Help: "", Text: "N/A"
		Text Prompt: "CPUFAN Speed", Help: "", Text: "N/A"
		Text Prompt: "SYSFAN1 Speed", Help: "", Text: "N/A"
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Text Prompt: "Fan4 Speed", Help: "", Text: "N/A"
			Text Prompt: "Fan5 Speed", Help: "", Text: "N/A"
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Text Prompt: "VCORE", Help: "", Text: "N/A"
			Text Prompt: "VIN1", Help: "", Text: "N/A"
			Text Prompt: "VIN2", Help: "", Text: "N/A"
			Text Prompt: "VIN3", Help: "", Text: "N/A"
			Text Prompt: "VIN4", Help: "", Text: "N/A"
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Text Prompt: "VSB3V", Help: "", Text: "N/A"
			Text Prompt: "VBAT", Help: "", Text: "N/A"
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "Smart Fan Function", Help: "", Flags: 0x0
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "CPUFAN1 Mode", Help: "Smart Fan Mode Select", QuestionFlags: 0x10, QuestionId: 0x370, VarStoreId: 0x1, VarOffset: 0x108E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				Default DefaultId: 0x0 Value: 1
				OneOfOption Option: "Full on Mode" Value: 0
				OneOfOption Option: "Automatic Mode" Value: 1, MfgDefault
				OneOfOption Option: "Manual Mode" Value: 2
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x370, Value: 0x2
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Numeric Prompt: "  Manual PWM Setting", Help: "Fan will work with this Manual PWM Value", QuestionFlags: 0x10, QuestionId: 0x371, VarStoreId: 0x1, VarOffset: 0x1094, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 100
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x370, Value: 0x1
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Numeric Prompt: "  Fan off temperature limit", Help: "Fan will off when temperature lower than this limit", QuestionFlags: 0x10, QuestionId: 0x372, VarStoreId: 0x1, VarOffset: 0x1090, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 45
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x370, Value: 0x1
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Numeric Prompt: "  Fan start temperature limit", Help: "Fan will work when temperature higher than this limit", QuestionFlags: 0x10, QuestionId: 0x373, VarStoreId: 0x1, VarOffset: 0x1091, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
					Default DefaultId: 0x0 Value: 50
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x370, Value: 0x1
				Not 
			End 
			Numeric Prompt: "  Fan full speed temperature limit", Help: "Fan will full speed when temperature higher than this limit", QuestionFlags: 0x10, QuestionId: 0x374, VarStoreId: 0x1, VarOffset: 0x1092, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5A, Step: 0x1
				Default DefaultId: 0x0 Value: 75
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x370, Value: 0x1
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Numeric Prompt: "  Fan start PWM", Help: "  Fan will stat with this PWM value.", QuestionFlags: 0x10, QuestionId: 0x375, VarStoreId: 0x1, VarOffset: 0x1093, Flags: 0x10, Size: 8, Min: 0x46, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 90
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x370, Value: 0x1
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Numeric Prompt: "  PWM SLOPE SETTING", Help: "PWM SLOPE Selection", QuestionFlags: 0x10, QuestionId: 0x376, VarStoreId: 0x1, VarOffset: 0x108F, Flags: 0x10, Size: 8, Min: 0x2, Max: 0xF, Step: 0x1
					Default DefaultId: 0x0 Value: 8
				End 
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "SYSFAN1 Mode", Help: "Smart Fan Mode Select", QuestionFlags: 0x10, QuestionId: 0x377, VarStoreId: 0x1, VarOffset: 0x1095, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				Default DefaultId: 0x0 Value: 1
				OneOfOption Option: "Full on Mode" Value: 0, MfgDefault
				OneOfOption Option: "Automatic Mode" Value: 1
				OneOfOption Option: "Manual Mode" Value: 2
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x377, Value: 0x2
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Numeric Prompt: "  Manual PWM Setting", Help: "Fan will work with this Manual PWM Value", QuestionFlags: 0x10, QuestionId: 0x378, VarStoreId: 0x1, VarOffset: 0x1096, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
					Default DefaultId: 0x0 Value: 127
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "SYSFAN34 Mode", Help: "Smart Fan Mode Select", QuestionFlags: 0x10, QuestionId: 0x379, VarStoreId: 0x1, VarOffset: 0x1097, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					Default DefaultId: 0x0 Value: 1
					OneOfOption Option: "Full on Mode" Value: 0
					OneOfOption Option: "Automatic Mode" Value: 1, MfgDefault
					OneOfOption Option: "Manual Mode" Value: 2
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x379, Value: 0x2
					Not 
				End 
				GrayOutIf 
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Numeric Prompt: "  Manual PWM Setting", Help: "Fan will work with this Manual PWM Value", QuestionFlags: 0x10, QuestionId: 0x37A, VarStoreId: 0x1, VarOffset: 0x1098, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
						Default DefaultId: 0x0 Value: 127
					End 
				End 
			End 
		End 
	End 
	Form FormId: 0x280C, Title: "Intel(R) Bios Guard Technology"
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Intel Bios Guard Support", Help: "Enable/Disable Intel Bios Guard Support", QuestionFlags: 0x10, QuestionId: 0x37B, VarStoreId: 0x1, VarOffset: 0x1099, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x0 Value: 0
				OneOfOption Option: "Disabled" Value: 0, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
	End 
	Form FormId: 0x2810, Title: "Intel TXT Information"
		Subtitle Prompt: "Intel TXT Information", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "Chipset", Help: "Chipset is production or debug Fused", Text: "Debug Fused"
		Text Prompt: "BiosAcm", Help: "BiosAcm is production or debug Fused", Text: "Debug Fused"
		Text Prompt: "Chipset Txt", Help: "Chipset support Txt", Text: "Not Supported"
		Text Prompt: "Cpu Txt", Help: "Cpu support Txt", Text: "Not Supported"
		Text Prompt: "Error Code", Help: "This holds the Intel TXT shutdown error code.", Text: "None"
		Text Prompt: "  Class Code", Help: "Error code[9:4]", Text: "None"
		Text Prompt: "  Major Code", Help: "Error code[14:10]", Text: "None"
		Text Prompt: "  Minor Code", Help: "Error code[24:16]", Text: "None"
	End 
	Form FormId: 0x2813, Title: "AMI Graphic Output Protocol Policy"
		Subtitle Prompt: "Unknown Device", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "Unknown Driver", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCB6, Value: 0x1
				Not 
			End 
			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2814, VarStoreId: 0x1, VarOffset: 0x109E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x0, Step: 0x0
				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCB6, Value: 0x2
				Not 
			End 
			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2815, VarStoreId: 0x1, VarOffset: 0x109E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault
				OneOfOption Option: "Unknown Device" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCB6, Value: 0x3
				Not 
			End 
			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2816, VarStoreId: 0x1, VarOffset: 0x109E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault
				OneOfOption Option: "Unknown Device" Value: 1
				OneOfOption Option: "Unknown Device" Value: 2
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCB6, Value: 0x4
				Not 
			End 
			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2817, VarStoreId: 0x1, VarOffset: 0x109E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault
				OneOfOption Option: "Unknown Device" Value: 1
				OneOfOption Option: "Unknown Device" Value: 2
				OneOfOption Option: "Unknown Device" Value: 3
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCB6, Value: 0x5
				Not 
			End 
			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2818, VarStoreId: 0x1, VarOffset: 0x109E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault
				OneOfOption Option: "Unknown Device" Value: 1
				OneOfOption Option: "Unknown Device" Value: 2
				OneOfOption Option: "Unknown Device" Value: 3
				OneOfOption Option: "Unknown Device" Value: 4
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCB6, Value: 0x6
				Not 
			End 
			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x2819, VarStoreId: 0x1, VarOffset: 0x109E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault
				OneOfOption Option: "Unknown Device" Value: 1
				OneOfOption Option: "Unknown Device" Value: 2
				OneOfOption Option: "Unknown Device" Value: 3
				OneOfOption Option: "Unknown Device" Value: 4
				OneOfOption Option: "Unknown Device" Value: 5
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCB6, Value: 0x7
				Not 
			End 
			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x281A, VarStoreId: 0x1, VarOffset: 0x109E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault
				OneOfOption Option: "Unknown Device" Value: 1
				OneOfOption Option: "Unknown Device" Value: 2
				OneOfOption Option: "Unknown Device" Value: 3
				OneOfOption Option: "Unknown Device" Value: 4
				OneOfOption Option: "Unknown Device" Value: 5
				OneOfOption Option: "Unknown Device" Value: 6
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCB6, Value: 0x8
				Not 
			End 
			OneOf Prompt: "Output Select", Help: "Output Interface", QuestionFlags: 0x4, QuestionId: 0x281B, VarStoreId: 0x1, VarOffset: 0x109E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
				OneOfOption Option: "Unknown Device" Value: 0, Default, MfgDefault
				OneOfOption Option: "Unknown Device" Value: 1
				OneOfOption Option: "Unknown Device" Value: 2
				OneOfOption Option: "Unknown Device" Value: 3
				OneOfOption Option: "Unknown Device" Value: 4
				OneOfOption Option: "Unknown Device" Value: 5
				OneOfOption Option: "Unknown Device" Value: 6
				OneOfOption Option: "Unknown Device" Value: 7
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCB5, Value: 0x0
			Numeric Prompt: "Brightnesst Setting", Help: "Set Gop Brightnesst value", QuestionFlags: 0x4, QuestionId: 0x281C, VarStoreId: 0x1, VarOffset: 0x109F, Flags: 0x12, Size: 32, Min: 0x0, Max: 0xFFFFFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 255
				OneOfOption Option: "Brightnesst Setting" Value: 0, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xCB4, Value: 0x0
			OneOf Prompt: "BIST Enable", Help: "Starts or stops the BIST on the integrated display panel.", QuestionFlags: 0x14, QuestionId: 0x281D, VarStoreId: 0x1, VarOffset: 0x10A3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
	End 
	Form FormId: 0x281F, Title: "PCI Subsystem Settings"
		Text Prompt: "PCI Bus Driver Version", Help: "PCI, PCI-X and PCI Express Settings.", Text: "00.00"
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "PCI Devices Common Settings:", Help: "", Flags: 0x0
		End 
		SuppressIf 
			Uint64 Value: 0x1
				Uint64 Value: 0x0
				Equal 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "PCI Latency Timer", Help: "Value to be programmed into PCI Latency Timer Register.", QuestionFlags: 0x10, QuestionId: 0x37C, VarStoreId: 0x1, VarOffset: 0x10A7, Flags: 0x10, Size: 8, Min: 0x20, Max: 0xF8, Step: 0x0
					OneOfOption Option: "32 PCI Bus Clocks" Value: 32, Default, MfgDefault
					OneOfOption Option: "64 PCI Bus Clocks" Value: 64
					OneOfOption Option: "96 PCI Bus Clocks" Value: 96
					OneOfOption Option: "128 PCI Bus Clocks" Value: 128
					OneOfOption Option: "160 PCI Bus Clocks" Value: 160
					OneOfOption Option: "192 PCI Bus Clocks" Value: 192
					OneOfOption Option: "224 PCI Bus Clocks" Value: 224
					OneOfOption Option: "248 PCI Bus Clocks" Value: 248
				End 
			End 
		End 
		SuppressIf 
			Uint64 Value: 0x1
				Uint64 Value: 0x0
				Equal 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "PCI-X Latency Timer", Help: "Value to be programmed into PCI Latency Timer Register.", QuestionFlags: 0x10, QuestionId: 0x37D, VarStoreId: 0x1, VarOffset: 0x10AB, Flags: 0x10, Size: 8, Min: 0x20, Max: 0xF8, Step: 0x0
					OneOfOption Option: "32 PCI Bus Clocks" Value: 32
					OneOfOption Option: "64 PCI Bus Clocks" Value: 64, Default, MfgDefault
					OneOfOption Option: "96 PCI Bus Clocks" Value: 96
					OneOfOption Option: "128 PCI Bus Clocks" Value: 128
					OneOfOption Option: "160 PCI Bus Clocks" Value: 160
					OneOfOption Option: "192 PCI Bus Clocks" Value: 192
					OneOfOption Option: "224 PCI Bus Clocks" Value: 224
					OneOfOption Option: "248 PCI Bus Clocks" Value: 248
				End 
			End 
		End 
		SuppressIf 
			Uint64 Value: 0x1
				Uint64 Value: 0x0
				Equal 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "VGA Palette Snoop", Help: "Enables or Disables VGA Palette Registers Snooping.", QuestionFlags: 0x10, QuestionId: 0x37E, VarStoreId: 0x1, VarOffset: 0x10A8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
		End 
		SuppressIf 
			Uint64 Value: 0x1
				Uint64 Value: 0x0
				Equal 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "PERR# Generation", Help: "Enables or Disables PCI Device to Generate PERR#.", QuestionFlags: 0x10, QuestionId: 0x37F, VarStoreId: 0x1, VarOffset: 0x10A9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
		End 
		SuppressIf 
			Uint64 Value: 0x1
				Uint64 Value: 0x0
				Equal 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "SERR# Generation", Help: "Enables or Disables PCI Device to Generate SERR#.", QuestionFlags: 0x10, QuestionId: 0x380, VarStoreId: 0x1, VarOffset: 0x10AA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
		End 
		SuppressIf 
			Uint64 Value: 0x1
				Uint64 Value: 0x0
				Equal 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "Above 4G Decoding", Help: "Enables or Disables 64bit capable Devices to be Decoded in Above 4G Address Space (Only if System Supports 64 bit PCI Decoding).", QuestionFlags: 0x10, QuestionId: 0x381, VarStoreId: 0x1, VarOffset: 0x10A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1
					Default DefaultId: 0x0 Value: 0
					Default DefaultId: 0x1 Value: 0
				End 
			End 
		End 
		SuppressIf 
			Uint64 Value: 0x1
				Uint64 Value: 0x0
				Equal 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "BME DMA Mitigation", Help: "Re-enable Bus Master Attribute disabled during Pci enumeration for PCI Bridges after SMM Locked ", QuestionFlags: 0x10, QuestionId: 0x382, VarStoreId: 0x1, VarOffset: 0x10A6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1
					Default DefaultId: 0x0 Value: 0
					Default DefaultId: 0x1 Value: 0
				End 
			End 
		End 
		SuppressIf 
			Uint64 Value: 0x0
				Uint64 Value: 0x0
				Equal 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "Don't Reset VC-TC Mapping", Help: "If system has Vitrtual Channels, Software can reset Traffic Class mapping through Virtual Channels, to it's default state. Setting this option to Enabled will not modify VC Resources.", QuestionFlags: 0x10, QuestionId: 0x383, VarStoreId: 0x1, VarOffset: 0x10B8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			Uint64 Value: 0x1
				Uint64 Value: 0x0
				Equal 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Ref Prompt: "PCI Hot-Plug Settings", Help: "Change PCI Express Hot-Plug and Standard HP Controller Settings.", QuestionFlags: 0x0, QuestionId: 0x384, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2822
			End 
		End 
	End 
	Form FormId: 0x2822, Title: "PCI Hot-Plug Settings"
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "PCI Hot-Plug Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "BIOS Hot-Plug Support", Help: "If ENABLED allows BIOS build in Hot-Pug support. Use this feature if OS does not support PCI Express and SHPC hot-plug natively.", QuestionFlags: 0x10, QuestionId: 0x385, VarStoreId: 0x1, VarOffset: 0x10C7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x385, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "PCI Buses Padding", Help: "Padd PCI Buses behind the bridge for Hot-Plug.", QuestionFlags: 0x10, QuestionId: 0x386, VarStoreId: 0x1, VarOffset: 0x10C8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "1" Value: 1, Default, MfgDefault
					OneOfOption Option: "2" Value: 2
					OneOfOption Option: "3" Value: 3
					OneOfOption Option: "4" Value: 4
					OneOfOption Option: "5" Value: 5
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x385, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "I/O Resources Padding", Help: "Padd PCI I/O Resources behind the bridge for Hot-Plug.", QuestionFlags: 0x10, QuestionId: 0x387, VarStoreId: 0x1, VarOffset: 0x10C9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x20, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "4 K" Value: 4, Default, MfgDefault
					OneOfOption Option: "8 K" Value: 8
					OneOfOption Option: "16 K" Value: 16
					OneOfOption Option: "32 K" Value: 32
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x385, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "MMIO 32 bit Resources Padding", Help: "Padd PCI MMIO 32-bit Resources behind the bridge for Hot-Plug.", QuestionFlags: 0x10, QuestionId: 0x388, VarStoreId: 0x1, VarOffset: 0x10CA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "1 M" Value: 1
					OneOfOption Option: "2 M" Value: 2
					OneOfOption Option: "4 M" Value: 4
					OneOfOption Option: "8 M" Value: 8
					OneOfOption Option: "16 M" Value: 16, Default, MfgDefault
					OneOfOption Option: "32 M" Value: 32
					OneOfOption Option: "64 M" Value: 64
					OneOfOption Option: "128 M" Value: 128
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x385, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "PFMMIO 32 bit Resources Padding", Help: "Padd PCI MMIO 32-bit Prefetchable Resources behind the bridge for Hot-Plug.", QuestionFlags: 0x10, QuestionId: 0x389, VarStoreId: 0x1, VarOffset: 0x10CB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "1 M" Value: 1
					OneOfOption Option: "2 M" Value: 2
					OneOfOption Option: "4 M" Value: 4
					OneOfOption Option: "8 M" Value: 8
					OneOfOption Option: "16 M" Value: 16, Default, MfgDefault
					OneOfOption Option: "32 M" Value: 32
					OneOfOption Option: "64 M" Value: 64
					OneOfOption Option: "128 M" Value: 128
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x385, Value: 0x0
				EqIdVal QuestionId: 0x381, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "PFMMIO 64 bit Resources Padding", Help: "Padd PCI MMIO 64-bit Prefetchable Resources behind the bridge for Hot-Plug.", QuestionFlags: 0x10, QuestionId: 0x38A, VarStoreId: 0x1, VarOffset: 0x10CE, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x2000, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "1 M" Value: 1
					OneOfOption Option: "2 M" Value: 2
					OneOfOption Option: "4 M" Value: 4
					OneOfOption Option: "8 M" Value: 8
					OneOfOption Option: "16 M" Value: 16
					OneOfOption Option: "32 M" Value: 32
					OneOfOption Option: "64 M" Value: 64
					OneOfOption Option: "128 M" Value: 128
					OneOfOption Option: "256 M" Value: 256
					OneOfOption Option: "512 M" Value: 512
					OneOfOption Option: "1 G" Value: 1024
					OneOfOption Option: "2 G" Value: 2048
					OneOfOption Option: "4 G" Value: 4096
					OneOfOption Option: "8 G" Value: 8192
				End 
				Subtitle Prompt: "", Help: "", Flags: 0x0
				End 
				Subtitle Prompt: "WARNING:
Due to the Bridge Architecture Specification
Software can not apply selected padding for
64 and 32 bit PFMMIO window at the same time.
User must pick which PFMMIO he wants to padd
by setting another resource to Disable state.
If both PFMMIO set, 32 bit resource will be used.", Help: "", Flags: 0x0
				End 
			End 
		End 
	End 
	Form FormId: 0x2827, Title: "USB Configuration"
		Subtitle Prompt: "USB Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "USB Module Version", Help: "", Text: "00.00"
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "USB Controllers:", Help: "", Text: ""
		Subtitle Prompt: "N/A", Help: "", Flags: 0x0
		End 
		Text Prompt: "USB Devices:", Help: "", Text: ""
		Subtitle Prompt: "N/A", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdId QuestionId: 0x38B, OtherQuestionId: 0x38B
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "USB Support", Help: "USB Support Parameters", QuestionFlags: 0x10, QuestionId: 0x38B, VarStoreId: 0x2D, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "Legacy USB Support", Help: "Enables Legacy USB support. AUTO option disables legacy support if no USB devices are connected. DISABLE option will keep USB devices available only for EFI applications.", QuestionFlags: 0x10, QuestionId: 0x38C, VarStoreId: 0x2D, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Disabled" Value: 1
					OneOfOption Option: "Auto" Value: 2
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCB1, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "USB 2.0 Controller Mode", Help: "Configures the USB 2.0 controller in HiSpeed (480Mbps) or FullSpeed (12Mbps).", QuestionFlags: 0x10, QuestionId: 0x38D, VarStoreId: 0x2D, VarOffset: 0x1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "HiSpeed" Value: 1, Default, MfgDefault
					OneOfOption Option: "FullSpeed" Value: 0
				End 
			End 
		End 
		SuppressIf 
			True 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "XHCI Legacy Support", Help: "Enable/Disable XHCI Controller Legacy support.", QuestionFlags: 0x10, QuestionId: 0x38E, VarStoreId: 0x2D, VarOffset: 0x1A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					OneOfOption Option: "Disabled" Value: 0
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCB0, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "XHCI Hand-off", Help: "This is a workaround for OSes without XHCI hand-off support. The XHCI ownership change should be claimed by XHCI driver.", QuestionFlags: 0x10, QuestionId: 0x38F, VarStoreId: 0x2D, VarOffset: 0x1B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1
					OneOfOption Option: "Disabled" Value: 0
					Default DefaultId: 0x0 Value: 1
					Default DefaultId: 0x1 Value: 1
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCB1, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "EHCI Hand-off", Help: "This is a workaround for OSes without EHCI hand-off support. The EHCI ownership change should be claimed by EHCI driver.", QuestionFlags: 0x10, QuestionId: 0x390, VarStoreId: 0x2D, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0xCB3, Value: 0x0
					EqIdVal QuestionId: 0xCB2, Value: 0x0
					And 
					EqIdVal QuestionId: 0xCB1, Value: 0x0
					And 
					EqIdVal QuestionId: 0xCB0, Value: 0x0
					And 
					Or 
				End 
				OneOf Prompt: "USB Mass Storage Driver Support", Help: "Enable/Disable USB Mass Storage Driver Support.", QuestionFlags: 0x10, QuestionId: 0x391, VarStoreId: 0x2D, VarOffset: 0x1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "Port 60/64 Emulation", Help: "Enables I/O port 60h/64h emulation support. This should be enabled for the complete USB keyboard legacy support for non-USB aware OSes.", QuestionFlags: 0x10, QuestionId: 0x392, VarStoreId: 0x2D, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1
					Default DefaultId: 0x0 Value: 1
					Default DefaultId: 0x1 Value: 1
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Text Prompt: "USB hardware delays and time-outs:", Help: "", Text: ""
			SuppressIf 
				EqIdVal QuestionId: 0x38B, Value: 0x0
				GrayOutIf 
					EqIdVal QuestionId: 0xC42, Value: 0x1
						EqIdVal QuestionId: 0xCB3, Value: 0x0
						EqIdVal QuestionId: 0xCB2, Value: 0x0
						And 
						EqIdVal QuestionId: 0xCB1, Value: 0x0
						And 
						EqIdVal QuestionId: 0xCB0, Value: 0x0
						And 
						Or 
					End 
					OneOf Prompt: "USB transfer time-out", Help: "The time-out value for Control, Bulk, and Interrupt transfers.", QuestionFlags: 0x10, QuestionId: 0x393, VarStoreId: 0x2D, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x14, Step: 0x0
						OneOfOption Option: "1 sec" Value: 1
						OneOfOption Option: "5 sec" Value: 5
						OneOfOption Option: "10 sec" Value: 10
						OneOfOption Option: "20 sec" Value: 20, Default, MfgDefault
					End 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x38B, Value: 0x0
				GrayOutIf 
					EqIdVal QuestionId: 0xC42, Value: 0x1
						EqIdVal QuestionId: 0xCB3, Value: 0x0
						EqIdVal QuestionId: 0xCB2, Value: 0x0
						And 
						EqIdVal QuestionId: 0xCB1, Value: 0x0
						And 
						EqIdVal QuestionId: 0xCB0, Value: 0x0
						And 
						Or 
					End 
					OneOf Prompt: "Device reset time-out", Help: "USB mass storage device Start Unit command time-out.", QuestionFlags: 0x10, QuestionId: 0x394, VarStoreId: 0x2D, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
						OneOfOption Option: "10 sec" Value: 0
						OneOfOption Option: "20 sec" Value: 1, Default, MfgDefault
						OneOfOption Option: "30 sec" Value: 2
						OneOfOption Option: "40 sec" Value: 3
					End 
				End 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0xCB3, Value: 0x0
					EqIdVal QuestionId: 0xCB2, Value: 0x0
					And 
					EqIdVal QuestionId: 0xCB1, Value: 0x0
					And 
					EqIdVal QuestionId: 0xCB0, Value: 0x0
					And 
					Or 
				End 
				OneOf Prompt: "Device power-up delay", Help: "Maximum time the device will take before it properly reports itself to the Host Controller. 'Auto' uses default value: for a Root port it is 100 ms, for a Hub port the delay is taken from Hub descriptor.", QuestionFlags: 0x10, QuestionId: 0x395, VarStoreId: 0x2D, VarOffset: 0x1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Manual" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x395, Value: 0x0
				GrayOutIf 
					EqIdVal QuestionId: 0xC42, Value: 0x1
						EqIdVal QuestionId: 0xCB3, Value: 0x0
						EqIdVal QuestionId: 0xCB2, Value: 0x0
						And 
						EqIdVal QuestionId: 0xCB1, Value: 0x0
						And 
						EqIdVal QuestionId: 0xCB0, Value: 0x0
						And 
						Or 
					End 
					Numeric Prompt: "Device power-up delay in seconds", Help: "Delay range is 1..40 seconds, in one second increments", QuestionFlags: 0x10, QuestionId: 0x396, VarStoreId: 0x2D, VarOffset: 0x1D, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x28, Step: 0x1
						Default DefaultId: 0x0 Value: 5
						Default DefaultId: 0x1 Value: 5
					End 
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCAF, Value: 0x0
				Or 
			End 
			Text Prompt: "Mass Storage Devices:", Help: "", Text: ""
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCAE, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x397, VarStoreId: 0x2D, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCAD, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x398, VarStoreId: 0x2D, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCAC, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x399, VarStoreId: 0x2D, VarOffset: 0xC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCAB, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x39A, VarStoreId: 0x2D, VarOffset: 0xD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCAA, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x39B, VarStoreId: 0x2D, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCA9, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x39C, VarStoreId: 0x2D, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCA8, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x39D, VarStoreId: 0x2D, VarOffset: 0x10, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCA7, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x39E, VarStoreId: 0x2D, VarOffset: 0x11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCA6, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x39F, VarStoreId: 0x2D, VarOffset: 0x12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCA5, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x3A0, VarStoreId: 0x2D, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCA4, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x3A1, VarStoreId: 0x2D, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCA3, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x3A2, VarStoreId: 0x2D, VarOffset: 0x15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCA2, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x3A3, VarStoreId: 0x2D, VarOffset: 0x16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCA1, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x3A4, VarStoreId: 0x2D, VarOffset: 0x17, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xCA0, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x3A5, VarStoreId: 0x2D, VarOffset: 0x18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x38B, Value: 0x0
				EqIdVal QuestionId: 0xC9F, Value: 0x0
				Or 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
					EqIdVal QuestionId: 0x38C, Value: 0x1
					Or 
				End 
				OneOf Prompt: "N/A", Help: "Mass storage device emulation type. 'AUTO' enumerates devices according to their media format. Optical drives are emulated as 'CDROM', drives with no media will be emulated according to a drive type.", QuestionFlags: 0x10, QuestionId: 0x3A6, VarStoreId: 0x2D, VarOffset: 0x19, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
					OneOfOption Option: "CD-ROM" Value: 4
				End 
			End 
		End 
		Text Prompt: "", Help: "", Text: ""
		SuppressIf 
			True 
			SuppressIf 
				EqIdVal QuestionId: 0xC41, Value: 0xB
				Action Prompt: "", Help: "", QuestionFlags: 0x4, QuestionId: 0x2828, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, QuestionConfig: ""
				End 
			End 
		End 
	End 
	Form FormId: 0x282A, Title: "CSM Configuration"
		Subtitle Prompt: "Compatibility Support Module Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC4D, Value: 0x1
			OneOf Prompt: "CSM Support", Help: "Enable/Disable CSM Support.", QuestionFlags: 0x14, QuestionId: 0x2829, VarStoreId: 0x1, VarOffset: 0x10D0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x0 Value: 1
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2829, Value: 0x0
				Subtitle Prompt: "", Help: "", Flags: 0x0
				End 
				Text Prompt: "CSM16 Module Version", Help: "CSM16 Module Version", Text: "N/A, reset required"
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					Subtitle Prompt: "", Help: "", Flags: 0x0
					End 
					OneOf Prompt: "GateA20 Active", Help: "UPON REQUEST - GA20 can be disabled using BIOS services. ALWAYS - do not allow disabling GA20; this option is useful when any RT code is executed above 1MB.", QuestionFlags: 0x10, QuestionId: 0x3A7, VarStoreId: 0x1, VarOffset: 0x10D4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Upon Request" Value: 0, Default, MfgDefault
						OneOfOption Option: "Always" Value: 1
					End 
					SuppressIf 
						EqIdVal QuestionId: 0x3AC, Value: 0x2
							Not 
						End 
						OneOf Prompt: "Option ROM Messages", Help: "Set display mode for Option ROM", QuestionFlags: 0x10, QuestionId: 0x3A8, VarStoreId: 0x1, VarOffset: 0x10D1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
							OneOfOption Option: "Force BIOS" Value: 1, Default, MfgDefault
							OneOfOption Option: "Keep Current" Value: 0
						End 
					End 
					OneOf Prompt: "INT19 Trap Response", Help: "BIOS reaction on INT19 trapping by Option ROM: IMMEDIATE - execute the trap right away; POSTPONED - execute the trap during legacy boot.", QuestionFlags: 0x10, QuestionId: 0x3A9, VarStoreId: 0x1, VarOffset: 0x10D2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Immediate" Value: 1
						OneOfOption Option: "Postponed" Value: 0, Default, MfgDefault
					End 
					Subtitle Prompt: "", Help: "", Flags: 0x0
					End 
					OneOf Prompt: "Boot option filter", Help: "This option controls Legacy/UEFI ROMs priority", QuestionFlags: 0x10, QuestionId: 0x3AA, VarStoreId: 0x1, VarOffset: 0x10D5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "UEFI and Legacy" Value: 0, MfgDefault
						OneOfOption Option: "Legacy only" Value: 1
						OneOfOption Option: "UEFI only" Value: 2
					End 
				End 
				Subtitle Prompt: "", Help: "", Flags: 0x0
				End 
				Subtitle Prompt: "Option ROM execution", Help: "", Flags: 0x0
				End 
				OneOf Prompt: "Launch Network PXE OpROM", Help: "Controls the execution of UEFI and Legacy PXE OpROM", QuestionFlags: 0x10, QuestionId: 0x3AB, VarStoreId: 0x1, VarOffset: 0x10D6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					Default DefaultId: 0x0 Value: 0
					OneOfOption Option: "Do not launch" Value: 0, MfgDefault
					SuppressIf 
						Uint64 Value: 0x0
							Uint64 Value: 0x0
							Equal 
						End 
						OneOfOption Option: "UEFI" Value: 1
					End 
					OneOfOption Option: "Legacy" Value: 2
				End 
				OneOf Prompt: "Video", Help: "Controls the execution of UEFI and Legacy Video OpROM", QuestionFlags: 0x10, QuestionId: 0x3AC, VarStoreId: 0x1, VarOffset: 0x10D8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					Default DefaultId: 0x0 Value: 2
					OneOfOption Option: "Do not launch" Value: 0
					OneOfOption Option: "UEFI" Value: 1, MfgDefault
					OneOfOption Option: "Legacy" Value: 2
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					OneOf Prompt: "Storage", Help: "Controls the execution of UEFI and Legacy Storage OpROM", QuestionFlags: 0x10, QuestionId: 0x3AD, VarStoreId: 0x1, VarOffset: 0x10D7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
						Default DefaultId: 0x0 Value: 1
						OneOfOption Option: "Do not launch" Value: 0
						OneOfOption Option: "UEFI" Value: 1, MfgDefault
						OneOfOption Option: "Legacy" Value: 2
					End 
					OneOf Prompt: "Other PCI devices", Help: "Determines OpROM execution policy for devices other than Network, Storage, or Video", QuestionFlags: 0x10, QuestionId: 0x3AE, VarStoreId: 0x1, VarOffset: 0x10D9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
						OneOfOption Option: "Do not launch" Value: 0
						OneOfOption Option: "UEFI" Value: 1, Default, MfgDefault
						OneOfOption Option: "Legacy" Value: 2
					End 
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC4D, Value: 0x0
			Subtitle Prompt: "CSM configuration is disabled.", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "Compatibility Support Module is not loaded", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "due to active UEFI Secure Boot mode.", Help: "", Flags: 0x0
			End 
		End 
	End 
	Form FormId: 0x28ED, Title: "SDIO Configuration"
		Subtitle Prompt: "SDIO Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "SDIO Access Mode", Help: "Auto Option: Access SD device in DMA mode if controller supports it,otherwise in PIO mode.DMA Option: Access SD device in DMA mode.PIO Option: Access SD device in PIO mode.", QuestionFlags: 0x10, QuestionId: 0x3AF, VarStoreId: 0x2E, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "ADMA" Value: 1
				OneOfOption Option: "SDMA" Value: 2
				OneOfOption Option: "PIO" Value: 3
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC9E, Value: 0x0
			Text Prompt: "Mass Storage Devices:", Help: "", Text: ""
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "", Help: "", Text: ""
		Text Prompt: "", Help: "", Text: ""
		SuppressIf 
			EqIdValList QuestionId: 0xC9E, Values: [1, 2, 3, 4, 5, 6, 7, 8]
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x3B0, VarStoreId: 0x2E, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "", Help: "", Text: ""
		Text Prompt: "", Help: "", Text: ""
		SuppressIf 
			EqIdValList QuestionId: 0xC9E, Values: [2, 3, 4, 5, 6, 7, 8]
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x3B1, VarStoreId: 0x2E, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "", Help: "", Text: ""
		Text Prompt: "", Help: "", Text: ""
		SuppressIf 
			EqIdValList QuestionId: 0xC9E, Values: [3, 4, 5, 6, 7, 8]
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x3B2, VarStoreId: 0x2E, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "", Help: "", Text: ""
		Text Prompt: "", Help: "", Text: ""
		SuppressIf 
			EqIdValList QuestionId: 0xC9E, Values: [4, 5, 6, 7, 8]
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x3B3, VarStoreId: 0x2E, VarOffset: 0x1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "", Help: "", Text: ""
		Text Prompt: "", Help: "", Text: ""
		SuppressIf 
			EqIdValList QuestionId: 0xC9E, Values: [5, 6, 7, 8]
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x3B4, VarStoreId: 0x2E, VarOffset: 0x26, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "", Help: "", Text: ""
		Text Prompt: "", Help: "", Text: ""
		SuppressIf 
			EqIdValList QuestionId: 0xC9E, Values: [6, 7, 8]
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x3B5, VarStoreId: 0x2E, VarOffset: 0x2F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "", Help: "", Text: ""
		Text Prompt: "", Help: "", Text: ""
		SuppressIf 
			EqIdValList QuestionId: 0xC9E, Values: [7, 8]
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x3B6, VarStoreId: 0x2E, VarOffset: 0x38, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "", Help: "", Text: ""
		Text Prompt: "", Help: "", Text: ""
		SuppressIf 
			EqIdValList QuestionId: 0xC9E, Values: [8]
				Not 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xC42, Value: 0x1
				OneOf Prompt: "", Help: "Mass storage device emulation type. 'AUTO' enumerates devices less than 530MB as floppies. Forced FDD option can be used to force HDD formatted drive to boot as FDD.", QuestionFlags: 0x10, QuestionId: 0x3B7, VarStoreId: 0x2E, VarOffset: 0x41, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
					OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
					OneOfOption Option: "Floppy" Value: 1
					OneOfOption Option: "Forced FDD" Value: 2
					OneOfOption Option: "Hard Disk" Value: 3
				End 
			End 
		End 
	End 
	Form FormId: 0x290E, Title: "Switchable Graphics"
		GrayOutIf 
			EqIdVal QuestionId: 0x3FA, Value: 0x4
				Not 
			End 
			OneOf Prompt: "SG Mode Select", Help: "MUXed vs. MUX-less          (nVidia-Optimus, ATI-PX4.0/PX5.0) Note!!! Either mode requires PrimaryDisplay set to 'SG'", QuestionFlags: 0x10, QuestionId: 0x3B8, VarStoreId: 0x1, VarOffset: 0x10DA, Flags: 0x10, Size: 8, Min: 0x2, Max: 0x2, Step: 0x0
				OneOfOption Option: "Muxless" Value: 2, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x3FA, Value: 0x4
				Not 
				EqIdVal QuestionId: 0xC9D, Value: 0x0
				Or 
			End 
		End 
	End 
	Form FormId: 0x2713, Title: "Chipset"
		Ref Prompt: "System Agent (SA) Configuration", Help: "System Agent (SA) Parameters", QuestionFlags: 0x0, QuestionId: 0x3B9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x273D
		Ref Prompt: "PCH-IO Configuration", Help: "PCH Parameters", QuestionFlags: 0x0, QuestionId: 0x3BA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2754
	End 
	Form FormId: 0x273C, Title: "Memory Configuration"
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "Memory Thermal Configuration", Help: "Memory Thermal Configuration Options", QuestionFlags: 0x0, QuestionId: 0x3BB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x274D
			Ref Prompt: "Memory Training Algorithms", Help: "Enable/Disable Memory Training Algorithms.", QuestionFlags: 0x0, QuestionId: 0x3BC, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x274C
		End 
		Subtitle Prompt: "Memory Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "Memory RC Version", Help: "Memory RC Version", Text: "N/A"
		Text Prompt: "Memory Frequency", Help: "Displays the Frequency of Memory", Text: "N/A"
		Text Prompt: "Memory Timings (tCL-tRCD-tRP-tRAS)", Help: "Memory Timings", Text: "N/A"
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "Channel 0 Slot 0", Help: "Channel Slot Subtitle", Text: "N/A"
		SuppressIf 
			EqIdVal QuestionId: 0xC9C, Value: 0x0
			Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A"
			Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A"
			Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown"
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x3DB, Value: 0x2
			Text Prompt: "Channel 0 Slot 1", Help: "Channel Slot Subtitle", Text: "N/A"
			SuppressIf 
				EqIdVal QuestionId: 0xC9B, Value: 0x0
				Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A"
				Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A"
				Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown"
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x3DC, Value: 0x3
			Text Prompt: "Channel 1 Slot 0", Help: "Channel Slot Subtitle", Text: "N/A"
			SuppressIf 
				EqIdVal QuestionId: 0xC9A, Value: 0x0
				Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A"
				Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A"
				Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown"
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0x3DC, Values: [2, 3]
			Text Prompt: "Channel 1 Slot 1", Help: "Channel Slot Subtitle", Text: "N/A"
			SuppressIf 
				EqIdVal QuestionId: 0xC99, Value: 0x0
				Text Prompt: "    Size", Help: "Memory Size in the Slot.", Text: "N/A"
				Text Prompt: "    Number of Ranks", Help: "Number of Ranks in the slot", Text: "N/A"
				Text Prompt: "    Manufacturer", Help: "DIMM / DRAM Manufacturer Value", Text: "UnKnown"
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Text Prompt: "Memory ratio/reference clock options moved to Overclock->Memory->Custom Profile menu", Help: "", Text: ""
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			OneOf Prompt: "MRC ULT Safe Config", Help: "MRC ULT Safe Config for PO", QuestionFlags: 0x10, QuestionId: 0x3BD, VarStoreId: 0x1, VarOffset: 0x93B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Memory Test on Warm Boot", Help: "Enable Or Disable Base Memory Test Run on Warm Boot", QuestionFlags: 0x10, QuestionId: 0x3BE, VarStoreId: 0x1, VarOffset: 0x78A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		OneOf Prompt: "Maximum Memory Frequency", Help: "Maximum Memory Frequency Selections in Mhz.", QuestionFlags: 0x10, QuestionId: 0x3BF, VarStoreId: 0x1, VarOffset: 0x8AC, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1838, Step: 0x0
			OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x2
				OneOfOption Option: "1067" Value: 1067
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x1
				OneOfOption Option: "1200" Value: 1200
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x2
				OneOfOption Option: "1333" Value: 1333
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x1
				OneOfOption Option: "1400" Value: 1400
			End 
			OneOfOption Option: "1600" Value: 1600
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x1
				OneOfOption Option: "1800" Value: 1800
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x2
				OneOfOption Option: "1867" Value: 1867
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x1
				OneOfOption Option: "2000" Value: 2000
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x2
				OneOfOption Option: "2133" Value: 2133
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x1
				OneOfOption Option: "2200" Value: 2200
			End 
			OneOfOption Option: "2400" Value: 2400
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x1
				OneOfOption Option: "2600" Value: 2600
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x2
				OneOfOption Option: "2667" Value: 2667
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x1
				OneOfOption Option: "2800" Value: 2800
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x2
				OneOfOption Option: "2933" Value: 2933
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x1
				OneOfOption Option: "3000" Value: 3000
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x0
					EqIdVal QuestionId: 0x2E0, Value: 0x1
					Or 
				End 
				OneOfOption Option: "3100" Value: 3100
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x1
				OneOfOption Option: "3200" Value: 3200
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x1
				OneOfOption Option: "3400" Value: 3400
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x2
				OneOfOption Option: "3467" Value: 3467
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x1
				OneOfOption Option: "3600" Value: 3600
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x2
				OneOfOption Option: "3733" Value: 3733
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x1
				OneOfOption Option: "3800" Value: 3800
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x1
				OneOfOption Option: "4000" Value: 4000
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2E0, Value: 0x2
				OneOfOption Option: "4133" Value: 4133
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC98, Value: 0x6E0
					EqIdVal QuestionId: 0xC97, Value: 0x9
					And 
					QuestionRef1 QuestionId: 0xC96
					Uint8 Value: 0xA
					GreaterEqual 
					And 
					Not 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x1
					OneOfOption Option: "4200" Value: 4200
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x2
					OneOfOption Option: "4267" Value: 4267
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x1
					OneOfOption Option: "4400" Value: 4400
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x2
					OneOfOption Option: "4533" Value: 4533
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x1
					OneOfOption Option: "4600" Value: 4600
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x1
					OneOfOption Option: "4800" Value: 4800
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x1
					OneOfOption Option: "5000" Value: 5000
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x2
					OneOfOption Option: "5067" Value: 5067
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x1
					OneOfOption Option: "5200" Value: 5200
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x2
					OneOfOption Option: "5333" Value: 5333
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x1
					OneOfOption Option: "5400" Value: 5400
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x1
					OneOfOption Option: "5600" Value: 5600
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x1
					OneOfOption Option: "5800" Value: 5800
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x2
					OneOfOption Option: "5867" Value: 5867
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x1
					OneOfOption Option: "6000" Value: 6000
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x2
					OneOfOption Option: "6133" Value: 6133
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x2E0, Value: 0x1
					OneOfOption Option: "6200" Value: 6200
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			OneOf Prompt: "HOB Buffer Size", Help: "Size to set HOB Buffer", QuestionFlags: 0x10, QuestionId: 0x3C0, VarStoreId: 0x1, VarOffset: 0x8A9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "1B" Value: 1
				OneOfOption Option: "1KB" Value: 2
				OneOfOption Option: "Max (assuming 63KB total HOB size)" Value: 3
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC8C, Value: 0x2
					Not 
					EqIdVal QuestionId: 0xC8C, Value: 0x5
					Not 
					And 
					EqIdVal QuestionId: 0xC8C, Value: 0x4
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x44
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x4A
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x50
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x45
					Not 
					And 
					EqIdVal QuestionId: 0xC50, Value: 0x48
					Not 
					And 
					EqIdVal QuestionId: 0xC8C, Value: 0x3
					Not 
					And 
				End 
				OneOf Prompt: "ECC Support", Help: "Enable/disable DDR Ecc Support", QuestionFlags: 0x10, QuestionId: 0x3C1, VarStoreId: 0x1, VarOffset: 0x8AA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			OneOf Prompt: "Max TOLUD", Help: "Maximum Value of TOLUD. Dynamic assignment would adjust TOLUD automatically based on largest MMIO length of installed graphic controller", QuestionFlags: 0x10, QuestionId: 0x3C2, VarStoreId: 0x1, VarOffset: 0x8AB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xB, Step: 0x0
				OneOfOption Option: "Dynamic" Value: 0
				OneOfOption Option: "1 GB" Value: 1
				OneOfOption Option: "1.25 GB" Value: 2
				OneOfOption Option: "1.5 GB" Value: 3
				OneOfOption Option: "1.75 GB" Value: 4
				OneOfOption Option: "2 GB" Value: 5
				OneOfOption Option: "2.25 GB" Value: 6
				OneOfOption Option: "2.5 GB" Value: 7
				OneOfOption Option: "2.75 GB" Value: 8
				OneOfOption Option: "3 GB" Value: 9
				OneOfOption Option: "3.25 GB" Value: 10
				OneOfOption Option: "3.5 GB" Value: 11, Default, MfgDefault
			End 
			OneOf Prompt: "SA GV", Help: "System Agent Geyserville. Fixed Low/High: SA GV disabled, MRC only runs tasks from Low or High point. SA GV will be disabled on DT/Halo CPUs and before C0/J0, regardless of this setting.", QuestionFlags: 0x10, QuestionId: 0x3C3, VarStoreId: 0x1, VarOffset: 0x8C9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Fixed Low" Value: 1
				OneOfOption Option: "Fixed High" Value: 2
				OneOfOption Option: "Enabled" Value: 3
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x3C3, Value: 0x1
					Not 
					EqIdVal QuestionId: 0x3C3, Value: 0x3
					Not 
					And 
				End 
				OneOf Prompt: "SA GV Low Freq", Help: "System Agent Geyserville. Set frequency for low point. Default 1067 for LPDDR3/DDR3, 1333 for DDR4. NOTE: must be below or equal to the SA GV High frequency.", QuestionFlags: 0x10, QuestionId: 0x3C4, VarStoreId: 0x1, VarOffset: 0x8CA, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x74B, Step: 0x0
					OneOfOption Option: "MRC default" Value: 0, Default, MfgDefault
					OneOfOption Option: "1067" Value: 1067
					OneOfOption Option: "1200" Value: 1200
					OneOfOption Option: "1333" Value: 1333
					OneOfOption Option: "1400" Value: 1400
					OneOfOption Option: "1600" Value: 1600
					OneOfOption Option: "1800" Value: 1800
					OneOfOption Option: "1867" Value: 1867
				End 
			End 
			OneOf Prompt: "Retrain on Fast Fail", Help: "Restart MRC in Cold mode if SW MemTest fails during Fast flow. Default = Enabled", QuestionFlags: 0x10, QuestionId: 0x3C5, VarStoreId: 0x1, VarOffset: 0x8C1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "Command Tristate", Help: "Command Tristate Support.", QuestionFlags: 0x10, QuestionId: 0x3C6, VarStoreId: 0x1, VarOffset: 0x8C2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 1
			End 
			OneOf Prompt: "BER Support", Help: "Enable/Disable the Rank Margin Tool interpolation/extrapolation.", QuestionFlags: 0x10, QuestionId: 0x3C7, VarStoreId: 0x1, VarOffset: 0x78B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "Enable RH Prevention", Help: "Actively prevent Row Hammer", QuestionFlags: 0x10, QuestionId: 0x3C8, VarStoreId: 0x1, VarOffset: 0x93C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x3C8, Value: 0x0
				OneOf Prompt: "Row Hammer Solution", Help: "Type of method used to prevent Row Hammer", QuestionFlags: 0x10, QuestionId: 0x3C9, VarStoreId: 0x1, VarOffset: 0x93D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Hardware RHP" Value: 0, Default, MfgDefault
					OneOfOption Option: "2x Refresh" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x3C8, Value: 0x0
					EqIdVal QuestionId: 0x3C9, Value: 0x1
					Or 
				End 
				OneOf Prompt: "RH Activation Probability", Help: "Used to adjust MC for Hardware RHP.", QuestionFlags: 0x10, QuestionId: 0x3CA, VarStoreId: 0x1, VarOffset: 0x93E, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xF, Step: 0x0
					OneOfOption Option: "1/2^1" Value: 1
					OneOfOption Option: "1/2^2" Value: 2
					OneOfOption Option: "1/2^3" Value: 3
					OneOfOption Option: "1/2^4" Value: 4
					OneOfOption Option: "1/2^5" Value: 5
					OneOfOption Option: "1/2^6" Value: 6
					OneOfOption Option: "1/2^7" Value: 7
					OneOfOption Option: "1/2^8" Value: 8
					OneOfOption Option: "1/2^9" Value: 9
					OneOfOption Option: "1/2^10" Value: 10
					OneOfOption Option: "1/2^11" Value: 11, Default, MfgDefault
					OneOfOption Option: "1/2^12" Value: 12
					OneOfOption Option: "1/2^13" Value: 13
					OneOfOption Option: "1/2^14" Value: 14
					OneOfOption Option: "1/2^15" Value: 15
				End 
			End 
			OneOf Prompt: "Exit On Failure (MRC)", Help: "Exit On Failure for MRC training steps", QuestionFlags: 0x10, QuestionId: 0x3CB, VarStoreId: 0x1, VarOffset: 0x940, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "MC Lock", Help: "Enable/Disable capacity to lock or not MC registers", QuestionFlags: 0x10, QuestionId: 0x3CC, VarStoreId: 0x1, VarOffset: 0x8C3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "Probeless Trace", Help: "HD Port, GDXC IOT/MOT or Disabled", QuestionFlags: 0x10, QuestionId: 0x3CD, VarStoreId: 0x1, VarOffset: 0x8C5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "GDXC IOT/MOT" Value: 1
				OneOfOption Option: "HD Port" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x3CD, Value: 0x1
					Not 
				End 
				Numeric Prompt: "GDXC IOT size", Help: "Size of IOT and MOT is in 8 MB chunks", QuestionFlags: 0x10, QuestionId: 0x3CE, VarStoreId: 0x1, VarOffset: 0x8C6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x1
					Default DefaultId: 0x0 Value: 4
				End 
				Numeric Prompt: "GDXC MOT size", Help: "Size of IOT and MOT is in 8 MB chunks", QuestionFlags: 0x10, QuestionId: 0x3CF, VarStoreId: 0x1, VarOffset: 0x8C7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x80, Step: 0x1
					Default DefaultId: 0x0 Value: 12
				End 
				OneOf Prompt: "Memory Trace", Help: "Enable Memory Trace of Ch 0 to Ch 1 using Stacked Mode. Both channels must be of equal size. This option may change TOLUD and REMAP values as needed.", QuestionFlags: 0x10, QuestionId: 0x3D0, VarStoreId: 0x1, VarOffset: 0x8C8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0x3CD, Value: 0x0
					Not 
				End 
				OneOf Prompt: "Enable/Disable IED (Intel Enhanced Debug)", Help: "Intel Enhanced Debug requires 4MB SMM memory", QuestionFlags: 0x10, QuestionId: 0x3D1, VarStoreId: 0x1, VarOffset: 0x87F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "Ch Hash Support", Help: "Enable/Disable Channel Hash Support. NOTE: ONLY if Memory interleaved Mode", QuestionFlags: 0x10, QuestionId: 0x3D2, VarStoreId: 0x1, VarOffset: 0x8B1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			Numeric Prompt: "Ch Hash Mask", Help: "Set the BIT(s) to be included in the XOR function. NOTE BIT mask corresponds to BITS [19:6}. 0-Auto, Range 1-16,383.", QuestionFlags: 0x10, QuestionId: 0x3D3, VarStoreId: 0x1, VarOffset: 0x8B2, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "Ch Hash Interleaved Bit", Help: "Select the BIT to be used for Channel Interleaved mode. NOTE: BIT7 will interlave the channels at a 2 cacheline granularity, BIT8 at 4 and BIT9 at 8", QuestionFlags: 0x10, QuestionId: 0x3D4, VarStoreId: 0x1, VarOffset: 0x8B4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
				OneOfOption Option: "BIT6" Value: 0
				OneOfOption Option: "BIT7" Value: 1
				OneOfOption Option: "BIT8" Value: 2, Default, MfgDefault
				OneOfOption Option: "BIT9" Value: 3
				OneOfOption Option: "BIT10" Value: 4
				OneOfOption Option: "BIT11" Value: 5
				OneOfOption Option: "BIT12" Value: 6
				OneOfOption Option: "BIT13" Value: 7
			End 
			OneOf Prompt: "VC1 Read Metering", Help: "Enable/Disable VC1 Read Metering Feature (RdMeter)", QuestionFlags: 0x10, QuestionId: 0x3D5, VarStoreId: 0x1, VarOffset: 0x8B5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x3D5, Value: 0x0
				Numeric Prompt: "VC1 RdMeter Time Window", Help: "VC1 Read Metering Time Window: time window over which VC1 read request counter is tracked. Configurable for tens of microseconds window size.", QuestionFlags: 0x10, QuestionId: 0x3D6, VarStoreId: 0x1, VarOffset: 0x8B6, Flags: 0x12, Size: 32, Min: 0x0, Max: 0x1FFFF, Step: 0x1
					Default DefaultId: 0x0 Value: 800
				End 
				Numeric Prompt: "VC1 RdMeter Threshold", Help: "VC1 Read Metering Threshold: threshold of counter within time window.", QuestionFlags: 0x10, QuestionId: 0x3D7, VarStoreId: 0x1, VarOffset: 0x8BA, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
					Default DefaultId: 0x0 Value: 280
				End 
			End 
			Numeric Prompt: "Strong Weak Leaker", Help: "Value for StrongWkLeaker", QuestionFlags: 0x10, QuestionId: 0x3D8, VarStoreId: 0x1, VarOffset: 0x8BC, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x7, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "Memory Scrambler", Help: "Enable/Disable Memory Scrambler support.", QuestionFlags: 0x10, QuestionId: 0x3D9, VarStoreId: 0x1, VarOffset: 0x936, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "Force ColdReset", Help: "Force ColdReset OR Choose MrcColdBoot mode, when Coldboot is required during MRC execution. Note: If ME 5.0MB is present, ForceColdReset is required!", QuestionFlags: 0x10, QuestionId: 0x3DA, VarStoreId: 0x1, VarOffset: 0x937, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "Channel A DIMM Control", Help: "Channel A DIMM Control Support - Enable or Disable Dimms on Channel A.", QuestionFlags: 0x10, QuestionId: 0x3DB, VarStoreId: 0x1, VarOffset: 0x938, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Enable both DIMMs" Value: 0
				OneOfOption Option: "Disable DIMM0" Value: 1
				OneOfOption Option: "Disable DIMM1" Value: 2, Default, MfgDefault
				OneOfOption Option: "Disable both DIMMs" Value: 3
			End 
			OneOf Prompt: "Channel B DIMM Control", Help: "Channel B DIMM Control Support - Enable or Disable Dimms on Channel B.", QuestionFlags: 0x10, QuestionId: 0x3DC, VarStoreId: 0x1, VarOffset: 0x939, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Enable both DIMMs" Value: 0
				OneOfOption Option: "Disable DIMM0" Value: 1
				OneOfOption Option: "Disable DIMM1" Value: 2, Default, MfgDefault
				OneOfOption Option: "Disable both DIMMs" Value: 3
			End 
			OneOf Prompt: "Force Single Rank", Help: "When enabled, only Rank 0 will be used in each DIMM", QuestionFlags: 0x10, QuestionId: 0x3DD, VarStoreId: 0x1, VarOffset: 0x8BD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Memory Remap", Help: "Enable/Disable Memory Remap above 4GB", QuestionFlags: 0x10, QuestionId: 0x3DE, VarStoreId: 0x1, VarOffset: 0x93A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
			OneOf Prompt: "Time Measure", Help: "Enable/Disable printing of the time it takes to execute MRC.", QuestionFlags: 0x10, QuestionId: 0x3DF, VarStoreId: 0x1, VarOffset: 0x8AF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "DLL Weak Lock Support", Help: "Enable/Disable Dll Weaklock support", QuestionFlags: 0x10, QuestionId: 0x3E0, VarStoreId: 0x1, VarOffset: 0x785, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			Numeric Prompt: "Pwr Down Idle Timer", Help: "The minimum value should = to the worst case Roundtrip delay + Burst_Length. 0 means AUTO: 64 for ULX/ULT, 128 for DT/Halo", QuestionFlags: 0x10, QuestionId: 0x3E1, VarStoreId: 0x1, VarOffset: 0x784, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
				Default DefaultId: 0x1 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC98, Value: 0x6E0
					EqIdVal QuestionId: 0xC97, Value: 0x4
					EqIdVal QuestionId: 0xC96, Value: 0x0
					EqIdVal QuestionId: 0xC96, Value: 0x1
					Or 
					And 
					EqIdVal QuestionId: 0xC97, Value: 0x5
					EqIdVal QuestionId: 0xC96, Value: 0x0
					And 
					Or 
					And 
					Not 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC98, Value: 0x6E0
					EqIdVal QuestionId: 0xC97, Value: 0x4
					EqIdVal QuestionId: 0xC96, Value: 0x0
					EqIdVal QuestionId: 0xC96, Value: 0x1
					Or 
					And 
					EqIdVal QuestionId: 0xC97, Value: 0x5
					EqIdVal QuestionId: 0xC96, Value: 0x0
					And 
					Or 
					And 
				End 
				OneOf Prompt: "Mrc Fast Boot", Help: "Enable/Disable fast path thru the MRC", QuestionFlags: 0x10, QuestionId: 0x3E2, VarStoreId: 0x1, VarOffset: 0x8B0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "Lpddr Mem WL Set", Help: "Only applicable to LPDDR, Memory Write Latency Set selection (A is default, B will be used if memory devices support it)", QuestionFlags: 0x10, QuestionId: 0x3E3, VarStoreId: 0x1, VarOffset: 0x8BE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Set A" Value: 0
				OneOfOption Option: "Set B" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "BDAT ACPI Table Support", Help: "Enables support for the BDAT ACPI table.", QuestionFlags: 0x10, QuestionId: 0x3E4, VarStoreId: 0x1, VarOffset: 0x786, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0x3E4, Value: 0x0
				OneOf Prompt: "BDAT Memory Data Schema", Help: "Indicates the BDAT Schema version used to format test results for the BDAT ACPI table.", QuestionFlags: 0x10, QuestionId: 0x3E5, VarStoreId: 0x1, VarOffset: 0x788, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "2" Value: 0
					OneOfOption Option: "6B" Value: 1, Default, MfgDefault
				End 
				OneOf Prompt: "BDAT Memory Test Type", Help: "Indicates the type of Memory Training data to populate into the BDAT ACPI table.", QuestionFlags: 0x10, QuestionId: 0x3E6, VarStoreId: 0x1, VarOffset: 0x787, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Rank Margin Tool Rank" Value: 0, Default, MfgDefault
					SuppressIf 
						EqIdVal QuestionId: 0x3E5, Value: 0x0
						OneOfOption Option: "Rank Margin Tool Bit" Value: 1
						OneOfOption Option: "Margin 2D" Value: 2
					End 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x3E6, Value: 0x2
				Numeric Prompt: "Rank Margin Tool Loop Count", Help: "Specifies the Loop Count to be used during Rank Margin Tool Testing. 0 - AUTO", QuestionFlags: 0x10, QuestionId: 0x3E7, VarStoreId: 0x1, VarOffset: 0x789, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x20, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			OneOf Prompt: "EV Loader", Help: "Enable/Disable EV Loader Functionality", QuestionFlags: 0x10, QuestionId: 0x3E8, VarStoreId: 0x1, VarOffset: 0x8BF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "EV Loader Delay", Help: "Enable/Disable EV Loader 2 Second Delay", QuestionFlags: 0x10, QuestionId: 0x3E9, VarStoreId: 0x1, VarOffset: 0x8C0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
		End 
	End 
	Form FormId: 0x273D, Title: "System Agent (SA) Configuration"
		Subtitle Prompt: "System Agent (SA) Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "SA PCIe Code Version", Help: "SA PCIe", Text: "N/A"
		Text Prompt: "VT-d", Help: "VT-d capability", Text: "N/A"
		SuppressIf 
			EqIdVal QuestionId: 0xC94, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC95, Value: 0x1
				OneOf Prompt: "VT-d", Help: "VT-d capability", QuestionFlags: 0x10, QuestionId: 0x3EA, VarStoreId: 0x1, VarOffset: 0x87A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC94, Value: 0x0
				EqIdVal QuestionId: 0x3EA, Value: 0x0
				Or 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC93, Value: 0x0
				OneOf Prompt: "X2APIC Opt Out", Help: "Enable/Disable X2APIC_OPT_OUT bit", QuestionFlags: 0x10, QuestionId: 0x3EB, VarStoreId: 0x1, VarOffset: 0x880, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Ref Prompt: "Memory Configuration", Help: "Memory Configuration Parameters", QuestionFlags: 0x0, QuestionId: 0x3EC, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x273C
		Ref Prompt: "Graphics Configuration", Help: "Graphics Configuration", QuestionFlags: 0x0, QuestionId: 0x3ED, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x273E
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "DMI/OPI Configuration", Help: "Control various DMI functions.", QuestionFlags: 0x0, QuestionId: 0x3EE, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x273F
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC51, Value: 0x1
				Not 
			End 
			Ref Prompt: "PEG Port Configuration", Help: "PEG Port Options", QuestionFlags: 0x0, QuestionId: 0x3EF, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2744
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			OneOf Prompt: "Stop Grant Configuration", Help: "Automatic/Manual stop grant configuration", QuestionFlags: 0x10, QuestionId: 0x3F0, VarStoreId: 0x1, VarOffset: 0x899, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Auto" Value: 1, Default, MfgDefault
				OneOfOption Option: "Manual" Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x3F0, Value: 0x1
				Numeric Prompt: "Number of Stop Grant Cycles", Help: "Selects number of Stop-Grant cycles.", QuestionFlags: 0x10, QuestionId: 0x3F1, VarStoreId: 0x1, VarOffset: 0x89A, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3F, Step: 0x0
					Default DefaultId: 0x0 Value: 1
				End 
			End 
			OneOf Prompt: "CHAP Device (B0:D7:F0)", Help: "Enable/Disable SA CHAP Device.", QuestionFlags: 0x10, QuestionId: 0x3F2, VarStoreId: 0x1, VarOffset: 0x878, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "Thermal Device (B0:D4:F0)", Help: "Enable/Disable SA Thermal Device.", QuestionFlags: 0x10, QuestionId: 0x3F3, VarStoreId: 0x1, VarOffset: 0x879, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "GMM Device (B0:D8:F0)", Help: "Enable/Disable SA GMM Device.", QuestionFlags: 0x10, QuestionId: 0x3F4, VarStoreId: 0x1, VarOffset: 0x87C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
			OneOf Prompt: "CRID Support", Help: "Enable/Disable CRID control for Intel SIPP", QuestionFlags: 0x14, QuestionId: 0x2739, VarStoreId: 0x1, VarOffset: 0x942, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x273A, Value: 0xF
				OneOf Prompt: "Above 4GB MMIO BIOS assignment", Help: "Enable/Disable above 4GB MemoryMappedIO BIOS assignment

This is enabled automatically when Aperture Size is set to 2048MB.", QuestionFlags: 0x10, QuestionId: 0x3F5, VarStoreId: 0x1, VarOffset: 0x87B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [7, 19]
								Uint64 Value: 0x0
								Uint64 Value: 0x1
								Conditional 
							End 
						End 
					End 
					OneOfOption Option: "Enabled" Value: 1
					OneOfOption Option: "Disabled" Value: 0
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC92, Value: 0x0
				GrayOutIf 
					EqIdVal QuestionId: 0xA39, Value: 0x0
					OneOf Prompt: "SKY CAM Device (B0:D5:F0)", Help: "Enable/Disable SA SKY CAM Device.", QuestionFlags: 0x10, QuestionId: 0x3F6, VarStoreId: 0x1, VarOffset: 0x87D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Enabled" Value: 1
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					End 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC91, Value: 0x1
					Not 
				End 
				OneOf Prompt: "eDRAM Mode", Help: "SW Mode eDRAM On or eDRAM Off", QuestionFlags: 0x10, QuestionId: 0x3F7, VarStoreId: 0x1, VarOffset: 0x87E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "SW Mode eDRAM Off" Value: 0
					OneOfOption Option: "SW Mode eDRAM On" Value: 1
					OneOfOption Option: "eDRAM HW Mode" Value: 2, Default
				End 
			End 
		End 
	End 
	Form FormId: 0x273E, Title: "Graphics Configuration"
		Subtitle Prompt: "Graphics Configuration", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8C, Value: 0x4
			Text Prompt: "IGFX VBIOS Version", Help: "IGFX VBIOS Version", Text: "N/A"
			Text Prompt: "IGFX GOP Version", Help: "IGFX GOP Version", Text: "N/A"
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC8C, Value: 0x4
				Numeric Prompt: "Graphics Turbo IMON Current", Help: "Graphics turbo IMON current values supported (14-31)", QuestionFlags: 0x10, QuestionId: 0x3F8, VarStoreId: 0x1, VarOffset: 0x8A8, Flags: 0x10, Size: 8, Min: 0xE, Max: 0x1F, Step: 0x1
					Default DefaultId: 0x0 Value: 31
				End 
			End 
			OneOf Prompt: "Skip Scaning of External Gfx Card", Help: "If Enable, it will not scan for External Gfx Card on PEG and PCH PCIE Ports", QuestionFlags: 0x10, QuestionId: 0x3F9, VarStoreId: 0x1, VarOffset: 0x941, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
		End 
		OneOf Prompt: "Primary Display", Help: "Select which of IGFX/PEG/PCI Graphics device should be Primary Display Or select SG for Switchable Gfx.", QuestionFlags: 0x10, QuestionId: 0x3FA, VarStoreId: 0x1, VarOffset: 0x89B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
			OneOfOption Option: "Auto" Value: 3, Default, MfgDefault
			OneOfOption Option: "IGFX" Value: 0
			SuppressIf 
				EqIdVal QuestionId: 0xC51, Value: 0x2
					EqIdVal QuestionId: 0xC8C, Value: 0x1
					EqIdVal QuestionId: 0xC8C, Value: 0x5
					Or 
					And 
				End 
				OneOfOption Option: "PEG" Value: 1
			End 
			OneOfOption Option: "PCI" Value: 2
			SuppressIf 
				EqIdVal QuestionId: 0xC8C, Value: 0x4
				OneOfOption Option: "SG" Value: 4
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8C, Value: 0x4
			OneOf Prompt: "Select PCIE Card", Help: "Select the card used on the platform
Auto       : Skip GPIO based Power Enable to dGPU
Elk Creek 4: DGPU Power Enable = ActiveLow
PEG Eval   : DGPU Power Enable = ActiveHigh", QuestionFlags: 0x10, QuestionId: 0x3FB, VarStoreId: 0x1, VarOffset: 0x89C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [74]
							Uint64 Value: 0x2
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Auto" Value: 2
				OneOfOption Option: "Elk Creek 4" Value: 0
				OneOfOption Option: "PEG Eval" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x3FA, Value: 0x4
				Not 
			End 
			Numeric Prompt: "SG Delay After Power Enable", Help: "Delay in milli-seconds after power enable", QuestionFlags: 0x0, QuestionId: 0x3FC, VarStoreId: 0x1, VarOffset: 0x89D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x0
				Default DefaultId: 0x0 Value: 300
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x3FA, Value: 0x4
				Not 
			End 
			Numeric Prompt: "SG Delay After Hold Reset", Help: "Delay in milli-seconds after hold reset", QuestionFlags: 0x0, QuestionId: 0x3FD, VarStoreId: 0x1, VarOffset: 0x8A5, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x0
				Default DefaultId: 0x0 Value: 100
			End 
		End 
		Ref Prompt: "External Gfx Card Primary Display Configuration", Help: "External Gfx Card Primary Display Configuration", QuestionFlags: 0x0, QuestionId: 0x3FE, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x280F
		SuppressIf 
			EqIdVal QuestionId: 0x3FA, Value: 0x4
				Not 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x4A
					Not 
				End 
				Numeric Prompt: "SG Delay After Off Method", Help: "Delay in milli-seconds after off method is called", QuestionFlags: 0x0, QuestionId: 0x3FF, VarStoreId: 0x1, VarOffset: 0x89F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [74]
								Uint64 Value: 0x0
								Uint64 Value: 0xC8
								Conditional 
							End 
						End 
					End 
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x3FA, Value: 0x4
				Not 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x4A
					Not 
				End 
				Numeric Prompt: "SG Delay After Link Enable", Help: "Delay in milli-seconds after link enable", QuestionFlags: 0x0, QuestionId: 0x400, VarStoreId: 0x1, VarOffset: 0x8A1, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3E8, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [74]
								Uint64 Value: 0x0
								Uint64 Value: 0xFA
								Conditional 
							End 
						End 
					End 
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x3FA, Value: 0x4
				Not 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x4A
					Not 
				End 
				OneOf Prompt: "Gen Speed Change in ACPI", Help: "Enable/Disable Gen Speed Change. In an _OFF call for PEG0, the link will be placed into Gen1 prior to entering L2. In the _ON call, after exiting L2 back to L0, the link will be put back in Gen3. This helps mitigate Gen3 framing errors on L2 entry", QuestionFlags: 0x10, QuestionId: 0x401, VarStoreId: 0x1, VarOffset: 0x8A3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [74]
								Uint64 Value: 0x0
								Uint64 Value: 0x1
								Conditional 
							End 
						End 
					End 
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC50, Value: 0x20
			OneOf Prompt: "Internal Graphics", Help: "Keep IGFX enabled based on the setup options.", QuestionFlags: 0x10, QuestionId: 0x402, VarStoreId: 0x1, VarOffset: 0x8A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		OneOf Prompt: "GTT Size", Help: "Select the GTT Size ", QuestionFlags: 0x10, QuestionId: 0x403, VarStoreId: 0x1, VarOffset: 0x7D7, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3, Step: 0x0
			OneOfOption Option: "2MB" Value: 1
			OneOfOption Option: "4MB" Value: 2
			OneOfOption Option: "8MB" Value: 3, Default, MfgDefault
		End 
		OneOf Prompt: "Aperture Size", Help: "Select the Aperture Size

Note : Above 4GB MMIO BIOS assignment is automatically enabled when selecting 2048MB aperture. To use this feature, please disable CSM Support.", QuestionFlags: 0x14, QuestionId: 0x273A, VarStoreId: 0x1, VarOffset: 0x7D8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
			OneOfOption Option: "128MB" Value: 0
			OneOfOption Option: "256MB" Value: 1, Default, MfgDefault
			OneOfOption Option: "512MB" Value: 3
			OneOfOption Option: "1024MB" Value: 7
			OneOfOption Option: "2048MB" Value: 15
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC50, Value: 0x20
			OneOf Prompt: "DVMT Pre-Allocated", Help: "Select DVMT 5.0 Pre-Allocated (Fixed) Graphics Memory size used by the Internal Graphics Device.", QuestionFlags: 0x14, QuestionId: 0x273B, VarStoreId: 0x1, VarOffset: 0x876, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFE, Step: 0x0
				OneOfOption Option: "0M" Value: 0
				OneOfOption Option: "32M" Value: 1, Default, MfgDefault
				OneOfOption Option: "64M" Value: 2
				OneOfOption Option: "4M" Value: 240
				OneOfOption Option: "8M" Value: 241
				OneOfOption Option: "12M" Value: 242
				OneOfOption Option: "16M" Value: 243
				OneOfOption Option: "20M" Value: 244
				OneOfOption Option: "24M" Value: 245
				OneOfOption Option: "28M" Value: 246
				OneOfOption Option: "32M/F7" Value: 247
				OneOfOption Option: "36M" Value: 248
				OneOfOption Option: "40M" Value: 249
				OneOfOption Option: "44M" Value: 250
				OneOfOption Option: "48M" Value: 251
				OneOfOption Option: "52M" Value: 252
				OneOfOption Option: "56M" Value: 253
				OneOfOption Option: "60M" Value: 254
			End 
		End 
		OneOf Prompt: "DVMT Total Gfx Mem", Help: "Select DVMT5.0 Total Graphic Memory size used by the Internal Graphics Device.", QuestionFlags: 0x10, QuestionId: 0x404, VarStoreId: 0x1, VarOffset: 0x877, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3, Step: 0x0
			OneOfOption Option: "256M" Value: 2, Default, MfgDefault
			OneOfOption Option: "128M" Value: 1
			OneOfOption Option: "MAX" Value: 3
		End 
		SuppressIf 
			True 
			OneOf Prompt: "Intel Graphics Pei Display Peim", Help: "Enable/Disable Pei (Early) Display", QuestionFlags: 0x10, QuestionId: 0x405, VarStoreId: 0x1, VarOffset: 0x7DB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC8C, Value: 0x4
				OneOf Prompt: "Gfx Low Power Mode", Help: "This option is applicable for SFF only.", QuestionFlags: 0x10, QuestionId: 0x406, VarStoreId: 0x1, VarOffset: 0x7D1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					OneOfOption Option: "Disabled" Value: 0
				End 
			End 
			SuppressIf 
				True 
				OneOf Prompt: "ALS Support", Help: "Valid only for ACPI.

Legacy = ALS Support through the IGFX INT10 function.

ACPI = ALS support through an ACPI ALS driver.", QuestionFlags: 0x10, QuestionId: 0x407, VarStoreId: 0x1, VarOffset: 0x7CE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Enabled" Value: 2
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC8C, Value: 0x4
				OneOf Prompt: "VDD Enable", Help: "Enable/Disable forcing of VDD in the BIOS", QuestionFlags: 0x10, QuestionId: 0x408, VarStoreId: 0x1, VarOffset: 0x7D9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "PM Support", Help: "Enable/Disable PM Support", QuestionFlags: 0x10, QuestionId: 0x409, VarStoreId: 0x1, VarOffset: 0x7DA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
			OneOf Prompt: "PAVP Enable", Help: "Enable/Disable PAVP", QuestionFlags: 0x10, QuestionId: 0x40A, VarStoreId: 0x1, VarOffset: 0x7DC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
			OneOf Prompt: "Cdynmax Clamping Enable", Help: "Enable/Disable Cdynmax Clamping", QuestionFlags: 0x10, QuestionId: 0x40B, VarStoreId: 0x1, VarOffset: 0x7DF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
			OneOf Prompt: "Cd Clock Frequency", Help: "Select the highest Cd Clock frequency supported by the platform", QuestionFlags: 0x10, QuestionId: 0x40C, VarStoreId: 0x1, VarOffset: 0x30, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "337.5 Mhz" Value: 0
				OneOfOption Option: "450 Mhz" Value: 1
				OneOfOption Option: "540 Mhz" Value: 2
				OneOfOption Option: "675 Mhz" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "IUER Button Enable", Help: "Enable/Disable IUER Button Functionality", QuestionFlags: 0x10, QuestionId: 0x40D, VarStoreId: 0x1, VarOffset: 0x947, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8C, Value: 0x4
				EqIdVal QuestionId: 0x3AC, Value: 0x2
				Not 
				Or 
				EqIdVal QuestionId: 0x2829, Value: 0x0
				Or 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC42, Value: 0x0
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Or 
				End 
				Ref Prompt: "LCD Control", Help: "LCD Control", QuestionFlags: 0x0, QuestionId: 0x40E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2749
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "Intel(R) Ultrabook Event Support", Help: "Intel(R) Ultrabook Event Support", QuestionFlags: 0x0, QuestionId: 0x40F, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x274A
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8C, Value: 0x4
				EqIdVal QuestionId: 0x3AC, Value: 0x2
				Not 
				Or 
				EqIdVal QuestionId: 0x2829, Value: 0x0
				Or 
			End 
			OneOf Prompt: "Primary IGFX Boot Display", Help: "Select the Video Device which will be activated during POST.
This has no effect if external graphics present.
Secondary boot display selection will appear based on your selection.
VGA modes will be supported only on primary display
", QuestionFlags: 0x10, QuestionId: 0x410, VarStoreId: 0x1, VarOffset: 0x7C6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x40, Step: 0x0
				OneOfOption Option: "VBIOS Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "VGA" Value: 4
				OneOfOption Option: "HDMI1" Value: 64
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x410, Value: 0x0
				OneOf Prompt: "Secondary IGFX Boot Display", Help: "Select Secondary Display Device", QuestionFlags: 0x10, QuestionId: 0x411, VarStoreId: 0x1, VarOffset: 0x7C7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x40, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "VGA" Value: 4
					OneOfOption Option: "HDMI1" Value: 64
				End 
			End 
		End 
	End 
	Form FormId: 0x273F, Title: "DMI/OPI Configuration"
		Subtitle Prompt: "DMI/OPI Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC51, Value: 0x1
				Not 
			End 
			Text Prompt: "DMI", Help: "DMI Link and Speed Information", Text: "N/A"
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "DMI Max Link Speed", Help: "Set DMI Speed Gen1/Gen2/Gen3", QuestionFlags: 0x10, QuestionId: 0x412, VarStoreId: 0x1, VarOffset: 0x883, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "DMI Gen3 Eq Phase 2", Help: "Perform Gen3 Equalization Phase 2", QuestionFlags: 0x10, QuestionId: 0x413, VarStoreId: 0x1, VarOffset: 0x886, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				InconsistentIf Error: "Phase 3 Eq must be Software or Static if Phase 2 is diabled"
					EqIdVal QuestionId: 0x413, Value: 0x0
						EqIdVal QuestionId: 0x414, Value: 0x1
						And 
					End 
				End 
			End 
			OneOf Prompt: "DMI Gen3 Eq Phase 3 Method", Help: "Select Method for Gen3 Equalization Phase 3", QuestionFlags: 0x10, QuestionId: 0x414, VarStoreId: 0x1, VarOffset: 0x887, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Adaptive Hardware Equalization" Value: 1
				OneOfOption Option: "Adaptive Software Equalization" Value: 2
				OneOfOption Option: "Static Equalization" Value: 3
				OneOfOption Option: "Disabled" Value: 4
				InconsistentIf Error: "Phase 3 Eq must be Software or Static if Phase 2 is diabled"
					EqIdVal QuestionId: 0x413, Value: 0x0
						EqIdVal QuestionId: 0x414, Value: 0x1
						And 
					End 
				End 
			End 
		End 
		OneOf Prompt: "DMI Vc1 Control", Help: "Enable/Disable DMI Vc1", QuestionFlags: 0x10, QuestionId: 0x415, VarStoreId: 0x1, VarOffset: 0x881, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Enabled" Value: 1
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
		End 
		OneOf Prompt: "DMI Vcm Control", Help: "Enable/Disable DMI Vcm", QuestionFlags: 0x10, QuestionId: 0x416, VarStoreId: 0x1, VarOffset: 0x882, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			OneOfOption Option: "Disabled" Value: 0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC51, Value: 0x1
				Not 
			End 
			OneOf Prompt: "Program Static Phase1 Eq", Help: "Program Phase1 Presets/CTLEp", QuestionFlags: 0x10, QuestionId: 0x417, VarStoreId: 0x1, VarOffset: 0x888, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x417, Value: 0x0
				Ref Prompt: " Gen3 Root Port Preset value for each Lane", Help: "Root Port preset value per lane for Gen3 Equalization", QuestionFlags: 0x0, QuestionId: 0x418, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2740
				Ref Prompt: " Gen3 Endpoint Preset value for each Lane", Help: "Endpoint preset value per lane for Gen3 Equalization", QuestionFlags: 0x0, QuestionId: 0x419, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2741
				Ref Prompt: " Gen3 Endpoint Hint value for each Lane", Help: "Endpoint Hint value per lane for Gen3 Equalization", QuestionFlags: 0x0, QuestionId: 0x41A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2742
			End 
			Ref Prompt: "Gen3 RxCTLE Control", Help: "Gen3 RxCTLE Control per Bundle", QuestionFlags: 0x0, QuestionId: 0x41B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2743
			OneOf Prompt: "DMI Link ASPM Control", Help: "Enable/Disable the control of Active State Power Management on SA side of the DMI Link.", QuestionFlags: 0x10, QuestionId: 0x41C, VarStoreId: 0x1, VarOffset: 0x897, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L1" Value: 2, Default, MfgDefault
			End 
			OneOf Prompt: "DMI Extended Sync Control", Help: "Enable DMI Extended Synchronization.", QuestionFlags: 0x10, QuestionId: 0x41D, VarStoreId: 0x1, VarOffset: 0x898, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "DMI De-emphasis Control", Help: "Configure the De-emphasis control on DMI", QuestionFlags: 0x10, QuestionId: 0x41E, VarStoreId: 0x1, VarOffset: 0x885, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "-6 dB" Value: 0
				OneOfOption Option: "-3.5 dB" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "DMI IOT", Help: "Enable/Disable DMI IOT", QuestionFlags: 0x10, QuestionId: 0x41F, VarStoreId: 0x1, VarOffset: 0x884, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
		End 
	End 
	Form FormId: 0x2740, Title: " Gen3 Root Port Preset value for each Lane"
		Subtitle Prompt: " Gen3 Root Port Preset value for each Lane", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: " Lane 0", Help: " Value for Lane 0", QuestionFlags: 0x10, QuestionId: 0x420, VarStoreId: 0x1, VarOffset: 0x889, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 4
		End 
		Numeric Prompt: " Lane 1", Help: " Value for Lane 1", QuestionFlags: 0x10, QuestionId: 0x421, VarStoreId: 0x1, VarOffset: 0x88A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 4
		End 
		Numeric Prompt: " Lane 2", Help: " Value for Lane 2", QuestionFlags: 0x10, QuestionId: 0x422, VarStoreId: 0x1, VarOffset: 0x88B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 4
		End 
		Numeric Prompt: " Lane 3", Help: " Value for Lane 3", QuestionFlags: 0x10, QuestionId: 0x423, VarStoreId: 0x1, VarOffset: 0x88C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 4
		End 
	End 
	Form FormId: 0x2741, Title: " Gen3 Endpoint Preset value for each Lane"
		Subtitle Prompt: " Gen3 Endpoint Preset value for each Lane", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: " Lane 0", Help: " Value for Lane 0", QuestionFlags: 0x10, QuestionId: 0x424, VarStoreId: 0x1, VarOffset: 0x88D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 1", Help: " Value for Lane 1", QuestionFlags: 0x10, QuestionId: 0x425, VarStoreId: 0x1, VarOffset: 0x88E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 2", Help: " Value for Lane 2", QuestionFlags: 0x10, QuestionId: 0x426, VarStoreId: 0x1, VarOffset: 0x88F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 3", Help: " Value for Lane 3", QuestionFlags: 0x10, QuestionId: 0x427, VarStoreId: 0x1, VarOffset: 0x890, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
	End 
	Form FormId: 0x2742, Title: " Gen3 Endpoint Hint value for each Lane"
		Subtitle Prompt: " Gen3 Endpoint Hint value for each Lane", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: " Lane 0", Help: " Value for Lane 0", QuestionFlags: 0x10, QuestionId: 0x428, VarStoreId: 0x1, VarOffset: 0x891, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: " Lane 1", Help: " Value for Lane 1", QuestionFlags: 0x10, QuestionId: 0x429, VarStoreId: 0x1, VarOffset: 0x892, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: " Lane 2", Help: " Value for Lane 2", QuestionFlags: 0x10, QuestionId: 0x42A, VarStoreId: 0x1, VarOffset: 0x893, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: " Lane 3", Help: " Value for Lane 3", QuestionFlags: 0x10, QuestionId: 0x42B, VarStoreId: 0x1, VarOffset: 0x894, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
	End 
	Form FormId: 0x2743, Title: "Gen3 RxCTLE Control"
		Subtitle Prompt: "Gen3 RxCTLE Control", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "Bundle0", Help: "Gen3 RxCTLE setting for Bundle0 (Lane0, Lane1)", QuestionFlags: 0x10, QuestionId: 0x42C, VarStoreId: 0x1, VarOffset: 0x895, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 3
		End 
		Numeric Prompt: "Bundle1", Help: "Gen3 RxCTLE setting for Bundle1 (Lane2, Lane3)", QuestionFlags: 0x10, QuestionId: 0x42D, VarStoreId: 0x1, VarOffset: 0x896, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 3
		End 
	End 
	Form FormId: 0x2744, Title: "PEG Port Configuration"
		Subtitle Prompt: "PEG Port Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "PEG 0:1:0", Help: "PEG 0:1:0 Link and Speed Information", Text: "Not Present"
		OneOf Prompt: "  Enable Root Port", Help: "Enable or Disable the Root Port", QuestionFlags: 0x10, QuestionId: 0x42E, VarStoreId: 0x1, VarOffset: 0x7EC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x2
						Uint64 Value: 0x1
						Conditional 
					End 
				End 
			End 
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1
			OneOfOption Option: "Auto" Value: 2, MfgDefault
		End 
		OneOf Prompt: "  Max Link Speed", Help: "Configure PEG 0:1:0 Max Speed", QuestionFlags: 0x10, QuestionId: 0x42F, VarStoreId: 0x1, VarOffset: 0x7EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
			OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
			OneOfOption Option: "Gen1" Value: 1
			OneOfOption Option: "Gen2" Value: 2
			OneOfOption Option: "Gen3" Value: 3
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC90, Value: 0x0
			OneOf Prompt: "  Max Link Width", Help: "Force PEG link to retrain to X1/2/4/8", QuestionFlags: 0x10, QuestionId: 0x430, VarStoreId: 0x1, VarOffset: 0x7F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Force X1" Value: 1
				OneOfOption Option: "Force X2" Value: 2
				OneOfOption Option: "Force X4" Value: 3
				OneOfOption Option: "Force X8" Value: 4
			End 
			OneOf Prompt: "  Power Down Unused Lanes", Help: "Power Down Unused Lanes.
Disabled: No power saving
Auto: Bios will power down unused lanes based on the max possible link width", QuestionFlags: 0x10, QuestionId: 0x431, VarStoreId: 0x1, VarOffset: 0x7F5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Auto" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Gen3 Eq Phase 2", Help: "Perform Gen3 Equalization Phase 2", QuestionFlags: 0x10, QuestionId: 0x432, VarStoreId: 0x1, VarOffset: 0x7FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				InconsistentIf Error: "Phase 3 Eq must be Software or Static if Phase 2 is diabled"
					EqIdVal QuestionId: 0x432, Value: 0x0
						EqIdVal QuestionId: 0x433, Value: 0x1
						And 
					End 
				End 
			End 
			OneOf Prompt: "  Gen3 Eq Phase 3 Method", Help: "Select Method for Gen3 Equalization Phase 3", QuestionFlags: 0x10, QuestionId: 0x433, VarStoreId: 0x1, VarOffset: 0x7FC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [74]
							Uint64 Value: 0x0
							Uint64 Value: 0x3
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Auto" Value: 0
				OneOfOption Option: "Adaptive Hardware Equalization" Value: 1
				OneOfOption Option: "Adaptive Software Equalization" Value: 2
				OneOfOption Option: "Static Equalization" Value: 3
				OneOfOption Option: "Disabled" Value: 4
				InconsistentIf Error: "Phase 3 Eq must be Software or Static if Phase 2 is diabled"
					EqIdVal QuestionId: 0x432, Value: 0x0
						EqIdVal QuestionId: 0x433, Value: 0x1
						And 
					End 
				End 
			End 
			OneOf Prompt: "  ASPM", Help: "Control ASPM support for the PEG 0.  This has no effect if PEG is not the currently active device.", QuestionFlags: 0x10, QuestionId: 0x434, VarStoreId: 0x1, VarOffset: 0x7E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
				OneOfOption Option: "ASPM L0s" Value: 1
				OneOfOption Option: "ASPM L1" Value: 2
				OneOfOption Option: "ASPM L0sL1" Value: 3
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x434, Value: 0x0
					EqIdVal QuestionId: 0x434, Value: 0x2
					Or 
					EqIdVal QuestionId: 0x434, Value: 0x4
					Or 
				End 
				OneOf Prompt: "    ASPM L0s", Help: "PEG0: Enable PCIe ASPM L0s.", QuestionFlags: 0x10, QuestionId: 0x435, VarStoreId: 0x1, VarOffset: 0x7E9, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3, Step: 0x0
					OneOfOption Option: "Root Port Only" Value: 1
					OneOfOption Option: "Endpoint Port Only" Value: 2
					OneOfOption Option: "Both Root and Endpoint Ports" Value: 3, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "  De-emphasis Control", Help: "PEG0: Configure the De-emphasis control on PEG", QuestionFlags: 0x10, QuestionId: 0x436, VarStoreId: 0x1, VarOffset: 0x802, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "-6 dB" Value: 0
				OneOfOption Option: "-3.5 dB" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  OBFF", Help: "CPU PEG0 (0,1,0) OBFF Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x437, VarStoreId: 0x1, VarOffset: 0x80B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  LTR", Help: "CPU PEG0 (0,1,0) Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x438, VarStoreId: 0x1, VarOffset: 0x808, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		Numeric Prompt: "  PEG0 Slot Power Limit Value", Help: "Sets the upper limit on power supplied by slot. Power limit (in Watts) is calculated by multiplying this value by the Slot Power Limit Scale. Values 0-255", QuestionFlags: 0x10, QuestionId: 0x439, VarStoreId: 0x1, VarOffset: 0x85C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 75
		End 
		OneOf Prompt: "  PEG0 Slot Power Limit Scale", Help: "Select the scale used for the Slot Power Limit Value.", QuestionFlags: 0x10, QuestionId: 0x43A, VarStoreId: 0x1, VarOffset: 0x859, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
			OneOfOption Option: "1.0x" Value: 0, Default, MfgDefault
			OneOfOption Option: "0.1x" Value: 1
			OneOfOption Option: "0.01x" Value: 2
			OneOfOption Option: "0.001x" Value: 3
		End 
		Numeric Prompt: "  PEG0 Physical Slot Number", Help: "Set the physical slot number attached to this Port. The number has to be globally unique within the chassis. Values  0-8191", QuestionFlags: 0x10, QuestionId: 0x43B, VarStoreId: 0x1, VarOffset: 0x85F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1FFF, Step: 0x1
			Default DefaultId: 0x0 Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x42E, Value: 0x1
				Not 
			End 
			OneOf Prompt: "PEG0 Hotplug", Help: "PCI Express Hot Plug Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x43C, VarStoreId: 0x1, VarOffset: 0x856, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x43C, Value: 0x1
				Not 
			End 
			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x43D, VarStoreId: 0x1, VarOffset: 0x865, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "Reseved Memory", Help: "Reserved Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x0, QuestionId: 0x43E, VarStoreId: 0x1, VarOffset: 0x868, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
			End 
			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x43F, VarStoreId: 0x1, VarOffset: 0x86E, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
				Default DefaultId: 0x0 Value: 4
			End 
		End 
		Text Prompt: "PEG 0:1:1", Help: "PEG 0:1:1 Link and Speed Information", Text: "Not Present"
		OneOf Prompt: "  Enable Root Port", Help: "Enable or Disable the Root Port", QuestionFlags: 0x10, QuestionId: 0x440, VarStoreId: 0x1, VarOffset: 0x7ED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1
			OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC50, Value: 0x4A
				Not 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x440, Value: 0x1
					Not 
				End 
				OneOf Prompt: "PEG1 Compliance Mode Test", Help: "PEG1 Compliance Mode Testing Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x441, VarStoreId: 0x1, VarOffset: 0x8A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
		End 
		OneOf Prompt: "  Max Link Speed", Help: "Configure PEG 0:1:1 Max Speed", QuestionFlags: 0x10, QuestionId: 0x442, VarStoreId: 0x1, VarOffset: 0x7F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
			OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
			OneOfOption Option: "Gen1" Value: 1
			OneOfOption Option: "Gen2" Value: 2
			OneOfOption Option: "Gen3" Value: 3
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8F, Value: 0x0
			OneOf Prompt: "  Max Link Width", Help: "Force PEG link to retrain to X1/2/4/8", QuestionFlags: 0x10, QuestionId: 0x443, VarStoreId: 0x1, VarOffset: 0x7F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Force X1" Value: 1
				OneOfOption Option: "Force X2" Value: 2
				OneOfOption Option: "Force X4" Value: 3
			End 
			OneOf Prompt: "  Power Down Unused Lanes", Help: "Power Down Unused Lanes.
Disabled: No power saving
Auto: Bios will power down unused lanes based on the max possible link width", QuestionFlags: 0x10, QuestionId: 0x444, VarStoreId: 0x1, VarOffset: 0x7F6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Auto" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Gen3 Eq Phase 2", Help: "Perform Gen3 Equalization Phase 2", QuestionFlags: 0x10, QuestionId: 0x445, VarStoreId: 0x1, VarOffset: 0x800, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				InconsistentIf Error: "Phase 3 Eq must be Software or Static if Phase 2 is diabled"
					EqIdVal QuestionId: 0x445, Value: 0x0
						EqIdVal QuestionId: 0x446, Value: 0x1
						And 
					End 
				End 
			End 
			OneOf Prompt: "  Gen3 Eq Phase 3 Method", Help: "Select Method for Gen3 Equalization Phase 3", QuestionFlags: 0x10, QuestionId: 0x446, VarStoreId: 0x1, VarOffset: 0x7FD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Adaptive Hardware Equalization" Value: 1
				OneOfOption Option: "Adaptive Software Equalization" Value: 2
				OneOfOption Option: "Static Equalization" Value: 3
				OneOfOption Option: "Disabled" Value: 4
				InconsistentIf Error: "Phase 3 Eq must be Software or Static if Phase 2 is diabled"
					EqIdVal QuestionId: 0x445, Value: 0x0
						EqIdVal QuestionId: 0x446, Value: 0x1
						And 
					End 
				End 
			End 
			OneOf Prompt: "  ASPM", Help: "Control ASPM support for the PEG 1.  This has no effect if PEG is not the currently active device.", QuestionFlags: 0x10, QuestionId: 0x447, VarStoreId: 0x1, VarOffset: 0x7E7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
				OneOfOption Option: "ASPM L0s" Value: 1
				OneOfOption Option: "ASPM L1" Value: 2
				OneOfOption Option: "ASPM L0sL1" Value: 3
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x447, Value: 0x0
					EqIdVal QuestionId: 0x447, Value: 0x2
					Or 
					EqIdVal QuestionId: 0x447, Value: 0x4
					Or 
				End 
				OneOf Prompt: "    ASPM L0s", Help: "PEG1: Enable PCIe ASPM L0s.", QuestionFlags: 0x10, QuestionId: 0x448, VarStoreId: 0x1, VarOffset: 0x7EA, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3, Step: 0x0
					OneOfOption Option: "Root Port Only" Value: 1
					OneOfOption Option: "Endpoint Port Only" Value: 2
					OneOfOption Option: "Both Root and Endpoint Ports" Value: 3, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "  De-emphasis Control", Help: "PEG1: Configure the De-emphasis control on PEG", QuestionFlags: 0x10, QuestionId: 0x449, VarStoreId: 0x1, VarOffset: 0x803, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "-6 dB" Value: 0
				OneOfOption Option: "-3.5 dB" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  OBFF", Help: "CPU PEG1 (0,1,1) OBFF Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x44A, VarStoreId: 0x1, VarOffset: 0x80C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  LTR", Help: "CPU PEG1 (0,1,1) Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x44B, VarStoreId: 0x1, VarOffset: 0x809, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		Numeric Prompt: "  PEG1 Slot Power Limit Value", Help: "Sets the upper limit on power supplied by slot. Power limit (in Watts) is calculated by multiplying this value by the Slot Power Limit Scale. Values 0-255", QuestionFlags: 0x10, QuestionId: 0x44C, VarStoreId: 0x1, VarOffset: 0x85D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 75
		End 
		OneOf Prompt: "  PEG1 Slot Power Limit Scale", Help: "Select the scale used for the Slot Power Limit Value.", QuestionFlags: 0x10, QuestionId: 0x44D, VarStoreId: 0x1, VarOffset: 0x85A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
			OneOfOption Option: "1.0x" Value: 0, Default, MfgDefault
			OneOfOption Option: "0.1x" Value: 1
			OneOfOption Option: "0.01x" Value: 2
			OneOfOption Option: "0.001x" Value: 3
		End 
		Numeric Prompt: "  PEG1 Physical Slot Number", Help: "Set the physical slot number attached to this Port. The number has to be globally unique within the chassis. Values  0-8191", QuestionFlags: 0x10, QuestionId: 0x44E, VarStoreId: 0x1, VarOffset: 0x861, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1FFF, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x440, Value: 0x1
				Not 
			End 
			OneOf Prompt: "PEG1 Hotplug", Help: "PCI Express Hot Plug Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x44F, VarStoreId: 0x1, VarOffset: 0x857, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x44F, Value: 0x1
				Not 
			End 
			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x450, VarStoreId: 0x1, VarOffset: 0x866, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "Reseved Memory", Help: "Reserved Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x0, QuestionId: 0x451, VarStoreId: 0x1, VarOffset: 0x86A, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
			End 
			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x452, VarStoreId: 0x1, VarOffset: 0x86F, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
				Default DefaultId: 0x0 Value: 4
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8C, Value: 0x4
			Text Prompt: "PEG 0:1:2", Help: "PEG 0:1:2 Link and Speed Information", Text: "Not Present"
			OneOf Prompt: "  Enable Root Port", Help: "Enable or Disable the Root Port", QuestionFlags: 0x10, QuestionId: 0x453, VarStoreId: 0x1, VarOffset: 0x7EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
			End 
			OneOf Prompt: "  Max Link Speed", Help: "Configure PEG 0:1:2 Max Speed", QuestionFlags: 0x10, QuestionId: 0x454, VarStoreId: 0x1, VarOffset: 0x7F1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8E, Value: 0x0
			OneOf Prompt: "  Max Link Width", Help: "Force PEG link to retrain to X1/2/4/8", QuestionFlags: 0x10, QuestionId: 0x455, VarStoreId: 0x1, VarOffset: 0x7F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Force X1" Value: 1
				OneOfOption Option: "Force X2" Value: 2
			End 
			OneOf Prompt: "  Power Down Unused Lanes", Help: "Power Down Unused Lanes.
Disabled: No power saving
Auto: Bios will power down unused lanes based on the max possible link width", QuestionFlags: 0x10, QuestionId: 0x456, VarStoreId: 0x1, VarOffset: 0x7F7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Auto" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Gen3 Eq Phase 2", Help: "Perform Gen3 Equalization Phase 2", QuestionFlags: 0x10, QuestionId: 0x457, VarStoreId: 0x1, VarOffset: 0x801, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				InconsistentIf Error: "Phase 3 Eq must be Software or Static if Phase 2 is diabled"
					EqIdVal QuestionId: 0x457, Value: 0x0
						EqIdVal QuestionId: 0x458, Value: 0x1
						And 
					End 
				End 
			End 
			OneOf Prompt: "  Gen3 Eq Phase 3 Method", Help: "Select Method for Gen3 Equalization Phase 3", QuestionFlags: 0x10, QuestionId: 0x458, VarStoreId: 0x1, VarOffset: 0x7FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Adaptive Hardware Equalization" Value: 1
				OneOfOption Option: "Adaptive Software Equalization" Value: 2
				OneOfOption Option: "Static Equalization" Value: 3
				OneOfOption Option: "Disabled" Value: 4
				InconsistentIf Error: "Phase 3 Eq must be Software or Static if Phase 2 is diabled"
					EqIdVal QuestionId: 0x457, Value: 0x0
						EqIdVal QuestionId: 0x458, Value: 0x1
						And 
					End 
				End 
			End 
			OneOf Prompt: "  ASPM", Help: "Control ASPM support for the PEG 2.  This has no effect if PEG is not the currently active device.", QuestionFlags: 0x10, QuestionId: 0x459, VarStoreId: 0x1, VarOffset: 0x7E8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
				OneOfOption Option: "ASPM L0s" Value: 1
				OneOfOption Option: "ASPM L1" Value: 2
				OneOfOption Option: "ASPM L0sL1" Value: 3
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x459, Value: 0x0
					EqIdVal QuestionId: 0x459, Value: 0x2
					Or 
					EqIdVal QuestionId: 0x459, Value: 0x4
					Or 
				End 
				OneOf Prompt: "    ASPM L0s", Help: "PEG2: Enable PCIe ASPM L0s.", QuestionFlags: 0x10, QuestionId: 0x45A, VarStoreId: 0x1, VarOffset: 0x7EB, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x3, Step: 0x0
					OneOfOption Option: "Root Port Only" Value: 1
					OneOfOption Option: "Endpoint Port Only" Value: 2
					OneOfOption Option: "Both Root and Endpoint Ports" Value: 3, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "  De-emphasis Control", Help: "PEG2: Configure the De-emphasis control on PEG", QuestionFlags: 0x10, QuestionId: 0x45B, VarStoreId: 0x1, VarOffset: 0x804, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "-6 dB" Value: 0
				OneOfOption Option: "-3.5 dB" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  OBFF", Help: "CPU PEG2 (0,1,2) OBFF Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x45C, VarStoreId: 0x1, VarOffset: 0x80D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  LTR", Help: "CPU PEG2 (0,1,2) Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x45D, VarStoreId: 0x1, VarOffset: 0x80A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
		Numeric Prompt: "  PEG2 Slot Power Limit Value", Help: "Sets the upper limit on power supplied by slot. Power limit (in Watts) is calculated by multiplying this value by the Slot Power Limit Scale. Values 0-255", QuestionFlags: 0x10, QuestionId: 0x45E, VarStoreId: 0x1, VarOffset: 0x85E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 75
		End 
		OneOf Prompt: "  PEG2 Slot Power Limit Scale", Help: "Select the scale used for the Slot Power Limit Value.", QuestionFlags: 0x10, QuestionId: 0x45F, VarStoreId: 0x1, VarOffset: 0x85B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
			OneOfOption Option: "1.0x" Value: 0, Default, MfgDefault
			OneOfOption Option: "0.1x" Value: 1
			OneOfOption Option: "0.01x" Value: 2
			OneOfOption Option: "0.001x" Value: 3
		End 
		Numeric Prompt: "  PEG2 Physical Slot Number", Help: "Set the physical slot number attached to this Port. The number has to be globally unique within the chassis. Values  0-8191", QuestionFlags: 0x10, QuestionId: 0x460, VarStoreId: 0x1, VarOffset: 0x863, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1FFF, Step: 0x1
			Default DefaultId: 0x0 Value: 3
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x453, Value: 0x1
				Not 
			End 
			OneOf Prompt: "PEG2 Hotplug", Help: "PCI Express Hot Plug Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x461, VarStoreId: 0x1, VarOffset: 0x858, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x461, Value: 0x1
				Not 
			End 
			Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x462, VarStoreId: 0x1, VarOffset: 0x867, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "Reseved Memory", Help: "Reserved Memory for this Root Bridge (1-4096) MB", QuestionFlags: 0x0, QuestionId: 0x463, VarStoreId: 0x1, VarOffset: 0x86C, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
			End 
			Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x464, VarStoreId: 0x1, VarOffset: 0x870, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
				Default DefaultId: 0x0 Value: 4
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC90, Value: 0x0
			OneOf Prompt: "PEG0 Max Payload size", Help: "Select PEG0 Max Payload Size; Choose Auto(Default Device Capability) or force to 128/256 Bytes", QuestionFlags: 0x10, QuestionId: 0x465, VarStoreId: 0x1, VarOffset: 0x805, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
				OneOfOption Option: "Auto" Value: 255, Default, MfgDefault
				OneOfOption Option: "128" Value: 0
				OneOfOption Option: "256 TLP" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8F, Value: 0x0
			OneOf Prompt: "PEG1 Max Payload size", Help: "Select PEG1 Max Payload Size; Choose Auto(Default Device Capability) or force to 128/256 Bytes", QuestionFlags: 0x10, QuestionId: 0x466, VarStoreId: 0x1, VarOffset: 0x806, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
				OneOfOption Option: "Auto" Value: 255, Default, MfgDefault
				OneOfOption Option: "128" Value: 0
				OneOfOption Option: "256 TLP" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8E, Value: 0x0
			OneOf Prompt: "PEG2 Max Payload size", Help: "Select PEG2 Max Payload Size; Choose Auto(Default Device Capability) or force to 128/256 Bytes", QuestionFlags: 0x10, QuestionId: 0x467, VarStoreId: 0x1, VarOffset: 0x807, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
				OneOfOption Option: "Auto" Value: 255, Default, MfgDefault
				OneOfOption Option: "128" Value: 0
				OneOfOption Option: "256 TLP" Value: 1
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Ref Prompt: "PEG Port Feature Configuration", Help: "PEG Port Feature Configuration", QuestionFlags: 0x0, QuestionId: 0x468, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x280E
		OneOf Prompt: "Program PCIe ASPM after OpROM", Help: "Enabled: PCIe ASPM will be programmed after OpROM.
Disabled: PCIe ASPM will be programmed before OpROM.", QuestionFlags: 0x10, QuestionId: 0x469, VarStoreId: 0x1, VarOffset: 0x84B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Program Static Phase1 Eq", Help: "Program Phase1 Presets/CTLEp", QuestionFlags: 0x10, QuestionId: 0x46A, VarStoreId: 0x1, VarOffset: 0x80E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x46A, Value: 0x0
			Ref Prompt: " Gen3 Root Port Preset value for each Lane", Help: "Root Port preset value per lane for Gen3 Equalization", QuestionFlags: 0x0, QuestionId: 0x46B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2745
			Ref Prompt: " Gen3 Endpoint Preset value for each Lane", Help: "Endpoint preset value per lane for Gen3 Equalization", QuestionFlags: 0x0, QuestionId: 0x46C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2746
			Ref Prompt: " Gen3 Endpoint Hint value for each Lane", Help: "Endpoint Hint value per lane for Gen3 Equalization", QuestionFlags: 0x0, QuestionId: 0x46D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2747
		End 
		Ref Prompt: "Gen3 RxCTLE Control", Help: "Gen3 RxCTLE Control per Bundle", QuestionFlags: 0x0, QuestionId: 0x46E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2748
		Text Prompt: "Gen3 Adaptive Software Equalization", Help: "Gen3 Adaptive Software Equalization", Text: ""
		OneOf Prompt: "  Always Attempt SW EQ", Help: "Always Attempt SW EQ, even it has been done once", QuestionFlags: 0x10, QuestionId: 0x46F, VarStoreId: 0x1, VarOffset: 0x84A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "  Number of Presets to test", Help: "Choose between 7,3,5,8 and 0-9. Auto = current default (7,3,5,8 for SKL.)  Do not change from the default unless debugging.", QuestionFlags: 0x10, QuestionId: 0x470, VarStoreId: 0x1, VarOffset: 0x855, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "7, 3, 5, 8" Value: 0
			OneOfOption Option: "0 - 9" Value: 1
			OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
		End 
		OneOf Prompt: "  Allow PERST# GPIO Usage", Help: "Enable/Disable GPIO-based resets to PEG endpoint(s) during margin search, if needed", QuestionFlags: 0x10, QuestionId: 0x471, VarStoreId: 0x1, VarOffset: 0x84C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "  SW EQ Enable VOC", Help: "Select Jitter & VOC test mode (default) or Jitter only test mode.  Auto will current default (Enabled)", QuestionFlags: 0x10, QuestionId: 0x472, VarStoreId: 0x1, VarOffset: 0x850, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Jitter Only Test Mode" Value: 0
			OneOfOption Option: "Jitter & VOC Test Mode" Value: 1
			OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
		End 
		Numeric Prompt: "  Jitter Dwell Time", Help: "PEG Gen3 Preset Search dwell time [0..65535] in [usec]", QuestionFlags: 0x10, QuestionId: 0x473, VarStoreId: 0x1, VarOffset: 0x848, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
			Default DefaultId: 0x0 Value: 3000
		End 
		Numeric Prompt: "  Jitter Error Target", Help: "The margin search error target value [1..65535]", QuestionFlags: 0x10, QuestionId: 0x474, VarStoreId: 0x1, VarOffset: 0x84D, Flags: 0x11, Size: 16, Min: 0x1, Max: 0xFFFF, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "  VOC Dwell Time", Help: "The VOC margin search dwell time [0..65535] in [usec]", QuestionFlags: 0x10, QuestionId: 0x475, VarStoreId: 0x1, VarOffset: 0x851, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
			Default DefaultId: 0x0 Value: 10000
		End 
		Numeric Prompt: "  VOC Error Target", Help: "The VOC margin search error target value [1..65535]", QuestionFlags: 0x10, QuestionId: 0x476, VarStoreId: 0x1, VarOffset: 0x853, Flags: 0x11, Size: 16, Min: 0x1, Max: 0xFFFF, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		OneOf Prompt: "Generate BDAT PEG Margin Data", Help: "Enable to generate BDAT PCIe margin tables", QuestionFlags: 0x10, QuestionId: 0x477, VarStoreId: 0x1, VarOffset: 0x84F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Generate Port Jitter Data" Value: 1
		End 
		OneOf Prompt: "PCIe Rx CEM Test Mode", Help: "Enable/Disable PEG Rx CEM Loopback Mode", QuestionFlags: 0x10, QuestionId: 0x478, VarStoreId: 0x1, VarOffset: 0x7F8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x478, Value: 0x0
			Numeric Prompt: "  PEG Lane number for Test", Help: "  PEG Lane number for Rx CEM Loopback mode (0 ~ 15)", QuestionFlags: 0x10, QuestionId: 0x479, VarStoreId: 0x1, VarOffset: 0x7F9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "  Non-Protocol Awareness", Help: "  Enable/Disable Non-Protocol Awareness", QuestionFlags: 0x10, QuestionId: 0x47A, VarStoreId: 0x1, VarOffset: 0x7FA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		OneOf Prompt: "PCIe Spread Spectrum Clocking", Help: "Allows disableing Spread Spectrum Clocking for compliance testing", QuestionFlags: 0x10, QuestionId: 0x47B, VarStoreId: 0x1, VarOffset: 0x7FB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Disabled" Value: 1
		End 
	End 
	Form FormId: 0x2745, Title: " Gen3 Root Port Preset value for each Lane"
		Subtitle Prompt: " Gen3 Root Port Preset value for each Lane", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: " Lane 0", Help: " Value for Lane 0", QuestionFlags: 0x10, QuestionId: 0x47C, VarStoreId: 0x1, VarOffset: 0x80F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x4
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 1", Help: " Value for Lane 1", QuestionFlags: 0x10, QuestionId: 0x47D, VarStoreId: 0x1, VarOffset: 0x810, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x4
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 2", Help: " Value for Lane 2", QuestionFlags: 0x10, QuestionId: 0x47E, VarStoreId: 0x1, VarOffset: 0x811, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x4
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 3", Help: " Value for Lane 3", QuestionFlags: 0x10, QuestionId: 0x47F, VarStoreId: 0x1, VarOffset: 0x812, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x4
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 4", Help: " Value for Lane 4", QuestionFlags: 0x10, QuestionId: 0x480, VarStoreId: 0x1, VarOffset: 0x813, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x4
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 5", Help: " Value for Lane 5", QuestionFlags: 0x10, QuestionId: 0x481, VarStoreId: 0x1, VarOffset: 0x814, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x4
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 6", Help: " Value for Lane 6", QuestionFlags: 0x10, QuestionId: 0x482, VarStoreId: 0x1, VarOffset: 0x815, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x4
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 7", Help: " Value for Lane 7", QuestionFlags: 0x10, QuestionId: 0x483, VarStoreId: 0x1, VarOffset: 0x816, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x4
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 8", Help: " Value for Lane 8", QuestionFlags: 0x10, QuestionId: 0x484, VarStoreId: 0x1, VarOffset: 0x817, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 9", Help: " Value for Lane 9", QuestionFlags: 0x10, QuestionId: 0x485, VarStoreId: 0x1, VarOffset: 0x818, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 10", Help: " Value for Lane 10", QuestionFlags: 0x10, QuestionId: 0x486, VarStoreId: 0x1, VarOffset: 0x819, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 11", Help: " Value for Lane 11", QuestionFlags: 0x10, QuestionId: 0x487, VarStoreId: 0x1, VarOffset: 0x81A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 12", Help: " Value for Lane 12", QuestionFlags: 0x10, QuestionId: 0x488, VarStoreId: 0x1, VarOffset: 0x81B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 13", Help: " Value for Lane 13", QuestionFlags: 0x10, QuestionId: 0x489, VarStoreId: 0x1, VarOffset: 0x81C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 14", Help: " Value for Lane 14", QuestionFlags: 0x10, QuestionId: 0x48A, VarStoreId: 0x1, VarOffset: 0x81D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 15", Help: " Value for Lane 15", QuestionFlags: 0x10, QuestionId: 0x48B, VarStoreId: 0x1, VarOffset: 0x81E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
	End 
	Form FormId: 0x2746, Title: " Gen3 Endpoint Preset value for each Lane"
		Subtitle Prompt: " Gen3 Endpoint Preset value for each Lane", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: " Lane 0", Help: " Value for Lane 0", QuestionFlags: 0x10, QuestionId: 0x48C, VarStoreId: 0x1, VarOffset: 0x81F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 1", Help: " Value for Lane 1", QuestionFlags: 0x10, QuestionId: 0x48D, VarStoreId: 0x1, VarOffset: 0x820, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 2", Help: " Value for Lane 2", QuestionFlags: 0x10, QuestionId: 0x48E, VarStoreId: 0x1, VarOffset: 0x821, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 3", Help: " Value for Lane 3", QuestionFlags: 0x10, QuestionId: 0x48F, VarStoreId: 0x1, VarOffset: 0x822, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 4", Help: " Value for Lane 4", QuestionFlags: 0x10, QuestionId: 0x490, VarStoreId: 0x1, VarOffset: 0x823, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 5", Help: " Value for Lane 5", QuestionFlags: 0x10, QuestionId: 0x491, VarStoreId: 0x1, VarOffset: 0x824, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 6", Help: " Value for Lane 6", QuestionFlags: 0x10, QuestionId: 0x492, VarStoreId: 0x1, VarOffset: 0x825, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 7", Help: " Value for Lane 7", QuestionFlags: 0x10, QuestionId: 0x493, VarStoreId: 0x1, VarOffset: 0x826, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x7
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 8", Help: " Value for Lane 8", QuestionFlags: 0x10, QuestionId: 0x494, VarStoreId: 0x1, VarOffset: 0x827, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 9", Help: " Value for Lane 9", QuestionFlags: 0x10, QuestionId: 0x495, VarStoreId: 0x1, VarOffset: 0x828, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 10", Help: " Value for Lane 10", QuestionFlags: 0x10, QuestionId: 0x496, VarStoreId: 0x1, VarOffset: 0x829, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 11", Help: " Value for Lane 11", QuestionFlags: 0x10, QuestionId: 0x497, VarStoreId: 0x1, VarOffset: 0x82A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 12", Help: " Value for Lane 12", QuestionFlags: 0x10, QuestionId: 0x498, VarStoreId: 0x1, VarOffset: 0x82B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 13", Help: " Value for Lane 13", QuestionFlags: 0x10, QuestionId: 0x499, VarStoreId: 0x1, VarOffset: 0x82C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 14", Help: " Value for Lane 14", QuestionFlags: 0x10, QuestionId: 0x49A, VarStoreId: 0x1, VarOffset: 0x82D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
		Numeric Prompt: " Lane 15", Help: " Value for Lane 15", QuestionFlags: 0x10, QuestionId: 0x49B, VarStoreId: 0x1, VarOffset: 0x82E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x9, Step: 0x1
			Default DefaultId: 0x0 Value: 7
		End 
	End 
	Form FormId: 0x2747, Title: " Gen3 Endpoint Hint value for each Lane"
		Subtitle Prompt: " Gen3 Endpoint Hint value for each Lane", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: " Lane 0", Help: " Value for Lane 0", QuestionFlags: 0x10, QuestionId: 0x49C, VarStoreId: 0x1, VarOffset: 0x82F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x2
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 1", Help: " Value for Lane 1", QuestionFlags: 0x10, QuestionId: 0x49D, VarStoreId: 0x1, VarOffset: 0x830, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x2
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 2", Help: " Value for Lane 2", QuestionFlags: 0x10, QuestionId: 0x49E, VarStoreId: 0x1, VarOffset: 0x831, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x2
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 3", Help: " Value for Lane 3", QuestionFlags: 0x10, QuestionId: 0x49F, VarStoreId: 0x1, VarOffset: 0x832, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x2
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 4", Help: " Value for Lane 4", QuestionFlags: 0x10, QuestionId: 0x4A0, VarStoreId: 0x1, VarOffset: 0x833, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x2
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 5", Help: " Value for Lane 5", QuestionFlags: 0x10, QuestionId: 0x4A1, VarStoreId: 0x1, VarOffset: 0x834, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x2
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 6", Help: " Value for Lane 6", QuestionFlags: 0x10, QuestionId: 0x4A2, VarStoreId: 0x1, VarOffset: 0x835, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x2
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 7", Help: " Value for Lane 7", QuestionFlags: 0x10, QuestionId: 0x4A3, VarStoreId: 0x1, VarOffset: 0x836, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [74]
						Uint64 Value: 0x2
						Uint64 Value: 0x6
						Conditional 
					End 
				End 
			End 
		End 
		Numeric Prompt: " Lane 8", Help: " Value for Lane 8", QuestionFlags: 0x10, QuestionId: 0x4A4, VarStoreId: 0x1, VarOffset: 0x837, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: " Lane 9", Help: " Value for Lane 9", QuestionFlags: 0x10, QuestionId: 0x4A5, VarStoreId: 0x1, VarOffset: 0x838, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: " Lane 10", Help: " Value for Lane 10", QuestionFlags: 0x10, QuestionId: 0x4A6, VarStoreId: 0x1, VarOffset: 0x839, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: " Lane 11", Help: " Value for Lane 11", QuestionFlags: 0x10, QuestionId: 0x4A7, VarStoreId: 0x1, VarOffset: 0x83A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: " Lane 12", Help: " Value for Lane 12", QuestionFlags: 0x10, QuestionId: 0x4A8, VarStoreId: 0x1, VarOffset: 0x83B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: " Lane 13", Help: " Value for Lane 13", QuestionFlags: 0x10, QuestionId: 0x4A9, VarStoreId: 0x1, VarOffset: 0x83C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: " Lane 14", Help: " Value for Lane 14", QuestionFlags: 0x10, QuestionId: 0x4AA, VarStoreId: 0x1, VarOffset: 0x83D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: " Lane 15", Help: " Value for Lane 15", QuestionFlags: 0x10, QuestionId: 0x4AB, VarStoreId: 0x1, VarOffset: 0x83E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
	End 
	Form FormId: 0x2748, Title: "Gen3 RxCTLE Control"
		Subtitle Prompt: "Gen3 RxCTLE Control", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "Bundle0", Help: "Gen3 RxCTLE setting for Bundle0 (Lane0, Lane1)", QuestionFlags: 0x10, QuestionId: 0x4AC, VarStoreId: 0x1, VarOffset: 0x83F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Bundle1", Help: "Gen3 RxCTLE setting for Bundle1 (Lane2, Lane3)", QuestionFlags: 0x10, QuestionId: 0x4AD, VarStoreId: 0x1, VarOffset: 0x840, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Bundle2", Help: "Gen3 RxCTLE setting for Bundle2 (Lane4, Lane5)", QuestionFlags: 0x10, QuestionId: 0x4AE, VarStoreId: 0x1, VarOffset: 0x841, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Bundle3", Help: "Gen3 RxCTLE setting for Bundle3 (Lane6, Lane7)", QuestionFlags: 0x10, QuestionId: 0x4AF, VarStoreId: 0x1, VarOffset: 0x842, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Bundle4", Help: "Gen3 RxCTLE setting for Bundle4 (Lane8, Lane9)", QuestionFlags: 0x10, QuestionId: 0x4B0, VarStoreId: 0x1, VarOffset: 0x843, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Bundle5", Help: "Gen3 RxCTLE setting for Bundle5 (Lane10, Lane11)", QuestionFlags: 0x10, QuestionId: 0x4B1, VarStoreId: 0x1, VarOffset: 0x844, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Bundle6", Help: "Gen3 RxCTLE setting for Bundle6 (Lane12, Lane13)", QuestionFlags: 0x10, QuestionId: 0x4B2, VarStoreId: 0x1, VarOffset: 0x845, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		Numeric Prompt: "Bundle7", Help: "Gen3 RxCTLE setting for Bundle7 (Lane14, Lane15)", QuestionFlags: 0x10, QuestionId: 0x4B3, VarStoreId: 0x1, VarOffset: 0x846, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 0
		End 
		OneOf Prompt: "RxCTLE Override", Help: "When Enabled, it overrides PEG's RxCTLE adaptive behavior", QuestionFlags: 0x10, QuestionId: 0x4B4, VarStoreId: 0x1, VarOffset: 0x847, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
	End 
	Form FormId: 0x2749, Title: "LCD Control"
		Subtitle Prompt: "LCD Control", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "LCD Panel Type", Help: "Select LCD panel used by Internal Graphics Device by selecting the appropriate setup item.", QuestionFlags: 0x10, QuestionId: 0x4B5, VarStoreId: 0x1, VarOffset: 0x7C8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x10, Step: 0x0
			Default DefaultId: 0x0 Value: 15
			OneOfOption Option: "VBIOS Default" Value: 0, MfgDefault
			OneOfOption Option: "640x480    LVDS" Value: 1
			OneOfOption Option: "800x600    LVDS" Value: 2
			OneOfOption Option: "1024x768   LVDS1" Value: 3
			OneOfOption Option: "1280x1024  LVDS" Value: 4
			OneOfOption Option: "1400x1050  LVDS1" Value: 5
			OneOfOption Option: "1400x1050  LVDS2" Value: 6
			OneOfOption Option: "1600x1200  LVDS" Value: 7
			OneOfOption Option: "1366x768   LVDS" Value: 8
			OneOfOption Option: "1680x1050  LVDS" Value: 9
			OneOfOption Option: "1920x1200  LVDS" Value: 10
			OneOfOption Option: "1440x900   LVDS" Value: 11
			OneOfOption Option: "1600x900   LVDS" Value: 12
			OneOfOption Option: "1024x768   LVDS2" Value: 13
			OneOfOption Option: "1280x800   LVDS" Value: 14
			OneOfOption Option: "1920x1080  LVDS" Value: 15
			OneOfOption Option: "2048x1536  LVDS" Value: 16
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			OneOf Prompt: "Panel Scaling", Help: "Select the LCD panel scaling option used by the Internal Graphics Device.", QuestionFlags: 0x10, QuestionId: 0x4B6, VarStoreId: 0x1, VarOffset: 0x7C9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Off" Value: 1
				OneOfOption Option: "Force Scaling" Value: 6
			End 
		End 
		OneOf Prompt: "Backlight Control", Help: "Back Light Control Setting", QuestionFlags: 0x10, QuestionId: 0x4B7, VarStoreId: 0x1, VarOffset: 0x7CB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			Default DefaultId: 0x0 Value: 0
			OneOfOption Option: "PWM Inverted" Value: 0
			OneOfOption Option: "PWM Normal" Value: 2, MfgDefault
		End 
		OneOf Prompt: "Active LFP", Help: "Select the Active LFP Configuration.

No LVDS:VBIOS does not enable LVDS.
Int-LVDS:VBIOS enables LVDS driver by Integrated encoder.
SDVO LVDS:VBIOS enables LVDS driver by SDVO encoder.
eDP Port-A:LFP Driven by Int-DisplayPort encoder from Port-A.
eDP Port-D:LFP Driven by Int-DisplayPort encoder from Port-D(through PCH).", QuestionFlags: 0x10, QuestionId: 0x4B8, VarStoreId: 0x1, VarOffset: 0x7D2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
			Default DefaultId: 0x0 Value: 0
			OneOfOption Option: "No eDP" Value: 0
			OneOfOption Option: "eDP Port-A" Value: 3, MfgDefault
		End 
		OneOf Prompt: "Panel Color Depth", Help: "Select the LFP Panel Color Depth", QuestionFlags: 0x10, QuestionId: 0x4B9, VarStoreId: 0x1, VarOffset: 0x7D3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			Default DefaultId: 0x0 Value: 1
			OneOfOption Option: "18 Bit" Value: 0, MfgDefault
			OneOfOption Option: "24 Bit" Value: 1
		End 
		OneOf Prompt: "LVDS Channel Select", Help: "Select the LVDS Channel", QuestionFlags: 0x10, QuestionId: 0x4BA, VarStoreId: 0x1, VarOffset: 0x7D4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			Default DefaultId: 0x0 Value: 1
			OneOfOption Option: "Singe Channel" Value: 0
			OneOfOption Option: "Dual  Channel" Value: 1, MfgDefault
		End 
		OneOf Prompt: "Brightness Mode Setting", Help: "External means eDP,Internal means LVDS Chipset", QuestionFlags: 0x10, QuestionId: 0x4BB, VarStoreId: 0x1, VarOffset: 0x7D6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Bypass" Value: 0, Default, MfgDefault
			OneOfOption Option: "Internal" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x4BB, Value: 0x0
			OneOf Prompt: "Brightnesst Setting", Help: "Set Gop Brightnesst value", QuestionFlags: 0x10, QuestionId: 0x4BC, VarStoreId: 0x1, VarOffset: 0x7D5, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xA, Step: 0x0
				OneOfOption Option: "Brightness 10%" Value: 1
				OneOfOption Option: "Brightness 20%" Value: 2
				OneOfOption Option: "Brightness 30%" Value: 3
				OneOfOption Option: "Brightness 40%" Value: 4
				OneOfOption Option: "Brightness 50%" Value: 5
				OneOfOption Option: "Brightness 60%" Value: 6
				OneOfOption Option: "Brightness 70%" Value: 7
				OneOfOption Option: "Brightness 80%" Value: 8
				OneOfOption Option: "Brightness 90%" Value: 9
				OneOfOption Option: "Brightness 100%" Value: 10, Default, MfgDefault
			End 
		End 
		Numeric Prompt: "Backlight Brightness", Help: "Set VBIOS Brightness.
Range : 0-255.", QuestionFlags: 0x0, QuestionId: 0x4BD, VarStoreId: 0x1, VarOffset: 0x7DE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			Default DefaultId: 0x0 Value: 255
		End 
	End 
	Form FormId: 0x274A, Title: "Intel(R) Ultrabook Event Support"
		Subtitle Prompt: "Intel(R) Ultrabook Event Support", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "IUER Slate Enable", Help: "Enable/Disable IUER Slate Functionality", QuestionFlags: 0x10, QuestionId: 0x4BE, VarStoreId: 0x1, VarOffset: 0x948, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x4BE, Value: 0x0
			OneOf Prompt: "  Slate Mode boot value", Help: "Choose Slate or Laptop as boot mode.", QuestionFlags: 0x10, QuestionId: 0x4BF, VarStoreId: 0x1, VarOffset: 0x943, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Slate Mode" Value: 0
				OneOfOption Option: "Laptop Mode" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Slate Mode on S3 and S4 resume", Help: "Keep it the same as Sx entry or toggle it.", QuestionFlags: 0x10, QuestionId: 0x4C0, VarStoreId: 0x1, VarOffset: 0x944, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "No change" Value: 0, Default, MfgDefault
				OneOfOption Option: "Toggle" Value: 1
			End 
		End 
		OneOf Prompt: "IUER Dock Enable", Help: "Enable/Disable IUER Dock Functionality", QuestionFlags: 0x10, QuestionId: 0x4C1, VarStoreId: 0x1, VarOffset: 0x949, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x4C1, Value: 0x0
			OneOf Prompt: "  Dock Mode boot value", Help: "Choose Docked or Undocked as boot mode.", QuestionFlags: 0x10, QuestionId: 0x4C2, VarStoreId: 0x1, VarOffset: 0x945, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Undocked" Value: 0, Default, MfgDefault
				OneOfOption Option: "Docked" Value: 1
			End 
			OneOf Prompt: "  Dock Mode upon S3 and S4 resume", Help: "Keep it the same as Sx entry or toggle it.", QuestionFlags: 0x10, QuestionId: 0x4C3, VarStoreId: 0x1, VarOffset: 0x946, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "No change" Value: 0, Default, MfgDefault
				OneOfOption Option: "Toggle" Value: 1
			End 
		End 
	End 
	Form FormId: 0x274B, Title: "GT - Power Management Control"
		Subtitle Prompt: "GT - Power Management Control", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x409, Value: 0x0
			OneOf Prompt: "RC6(Render Standby)", Help: "Check to enable render standby support.", QuestionFlags: 0x10, QuestionId: 0x4C4, VarStoreId: 0x1, VarOffset: 0x7CA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
		End 
		OneOf Prompt: "Maximum GT frequency", Help: "Auto Updated", QuestionFlags: 0x10, QuestionId: 0x4C5, VarStoreId: 0x1, VarOffset: 0x7E0, Flags: 0x10, Size: 8, Min: 0x2, Max: 0xFF, Step: 0x0
			OneOfOption Option: "Default Max Frequency" Value: 255, Default, MfgDefault
			OneOfOption Option: "100Mhz" Value: 2
			OneOfOption Option: "150Mhz" Value: 3
			OneOfOption Option: "200Mhz" Value: 4
			OneOfOption Option: "250Mhz" Value: 5
			OneOfOption Option: "300Mhz" Value: 6
			OneOfOption Option: "350Mhz" Value: 7
			OneOfOption Option: "400Mhz" Value: 8
			OneOfOption Option: "450Mhz" Value: 9
			OneOfOption Option: "500Mhz" Value: 10
			OneOfOption Option: "550Mhz" Value: 11
			OneOfOption Option: "600Mhz" Value: 12
			OneOfOption Option: "650Mhz" Value: 13
			OneOfOption Option: "700Mhz" Value: 14
			OneOfOption Option: "750Mhz" Value: 15
			OneOfOption Option: "800Mhz" Value: 16
			OneOfOption Option: "850Mhz" Value: 17
			OneOfOption Option: "900Mhz" Value: 18
			OneOfOption Option: "950Mhz" Value: 19
			OneOfOption Option: "1000Mhz" Value: 20
			OneOfOption Option: "1050Mhz" Value: 21
			OneOfOption Option: "1100Mhz" Value: 22
			OneOfOption Option: "1150Mhz" Value: 23
			OneOfOption Option: "1200Mhz" Value: 24
		End 
	End 
	Form FormId: 0x274C, Title: "Memory Training Algorithms"
		OneOf Prompt: "Early Command Training", Help: "Early Command Training", QuestionFlags: 0x10, QuestionId: 0x4C6, VarStoreId: 0x1, VarOffset: 0x8CC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "SenseAmp Offset Training", Help: "SenseAmp Offset Training", QuestionFlags: 0x10, QuestionId: 0x4C7, VarStoreId: 0x1, VarOffset: 0x8CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Early ReadMPR Timing Centering 2D", Help: "", QuestionFlags: 0x10, QuestionId: 0x4C8, VarStoreId: 0x1, VarOffset: 0x8CE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Read MPR Training", Help: "Read MPR Training", QuestionFlags: 0x10, QuestionId: 0x4C9, VarStoreId: 0x1, VarOffset: 0x8CF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Receive Enable Training", Help: "Receive Enable Training", QuestionFlags: 0x10, QuestionId: 0x4CA, VarStoreId: 0x1, VarOffset: 0x8D0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Jedec Write Leveling", Help: "Jedec Write Leveling", QuestionFlags: 0x10, QuestionId: 0x4CB, VarStoreId: 0x1, VarOffset: 0x8D1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Early Write Time Centering 2D", Help: "Early Write Time Centering 2D", QuestionFlags: 0x10, QuestionId: 0x4CC, VarStoreId: 0x1, VarOffset: 0x8D2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Early Write Drive Strength/Equalization", Help: "", QuestionFlags: 0x10, QuestionId: 0x4CD, VarStoreId: 0x1, VarOffset: 0x974, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Early Read Time Centering 2D", Help: "", QuestionFlags: 0x10, QuestionId: 0x4CE, VarStoreId: 0x1, VarOffset: 0x8D3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Write Timing Centering 1D", Help: "Write Timing Centering 1D", QuestionFlags: 0x10, QuestionId: 0x4CF, VarStoreId: 0x1, VarOffset: 0x8D4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Write Voltage Centering 1D", Help: "", QuestionFlags: 0x10, QuestionId: 0x4D0, VarStoreId: 0x1, VarOffset: 0x8D5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Read Timing Centering 1D", Help: "Read Timing Centering 1D", QuestionFlags: 0x10, QuestionId: 0x4D1, VarStoreId: 0x1, VarOffset: 0x8D6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Dimm ODT Training*", Help: "Dimm On-Die Termination Training", QuestionFlags: 0x10, QuestionId: 0x4D2, VarStoreId: 0x1, VarOffset: 0x8D7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x4D2, Value: 0x0
			OneOf Prompt: "  Max RTT_WR", Help: "Caps the maximum RTT_WR in power training.", QuestionFlags: 0x10, QuestionId: 0x4D3, VarStoreId: 0x1, VarOffset: 0x93F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "ODT Off" Value: 0, Default, MfgDefault
				OneOfOption Option: "120 Ohms" Value: 1
			End 
		End 
		OneOf Prompt: "DIMM RON Training*", Help: "DIMM RON Training", QuestionFlags: 0x10, QuestionId: 0x4D4, VarStoreId: 0x1, VarOffset: 0x8D8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Write Drive Strength/Equalization 2D*", Help: "", QuestionFlags: 0x10, QuestionId: 0x4D5, VarStoreId: 0x1, VarOffset: 0x8D9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Write Slew Rate Training*", Help: "Write Slew Rate Training", QuestionFlags: 0x10, QuestionId: 0x4D6, VarStoreId: 0x1, VarOffset: 0x8DA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Read ODT Training*", Help: "Read On-Die Termination Training", QuestionFlags: 0x10, QuestionId: 0x4D7, VarStoreId: 0x1, VarOffset: 0x8DB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Read Equalization Training*", Help: "Read Equalization Training", QuestionFlags: 0x10, QuestionId: 0x4D8, VarStoreId: 0x1, VarOffset: 0x8DC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Read Amplifier Training*", Help: "Read Amplifier Training", QuestionFlags: 0x10, QuestionId: 0x4D9, VarStoreId: 0x1, VarOffset: 0x8DD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Write Timing Centering 2D", Help: "Write Dq-Dqs Timing Centering 2D", QuestionFlags: 0x10, QuestionId: 0x4DA, VarStoreId: 0x1, VarOffset: 0x8DE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Read Timing Centering 2D", Help: "Read Dq-Dqs Timing Centering 2D", QuestionFlags: 0x10, QuestionId: 0x4DB, VarStoreId: 0x1, VarOffset: 0x8DF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Command Voltage Centering", Help: "Command Voltage Centering", QuestionFlags: 0x10, QuestionId: 0x4DC, VarStoreId: 0x1, VarOffset: 0x8E0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Write Voltage Centering 2D", Help: "Write Voltage Centering 2D", QuestionFlags: 0x10, QuestionId: 0x4DD, VarStoreId: 0x1, VarOffset: 0x8E1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Read Voltage Centering 2D", Help: "Read Voltage Centering 2D", QuestionFlags: 0x10, QuestionId: 0x4DE, VarStoreId: 0x1, VarOffset: 0x8E2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Late Command Training", Help: "Late Command Training", QuestionFlags: 0x10, QuestionId: 0x4DF, VarStoreId: 0x1, VarOffset: 0x8E3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Round Trip Latency", Help: "Round Trip Latency Training", QuestionFlags: 0x10, QuestionId: 0x4E0, VarStoreId: 0x1, VarOffset: 0x8E4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Turn Around Timing Training", Help: "Turn Around Timing Training", QuestionFlags: 0x10, QuestionId: 0x4E1, VarStoreId: 0x1, VarOffset: 0x8E5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Rank Margin Tool", Help: "Rank Margin Tool Training", QuestionFlags: 0x10, QuestionId: 0x4E2, VarStoreId: 0x1, VarOffset: 0x8E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Memory Test", Help: "Memory Test Training", QuestionFlags: 0x10, QuestionId: 0x4E3, VarStoreId: 0x1, VarOffset: 0x8E7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "DIMM SPD Alias Test", Help: "Test to determine if the SPD has been corrupted to cause memory aliasing.", QuestionFlags: 0x10, QuestionId: 0x4E4, VarStoreId: 0x1, VarOffset: 0x8E8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Receive Enable Centering 1D", Help: "Receive Enable Centering 1D", QuestionFlags: 0x10, QuestionId: 0x4E5, VarStoreId: 0x1, VarOffset: 0x8E9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Retrain Margin Check", Help: "Retrain Margin Check", QuestionFlags: 0x10, QuestionId: 0x4E6, VarStoreId: 0x1, VarOffset: 0x8EA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "Write Drive Strength Up/Dn independently", Help: "Write Drive Strength Up/Dn independently", QuestionFlags: 0x10, QuestionId: 0x4E7, VarStoreId: 0x1, VarOffset: 0x8EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "CMD Slew Rate Training", Help: "CMD Slew Rate Training", QuestionFlags: 0x10, QuestionId: 0x4E8, VarStoreId: 0x1, VarOffset: 0x8EC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "CMD Drive Strength / Tx Equalization", Help: "CMD Drive Strength / Tx Equalization", QuestionFlags: 0x10, QuestionId: 0x4E9, VarStoreId: 0x1, VarOffset: 0x8ED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "CMD Normalization", Help: "CMD Normalization", QuestionFlags: 0x10, QuestionId: 0x4EA, VarStoreId: 0x1, VarOffset: 0x8EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
	End 
	Form FormId: 0x274D, Title: "Memory Thermal Configuration"
		Subtitle Prompt: "Memory Thermal Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Ref Prompt: "Memory Power and Thermal Throttling", Help: ".", QuestionFlags: 0x0, QuestionId: 0x4EB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x274E
		OneOf Prompt: "Memory Thermal Management", Help: "Enable/Disable Memory Thermal Management.", QuestionFlags: 0x10, QuestionId: 0x4EC, VarStoreId: 0x1, VarOffset: 0x931, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x4EC, Value: 0x0
			OneOf Prompt: "PECI Injected Temperature", Help: "Enable/Disable memory temperatures to be injected to the processor via PECI.", QuestionFlags: 0x10, QuestionId: 0x4ED, VarStoreId: 0x1, VarOffset: 0x932, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "EXTTS# via TS-on-Board", Help: "Enable/Disable routing TS-on-Board's ALERT# and THERM# to EXTTS# pins on the PCH.", QuestionFlags: 0x10, QuestionId: 0x4EE, VarStoreId: 0x1, VarOffset: 0x933, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "EXTTS# via TS-on-DIMM", Help: "Enable/Disable routing TS-on-DIMM's ALERT# to EXTTS# pin on the PCH.", QuestionFlags: 0x10, QuestionId: 0x4EF, VarStoreId: 0x1, VarOffset: 0x934, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Virtual Temperature Sensor (VTS)", Help: "Enable/Disable Virtual Temperature Sensor (VTS).", QuestionFlags: 0x10, QuestionId: 0x4F0, VarStoreId: 0x1, VarOffset: 0x935, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
	End 
	Form FormId: 0x274E, Title: "Memory Power and Thermal Throttling"
		Subtitle Prompt: "Memory Power and Thermal Throttling", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "DDR PowerDown and idle counter", Help: "BIOS: BIOS is in control of DDR CKE mode and idle timer value. PCODE: pcode will manage the modes.", QuestionFlags: 0x10, QuestionId: 0x4F1, VarStoreId: 0x1, VarOffset: 0x8F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "PCODE" Value: 0
			OneOfOption Option: "BIOS" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "For LPDDR Only: DDR PowerDown and idle counter", Help: "For LPDDR Only: BIOS: BIOS is in control of DDR CKE mode and idle timer value. PCODE: pcode will manage the modes.", QuestionFlags: 0x10, QuestionId: 0x4F2, VarStoreId: 0x1, VarOffset: 0x8F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "PCODE" Value: 0
			OneOfOption Option: "BIOS" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "REFRESH_2X_MODE", Help: "0- Disabled 1-iMC enables 2xRef when Warm and Hot 2- iMC enables 2xRef when Hot", QuestionFlags: 0x10, QuestionId: 0x4F3, VarStoreId: 0x1, VarOffset: 0x8F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "1- Enabled for WARM or HOT" Value: 1
			OneOfOption Option: "2- Enabled HOT only" Value: 2
		End 
		OneOf Prompt: "LPDDR Thermal Sensor", Help: "When enabled, MC uses MR4 to read LPDDR thermal sensors", QuestionFlags: 0x10, QuestionId: 0x4F4, VarStoreId: 0x1, VarOffset: 0x8F5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "SelfRefresh Enable", Help: "Enable, Disable(Enable= Def)", QuestionFlags: 0x10, QuestionId: 0x4F5, VarStoreId: 0x1, VarOffset: 0x92A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		Numeric Prompt: "SelfRefresh IdleTimer", Help: "range [64K-1;512]in DLCK800s, (512= Def)", QuestionFlags: 0x10, QuestionId: 0x4F6, VarStoreId: 0x1, VarOffset: 0x92B, Flags: 0x11, Size: 16, Min: 0x200, Max: 0xFFFF, Step: 0x1
			Default DefaultId: 0x0 Value: 512
		End 
		OneOf Prompt: "Throttler CKEMin Defeature", Help: "On, Off", QuestionFlags: 0x10, QuestionId: 0x4F7, VarStoreId: 0x1, VarOffset: 0x92D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Enabled" Value: 1
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
		End 
		Numeric Prompt: "Throttler CKEMin Timer", Help: "Timer value for CKEMin, range[255;0]. Req'd min of SC_ROUND_T + BYTE_LENGTH (4)", QuestionFlags: 0x10, QuestionId: 0x4F8, VarStoreId: 0x1, VarOffset: 0x92E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 48
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC51, Value: 0x2
				Not 
			End 
			OneOf Prompt: "For LPDDR Only: Throttler CKEMin Defeature", Help: "For LPDDR Only: On, Off", QuestionFlags: 0x10, QuestionId: 0x4F9, VarStoreId: 0x1, VarOffset: 0x92F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
			Numeric Prompt: "For LPDDR Only: Throttler CKEMin Timer", Help: "For LPDDR Only: Timer value for CKEMin, range[255;0]. Req'd min of SC_ROUND_T + BYTE_LENGTH (4)", QuestionFlags: 0x10, QuestionId: 0x4FA, VarStoreId: 0x1, VarOffset: 0x930, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 64
			End 
		End 
		Ref Prompt: "Dram Power Meter", Help: ".", QuestionFlags: 0x0, QuestionId: 0x4FB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x274F
		Ref Prompt: "Memory Thermal Reporting", Help: ".", QuestionFlags: 0x0, QuestionId: 0x4FC, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2750
		Ref Prompt: "Memory RAPL", Help: ".", QuestionFlags: 0x0, QuestionId: 0x4FD, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2752
	End 
	Form FormId: 0x274F, Title: "Dram Power Meter"
		Subtitle Prompt: "Dram Power Meter", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Use user provided power weights, scale factor, and channel power floor values", Help: "Enabled: User provided power weights, scale factor, and channel power floor values are used. Disabled: BIOS sets power weights, scale factor, and channel power floor values based on DIMMs present in system.", QuestionFlags: 0x10, QuestionId: 0x4FE, VarStoreId: 0x1, VarOffset: 0x8F7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x4FE, Value: 0x0
			Numeric Prompt: "Energy Scale Factor", Help: "range[7;0]= [7.3;931.3]in pJ, (3= 116pJ Def)", QuestionFlags: 0x10, QuestionId: 0x4FF, VarStoreId: 0x1, VarOffset: 0x8F8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
				Default DefaultId: 0x0 Value: 4
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "Idle Energy Ch0Dimm0", Help: "Idle Energy Consumed for 1 clk w/dimm idle/cke on, range[63;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x500, VarStoreId: 0x1, VarOffset: 0x917, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 10
			End 
			Numeric Prompt: "PowerDown Energy Ch0Dimm0", Help: "PowerDown Energy Consumed w/dimm idle/cke off, range[63;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x501, VarStoreId: 0x1, VarOffset: 0x919, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 6
			End 
			Numeric Prompt: "Activate Energy Ch0Dimm0", Help: "Activate Energy Contribution, range[255;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x502, VarStoreId: 0x1, VarOffset: 0x91B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 172
			End 
			Numeric Prompt: "Read Energy Ch0Dimm0", Help: "Read Energy Contribution, range[255;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x503, VarStoreId: 0x1, VarOffset: 0x91D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 212
			End 
			Numeric Prompt: "Write Energy Ch0Dimm0", Help: "Write Energy Contribution, range[255;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x504, VarStoreId: 0x1, VarOffset: 0x91F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 221
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "Idle Energy Ch0Dimm1", Help: "Idle Energy Consumed for 1 clk w/dimm idle/cke on, range[63;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x505, VarStoreId: 0x1, VarOffset: 0x916, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 10
			End 
			Numeric Prompt: "PowerDown Energy Ch0Dimm1", Help: "PowerDown Energy Consumed w/dimm idle/cke off, range[63;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x506, VarStoreId: 0x1, VarOffset: 0x918, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 6
			End 
			Numeric Prompt: "Activate Energy Ch0Dimm1", Help: "Activate Energy Contribution, range[255;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x507, VarStoreId: 0x1, VarOffset: 0x91A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 172
			End 
			Numeric Prompt: "Read Energy Ch0Dimm1", Help: "Read Energy Contribution, range[255;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x508, VarStoreId: 0x1, VarOffset: 0x91C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 212
			End 
			Numeric Prompt: "Write Energy Ch0Dimm1", Help: "Write Energy Contribution, range[255;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x509, VarStoreId: 0x1, VarOffset: 0x91E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 221
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "Idle Energy Ch1Dimm0", Help: "Idle Energy Consumed for 1 clk w/dimm idle/cke on, range[63;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x50A, VarStoreId: 0x1, VarOffset: 0x921, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 10
			End 
			Numeric Prompt: "PowerDown Energy Ch1Dimm0", Help: "PowerDown Energy Consumed w/dimm idle/cke off, range[63;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x50B, VarStoreId: 0x1, VarOffset: 0x923, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 6
			End 
			Numeric Prompt: "Activate Energy Ch1Dimm0", Help: "Activate Energy Contribution, range[255;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x50C, VarStoreId: 0x1, VarOffset: 0x925, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 172
			End 
			Numeric Prompt: "Read Energy Ch1Dimm0", Help: "Read Energy Contribution, range[255;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x50D, VarStoreId: 0x1, VarOffset: 0x927, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 212
			End 
			Numeric Prompt: "Write Energy Ch1Dimm0", Help: "Write Energy Contribution, range[255;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x50E, VarStoreId: 0x1, VarOffset: 0x929, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 221
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "Idle Energy Ch1Dimm1", Help: "Idle Energy Consumed for 1 clk w/dimm idle/cke on, range[63;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x50F, VarStoreId: 0x1, VarOffset: 0x920, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 10
			End 
			Numeric Prompt: "PowerDown Energy Ch1Dimm1", Help: "PowerDown Energy Consumed w/dimm idle/cke off, range[63;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x510, VarStoreId: 0x1, VarOffset: 0x922, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 6
			End 
			Numeric Prompt: "Activate Energy Ch1Dimm1", Help: "Activate Energy Contribution, range[255;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x511, VarStoreId: 0x1, VarOffset: 0x924, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 172
			End 
			Numeric Prompt: "Read Energy Ch1Dimm1", Help: "Read Energy Contribution, range[255;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x512, VarStoreId: 0x1, VarOffset: 0x926, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 212
			End 
			Numeric Prompt: "Write Energy Ch1Dimm1", Help: "Write Energy Contribution, range[255;0],(0= Def)", QuestionFlags: 0x10, QuestionId: 0x513, VarStoreId: 0x1, VarOffset: 0x928, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 221
			End 
		End 
	End 
	Form FormId: 0x2750, Title: "Memory Thermal Reporting"
		OneOf Prompt: "Lock Thermal Management Registers", Help: "Enabled: lock several PCU registers related to DDR power/thermal management", QuestionFlags: 0x10, QuestionId: 0x514, VarStoreId: 0x1, VarOffset: 0x8F6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "Memory Thermal Reporting", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Extern Therm Status", Help: "Enabled: The value from EXTTS is used Disabled: Pcode ignores the EXTTS.", QuestionFlags: 0x10, QuestionId: 0x515, VarStoreId: 0x1, VarOffset: 0x8EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Closed Loop Therm Manage", Help: "Enabled: CLTM pcode algorithm will be used. Note: CLTM will preceed OLTM", QuestionFlags: 0x10, QuestionId: 0x516, VarStoreId: 0x1, VarOffset: 0x8F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Open Loop Therm Manage", Help: "Enabled: OLTM pcode algorithm will be used. Note: CLTM will preceed OLTM", QuestionFlags: 0x10, QuestionId: 0x517, VarStoreId: 0x1, VarOffset: 0x8F1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "Thermal Threshold Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "Warm Threshold Ch0 Dimm0", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x518, VarStoreId: 0x1, VarOffset: 0x906, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Warm Threshold Ch0 Dimm1", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x519, VarStoreId: 0x1, VarOffset: 0x907, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Hot Threshold Ch0 Dimm0", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x51A, VarStoreId: 0x1, VarOffset: 0x90A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Hot Threshold Ch0 Dimm1", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x51B, VarStoreId: 0x1, VarOffset: 0x90B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Warm Threshold Ch1 Dimm0", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x51C, VarStoreId: 0x1, VarOffset: 0x908, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Warm Threshold Ch1 Dimm1", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x51D, VarStoreId: 0x1, VarOffset: 0x909, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Hot Threshold Ch1 Dimm0", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x51E, VarStoreId: 0x1, VarOffset: 0x90C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Hot Threshold Ch1 Dimm1", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x51F, VarStoreId: 0x1, VarOffset: 0x90D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "Thermal Throttle Budget Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "Warm Budget Ch0 Dimm0", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x520, VarStoreId: 0x1, VarOffset: 0x90E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Warm Budget Ch0 Dimm1", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x521, VarStoreId: 0x1, VarOffset: 0x90F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Hot Budget Ch0 Dimm0", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x522, VarStoreId: 0x1, VarOffset: 0x912, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Hot Budget Ch0 Dimm1", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x523, VarStoreId: 0x1, VarOffset: 0x913, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Warm Budget Ch1 Dimm0", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x524, VarStoreId: 0x1, VarOffset: 0x910, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Warm Budget Ch1 Dimm1", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x525, VarStoreId: 0x1, VarOffset: 0x911, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Hot Budget Ch1 Dimm0", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x526, VarStoreId: 0x1, VarOffset: 0x914, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
		Numeric Prompt: "Hot Budget Ch1 Dimm1", Help: "range[255;0]=[31.875;0] in W for OLTM, [127.5;0] in C for CLTM", QuestionFlags: 0x10, QuestionId: 0x527, VarStoreId: 0x1, VarOffset: 0x915, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
			Default DefaultId: 0x0 Value: 255
		End 
	End 
	Form FormId: 0x2752, Title: "Memory RAPL"
		Subtitle Prompt: "Memory RAPL", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x4FE, Value: 0x0
			Numeric Prompt: "Rapl Power Floor Ch0", Help: "Power budget ,range[255;0], (0= 5.3W Def)", QuestionFlags: 0x10, QuestionId: 0x528, VarStoreId: 0x1, VarOffset: 0x8FA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "Rapl Power Floor Ch1", Help: "Power budget ,range[255;0],(0= 5.3W Def)", QuestionFlags: 0x10, QuestionId: 0x529, VarStoreId: 0x1, VarOffset: 0x8F9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "RAPL PL Lock", Help: "Enable= lock Rapl Limit register , Disable(Disable= Def)", QuestionFlags: 0x10, QuestionId: 0x52A, VarStoreId: 0x1, VarOffset: 0x8FB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "RAPL PL 1 enable", Help: "Enable= enable, Disable(Disable= Def)", QuestionFlags: 0x10, QuestionId: 0x52B, VarStoreId: 0x1, VarOffset: 0x903, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		Numeric Prompt: "RAPL PL 1 Power", Help: "range[0;2^14-1]= [2047.875;0]in W, (0= Def)", QuestionFlags: 0x10, QuestionId: 0x52C, VarStoreId: 0x1, VarOffset: 0x904, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FFF, Step: 0x1
			Default DefaultId: 0x0 Value: Other
				Value 
					Uint64 Value: 0x0
				End 
			End 
		End 
		Numeric Prompt: "RAPL PL 1 WindowX", Help: "Power PL 1 time window X value, (1/1024)*(1+(x/4))*(2^y) (0=Def)", QuestionFlags: 0x10, QuestionId: 0x52D, VarStoreId: 0x1, VarOffset: 0x901, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x1
			Default DefaultId: 0x0 Value: Other
				Value 
					Uint64 Value: 0x0
				End 
			End 
		End 
		Numeric Prompt: "RAPL PL 1 WindowY", Help: "Power PL 1 time window Y value, (1/1024)*(1+(x/4))*(2^y) (0=Def)", QuestionFlags: 0x10, QuestionId: 0x52E, VarStoreId: 0x1, VarOffset: 0x902, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
			Default DefaultId: 0x0 Value: Other
				Value 
					Uint64 Value: 0x0
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "RAPL PL 2 enable", Help: "Enable= enable, Disable(Disable= Def)", QuestionFlags: 0x10, QuestionId: 0x52F, VarStoreId: 0x1, VarOffset: 0x8FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		Numeric Prompt: "RAPL PL 2 Power", Help: "range[0;2^14-1]= [2047.875;0]in W, (0= Def)", QuestionFlags: 0x10, QuestionId: 0x530, VarStoreId: 0x1, VarOffset: 0x8FF, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FFF, Step: 0x1
			Default DefaultId: 0x0 Value: 222
		End 
		Numeric Prompt: "RAPL PL 2 WindowX", Help: "Power PL 2 time window X value, (1/1024)*(1+(x/4))*(2^y) (0=Def)", QuestionFlags: 0x10, QuestionId: 0x531, VarStoreId: 0x1, VarOffset: 0x8FC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x1
			Default DefaultId: 0x0 Value: 1
		End 
		Numeric Prompt: "RAPL PL 2 WindowY", Help: "Power PL 2 time window Y value, (1/1024)*(1+(x/4))*(2^y) (0=Def)", QuestionFlags: 0x10, QuestionId: 0x532, VarStoreId: 0x1, VarOffset: 0x8FD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
			Default DefaultId: 0x0 Value: 10
		End 
	End 
	Form FormId: 0x2754, Title: "PCH-IO Configuration"
		Subtitle Prompt: "PCH-IO Configuration", Help: "", Flags: 0x0
		End 
		Text Prompt: "Name", Help: "PCH Name", Text: "UnKnown"
		Text Prompt: "PCH SKU", Help: "PCH SKU", Text: "UnKnown"
		Text Prompt: "Stepping", Help: "PCH Stepping", Text: "UnKnown"
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Ref Prompt: "PCI Express Configuration", Help: "PCI Express Configuration settings", QuestionFlags: 0x0, QuestionId: 0x533, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2755
		Ref Prompt: "SATA And RST Configuration", Help: "SATA Device Options Settings", QuestionFlags: 0x0, QuestionId: 0x534, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2757
		Ref Prompt: "USB Configuration", Help: "USB Configuration settings", QuestionFlags: 0x0, QuestionId: 0x535, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2756
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "Security Configuration", Help: "Security Configuration settings", QuestionFlags: 0x0, QuestionId: 0x536, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2775
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8C, Value: 0x4
			Ref Prompt: "HD Audio Configuration", Help: "HD Audio Subsystem Configuration Settings", QuestionFlags: 0x0, QuestionId: 0x537, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2772
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "SerialIo Configuration", Help: "SerialIo Configuration Settings", QuestionFlags: 0x0, QuestionId: 0x538, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2776
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC50, Values: [4, 20, 10, 26, 8, 11, 7, 19, 3, 27, 5, 131, 12, 33, 32]
				Not 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC42, Value: 0x0
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Or 
				End 
				Ref Prompt: "SkyCam Configuration", Help: "SkyCam Configuration", QuestionFlags: 0x0, QuestionId: 0x539, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2784
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC51, Value: 0x2
				Not 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC42, Value: 0x0
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Or 
				End 
				Ref Prompt: "SCS Configuration", Help: "Storage and Communication Subsystem (SCS) Configuration", QuestionFlags: 0x0, QuestionId: 0x53A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2785
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8C, Value: 0x4
			SuppressIf 
				EqIdVal QuestionId: 0xC42, Value: 0x0
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Or 
				End 
				Ref Prompt: "ISH Configuration", Help: "Integrated Sensor Hub (ISH) Configuration", QuestionFlags: 0x0, QuestionId: 0x53B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2786
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "TraceHub Configuration Menu", Help: "TraceHub Configuration Settings", QuestionFlags: 0x0, QuestionId: 0x53C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2787
			Ref Prompt: "Pch Thermal Throttling Control", Help: "Pch Thermal Throttling Control", QuestionFlags: 0x0, QuestionId: 0x53D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2788
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Ref Prompt: "SB Porting Configuration", Help: "SB Porting Configuration.", QuestionFlags: 0x0, QuestionId: 0x53E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27E2
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "DCI enable (HDCIEN)", Help: "When DCI is Enabled, it is taken as user consent to enable the DCI which allows debug over the USB3 interface. When Disabled, the host control is not enabling DCI feature.", QuestionFlags: 0x10, QuestionId: 0x53F, VarStoreId: 0x1, VarOffset: 0x994, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0xA
					Not 
					EqIdVal QuestionId: 0xC50, Value: 0x1A
					Not 
					And 
				End 
				OneOf Prompt: "USB/UART", Help: "The UART/USB selector for kernel debug on RVP5", QuestionFlags: 0x10, QuestionId: 0x540, VarStoreId: 0x1, VarOffset: 0x32, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "UART" Value: 0, Default, MfgDefault
					OneOfOption Option: "USB" Value: 1
				End 
			End 
			OneOf Prompt: "Debug Port Selection", Help: "Select Kernel Debug Port and report in ACPI DBG2 table", QuestionFlags: 0x10, QuestionId: 0x541, VarStoreId: 0x1, VarOffset: 0x992, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Legacy UART" Value: 0, Default, MfgDefault
				SuppressIf 
					EqIdVal QuestionId: 0x9F9, Value: 0x1
						EqIdVal QuestionId: 0x9F3, Value: 0x1
						Or 
						EqIdVal QuestionId: 0x9F4, Value: 0x1
						Or 
					End 
					OneOfOption Option: "SERIALIO UART2" Value: 3
				End 
			End 
			OneOf Prompt: "GNSS", Help: "ISH - GNSS is connected to ISH (need ISH enabled). SerialIO UART - GNSS is connected to SerialIO (need SerialIO UART1 enabled)", QuestionFlags: 0x10, QuestionId: 0x542, VarStoreId: 0x1, VarOffset: 0x288, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				SuppressIf 
					EqIdVal QuestionId: 0x9F8, Value: 0x0
					OneOfOption Option: "SerialIO UART" Value: 1
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xA67, Value: 0x0
					OneOfOption Option: "ISH" Value: 2
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x542, Value: 0x0
				OneOf Prompt: "GNSS Device Model", Help: "GNSS Device Model", QuestionFlags: 0x10, QuestionId: 0x543, VarStoreId: 0x1, VarOffset: 0x287, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x0, Step: 0x0
					OneOfOption Option: "CG2000" Value: 0, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC8D, Value: 0x0
				OneOf Prompt: "PCH LAN Controller", Help: "Enable/Disable onboard NIC.", QuestionFlags: 0x10, QuestionId: 0x544, VarStoreId: 0x1, VarOffset: 0x993, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1, Default
					OneOfOption Option: "Disabled" Value: 0
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC8D, Value: 0x1
				Text Prompt: "PCH LAN Controller", Help: "", Text: "No GbE Region"
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC8C, Value: 0x1
					Not 
					EqIdVal QuestionId: 0xC8C, Value: 0x5
					Not 
					And 
				End 
				OneOf Prompt: "Sensor Hub Type", Help: "Choose the Sensor Hub Type, 'None' will Suppress 'I2C Sensor Hub' Setup Option','I2C' Will Suppress 'ALS' Setup Option and 'USB' will Suppress Both I2C and ALS.", QuestionFlags: 0x10, QuestionId: 0x545, VarStoreId: 0x1, VarOffset: 0x31, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "None" Value: 0, Default, MfgDefault
					OneOfOption Option: "I2C Sensor Hub" Value: 1
					OneOfOption Option: "USB Sensor Hub" Value: 2
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
				OneOf Prompt: "DeepSx Power Policies", Help: "configure the DeepSx Mode configuration.", QuestionFlags: 0x10, QuestionId: 0x546, VarStoreId: 0x1, VarOffset: 0x98E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					SuppressIf 
						EqIdVal QuestionId: 0xC8C, Value: 0x2
							EqIdVal QuestionId: 0xC8C, Value: 0x4
							Or 
							EqIdVal QuestionId: 0xC8C, Value: 0x3
							Or 
						End 
						OneOfOption Option: "Enabled in S4-S5/Battery" Value: 3
						OneOfOption Option: "Enabled in S3-S4-S5/Battery" Value: 5
						OneOfOption Option: "Enabled in S3-S4-S5" Value: 6
					End 
					OneOfOption Option: "Enabled in S4-S5" Value: 4
				End 
			End 
			OneOf Prompt: "LAN Wake From DeepSx", Help: "Wake from DeepSx by the assertion of LAN_WAKE# pin", QuestionFlags: 0x10, QuestionId: 0x547, VarStoreId: 0x1, VarOffset: 0x98F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x544, Value: 0x0
				OneOf Prompt: "  Wake on LAN Enable", Help: "Enable/Disable integrated LAN to wake the system.", QuestionFlags: 0x10, QuestionId: 0x548, VarStoreId: 0x1, VarOffset: 0x996, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					OneOfOption Option: "Disabled" Value: 0
				End 
				OneOf Prompt: "  SLP_LAN# Low on DC Power", Help: "Enable/Disable SLP_LAN# Low on DC Power.", QuestionFlags: 0x10, QuestionId: 0x549, VarStoreId: 0x1, VarOffset: 0x997, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					OneOfOption Option: "Disabled" Value: 0
				End 
				OneOf Prompt: "K1 off", Help: "Enable or disable K1 off feature (CLKREQ).", QuestionFlags: 0x10, QuestionId: 0x54A, VarStoreId: 0x1, VarOffset: 0x998, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					OneOfOption Option: "Disabled" Value: 0
				End 
			End 
			OneOf Prompt: "Wake on WLAN and BT Enable", Help: "Enable/Disable PCI Express Wireless LAN and Bluetooth to wake the system. ", QuestionFlags: 0x10, QuestionId: 0x54B, VarStoreId: 0x1, VarOffset: 0x999, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x54B, Value: 0x0
				OneOf Prompt: "DeepSx Wake on WLAN and BT Enable", Help: "Enable/Disable PCI Express Wireless LAN and Bluetooth to wake the system from DeepSx. ", QuestionFlags: 0x10, QuestionId: 0x54C, VarStoreId: 0x1, VarOffset: 0x99A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "Disable DSX ACPRESENT PullDown", Help: "Disable PCH internal ACPRESENT PullDown when DeepSx or G3 exit.", QuestionFlags: 0x10, QuestionId: 0x54D, VarStoreId: 0x1, VarOffset: 0x990, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "CLKRUN# logic", Help: "Enable the CLKRUN# logic to stop the PCI clocks.", QuestionFlags: 0x10, QuestionId: 0x54E, VarStoreId: 0x1, VarOffset: 0x99B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "Serial IRQ Mode", Help: "Configure Serial IRQ Mode.", QuestionFlags: 0x10, QuestionId: 0x54F, VarStoreId: 0x1, VarOffset: 0x9A6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x0 Value: 1
				OneOfOption Option: "Quiet" Value: 0, MfgDefault
				OneOfOption Option: "Continuous" Value: 1
			End 
			OneOf Prompt: "Port 61h Bit-4 Emulation", Help: "Emulation of Port 61h bit-4 toggling in SMM", QuestionFlags: 0x10, QuestionId: 0x550, VarStoreId: 0x1, VarOffset: 0x9A7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				True 
				OneOf Prompt: "High Precision Timer", Help: "Enable or Disable the High Precision Event Timer.", QuestionFlags: 0x10, QuestionId: 0x551, VarStoreId: 0x1, VarOffset: 0x9A2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "State After G3", Help: "Specify what state to go to when power is re-applied after a power failure (G3 state).", QuestionFlags: 0x10, QuestionId: 0x552, VarStoreId: 0x1, VarOffset: 0x9A3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "S0 State" Value: 0
				OneOfOption Option: "S5 State" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "Port 80h Redirection", Help: "Control where the Port 80h cycles are sent.", QuestionFlags: 0x10, QuestionId: 0x553, VarStoreId: 0x1, VarOffset: 0x9A4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "LPC Bus" Value: 0, Default, MfgDefault
				OneOfOption Option: "PCIE Bus" Value: 1
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0x553, Value: 0x0
					Not 
				End 
				OneOf Prompt: "Enhance Port 80h LPC Decoding", Help: "Support the word/dword decoding of port 80h behind LPC", QuestionFlags: 0x10, QuestionId: 0x554, VarStoreId: 0x1, VarOffset: 0x9A5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "Compatible Revision ID", Help: "Enable/Disable the PCH Compatible Revision ID feature", QuestionFlags: 0x14, QuestionId: 0x2753, VarStoreId: 0x1, VarOffset: 0x99F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x0 Value: 0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, MfgDefault
			End 
			OneOf Prompt: "PCH Cross Throttling", Help: "Enable/Disable the PCH Cross Throttling feature. Only ULT support this feature.", QuestionFlags: 0x10, QuestionId: 0x555, VarStoreId: 0x1, VarOffset: 0xF45, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "Disable Energy Reporting", Help: "TRUE: Disable Energy Report. FALSE: Enable Energy Report. MUST set it as FALSE. This is only for test purpose.", QuestionFlags: 0x10, QuestionId: 0x556, VarStoreId: 0x1, VarOffset: 0x99C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "FALSE" Value: 0, Default, MfgDefault
				OneOfOption Option: "TRUE" Value: 1
			End 
			OneOf Prompt: "Enable TCO Timer", Help: "Enable/Disable TCO timer. When disabled, it disables PCH ACPI timer, and stops TCO timer.", QuestionFlags: 0x10, QuestionId: 0x557, VarStoreId: 0x1, VarOffset: 0x99D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Pcie Pll SSC", Help: "Pcie Pll SSC percentage.AUTO - Keep hw default, no BIOS override. Range is 0.0%-2.0%.", QuestionFlags: 0x10, QuestionId: 0x558, VarStoreId: 0x1, VarOffset: 0x9A8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
				OneOfOption Option: "Auto" Value: 255, Default, MfgDefault
				OneOfOption Option: "0.0%" Value: 0
				OneOfOption Option: "0.1%" Value: 1
				OneOfOption Option: "0.2%" Value: 2
				OneOfOption Option: "0.3%" Value: 3
				OneOfOption Option: "0.4%" Value: 4
				OneOfOption Option: "0.5%" Value: 5
				OneOfOption Option: "0.6%" Value: 6
				OneOfOption Option: "0.7%" Value: 7
				OneOfOption Option: "0.8%" Value: 8
				OneOfOption Option: "0.9%" Value: 9
				OneOfOption Option: "1.0%" Value: 10
				OneOfOption Option: "1.1%" Value: 11
				OneOfOption Option: "1.2%" Value: 12
				OneOfOption Option: "1.3%" Value: 13
				OneOfOption Option: "1.4%" Value: 14
				OneOfOption Option: "1.5%" Value: 15
				OneOfOption Option: "1.6%" Value: 16
				OneOfOption Option: "1.7%" Value: 17
				OneOfOption Option: "1.8%" Value: 18
				OneOfOption Option: "1.9%" Value: 19
				OneOfOption Option: "2.0%" Value: 20
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC51, Value: 0x2
					Not 
					EqIdVal QuestionId: 0xC50, Value: 0x42
					Not 
					And 
					EqIdVal QuestionId: 0xC8C, Value: 0x4
					Not 
					And 
				End 
				OneOf Prompt: "IOAPIC 24-119 Entries", Help: "Enables/Disables IOAPIC 24-119 Entries. IRQ24-119 may be used by PCH devices. Disabling those interrupts may cause certain devices failure.", QuestionFlags: 0x10, QuestionId: 0x559, VarStoreId: 0x1, VarOffset: 0xF44, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "Unlock PCH P2SB", Help: "Unlock PCH P2SB SBI and Configuration space by PSF", QuestionFlags: 0x10, QuestionId: 0x55A, VarStoreId: 0x1, VarOffset: 0xF9B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Flash Protection Range Registers (FPRR)", Help: "Enable Flash Protection Range Registers", QuestionFlags: 0x10, QuestionId: 0x55B, VarStoreId: 0x1, VarOffset: 0xF9C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "SPD Write Disable", Help: "Enable/Disable setting SPD Write Disable. For security recommendations, SPD write disable bit must be set.", QuestionFlags: 0x10, QuestionId: 0x55C, VarStoreId: 0x1, VarOffset: 0xF9A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "FALSE" Value: 0
				OneOfOption Option: "TRUE" Value: 1, Default, MfgDefault
			End 
			CheckBox Prompt: "ChipsetInit HECI Message", Help: "Enable/Disable ChipsetInit HECI Message (disable will prevent the HSIO version check and HSIO init messages from being sent).", QuestionFlags: 0x10, QuestionId: 0x55D, VarStoreId: 0x1, VarOffset: 0xF9D, Flags: 0x1, Default: Enabled, MfgDefault: Disabled
			End 
			OneOf Prompt: "Bypass ChipsetInit sync reset", Help: "Setting this option to skip ChipsetInit sync reset", QuestionFlags: 0x10, QuestionId: 0x55E, VarStoreId: 0x1, VarOffset: 0xF9E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
	End 
	Form FormId: 0x2755, Title: "PCI Express Configuration"
		Subtitle Prompt: "PCI Express Configuration", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCI Express Clock Gating", Help: "PCI Express Clock Gating Enable/Disable for each root port.", QuestionFlags: 0x10, QuestionId: 0x55F, VarStoreId: 0x1, VarOffset: 0xA3D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 1
				OneOfOption Option: "Enabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "Legacy IO Low Latency", Help: "Set to enable low latenc of legacy IO. Some systems require lower IO latency irrespective of power. This is a tradeoff between power and IO latency.", QuestionFlags: 0x10, QuestionId: 0x560, VarStoreId: 0x1, VarOffset: 0xFE8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default
				OneOfOption Option: "Enabled" Value: 1
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0x560, Value: 0x1
				OneOf Prompt: "DMI Link ASPM Control", Help: "The control of Active State Power Management of the DMI Link.
Auto is equal to POR setting.", QuestionFlags: 0x10, QuestionId: 0x561, VarStoreId: 0x1, VarOffset: 0xDCD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			Text Prompt: "PCIE Port assigned to LAN", Help: "", Text: "6"
			OneOf Prompt: "Port8xh Decode", Help: "PCI Express Port8xh Decode Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x562, VarStoreId: 0x1, VarOffset: 0xA3E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x562, Value: 0x0
				Numeric Prompt: "  Port8xh Decode Port#", Help: "Select PCI Express Port8xh Decode Root Port. User to ensure port availability", QuestionFlags: 0x10, QuestionId: 0x563, VarStoreId: 0x1, VarOffset: 0xA3F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			OneOf Prompt: "Peer Memory Write Enable", Help: "Peer Memory Write Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x564, VarStoreId: 0x1, VarOffset: 0xA40, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "Compliance Test Mode", Help: "Enable when using Compliance Load Board", QuestionFlags: 0x10, QuestionId: 0x565, VarStoreId: 0x1, VarOffset: 0xA41, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "PCIe-USB Glitch W/A", Help: "PCIe-USB Glitch W/A for bad USB device(s) connected behind PCIE/PEG Port.", QuestionFlags: 0x10, QuestionId: 0x566, VarStoreId: 0x1, VarOffset: 0xA42, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "PCIe function swap", Help: "When Disabled, prevents PCIE rootport function swap. If any function other than 0th is enabled, 0th will become visible.", QuestionFlags: 0x10, QuestionId: 0x567, VarStoreId: 0x1, VarOffset: 0xC89, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			Ref Prompt: "PCI Express Gen3 Eq Lanes", Help: "PCI Express Gen3 Equalization settings per PCIe lane", QuestionFlags: 0x0, QuestionId: 0x568, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2759
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
		End 
		Ref Prompt: "PCI Express Root Port 1", Help: "PCI Express Root Port 1 Settings.", QuestionFlags: 0x0, QuestionId: 0x569, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x275A
		SuppressIf 
			EqIdVal QuestionId: 0xC8B, Value: 0x0
				Not 
			End 
			Ref Prompt: "PCI Express Root Port 2", Help: "PCI Express Root Port 2 Settings.", QuestionFlags: 0x0, QuestionId: 0x56A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x275B
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8B, Value: 0x3
				EqIdVal QuestionId: 0xC88, Value: 0x3
				Or 
			End 
			Ref Prompt: "PCI Express Root Port 3", Help: "PCI Express Root Port 3 Settings.", QuestionFlags: 0x0, QuestionId: 0x56B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x275C
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC8B, Values: [2, 3]
				EqIdVal QuestionId: 0xC88, Value: 0x4
				Or 
			End 
			Ref Prompt: "PCI Express Root Port 4", Help: "PCI Express Root Port 4 Settings.", QuestionFlags: 0x0, QuestionId: 0x56C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x275D
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC88, Value: 0x5
			Ref Prompt: "PCI Express Root Port 5", Help: "PCI Express Root Port 5 Settings.", QuestionFlags: 0x0, QuestionId: 0x56D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x275E
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8A, Value: 0x0
				Not 
			End 
			Ref Prompt: "PCI Express Root Port 6", Help: "PCI Express Root Port 6 Settings.", QuestionFlags: 0x0, QuestionId: 0x56E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x275F
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC8A, Value: 0x3
			Ref Prompt: "PCI Express Root Port 7", Help: "PCI Express Root Port 7 Settings.", QuestionFlags: 0x0, QuestionId: 0x56F, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2760
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC8A, Values: [2, 3]
			Ref Prompt: "PCI Express Root Port 8", Help: "PCI Express Root Port 8 Settings.", QuestionFlags: 0x0, QuestionId: 0x570, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2761
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC88, Value: 0x9
			Ref Prompt: "PCI Express Root Port 9", Help: "PCI Express Root Port 9 Settings.", QuestionFlags: 0x0, QuestionId: 0x571, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2762
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC89, Value: 0x0
				Not 
				EqIdVal QuestionId: 0xC88, Value: 0xA
				Or 
			End 
			Ref Prompt: "PCI Express Root Port 10", Help: "PCI Express Root Port 10 Settings.", QuestionFlags: 0x0, QuestionId: 0x572, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2763
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC50, Values: [32]
				EqIdVal QuestionId: 0xC89, Value: 0x3
				Or 
			End 
			Ref Prompt: "PCI Express Root Port 11", Help: "PCI Express Root Port 11 Settings.", QuestionFlags: 0x0, QuestionId: 0x573, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2764
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC89, Values: [2, 3]
				EqIdVal QuestionId: 0xC88, Value: 0xC
				Or 
			End 
			Ref Prompt: "PCI Express Root Port 12", Help: "PCI Express Root Port 12 Settings.", QuestionFlags: 0x0, QuestionId: 0x574, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2765
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC51, Value: 0x1
				Not 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC88, Value: 0xD
				Ref Prompt: "PCI Express Root Port 13", Help: "PCI Express Root Port 13 Settings.", QuestionFlags: 0x0, QuestionId: 0x575, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2766
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC87, Value: 0x0
					Not 
				End 
				Ref Prompt: "PCI Express Root Port 14", Help: "PCI Express Root Port 14 Settings.", QuestionFlags: 0x0, QuestionId: 0x576, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2767
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC87, Value: 0x3
				Ref Prompt: "PCI Express Root Port 15", Help: "PCI Express Root Port 15 Settings.", QuestionFlags: 0x0, QuestionId: 0x577, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2768
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xC87, Values: [2, 3]
				Ref Prompt: "PCI Express Root Port 16", Help: "PCI Express Root Port 16 Settings.", QuestionFlags: 0x0, QuestionId: 0x578, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2769
			End 
			Ref Prompt: "PCI Express Root Port 17", Help: "PCI Express Root Port 17 Settings.", QuestionFlags: 0x0, QuestionId: 0x579, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x276A
			SuppressIf 
				EqIdVal QuestionId: 0xC86, Value: 0x0
					Not 
				End 
				Ref Prompt: "PCI Express Root Port 18", Help: "PCI Express Root Port 18 Settings.", QuestionFlags: 0x0, QuestionId: 0x57A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x276B
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC86, Value: 0x3
				Ref Prompt: "PCI Express Root Port 19", Help: "PCI Express Root Port 19 Settings.", QuestionFlags: 0x0, QuestionId: 0x57B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x276C
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xC86, Values: [2, 3]
				Ref Prompt: "PCI Express Root Port 20", Help: "PCI Express Root Port 20 Settings.", QuestionFlags: 0x0, QuestionId: 0x57C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x276D
			End 
			Ref Prompt: "PCI Express Root Port 21", Help: "PCI Express Root Port 21 Settings.", QuestionFlags: 0x0, QuestionId: 0x57D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x276E
			SuppressIf 
				EqIdVal QuestionId: 0xC85, Value: 0x0
					Not 
				End 
				Ref Prompt: "PCI Express Root Port 22", Help: "PCI Express Root Port 22 Settings.", QuestionFlags: 0x0, QuestionId: 0x57E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x276F
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC85, Value: 0x3
				Ref Prompt: "PCI Express Root Port 23", Help: "PCI Express Root Port 23 Settings.", QuestionFlags: 0x0, QuestionId: 0x57F, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2770
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xC85, Values: [2, 3]
				Ref Prompt: "PCI Express Root Port 24", Help: "PCI Express Root Port 24 Settings.", QuestionFlags: 0x0, QuestionId: 0x580, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2771
			End 
		End 
	End 
	Form FormId: 0x2756, Title: "USB Configuration"
		Subtitle Prompt: "USB Configuration", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC84, Value: 0x0
			OneOf Prompt: "SSIC Port 1", Help: "Enable/Disable support for SSIC.", QuestionFlags: 0x10, QuestionId: 0x581, VarStoreId: 0x1, VarOffset: 0x9C8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC83, Value: 0x0
			OneOf Prompt: "SSIC Port 2", Help: "Enable/Disable support for SSIC.", QuestionFlags: 0x10, QuestionId: 0x582, VarStoreId: 0x1, VarOffset: 0x9C9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
		End 
		OneOf Prompt: "XHCI Disable Compliance Mode", Help: "Options to disable Compliance Mode. Default is FALSE to not disable Compliance Mode. Set TRUE to disable Compliance Mode.", QuestionFlags: 0x10, QuestionId: 0x583, VarStoreId: 0x1, VarOffset: 0x9C7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "FALSE" Value: 0, Default, MfgDefault
			OneOfOption Option: "TRUE" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			OneOf Prompt: "xDCI Support", Help: "Enable/Disable xDCI (USB OTG Device).", QuestionFlags: 0x10, QuestionId: 0x584, VarStoreId: 0x1, VarOffset: 0x9CA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			OneOf Prompt: "USB Port Disable Override", Help: "Selectively Enable/Disable the corresponding USB port from reporting a Device Connection to the controller.", QuestionFlags: 0x10, QuestionId: 0x585, VarStoreId: 0x1, VarOffset: 0x9AC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Select Per-Pin" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x585, Value: 0x0
			OneOf Prompt: "USB SS Physical Connector #0", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x586, VarStoreId: 0x1, VarOffset: 0x9BD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "USB SS Physical Connector #1", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x587, VarStoreId: 0x1, VarOffset: 0x9BE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC82, Value: 0x7
				OneOf Prompt: "USB SS Physical Connector #2", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x588, VarStoreId: 0x1, VarOffset: 0x9BF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [7]
								Uint64 Value: 0x1
								Uint64 Value: 0x0
								Conditional 
							End 
						End 
					End 
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			OneOf Prompt: "USB SS Physical Connector #3", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x589, VarStoreId: 0x1, VarOffset: 0x9C0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "USB SS Physical Connector #4", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x58A, VarStoreId: 0x1, VarOffset: 0x9C1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
				OneOf Prompt: "USB SS Physical Connector #5", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x58B, VarStoreId: 0x1, VarOffset: 0x9C2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC51, Value: 0x1
					Not 
				End 
				OneOf Prompt: "USB SS Physical Connector #6", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x58C, VarStoreId: 0x1, VarOffset: 0x9C3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
				OneOf Prompt: "USB SS Physical Connector #7", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x58D, VarStoreId: 0x1, VarOffset: 0x9C4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
				OneOf Prompt: "USB SS Physical Connector #8", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x58E, VarStoreId: 0x1, VarOffset: 0x9C5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
				OneOf Prompt: "USB SS Physical Connector #9", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x58F, VarStoreId: 0x1, VarOffset: 0x9C6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "USB HS Physical Connector #0", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x590, VarStoreId: 0x1, VarOffset: 0x9AD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "USB HS Physical Connector #1", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x591, VarStoreId: 0x1, VarOffset: 0x9AE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "USB HS Physical Connector #2", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x592, VarStoreId: 0x1, VarOffset: 0x9AF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "USB HS Physical Connector #3", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x593, VarStoreId: 0x1, VarOffset: 0x9B0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "USB HS Physical Connector #4", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x594, VarStoreId: 0x1, VarOffset: 0x9B1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "USB HS Physical Connector #5", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x595, VarStoreId: 0x1, VarOffset: 0x9B2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
			OneOf Prompt: "USB HS Physical Connector #6", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x596, VarStoreId: 0x1, VarOffset: 0x9B3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
				OneOf Prompt: "USB HS Physical Connector #7", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x597, VarStoreId: 0x1, VarOffset: 0x9B4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					OneOfOption Option: "Disabled" Value: 0
				End 
			End 
			OneOf Prompt: "USB HS Physical Connector #8", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x598, VarStoreId: 0x1, VarOffset: 0x9B5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				OneOfOption Option: "Disabled" Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
				OneOf Prompt: "USB HS Physical Connector #9", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x599, VarStoreId: 0x1, VarOffset: 0x9B6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					OneOfOption Option: "Disabled" Value: 0
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC51, Value: 0x1
					Not 
				End 
				OneOf Prompt: "USB HS Physical Connector #10", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x59A, VarStoreId: 0x1, VarOffset: 0x9B7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
				OneOf Prompt: "USB HS Physical Connector #11", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x59B, VarStoreId: 0x1, VarOffset: 0x9B8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
				OneOf Prompt: "USB HS Physical Connector #12", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x59C, VarStoreId: 0x1, VarOffset: 0x9B9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
				OneOf Prompt: "USB HS Physical Connector #13", Help: "Enable/Disable this USB Physical Connector (physical port).  Once disabled, any USB devices plug into the connector will not be detected by BIOS or OS.", QuestionFlags: 0x10, QuestionId: 0x59D, VarStoreId: 0x1, VarOffset: 0x9BA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x545, Value: 0x2
				Not 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "USB Sensor Hub", Help: "USB Sensor Hub enable/disable", QuestionFlags: 0x10, QuestionId: 0x59E, VarStoreId: 0x1, VarOffset: 0x33, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
		End 
	End 
	Form FormId: 0x2757, Title: "SATA And RST Configuration"
		Subtitle Prompt: "SATA And RST Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "SATA Controller(s)", Help: "Enable/Disable SATA Device.", QuestionFlags: 0x10, QuestionId: 0x59F, VarStoreId: 0x1, VarOffset: 0x9CB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			OneOfOption Option: "Disabled" Value: 0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x59F, Value: 0x0
			OneOf Prompt: "SATA Mode Selection", Help: "Determines how SATA controller(s) operate.", QuestionFlags: 0x10, QuestionId: 0x5A0, VarStoreId: 0x1, VarOffset: 0x9CC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "AHCI" Value: 0, Default, MfgDefault
				SuppressIf 
					EqIdVal QuestionId: 0xC81, Value: 0x0
					OneOfOption Option: "RAID" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x5A0, Value: 0x1
					Not 
				End 
				GrayOutIf 
					EqIdVal QuestionId: 0xC80, Value: 0x63
					SuppressIf 
						EqIdVal QuestionId: 0xC7F, Value: 0x4
							Not 
							EqIdVal QuestionId: 0xC7F, Value: 0x2
							Not 
							And 
						End 
						GrayOutIf 
							EqIdVal QuestionId: 0x5A2, Value: 0x1
								EqIdVal QuestionId: 0xC7E, Value: 0x0
								Or 
							End 
							OneOf Prompt: "PCIe Storage Dev On Port 1", Help: "Enable/Disable RST Pcie Storage Remapping", QuestionFlags: 0x10, QuestionId: 0x5A1, VarStoreId: 0x1, VarOffset: 0xF9F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
								OneOfOption Option: "RST Controlled" Value: 1
								OneOfOption Option: "Not RST Controlled" Value: 0, Default, MfgDefault
							End 
						End 
					End 
					SuppressIf 
						EqIdVal QuestionId: 0xC7D, Value: 0x2
							Not 
						End 
						GrayOutIf 
							EqIdVal QuestionId: 0x5A1, Value: 0x1
								EqIdVal QuestionId: 0xC7C, Value: 0x0
								Or 
							End 
							OneOf Prompt: "PCIe Storage Dev On Port 3", Help: "Enable/Disable RST Pcie Storage Remapping", QuestionFlags: 0x10, QuestionId: 0x5A2, VarStoreId: 0x1, VarOffset: 0xFA1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
								OneOfOption Option: "RST Controlled" Value: 1
								OneOfOption Option: "Not RST Controlled" Value: 0, Default, MfgDefault
							End 
						End 
					End 
				End 
				GrayOutIf 
					EqIdVal QuestionId: 0xC7B, Value: 0x63
					SuppressIf 
						EqIdVal QuestionId: 0xC7A, Value: 0x4
							Not 
							EqIdVal QuestionId: 0xC7A, Value: 0x2
							Not 
							And 
						End 
						GrayOutIf 
							EqIdVal QuestionId: 0x5A4, Value: 0x1
								EqIdVal QuestionId: 0xC79, Value: 0x0
								Or 
							End 
							OneOf Prompt: "PCIe Storage Dev On Port 5", Help: "Enable/Disable RST Pcie Storage Remapping", QuestionFlags: 0x10, QuestionId: 0x5A3, VarStoreId: 0x1, VarOffset: 0xFA3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
								OneOfOption Option: "RST Controlled" Value: 1
								OneOfOption Option: "Not RST Controlled" Value: 0, Default, MfgDefault
							End 
						End 
					End 
					SuppressIf 
						EqIdVal QuestionId: 0xC78, Value: 0x2
							Not 
						End 
						GrayOutIf 
							EqIdVal QuestionId: 0x5A3, Value: 0x1
								EqIdVal QuestionId: 0xC77, Value: 0x0
								Or 
							End 
							OneOf Prompt: "PCIe Storage Dev On Port 7", Help: "Enable/Disable RST Pcie Storage Remapping", QuestionFlags: 0x10, QuestionId: 0x5A4, VarStoreId: 0x1, VarOffset: 0xFA5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
								OneOfOption Option: "RST Controlled" Value: 1
								OneOfOption Option: "Not RST Controlled" Value: 0, Default, MfgDefault
							End 
						End 
					End 
				End 
				GrayOutIf 
					EqIdVal QuestionId: 0xC76, Value: 0x63
					SuppressIf 
						EqIdVal QuestionId: 0xC75, Value: 0x4
							Not 
							EqIdVal QuestionId: 0xC75, Value: 0x2
							Not 
							And 
						End 
						GrayOutIf 
							EqIdVal QuestionId: 0x5A6, Value: 0x1
								EqIdVal QuestionId: 0xC74, Value: 0x0
								Or 
							End 
							OneOf Prompt: "PCIe Storage Dev On Port 9", Help: "Enable/Disable RST Pcie Storage Remapping", QuestionFlags: 0x10, QuestionId: 0x5A5, VarStoreId: 0x1, VarOffset: 0xFA7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
								OneOfOption Option: "RST Controlled" Value: 1
								OneOfOption Option: "Not RST Controlled" Value: 0, Default, MfgDefault
							End 
						End 
					End 
					SuppressIf 
						EqIdVal QuestionId: 0xC73, Value: 0x2
							Not 
						End 
						GrayOutIf 
							EqIdVal QuestionId: 0x5A5, Value: 0x1
								EqIdVal QuestionId: 0xC72, Value: 0x0
								Or 
							End 
							OneOf Prompt: "PCIe Storage Dev On Port 11", Help: "Enable/Disable RST Pcie Storage Remapping", QuestionFlags: 0x10, QuestionId: 0x5A6, VarStoreId: 0x1, VarOffset: 0xFA9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
								OneOfOption Option: "RST Controlled" Value: 1
								OneOfOption Option: "Not RST Controlled" Value: 0, Default, MfgDefault
							End 
						End 
					End 
				End 
				GrayOutIf 
					EqIdVal QuestionId: 0xC71, Value: 0x63
					SuppressIf 
						EqIdVal QuestionId: 0xC70, Value: 0x4
							Not 
							EqIdVal QuestionId: 0xC70, Value: 0x2
							Not 
							And 
						End 
						GrayOutIf 
							EqIdVal QuestionId: 0x5A8, Value: 0x1
								EqIdVal QuestionId: 0xC6F, Value: 0x0
								Or 
							End 
							OneOf Prompt: "PCIe Storage Dev On Port 13", Help: "Enable/Disable RST Pcie Storage Remapping", QuestionFlags: 0x10, QuestionId: 0x5A7, VarStoreId: 0x1, VarOffset: 0xFAB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
								OneOfOption Option: "RST Controlled" Value: 1
								OneOfOption Option: "Not RST Controlled" Value: 0, Default, MfgDefault
							End 
						End 
					End 
					SuppressIf 
						EqIdVal QuestionId: 0xC6E, Value: 0x2
							Not 
						End 
						GrayOutIf 
							EqIdVal QuestionId: 0x5A7, Value: 0x1
								EqIdVal QuestionId: 0xC6D, Value: 0x0
								Or 
							End 
							OneOf Prompt: "PCIe Storage Dev On Port 15", Help: "Enable/Disable RST Pcie Storage Remapping", QuestionFlags: 0x10, QuestionId: 0x5A8, VarStoreId: 0x1, VarOffset: 0xFAD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
								OneOfOption Option: "RST Controlled" Value: 1
								OneOfOption Option: "Not RST Controlled" Value: 0, Default, MfgDefault
							End 
						End 
					End 
				End 
				GrayOutIf 
					EqIdVal QuestionId: 0xC6C, Value: 0x63
					SuppressIf 
						EqIdVal QuestionId: 0xC6B, Value: 0x4
							Not 
							EqIdVal QuestionId: 0xC6B, Value: 0x2
							Not 
							And 
						End 
						GrayOutIf 
							EqIdVal QuestionId: 0x5AA, Value: 0x1
								EqIdVal QuestionId: 0xC6A, Value: 0x0
								Or 
							End 
							OneOf Prompt: "PCIe Storage Dev On Port 17", Help: "Enable/Disable RST Pcie Storage Remapping", QuestionFlags: 0x10, QuestionId: 0x5A9, VarStoreId: 0x1, VarOffset: 0xFAF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
								OneOfOption Option: "RST Controlled" Value: 1
								OneOfOption Option: "Not RST Controlled" Value: 0, Default, MfgDefault
							End 
						End 
					End 
					SuppressIf 
						EqIdVal QuestionId: 0xC69, Value: 0x2
							Not 
						End 
						GrayOutIf 
							EqIdVal QuestionId: 0x5A9, Value: 0x1
								EqIdVal QuestionId: 0xC68, Value: 0x0
								Or 
							End 
							OneOf Prompt: "PCIe Storage Dev On Port 19", Help: "Enable/Disable RST Pcie Storage Remapping", QuestionFlags: 0x10, QuestionId: 0x5AA, VarStoreId: 0x1, VarOffset: 0xFB1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
								OneOfOption Option: "RST Controlled" Value: 1
								OneOfOption Option: "Not RST Controlled" Value: 0, Default, MfgDefault
							End 
						End 
					End 
				End 
				GrayOutIf 
					EqIdVal QuestionId: 0xC67, Value: 0x63
					SuppressIf 
						EqIdVal QuestionId: 0xC66, Value: 0x4
							Not 
							EqIdVal QuestionId: 0xC66, Value: 0x2
							Not 
							And 
						End 
						GrayOutIf 
							EqIdVal QuestionId: 0x5AC, Value: 0x1
								EqIdVal QuestionId: 0xC65, Value: 0x0
								Or 
							End 
							OneOf Prompt: "PCIe Storage Dev On Port 21", Help: "Enable/Disable RST Pcie Storage Remapping", QuestionFlags: 0x10, QuestionId: 0x5AB, VarStoreId: 0x1, VarOffset: 0xFB3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
								OneOfOption Option: "RST Controlled" Value: 1
								OneOfOption Option: "Not RST Controlled" Value: 0, Default, MfgDefault
							End 
						End 
					End 
					SuppressIf 
						EqIdVal QuestionId: 0xC64, Value: 0x2
							Not 
						End 
						GrayOutIf 
							EqIdVal QuestionId: 0x5AB, Value: 0x1
								EqIdVal QuestionId: 0xC63, Value: 0x0
								Or 
							End 
							OneOf Prompt: "PCIe Storage Dev On Port 23", Help: "Enable/Disable RST Pcie Storage Remapping", QuestionFlags: 0x10, QuestionId: 0x5AC, VarStoreId: 0x1, VarOffset: 0xFB5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
								OneOfOption Option: "RST Controlled" Value: 1
								OneOfOption Option: "Not RST Controlled" Value: 0, Default, MfgDefault
							End 
						End 
					End 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC42, Value: 0x0
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Or 
				End 
				OneOf Prompt: "SATA Test Mode ", Help: "Test Mode Enable/Disable (Loop Back).", QuestionFlags: 0x10, QuestionId: 0x5AD, VarStoreId: 0x1, VarOffset: 0xA13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Enabled" Value: 1
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x5A0, Value: 0x1
					Not 
				End 
				OneOf Prompt: "RAID Device ID", Help: "Choose RAID Device ID", QuestionFlags: 0x10, QuestionId: 0x5AE, VarStoreId: 0x1, VarOffset: 0xFE9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Client" Value: 0, Default, MfgDefault
					OneOfOption Option: "Alternate" Value: 1
					SuppressIf 
						EqIdVal QuestionId: 0xC62, Value: 0x2
							Not 
						End 
						OneOfOption Option: "Server" Value: 2
					End 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x5AD, Value: 0x1
					EqIdVal QuestionId: 0x5A0, Value: 0x1
					Not 
					Or 
				End 
				Ref Prompt: "Software Feature Mask Configuration", Help: "RST Legacy OROM/RST UEFI driver will refer to the SWFM configuration to enable/disable the storage features.", QuestionFlags: 0x0, QuestionId: 0x5AF, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2758
				OneOf Prompt: "Aggressive LPM Support", Help: "Enable PCH to aggressively enter link power state.", QuestionFlags: 0x10, QuestionId: 0x5B0, VarStoreId: 0x1, VarOffset: 0xA12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			OneOf Prompt: "SATA Controller Speed", Help: "Indicates the maximum speed the SATA controller can support.", QuestionFlags: 0x10, QuestionId: 0x5B1, VarStoreId: 0x1, VarOffset: 0x98A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Text Prompt: "Serial ATA Port 0", Help: "", Text: "Empty"
			SuppressIf 
				EqIdVal QuestionId: 0xC42, Value: 0x0
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Or 
				End 
				Text Prompt: "  Software Preserve", Help: "", Text: "Unknown"
			End 
			SuppressIf 
				EqIdValList QuestionId: 0x5AD, Values: [1]
				OneOf Prompt: "  Port 0", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0x5B2, VarStoreId: 0x1, VarOffset: 0x9CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC61, Value: 0x1
				OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0x5B3, VarStoreId: 0x1, VarOffset: 0x9D5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 0
					OneOfOption Option: "Disabled" Value: 0, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported"
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC42, Value: 0x0
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Or 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x5B3, Value: 0x0
						EqIdVal QuestionId: 0xC60, Value: 0x0
						Or 
					End 
					OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0x5B4, VarStoreId: 0x1, VarOffset: 0x9DD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0
						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					End 
				End 
				OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0x5B5, VarStoreId: 0x1, VarOffset: 0x9E5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0x5B6, VarStoreId: 0x1, VarOffset: 0x9F5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault
					OneOfOption Option: "Solid State Drive" Value: 1
				End 
				OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x5B7, VarStoreId: 0x1, VarOffset: 0x9FD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [10, 26, 8, 70, 66, 67, 64, 65, 115, 116]
								EqIdValList QuestionId: 0xC50, Values: [20, 4, 5, 131]
								EqIdValList QuestionId: 0xC50, Values: [11, 27, 7, 19, 3]
								EqIdValList QuestionId: 0xC50, Values: [72, 69, 68, 80, 74]
								Uint64 Value: 0x0
								Uint64 Value: 0x4
								Conditional 
								Uint64 Value: 0x3
								Conditional 
								Uint64 Value: 0x2
								Conditional 
								Uint64 Value: 0x1
								Conditional 
							End 
						End 
					End 
					OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
					OneOfOption Option: "ISATA" Value: 1
					OneOfOption Option: "Direct Connect" Value: 2
					OneOfOption Option: "Flex" Value: 3
					OneOfOption Option: "M2" Value: 4
				End 
				OneOf Prompt: "  SATA Port 0 DevSlp", Help: "Enable/Disable SATA Port 0 DevSlp. Board rework for LP needed before enable.", QuestionFlags: 0x10, QuestionId: 0x5B8, VarStoreId: 0x1, VarOffset: 0xA14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0x5B9, VarStoreId: 0x1, VarOffset: 0xA1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				GrayOutIf 
					EqIdVal QuestionId: 0x5B9, Value: 0x0
					Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0x5BA, VarStoreId: 0x1, VarOffset: 0xA24, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0
						Default DefaultId: 0x0 Value: 625
					End 
					Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0x5BB, VarStoreId: 0x1, VarOffset: 0xA34, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
						Default DefaultId: 0x0 Value: 15
					End 
				End 
			End 
			Text Prompt: "Serial ATA Port 1", Help: "", Text: "Empty"
			SuppressIf 
				EqIdVal QuestionId: 0xC42, Value: 0x0
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Or 
				End 
				Text Prompt: "  Software Preserve", Help: "", Text: "Unknown"
			End 
			SuppressIf 
				EqIdValList QuestionId: 0x5AD, Values: [1]
				OneOf Prompt: "  Port 1", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0x5BC, VarStoreId: 0x1, VarOffset: 0x9CE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC5F, Value: 0x1
				OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0x5BD, VarStoreId: 0x1, VarOffset: 0x9D6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 0
					OneOfOption Option: "Disabled" Value: 0, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported"
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC42, Value: 0x0
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Or 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x5BD, Value: 0x0
						EqIdVal QuestionId: 0xC5E, Value: 0x0
						Or 
					End 
					OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0x5BE, VarStoreId: 0x1, VarOffset: 0x9DE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0
						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					End 
				End 
				OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0x5BF, VarStoreId: 0x1, VarOffset: 0x9E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0x5C0, VarStoreId: 0x1, VarOffset: 0x9F6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault
					OneOfOption Option: "Solid State Drive" Value: 1
				End 
				OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x5C1, VarStoreId: 0x1, VarOffset: 0x9FE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [72, 8, 10, 26, 69, 70, 66, 67, 68, 64, 65, 115, 116, 74]
								EqIdValList QuestionId: 0xC50, Values: [11, 12, 27, 7, 19, 3]
								EqIdValList QuestionId: 0xC50, Values: [20, 4, 5, 131, 32, 80]
								Uint64 Value: 0x0
								Uint64 Value: 0x4
								Conditional 
								Uint64 Value: 0x2
								Conditional 
								Uint64 Value: 0x1
								Conditional 
							End 
						End 
					End 
					OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
					OneOfOption Option: "ISATA" Value: 1
					OneOfOption Option: "Direct Connect" Value: 2
					OneOfOption Option: "Flex" Value: 3
					OneOfOption Option: "M2" Value: 4
				End 
				OneOf Prompt: "  SATA Port 1 DevSlp", Help: "Enable/Disable SATA Port 1 DevSlp. Board rework for LP needed before enable.", QuestionFlags: 0x10, QuestionId: 0x5C2, VarStoreId: 0x1, VarOffset: 0xA15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0x5C3, VarStoreId: 0x1, VarOffset: 0xA1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				GrayOutIf 
					EqIdVal QuestionId: 0x5C3, Value: 0x0
					Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0x5C4, VarStoreId: 0x1, VarOffset: 0xA26, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0
						Default DefaultId: 0x0 Value: 625
					End 
					Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0x5C5, VarStoreId: 0x1, VarOffset: 0xA35, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
						Default DefaultId: 0x0 Value: 15
					End 
				End 
			End 
			Text Prompt: "Serial ATA Port 2", Help: "", Text: "Empty"
			SuppressIf 
				EqIdVal QuestionId: 0xC42, Value: 0x0
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Or 
				End 
				Text Prompt: "  Software Preserve", Help: "", Text: "Unknown"
			End 
			SuppressIf 
				EqIdValList QuestionId: 0x5AD, Values: [1]
				OneOf Prompt: "  Port 2", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0x5C6, VarStoreId: 0x1, VarOffset: 0x9CF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC5D, Value: 0x1
				OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0x5C7, VarStoreId: 0x1, VarOffset: 0x9D7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 0
					OneOfOption Option: "Disabled" Value: 0, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported"
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC42, Value: 0x0
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Or 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x5C7, Value: 0x0
						EqIdVal QuestionId: 0xC5C, Value: 0x0
						Or 
					End 
					OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0x5C8, VarStoreId: 0x1, VarOffset: 0x9DF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0
						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					End 
				End 
				OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0x5C9, VarStoreId: 0x1, VarOffset: 0x9E7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0x5CA, VarStoreId: 0x1, VarOffset: 0x9F7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault
					OneOfOption Option: "Solid State Drive" Value: 1
				End 
				OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x5CB, VarStoreId: 0x1, VarOffset: 0x9FF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					Default DefaultId: 0x1 Value: Other
						Value 
							EqIdValList QuestionId: 0xC50, Values: [72, 69, 70, 66, 67, 68, 64, 65, 115, 116, 74]
								EqIdValList QuestionId: 0xC50, Values: [80]
								Uint64 Value: 0x0
								Uint64 Value: 0x4
								Conditional 
								Uint64 Value: 0x1
								Conditional 
							End 
						End 
					End 
					OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
					OneOfOption Option: "ISATA" Value: 1
					OneOfOption Option: "Direct Connect" Value: 2
					OneOfOption Option: "Flex" Value: 3
					OneOfOption Option: "M2" Value: 4
				End 
				OneOf Prompt: "  SATA Port 2 DevSlp", Help: "Enable/Disable SATA Port 2 DevSlp. Board rework for LP needed before enable.", QuestionFlags: 0x10, QuestionId: 0x5CC, VarStoreId: 0x1, VarOffset: 0xA16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0x5CD, VarStoreId: 0x1, VarOffset: 0xA1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				GrayOutIf 
					EqIdVal QuestionId: 0x5CD, Value: 0x0
					Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0x5CE, VarStoreId: 0x1, VarOffset: 0xA28, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0
						Default DefaultId: 0x0 Value: Other
							Value 
								Uint64 Value: 0x271
							End 
						End 
					End 
					Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0x5CF, VarStoreId: 0x1, VarOffset: 0xA36, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
						Default DefaultId: 0x0 Value: 15
					End 
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC51, Value: 0x1
					Not 
				End 
				Text Prompt: "Serial ATA Port 3", Help: "", Text: "Empty"
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					Text Prompt: "  Software Preserve", Help: "", Text: "Unknown"
				End 
				SuppressIf 
					EqIdValList QuestionId: 0x5AD, Values: [1]
					OneOf Prompt: "  Port 3", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0x5D0, VarStoreId: 0x1, VarOffset: 0x9D0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0
						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC5B, Value: 0x1
					OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0x5D1, VarStoreId: 0x1, VarOffset: 0x9D8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "Disabled" Value: 0, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					SuppressIf 
						EqIdVal QuestionId: 0xC42, Value: 0x0
							EqIdVal QuestionId: 0xC42, Value: 0x1
							Or 
						End 
						Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported"
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					SuppressIf 
						EqIdVal QuestionId: 0x5D1, Value: 0x0
							EqIdVal QuestionId: 0xC5A, Value: 0x0
							Or 
						End 
						OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0x5D2, VarStoreId: 0x1, VarOffset: 0x9E0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
							OneOfOption Option: "Disabled" Value: 0
							OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
						End 
					End 
					OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0x5D3, VarStoreId: 0x1, VarOffset: 0x9E8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0x5D4, VarStoreId: 0x1, VarOffset: 0x9F8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault
						OneOfOption Option: "Solid State Drive" Value: 1
					End 
					OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x5D5, VarStoreId: 0x1, VarOffset: 0xA00, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
						Default DefaultId: 0x1 Value: Other
							Value 
								EqIdValList QuestionId: 0xC50, Values: [70, 66, 67, 64, 65, 115, 116]
									EqIdValList QuestionId: 0xC50, Values: [72, 69, 68, 74]
									EqIdValList QuestionId: 0xC50, Values: [80]
									Uint64 Value: 0x0
									Uint64 Value: 0x4
									Conditional 
									Uint64 Value: 0x3
									Conditional 
									Uint64 Value: 0x1
									Conditional 
								End 
							End 
						End 
						OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
						OneOfOption Option: "ISATA" Value: 1
						OneOfOption Option: "Direct Connect" Value: 2
						OneOfOption Option: "Flex" Value: 3
						OneOfOption Option: "M2" Value: 4
					End 
					OneOf Prompt: "  SATA Port 3 DevSlp", Help: "Enable/Disable SATA Port 3 DevSlp.", QuestionFlags: 0x10, QuestionId: 0x5D6, VarStoreId: 0x1, VarOffset: 0xA17, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0x5D7, VarStoreId: 0x1, VarOffset: 0xA1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					GrayOutIf 
						EqIdVal QuestionId: 0x5D7, Value: 0x0
						Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0x5D8, VarStoreId: 0x1, VarOffset: 0xA2A, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0
							Default DefaultId: 0x0 Value: 625
						End 
						Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0x5D9, VarStoreId: 0x1, VarOffset: 0xA37, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
							Default DefaultId: 0x0 Value: 15
						End 
					End 
				End 
				Text Prompt: "Serial ATA Port 4", Help: "", Text: "Empty"
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					Text Prompt: "  Software Preserve", Help: "", Text: "Unknown"
				End 
				SuppressIf 
					EqIdValList QuestionId: 0x5AD, Values: [1]
					OneOf Prompt: "  Port 4", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0x5DA, VarStoreId: 0x1, VarOffset: 0x9D1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0
						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC59, Value: 0x1
					OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0x5DB, VarStoreId: 0x1, VarOffset: 0x9D9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "Disabled" Value: 0, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					SuppressIf 
						EqIdVal QuestionId: 0xC42, Value: 0x0
							EqIdVal QuestionId: 0xC42, Value: 0x1
							Or 
						End 
						Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported"
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					SuppressIf 
						EqIdVal QuestionId: 0x5DB, Value: 0x0
							EqIdVal QuestionId: 0xC58, Value: 0x0
							Or 
						End 
						OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0x5DC, VarStoreId: 0x1, VarOffset: 0x9E1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
							OneOfOption Option: "Disabled" Value: 0
							OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
						End 
					End 
					OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0x5DD, VarStoreId: 0x1, VarOffset: 0x9E9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0x5DE, VarStoreId: 0x1, VarOffset: 0x9F9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault
						OneOfOption Option: "Solid State Drive" Value: 1
					End 
					OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x5DF, VarStoreId: 0x1, VarOffset: 0xA01, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
						Default DefaultId: 0x1 Value: Other
							Value 
								EqIdValList QuestionId: 0xC50, Values: [72, 69, 70, 67, 68, 64, 74]
									EqIdValList QuestionId: 0xC50, Values: [80, 115, 116]
									Uint64 Value: 0x0
									Uint64 Value: 0x1
									Conditional 
									Uint64 Value: 0x4
									Conditional 
								End 
							End 
						End 
						OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
						OneOfOption Option: "ISATA" Value: 1
						OneOfOption Option: "Direct Connect" Value: 2
						OneOfOption Option: "Flex" Value: 3
						OneOfOption Option: "M2" Value: 4
					End 
					OneOf Prompt: "  SATA Port 4 DevSlp", Help: "Enable/Disable SATA Port 4 DevSlp.", QuestionFlags: 0x10, QuestionId: 0x5E0, VarStoreId: 0x1, VarOffset: 0xA18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0x5E1, VarStoreId: 0x1, VarOffset: 0xA20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					GrayOutIf 
						EqIdVal QuestionId: 0x5E1, Value: 0x0
						Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0x5E2, VarStoreId: 0x1, VarOffset: 0xA2C, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0
							Default DefaultId: 0x0 Value: 625
						End 
						Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0x5E3, VarStoreId: 0x1, VarOffset: 0xA38, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
							Default DefaultId: 0x0 Value: 15
						End 
					End 
				End 
				Text Prompt: "Serial ATA Port 5", Help: "", Text: "Empty"
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					Text Prompt: "  Software Preserve", Help: "", Text: "Unknown"
				End 
				SuppressIf 
					EqIdValList QuestionId: 0x5AD, Values: [1]
					OneOf Prompt: "  Port 5", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0x5E4, VarStoreId: 0x1, VarOffset: 0x9D2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0
						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC57, Value: 0x1
					OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0x5E5, VarStoreId: 0x1, VarOffset: 0x9DA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "Disabled" Value: 0, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					SuppressIf 
						EqIdVal QuestionId: 0xC42, Value: 0x0
							EqIdVal QuestionId: 0xC42, Value: 0x1
							Or 
						End 
						Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported"
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					SuppressIf 
						EqIdVal QuestionId: 0x5E5, Value: 0x0
							EqIdVal QuestionId: 0xC56, Value: 0x0
							Or 
						End 
						OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0x5E6, VarStoreId: 0x1, VarOffset: 0x9E2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
							OneOfOption Option: "Disabled" Value: 0
							OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
						End 
					End 
					OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0x5E7, VarStoreId: 0x1, VarOffset: 0x9EA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0x5E8, VarStoreId: 0x1, VarOffset: 0x9FA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault
						OneOfOption Option: "Solid State Drive" Value: 1
					End 
					OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x5E9, VarStoreId: 0x1, VarOffset: 0xA02, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
						Default DefaultId: 0x1 Value: Other
							Value 
								EqIdValList QuestionId: 0xC50, Values: [8, 10, 26, 11, 7, 19, 3, 12, 27]
									EqIdValList QuestionId: 0xC50, Values: [80, 115, 116]
									Uint64 Value: 0x0
									Uint64 Value: 0x1
									Conditional 
									Uint64 Value: 0x4
									Conditional 
								End 
							End 
						End 
						OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
						OneOfOption Option: "ISATA" Value: 1
						OneOfOption Option: "Direct Connect" Value: 2
						OneOfOption Option: "Flex" Value: 3
						OneOfOption Option: "M2" Value: 4
					End 
					OneOf Prompt: "  SATA Port 5 DevSlp", Help: "Enable/Disable SATA Port 5 DevSlp.", QuestionFlags: 0x10, QuestionId: 0x5EA, VarStoreId: 0x1, VarOffset: 0xA19, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0x5EB, VarStoreId: 0x1, VarOffset: 0xA21, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					GrayOutIf 
						EqIdVal QuestionId: 0x5EB, Value: 0x0
						Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0x5EC, VarStoreId: 0x1, VarOffset: 0xA2E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0
							Default DefaultId: 0x0 Value: 625
						End 
						Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0x5ED, VarStoreId: 0x1, VarOffset: 0xA39, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
							Default DefaultId: 0x0 Value: 15
						End 
					End 
				End 
				Text Prompt: "Serial ATA Port 6", Help: "", Text: "Empty"
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					Text Prompt: "  Software Preserve", Help: "", Text: "Unknown"
				End 
				SuppressIf 
					EqIdValList QuestionId: 0x5AD, Values: [1]
					OneOf Prompt: "  Port 6", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0x5EE, VarStoreId: 0x1, VarOffset: 0x9D3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x1 Value: Other
							Value 
								EqIdValList QuestionId: 0xC50, Values: [80]
									Uint64 Value: 0x1
									Uint64 Value: 0x0
									Conditional 
								End 
							End 
						End 
						OneOfOption Option: "Disabled" Value: 0
						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC55, Value: 0x1
					OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0x5EF, VarStoreId: 0x1, VarOffset: 0x9DB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "Disabled" Value: 0, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					SuppressIf 
						EqIdVal QuestionId: 0xC42, Value: 0x0
							EqIdVal QuestionId: 0xC42, Value: 0x1
							Or 
						End 
						Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported"
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					SuppressIf 
						EqIdVal QuestionId: 0x5EF, Value: 0x0
							EqIdVal QuestionId: 0xC54, Value: 0x0
							Or 
						End 
						OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0x5F0, VarStoreId: 0x1, VarOffset: 0x9E3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
							OneOfOption Option: "Disabled" Value: 0
							OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
						End 
					End 
					OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0x5F1, VarStoreId: 0x1, VarOffset: 0x9EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0x5F2, VarStoreId: 0x1, VarOffset: 0x9FB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault
						OneOfOption Option: "Solid State Drive" Value: 1
					End 
					OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x5F3, VarStoreId: 0x1, VarOffset: 0xA03, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
						OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
						OneOfOption Option: "ISATA" Value: 1
						OneOfOption Option: "Direct Connect" Value: 2
						OneOfOption Option: "Flex" Value: 3
						OneOfOption Option: "M2" Value: 4
					End 
					OneOf Prompt: "  SATA Port 6 DevSlp", Help: "Enable/Disable SATA Port 6 DevSlp.", QuestionFlags: 0x10, QuestionId: 0x5F4, VarStoreId: 0x1, VarOffset: 0xA1A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0x5F5, VarStoreId: 0x1, VarOffset: 0xA22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					GrayOutIf 
						EqIdVal QuestionId: 0x5F5, Value: 0x0
						Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0x5F6, VarStoreId: 0x1, VarOffset: 0xA30, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0
							Default DefaultId: 0x0 Value: 625
						End 
						Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0x5F7, VarStoreId: 0x1, VarOffset: 0xA3A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
							Default DefaultId: 0x0 Value: 15
						End 
					End 
				End 
				Text Prompt: "Serial ATA Port 7", Help: "", Text: "Empty"
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					Text Prompt: "  Software Preserve", Help: "", Text: "Unknown"
				End 
				SuppressIf 
					EqIdValList QuestionId: 0x5AD, Values: [1]
					OneOf Prompt: "  Port 7", Help: "Enable or Disable SATA Port", QuestionFlags: 0x10, QuestionId: 0x5F8, VarStoreId: 0x1, VarOffset: 0x9D4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x1 Value: Other
							Value 
								EqIdValList QuestionId: 0xC50, Values: [80]
									Uint64 Value: 0x1
									Uint64 Value: 0x0
									Conditional 
								End 
							End 
						End 
						OneOfOption Option: "Disabled" Value: 0
						OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC53, Value: 0x1
					OneOf Prompt: "  Hot Plug", Help: "Designates this port as Hot Pluggable.", QuestionFlags: 0x10, QuestionId: 0x5F9, VarStoreId: 0x1, VarOffset: 0x9DC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						Default DefaultId: 0x0 Value: 0
						OneOfOption Option: "Disabled" Value: 0, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					SuppressIf 
						EqIdVal QuestionId: 0xC42, Value: 0x0
							EqIdVal QuestionId: 0xC42, Value: 0x1
							Or 
						End 
						Text Prompt: "  Configured as eSATA", Help: "", Text: "Hot Plug supported"
					End 
				End 
				SuppressIf 
					EqIdVal QuestionId: 0xC42, Value: 0x0
						EqIdVal QuestionId: 0xC42, Value: 0x1
						Or 
					End 
					SuppressIf 
						EqIdVal QuestionId: 0x5F9, Value: 0x0
							EqIdVal QuestionId: 0xC52, Value: 0x0
							Or 
						End 
						OneOf Prompt: "  Mechanical Presence Switch", Help: "Controls reporting if this port has an Mechanical Presence Switch.

Note: Requires hardware support.", QuestionFlags: 0x10, QuestionId: 0x5FA, VarStoreId: 0x1, VarOffset: 0x9E4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
							OneOfOption Option: "Disabled" Value: 0
							OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
						End 
					End 
					OneOf Prompt: "  Spin Up Device", Help: "If enabled for any of ports Staggerred Spin Up will be performed and only the drives which have this option enabled will spin up at boot. Otherwise all drives spin up at boot.", QuestionFlags: 0x10, QuestionId: 0x5FB, VarStoreId: 0x1, VarOffset: 0x9EC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					OneOf Prompt: "  SATA Device Type", Help: "Identify the SATA port is connected to Solid State Drive or Hard Disk Drive", QuestionFlags: 0x10, QuestionId: 0x5FC, VarStoreId: 0x1, VarOffset: 0x9FC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Hard Disk Drive" Value: 0, Default, MfgDefault
						OneOfOption Option: "Solid State Drive" Value: 1
					End 
					OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x5FD, VarStoreId: 0x1, VarOffset: 0xA04, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
						OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
						OneOfOption Option: "ISATA" Value: 1
						OneOfOption Option: "Direct Connect" Value: 2
						OneOfOption Option: "Flex" Value: 3
						OneOfOption Option: "M2" Value: 4
					End 
					OneOf Prompt: "  SATA Port 7 DevSlp", Help: "Enable/Disable SATA Port 7 DevSlp.", QuestionFlags: 0x10, QuestionId: 0x5FE, VarStoreId: 0x1, VarOffset: 0xA1B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					OneOf Prompt: "  DITO Configuration", Help: "Enable/Disable DITO Configuration", QuestionFlags: 0x10, QuestionId: 0x5FF, VarStoreId: 0x1, VarOffset: 0xA23, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
						OneOfOption Option: "Enabled" Value: 1
					End 
					GrayOutIf 
						EqIdVal QuestionId: 0x5FF, Value: 0x0
						Numeric Prompt: "  DITO Value", Help: "DITO Value", QuestionFlags: 0x10, QuestionId: 0x600, VarStoreId: 0x1, VarOffset: 0xA32, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x0
							Default DefaultId: 0x0 Value: 625
						End 
						Numeric Prompt: "  DM Value", Help: "DM Value", QuestionFlags: 0x10, QuestionId: 0x601, VarStoreId: 0x1, VarOffset: 0xA3B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
							Default DefaultId: 0x0 Value: 15
						End 
					End 
				End 
			End 
		End 
	End 
	Form FormId: 0x2758, Title: "Software Feature Mask Configuration"
		Subtitle Prompt: "Software Feature Mask Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "HDD Unlock", Help: "If enabled, indicates that the HDD password unlock in the OS is enabled.", QuestionFlags: 0x10, QuestionId: 0x602, VarStoreId: 0x1, VarOffset: 0xA0B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		OneOf Prompt: "LED Locate", Help: "If enabled, indicates that the LED/SGPIO hardware is attached and ping to locate feature is enabled on the OS.", QuestionFlags: 0x10, QuestionId: 0x603, VarStoreId: 0x1, VarOffset: 0xA0C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x5A0, Value: 0x1
				Not 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x2829, Value: 0x0
				OneOf Prompt: "Use RST Legacy OROM", Help: "Use RST Legacy OROM when CSM is Enabled.", QuestionFlags: 0x10, QuestionId: 0x604, VarStoreId: 0x1, VarOffset: 0xA3C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			OneOf Prompt: "RAID0", Help: "Enable/Disable RAID0 feature.", QuestionFlags: 0x10, QuestionId: 0x605, VarStoreId: 0x1, VarOffset: 0xA05, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "RAID1", Help: "Enable/Disable RAID1 feature.", QuestionFlags: 0x10, QuestionId: 0x606, VarStoreId: 0x1, VarOffset: 0xA06, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "RAID10", Help: "Enable/Disable RAID10 feature.", QuestionFlags: 0x10, QuestionId: 0x607, VarStoreId: 0x1, VarOffset: 0xA07, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "RAID5", Help: "Enable/Disable RAID5 feature.", QuestionFlags: 0x10, QuestionId: 0x608, VarStoreId: 0x1, VarOffset: 0xA08, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "Intel Rapid Recovery Technology", Help: "Enable/Disable Intel Rapid Recovery Technology.", QuestionFlags: 0x10, QuestionId: 0x609, VarStoreId: 0x1, VarOffset: 0xA09, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "OROM UI and BANNER", Help: "If enabled, then the OROM UI is shown. Otherwise, no OROM banner or information will be displayed if all disks and RAID volumes are Normal.", QuestionFlags: 0x10, QuestionId: 0x60A, VarStoreId: 0x1, VarOffset: 0xA0A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "IRRT Only on eSATA", Help: "If enabled, then only IRRT volumes can span internal and eSATA drives. If disabled, then any RAID volume can span internal and eSATA drives.", QuestionFlags: 0x10, QuestionId: 0x60B, VarStoreId: 0x1, VarOffset: 0xA0D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "Smart Response Technology", Help: "Enabled/Disable Smart Response Technology feature", QuestionFlags: 0x10, QuestionId: 0x60C, VarStoreId: 0x1, VarOffset: 0xA0E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "OROM UI Normal Delay", Help: "Select the delay time of the OROM UI Splash Screen in a normal status", QuestionFlags: 0x10, QuestionId: 0x60D, VarStoreId: 0x1, VarOffset: 0xA0F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "2 secs" Value: 0, Default, MfgDefault
				OneOfOption Option: "4 secs" Value: 1
				OneOfOption Option: "6 secs" Value: 2
				OneOfOption Option: "8 secs" Value: 3
			End 
			OneOf Prompt: "RST Force Form", Help: "Enable/Disable Form for Intel Rapid Storage Technology.", QuestionFlags: 0x10, QuestionId: 0x60E, VarStoreId: 0x1, VarOffset: 0xA10, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "System Acceleration with Intel(R) Optane(TM) Memory", Help: "Enable/Disable System Acceleration with Intel(R) Optane(TM) Memory feature.", QuestionFlags: 0x10, QuestionId: 0x60F, VarStoreId: 0x1, VarOffset: 0xFEA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "CPU attached storage", Help: "Enable/Disable RST CPU attached storage feature", QuestionFlags: 0x10, QuestionId: 0x610, VarStoreId: 0x1, VarOffset: 0xFEB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
		End 
	End 
	Form FormId: 0x2759, Title: "PCI Express Gen3 Eq Lanes"
		Numeric Prompt: "PCIE1  Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x611, VarStoreId: 0x1, VarOffset: 0xC41, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE1  Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x612, VarStoreId: 0x1, VarOffset: 0xC59, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE2  Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x613, VarStoreId: 0x1, VarOffset: 0xC42, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE2  Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x614, VarStoreId: 0x1, VarOffset: 0xC5A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE3  Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x615, VarStoreId: 0x1, VarOffset: 0xC43, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE3  Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x616, VarStoreId: 0x1, VarOffset: 0xC5B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE4  Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x617, VarStoreId: 0x1, VarOffset: 0xC44, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE4  Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x618, VarStoreId: 0x1, VarOffset: 0xC5C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE5  Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x619, VarStoreId: 0x1, VarOffset: 0xC45, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE5  Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x61A, VarStoreId: 0x1, VarOffset: 0xC5D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE6  Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x61B, VarStoreId: 0x1, VarOffset: 0xC46, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE6  Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x61C, VarStoreId: 0x1, VarOffset: 0xC5E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE7  Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x61D, VarStoreId: 0x1, VarOffset: 0xC47, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE7  Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x61E, VarStoreId: 0x1, VarOffset: 0xC5F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE8  Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x61F, VarStoreId: 0x1, VarOffset: 0xC48, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE8  Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x620, VarStoreId: 0x1, VarOffset: 0xC60, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE9  Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x621, VarStoreId: 0x1, VarOffset: 0xC49, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE9  Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x622, VarStoreId: 0x1, VarOffset: 0xC61, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE10 Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x623, VarStoreId: 0x1, VarOffset: 0xC4A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE10 Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x624, VarStoreId: 0x1, VarOffset: 0xC62, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE11 Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x625, VarStoreId: 0x1, VarOffset: 0xC4B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE11 Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x626, VarStoreId: 0x1, VarOffset: 0xC63, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE12 Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x627, VarStoreId: 0x1, VarOffset: 0xC4C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE12 Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x628, VarStoreId: 0x1, VarOffset: 0xC64, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE13 Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x629, VarStoreId: 0x1, VarOffset: 0xC4D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE13 Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x62A, VarStoreId: 0x1, VarOffset: 0xC65, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE14 Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x62B, VarStoreId: 0x1, VarOffset: 0xC4E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE14 Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x62C, VarStoreId: 0x1, VarOffset: 0xC66, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE15 Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x62D, VarStoreId: 0x1, VarOffset: 0xC4F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE15 Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x62E, VarStoreId: 0x1, VarOffset: 0xC67, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE16 Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x62F, VarStoreId: 0x1, VarOffset: 0xC50, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE16 Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x630, VarStoreId: 0x1, VarOffset: 0xC68, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE17 Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x631, VarStoreId: 0x1, VarOffset: 0xC51, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE17 Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x632, VarStoreId: 0x1, VarOffset: 0xC69, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE18 Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x633, VarStoreId: 0x1, VarOffset: 0xC52, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE18 Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x634, VarStoreId: 0x1, VarOffset: 0xC6A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE19 Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x635, VarStoreId: 0x1, VarOffset: 0xC53, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE19 Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x636, VarStoreId: 0x1, VarOffset: 0xC6B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Numeric Prompt: "PCIE20 Cm", Help: "", QuestionFlags: 0x0, QuestionId: 0x637, VarStoreId: 0x1, VarOffset: 0xC54, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		Numeric Prompt: "PCIE20 Cp", Help: "", QuestionFlags: 0x0, QuestionId: 0x638, VarStoreId: 0x1, VarOffset: 0xC6C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
			Default DefaultId: 0x0 Value: 2
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Override SW EQ settings", Help: "", QuestionFlags: 0x10, QuestionId: 0x639, VarStoreId: 0x1, VarOffset: 0xC8A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [7, 19]
						Uint64 Value: 0x0
						Uint64 Value: 0x1
						Conditional 
					End 
				End 
			End 
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x639, Value: 0x0
			Numeric Prompt: "Coeff0 Cm", Help: "", QuestionFlags: 0x10, QuestionId: 0x63A, VarStoreId: 0x1, VarOffset: 0xC8B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 6
			End 
			Numeric Prompt: "Coeff0 Cp", Help: "", QuestionFlags: 0x10, QuestionId: 0x63B, VarStoreId: 0x1, VarOffset: 0xC90, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 2
			End 
			Numeric Prompt: "Coeff1 Cm", Help: "", QuestionFlags: 0x10, QuestionId: 0x63C, VarStoreId: 0x1, VarOffset: 0xC8C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 4
			End 
			Numeric Prompt: "Coeff1 Cp", Help: "", QuestionFlags: 0x10, QuestionId: 0x63D, VarStoreId: 0x1, VarOffset: 0xC91, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 2
			End 
			Numeric Prompt: "Coeff2 Cm", Help: "", QuestionFlags: 0x10, QuestionId: 0x63E, VarStoreId: 0x1, VarOffset: 0xC8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 8
			End 
			Numeric Prompt: "Coeff2 Cp", Help: "", QuestionFlags: 0x10, QuestionId: 0x63F, VarStoreId: 0x1, VarOffset: 0xC92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 2
			End 
			Numeric Prompt: "Coeff3 Cm", Help: "", QuestionFlags: 0x10, QuestionId: 0x640, VarStoreId: 0x1, VarOffset: 0xC8E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 2
			End 
			Numeric Prompt: "Coeff3 Cp", Help: "", QuestionFlags: 0x10, QuestionId: 0x641, VarStoreId: 0x1, VarOffset: 0xC93, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 2
			End 
			Numeric Prompt: "Coeff4 Cm", Help: "", QuestionFlags: 0x10, QuestionId: 0x642, VarStoreId: 0x1, VarOffset: 0xC8F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 10
			End 
			Numeric Prompt: "Coeff4 Cp", Help: "", QuestionFlags: 0x10, QuestionId: 0x643, VarStoreId: 0x1, VarOffset: 0xC94, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3F, Step: 0x1
				Default DefaultId: 0x0 Value: 2
			End 
		End 
	End 
	Form FormId: 0x275A, Title: "PCI Express Root Port 1"
		OneOf Prompt: "PCI Express Root Port 1", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x644, VarStoreId: 0x1, VarOffset: 0xA49, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x644, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x645, VarStoreId: 0x1, VarOffset: 0xC71, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [20, 4, 5, 131]
							Uint64 Value: 0x0
							Uint64 Value: 0x2
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x646, VarStoreId: 0x1, VarOffset: 0xA61, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Auto" Value: 4
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x647, VarStoreId: 0x1, VarOffset: 0xBC9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x648, VarStoreId: 0x1, VarOffset: 0xBF9, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [7, 19]
							Uint64 Value: 0x2
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x649, VarStoreId: 0x1, VarOffset: 0xC11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x64A, VarStoreId: 0x1, VarOffset: 0xC29, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [7, 19]
							Uint64 Value: 0x7
							Uint64 Value: 0x5
							Conditional 
						End 
					End 
				End 
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x64B, VarStoreId: 0x1, VarOffset: 0xBE1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x64C, VarStoreId: 0x1, VarOffset: 0xA79, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x64D, VarStoreId: 0x1, VarOffset: 0xA91, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x64E, VarStoreId: 0x1, VarOffset: 0xAA9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x64F, VarStoreId: 0x1, VarOffset: 0xAC1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x650, VarStoreId: 0x1, VarOffset: 0xAD9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x651, VarStoreId: 0x1, VarOffset: 0xB09, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x652, VarStoreId: 0x1, VarOffset: 0xB21, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x653, VarStoreId: 0x1, VarOffset: 0xB39, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x654, VarStoreId: 0x1, VarOffset: 0xB51, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x655, VarStoreId: 0x1, VarOffset: 0xB69, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x656, VarStoreId: 0x1, VarOffset: 0xB81, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x657, VarStoreId: 0x1, VarOffset: 0xB99, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x658, VarStoreId: 0x1, VarOffset: 0xBB1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x659, VarStoreId: 0x1, VarOffset: 0xFB8, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x65A, VarStoreId: 0x1, VarOffset: 0xDCE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x65B, VarStoreId: 0x1, VarOffset: 0xDE6, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x65C, VarStoreId: 0x1, VarOffset: 0xE16, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE1 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x65D, VarStoreId: 0x1, VarOffset: 0xC95, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x65D, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x65E, VarStoreId: 0x1, VarOffset: 0xCC5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x65E, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x65F, VarStoreId: 0x1, VarOffset: 0xD25, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x660, VarStoreId: 0x1, VarOffset: 0xCDD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x661, VarStoreId: 0x1, VarOffset: 0xCF5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x661, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x662, VarStoreId: 0x1, VarOffset: 0xD55, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x663, VarStoreId: 0x1, VarOffset: 0xD0D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x664, VarStoreId: 0x1, VarOffset: 0xD85, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE1 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x665, VarStoreId: 0x1, VarOffset: 0xCAD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE1 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x666, VarStoreId: 0x1, VarOffset: 0xD9D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0
				OneOfOption Option: "No CLKREQ" Value: 1, Default, MfgDefault
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x666, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x667, VarStoreId: 0x1, VarOffset: 0xDB5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x668, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27E3
		End 
	End 
	Form FormId: 0x275B, Title: "PCI Express Root Port 2"
		OneOf Prompt: "PCI Express Root Port 2", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x669, VarStoreId: 0x1, VarOffset: 0xA4A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x669, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x66A, VarStoreId: 0x1, VarOffset: 0xC72, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x66B, VarStoreId: 0x1, VarOffset: 0xA62, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Auto" Value: 4
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x66C, VarStoreId: 0x1, VarOffset: 0xBCA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x66D, VarStoreId: 0x1, VarOffset: 0xBFA, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x66E, VarStoreId: 0x1, VarOffset: 0xC12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x66F, VarStoreId: 0x1, VarOffset: 0xC2A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x670, VarStoreId: 0x1, VarOffset: 0xBE2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x671, VarStoreId: 0x1, VarOffset: 0xA7A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x672, VarStoreId: 0x1, VarOffset: 0xA92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x673, VarStoreId: 0x1, VarOffset: 0xAAA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x674, VarStoreId: 0x1, VarOffset: 0xAC2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x675, VarStoreId: 0x1, VarOffset: 0xADA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x676, VarStoreId: 0x1, VarOffset: 0xB0A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x677, VarStoreId: 0x1, VarOffset: 0xB22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x678, VarStoreId: 0x1, VarOffset: 0xB3A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x679, VarStoreId: 0x1, VarOffset: 0xB52, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x67A, VarStoreId: 0x1, VarOffset: 0xB6A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x67B, VarStoreId: 0x1, VarOffset: 0xB82, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x67C, VarStoreId: 0x1, VarOffset: 0xB9A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x67D, VarStoreId: 0x1, VarOffset: 0xBB2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x67E, VarStoreId: 0x1, VarOffset: 0xFBA, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x2
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x67F, VarStoreId: 0x1, VarOffset: 0xDCF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x680, VarStoreId: 0x1, VarOffset: 0xDE8, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x681, VarStoreId: 0x1, VarOffset: 0xE17, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE2 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x682, VarStoreId: 0x1, VarOffset: 0xC96, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x682, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x683, VarStoreId: 0x1, VarOffset: 0xCC6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x683, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x684, VarStoreId: 0x1, VarOffset: 0xD27, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x685, VarStoreId: 0x1, VarOffset: 0xCDE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x686, VarStoreId: 0x1, VarOffset: 0xCF6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x686, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x687, VarStoreId: 0x1, VarOffset: 0xD57, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x688, VarStoreId: 0x1, VarOffset: 0xD0E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x689, VarStoreId: 0x1, VarOffset: 0xD86, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE2 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x68A, VarStoreId: 0x1, VarOffset: 0xCAE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE2 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x68B, VarStoreId: 0x1, VarOffset: 0xD9E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0
				OneOfOption Option: "No CLKREQ" Value: 1, Default, MfgDefault
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x68B, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x68C, VarStoreId: 0x1, VarOffset: 0xDB6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x68D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27E4
		End 
	End 
	Form FormId: 0x275C, Title: "PCI Express Root Port 3"
		OneOf Prompt: "PCI Express Root Port 3", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x68E, VarStoreId: 0x1, VarOffset: 0xA4B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x68E, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x68F, VarStoreId: 0x1, VarOffset: 0xC73, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [12, 8, 10, 26, 7, 19, 3, 11, 27]
							Uint64 Value: 0x0
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x690, VarStoreId: 0x1, VarOffset: 0xA63, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Auto" Value: 4
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x691, VarStoreId: 0x1, VarOffset: 0xBCB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x692, VarStoreId: 0x1, VarOffset: 0xBFB, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x693, VarStoreId: 0x1, VarOffset: 0xC13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x694, VarStoreId: 0x1, VarOffset: 0xC2B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x695, VarStoreId: 0x1, VarOffset: 0xBE3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x696, VarStoreId: 0x1, VarOffset: 0xA7B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x697, VarStoreId: 0x1, VarOffset: 0xA93, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x698, VarStoreId: 0x1, VarOffset: 0xAAB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x699, VarStoreId: 0x1, VarOffset: 0xAC3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x69A, VarStoreId: 0x1, VarOffset: 0xADB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x69B, VarStoreId: 0x1, VarOffset: 0xB0B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x69C, VarStoreId: 0x1, VarOffset: 0xB23, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x69D, VarStoreId: 0x1, VarOffset: 0xB3B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x69E, VarStoreId: 0x1, VarOffset: 0xB53, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x69F, VarStoreId: 0x1, VarOffset: 0xB6B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6A0, VarStoreId: 0x1, VarOffset: 0xB83, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x6A1, VarStoreId: 0x1, VarOffset: 0xB9B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6A2, VarStoreId: 0x1, VarOffset: 0xBB3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x6A3, VarStoreId: 0x1, VarOffset: 0xFBC, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x3
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x6A4, VarStoreId: 0x1, VarOffset: 0xDD0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x6A5, VarStoreId: 0x1, VarOffset: 0xDEA, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x6A6, VarStoreId: 0x1, VarOffset: 0xE18, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE3 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x6A7, VarStoreId: 0x1, VarOffset: 0xC97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x6A7, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x6A8, VarStoreId: 0x1, VarOffset: 0xCC7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x6A8, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x6A9, VarStoreId: 0x1, VarOffset: 0xD29, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x6AA, VarStoreId: 0x1, VarOffset: 0xCDF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x6AB, VarStoreId: 0x1, VarOffset: 0xCF7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x6AB, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x6AC, VarStoreId: 0x1, VarOffset: 0xD59, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x6AD, VarStoreId: 0x1, VarOffset: 0xD0F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x6AE, VarStoreId: 0x1, VarOffset: 0xD87, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE3 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x6AF, VarStoreId: 0x1, VarOffset: 0xCAF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE3 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x6B0, VarStoreId: 0x1, VarOffset: 0xD9F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0
				OneOfOption Option: "No CLKREQ" Value: 1, Default, MfgDefault
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x6B0, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x6B1, VarStoreId: 0x1, VarOffset: 0xDB7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x6B2, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27E5
		End 
	End 
	Form FormId: 0x275D, Title: "PCI Express Root Port 4"
		OneOf Prompt: "PCI Express Root Port 4", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x6B3, VarStoreId: 0x1, VarOffset: 0xA4C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x6B3, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x6B4, VarStoreId: 0x1, VarOffset: 0xC74, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [8, 10, 26, 11, 7, 19, 3, 12, 27]
							Uint64 Value: 0x0
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x6B5, VarStoreId: 0x1, VarOffset: 0xA64, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Auto" Value: 4
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x6B6, VarStoreId: 0x1, VarOffset: 0xBCC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x6B7, VarStoreId: 0x1, VarOffset: 0xBFC, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x6B8, VarStoreId: 0x1, VarOffset: 0xC14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x6B9, VarStoreId: 0x1, VarOffset: 0xC2C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x6BA, VarStoreId: 0x1, VarOffset: 0xBE4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6BB, VarStoreId: 0x1, VarOffset: 0xA7C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6BC, VarStoreId: 0x1, VarOffset: 0xA94, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6BD, VarStoreId: 0x1, VarOffset: 0xAAC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6BE, VarStoreId: 0x1, VarOffset: 0xAC4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6BF, VarStoreId: 0x1, VarOffset: 0xADC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6C0, VarStoreId: 0x1, VarOffset: 0xB0C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6C1, VarStoreId: 0x1, VarOffset: 0xB24, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6C2, VarStoreId: 0x1, VarOffset: 0xB3C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6C3, VarStoreId: 0x1, VarOffset: 0xB54, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6C4, VarStoreId: 0x1, VarOffset: 0xB6C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6C5, VarStoreId: 0x1, VarOffset: 0xB84, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x6C6, VarStoreId: 0x1, VarOffset: 0xB9C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6C7, VarStoreId: 0x1, VarOffset: 0xBB4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x6C8, VarStoreId: 0x1, VarOffset: 0xFBE, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x4
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x6C9, VarStoreId: 0x1, VarOffset: 0xDD1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x6CA, VarStoreId: 0x1, VarOffset: 0xDEC, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x6CB, VarStoreId: 0x1, VarOffset: 0xE19, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE4 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x6CC, VarStoreId: 0x1, VarOffset: 0xC98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x6CC, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x6CD, VarStoreId: 0x1, VarOffset: 0xCC8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x6CD, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x6CE, VarStoreId: 0x1, VarOffset: 0xD2B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x6CF, VarStoreId: 0x1, VarOffset: 0xCE0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x6D0, VarStoreId: 0x1, VarOffset: 0xCF8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x6D0, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x6D1, VarStoreId: 0x1, VarOffset: 0xD5B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x6D2, VarStoreId: 0x1, VarOffset: 0xD10, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x6D3, VarStoreId: 0x1, VarOffset: 0xD88, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE4 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x6D4, VarStoreId: 0x1, VarOffset: 0xCB0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE4 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x6D5, VarStoreId: 0x1, VarOffset: 0xDA0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0
				OneOfOption Option: "No CLKREQ" Value: 1, Default, MfgDefault
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x6D5, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x6D6, VarStoreId: 0x1, VarOffset: 0xDB8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x6D7, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27E6
		End 
	End 
	Form FormId: 0x275E, Title: "PCI Express Root Port 5"
		OneOf Prompt: "PCI Express Root Port 5", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x6D8, VarStoreId: 0x1, VarOffset: 0xA4D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			OneOfOption Option: "Disabled" Value: 0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x6D8, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x6D9, VarStoreId: 0x1, VarOffset: 0xC75, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x6DA, VarStoreId: 0x1, VarOffset: 0xA65, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Auto" Value: 4
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x6DB, VarStoreId: 0x1, VarOffset: 0xBCD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x6DC, VarStoreId: 0x1, VarOffset: 0xBFD, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x6DD, VarStoreId: 0x1, VarOffset: 0xC15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x6DE, VarStoreId: 0x1, VarOffset: 0xC2D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x6DF, VarStoreId: 0x1, VarOffset: 0xBE5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6E0, VarStoreId: 0x1, VarOffset: 0xA7D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6E1, VarStoreId: 0x1, VarOffset: 0xA95, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6E2, VarStoreId: 0x1, VarOffset: 0xAAD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6E3, VarStoreId: 0x1, VarOffset: 0xAC5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6E4, VarStoreId: 0x1, VarOffset: 0xADD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6E5, VarStoreId: 0x1, VarOffset: 0xB0D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6E6, VarStoreId: 0x1, VarOffset: 0xB25, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6E7, VarStoreId: 0x1, VarOffset: 0xB3D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6E8, VarStoreId: 0x1, VarOffset: 0xB55, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6E9, VarStoreId: 0x1, VarOffset: 0xB6D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6EA, VarStoreId: 0x1, VarOffset: 0xB85, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x6EB, VarStoreId: 0x1, VarOffset: 0xB9D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x6EC, VarStoreId: 0x1, VarOffset: 0xBB5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x6ED, VarStoreId: 0x1, VarOffset: 0xFC0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x5
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x6EE, VarStoreId: 0x1, VarOffset: 0xDD2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x6EF, VarStoreId: 0x1, VarOffset: 0xDEE, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x6F0, VarStoreId: 0x1, VarOffset: 0xE1A, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE5 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x6F1, VarStoreId: 0x1, VarOffset: 0xC99, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x6F1, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x6F2, VarStoreId: 0x1, VarOffset: 0xCC9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x6F2, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x6F3, VarStoreId: 0x1, VarOffset: 0xD2D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x6F4, VarStoreId: 0x1, VarOffset: 0xCE1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x6F5, VarStoreId: 0x1, VarOffset: 0xCF9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x6F5, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x6F6, VarStoreId: 0x1, VarOffset: 0xD5D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x6F7, VarStoreId: 0x1, VarOffset: 0xD11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x6F8, VarStoreId: 0x1, VarOffset: 0xD89, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE5 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x6F9, VarStoreId: 0x1, VarOffset: 0xCB1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE5 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x6FA, VarStoreId: 0x1, VarOffset: 0xDA1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0
				OneOfOption Option: "No CLKREQ" Value: 1, Default, MfgDefault
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x6FA, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x6FB, VarStoreId: 0x1, VarOffset: 0xDB9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x6FC, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27E7
		End 
	End 
	Form FormId: 0x275F, Title: "PCI Express Root Port 6"
		OneOf Prompt: "PCI Express Root Port 6", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x6FD, VarStoreId: 0x1, VarOffset: 0xA4E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x6FD, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x6FE, VarStoreId: 0x1, VarOffset: 0xC76, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [20, 4, 5, 131]
							Uint64 Value: 0x0
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x6FF, VarStoreId: 0x1, VarOffset: 0xA66, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x700, VarStoreId: 0x1, VarOffset: 0xBCE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x701, VarStoreId: 0x1, VarOffset: 0xBFE, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x702, VarStoreId: 0x1, VarOffset: 0xC16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x703, VarStoreId: 0x1, VarOffset: 0xC2E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x704, VarStoreId: 0x1, VarOffset: 0xBE6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x705, VarStoreId: 0x1, VarOffset: 0xA7E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x706, VarStoreId: 0x1, VarOffset: 0xA96, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x707, VarStoreId: 0x1, VarOffset: 0xAAE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x708, VarStoreId: 0x1, VarOffset: 0xAC6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x709, VarStoreId: 0x1, VarOffset: 0xADE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x70A, VarStoreId: 0x1, VarOffset: 0xB0E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x70B, VarStoreId: 0x1, VarOffset: 0xB26, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x70C, VarStoreId: 0x1, VarOffset: 0xB3E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x70D, VarStoreId: 0x1, VarOffset: 0xB56, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x70E, VarStoreId: 0x1, VarOffset: 0xB6E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x70F, VarStoreId: 0x1, VarOffset: 0xB86, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x710, VarStoreId: 0x1, VarOffset: 0xB9E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x711, VarStoreId: 0x1, VarOffset: 0xBB6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x712, VarStoreId: 0x1, VarOffset: 0xFC2, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x6
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x713, VarStoreId: 0x1, VarOffset: 0xDD3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x714, VarStoreId: 0x1, VarOffset: 0xDF0, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x715, VarStoreId: 0x1, VarOffset: 0xE1B, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE6 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x716, VarStoreId: 0x1, VarOffset: 0xC9A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x716, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x717, VarStoreId: 0x1, VarOffset: 0xCCA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x717, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x718, VarStoreId: 0x1, VarOffset: 0xD2F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x719, VarStoreId: 0x1, VarOffset: 0xCE2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x71A, VarStoreId: 0x1, VarOffset: 0xCFA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x71A, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x71B, VarStoreId: 0x1, VarOffset: 0xD5F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x71C, VarStoreId: 0x1, VarOffset: 0xD12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x71D, VarStoreId: 0x1, VarOffset: 0xD8A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE6 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x71E, VarStoreId: 0x1, VarOffset: 0xCB2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE6 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x71F, VarStoreId: 0x1, VarOffset: 0xDA2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0
				OneOfOption Option: "No CLKREQ" Value: 1, Default, MfgDefault
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x71F, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x720, VarStoreId: 0x1, VarOffset: 0xDBA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x721, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27E8
		End 
	End 
	Form FormId: 0x2760, Title: "PCI Express Root Port 7"
		OneOf Prompt: "PCI Express Root Port 7", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x722, VarStoreId: 0x1, VarOffset: 0xA4F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x722, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x723, VarStoreId: 0x1, VarOffset: 0xC77, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [70, 66, 67, 64, 65]
							Uint64 Value: 0x0
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x724, VarStoreId: 0x1, VarOffset: 0xA67, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x725, VarStoreId: 0x1, VarOffset: 0xBCF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x726, VarStoreId: 0x1, VarOffset: 0xBFF, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x727, VarStoreId: 0x1, VarOffset: 0xC17, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x728, VarStoreId: 0x1, VarOffset: 0xC2F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x729, VarStoreId: 0x1, VarOffset: 0xBE7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x72A, VarStoreId: 0x1, VarOffset: 0xA7F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x72B, VarStoreId: 0x1, VarOffset: 0xA97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x72C, VarStoreId: 0x1, VarOffset: 0xAAF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x72D, VarStoreId: 0x1, VarOffset: 0xAC7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x72E, VarStoreId: 0x1, VarOffset: 0xADF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x72F, VarStoreId: 0x1, VarOffset: 0xB0F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x730, VarStoreId: 0x1, VarOffset: 0xB27, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x731, VarStoreId: 0x1, VarOffset: 0xB3F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x732, VarStoreId: 0x1, VarOffset: 0xB57, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x733, VarStoreId: 0x1, VarOffset: 0xB6F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x734, VarStoreId: 0x1, VarOffset: 0xB87, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x735, VarStoreId: 0x1, VarOffset: 0xB9F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x736, VarStoreId: 0x1, VarOffset: 0xBB7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x737, VarStoreId: 0x1, VarOffset: 0xFC4, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x7
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x738, VarStoreId: 0x1, VarOffset: 0xDD4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 7
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x739, VarStoreId: 0x1, VarOffset: 0xDF2, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 17
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x73A, VarStoreId: 0x1, VarOffset: 0xE1C, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 16
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE7 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x73B, VarStoreId: 0x1, VarOffset: 0xC9B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x73B, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x73C, VarStoreId: 0x1, VarOffset: 0xCCB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x73C, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x73D, VarStoreId: 0x1, VarOffset: 0xD31, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x73E, VarStoreId: 0x1, VarOffset: 0xCE3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x73F, VarStoreId: 0x1, VarOffset: 0xCFB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x73F, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x740, VarStoreId: 0x1, VarOffset: 0xD61, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x741, VarStoreId: 0x1, VarOffset: 0xD13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x742, VarStoreId: 0x1, VarOffset: 0xD8B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE7 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x743, VarStoreId: 0x1, VarOffset: 0xCB3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE7 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x744, VarStoreId: 0x1, VarOffset: 0xDA3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "No CLKREQ" Value: 1
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x744, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x745, VarStoreId: 0x1, VarOffset: 0xDBB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x746, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27E9
		End 
	End 
	Form FormId: 0x2761, Title: "PCI Express Root Port 8"
		OneOf Prompt: "PCI Express Root Port 8", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x747, VarStoreId: 0x1, VarOffset: 0xA50, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x747, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x748, VarStoreId: 0x1, VarOffset: 0xC78, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [72, 69, 70, 66, 67, 68, 64, 65, 74]
							Uint64 Value: 0x0
							Uint64 Value: 0x1
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x749, VarStoreId: 0x1, VarOffset: 0xA68, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x74A, VarStoreId: 0x1, VarOffset: 0xBD0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x74B, VarStoreId: 0x1, VarOffset: 0xC00, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x74C, VarStoreId: 0x1, VarOffset: 0xC18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x74D, VarStoreId: 0x1, VarOffset: 0xC30, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x74E, VarStoreId: 0x1, VarOffset: 0xBE8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x74F, VarStoreId: 0x1, VarOffset: 0xA80, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x750, VarStoreId: 0x1, VarOffset: 0xA98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x751, VarStoreId: 0x1, VarOffset: 0xAB0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x752, VarStoreId: 0x1, VarOffset: 0xAC8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x753, VarStoreId: 0x1, VarOffset: 0xAE0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x754, VarStoreId: 0x1, VarOffset: 0xB10, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x755, VarStoreId: 0x1, VarOffset: 0xB28, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x756, VarStoreId: 0x1, VarOffset: 0xB40, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x757, VarStoreId: 0x1, VarOffset: 0xB58, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x758, VarStoreId: 0x1, VarOffset: 0xB70, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x759, VarStoreId: 0x1, VarOffset: 0xB88, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x75A, VarStoreId: 0x1, VarOffset: 0xBA0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x75B, VarStoreId: 0x1, VarOffset: 0xBB8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x75C, VarStoreId: 0x1, VarOffset: 0xFC6, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x8
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x75D, VarStoreId: 0x1, VarOffset: 0xDD5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 7
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x75E, VarStoreId: 0x1, VarOffset: 0xDF4, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 17
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x75F, VarStoreId: 0x1, VarOffset: 0xE1D, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 8
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE8 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x760, VarStoreId: 0x1, VarOffset: 0xC9C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x760, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x761, VarStoreId: 0x1, VarOffset: 0xCCC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x761, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x762, VarStoreId: 0x1, VarOffset: 0xD33, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x763, VarStoreId: 0x1, VarOffset: 0xCE4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x764, VarStoreId: 0x1, VarOffset: 0xCFC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x764, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x765, VarStoreId: 0x1, VarOffset: 0xD63, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x766, VarStoreId: 0x1, VarOffset: 0xD14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x767, VarStoreId: 0x1, VarOffset: 0xD8C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE8 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x768, VarStoreId: 0x1, VarOffset: 0xCB4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE8 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x769, VarStoreId: 0x1, VarOffset: 0xDA4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0
				OneOfOption Option: "No CLKREQ" Value: 1, Default, MfgDefault
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x769, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x76A, VarStoreId: 0x1, VarOffset: 0xDBC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x76B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27EA
		End 
	End 
	Form FormId: 0x2762, Title: "PCI Express Root Port 9"
		OneOf Prompt: "PCI Express Root Port 9", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x76C, VarStoreId: 0x1, VarOffset: 0xA51, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			Default DefaultId: 0x1 Value: Other
				Value 
					EqIdValList QuestionId: 0xC50, Values: [20]
						Uint64 Value: 0x1
						Uint64 Value: 0x0
						Conditional 
					End 
				End 
			End 
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			OneOfOption Option: "Disabled" Value: 0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x76C, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x76D, VarStoreId: 0x1, VarOffset: 0xC79, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [70, 67, 64, 68, 69, 72, 66, 65, 74]
							EqIdValList QuestionId: 0xC50, Values: [8, 10, 26, 11, 7, 19, 3, 27, 12]
							Uint64 Value: 0x0
							Uint64 Value: 0x4
							Conditional 
							Uint64 Value: 0x2
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x76E, VarStoreId: 0x1, VarOffset: 0xA69, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Auto" Value: 4
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x76F, VarStoreId: 0x1, VarOffset: 0xBD1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x770, VarStoreId: 0x1, VarOffset: 0xC01, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x771, VarStoreId: 0x1, VarOffset: 0xC19, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x772, VarStoreId: 0x1, VarOffset: 0xC31, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x773, VarStoreId: 0x1, VarOffset: 0xBE9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x774, VarStoreId: 0x1, VarOffset: 0xA81, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x775, VarStoreId: 0x1, VarOffset: 0xA99, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x776, VarStoreId: 0x1, VarOffset: 0xAB1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x777, VarStoreId: 0x1, VarOffset: 0xAC9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x778, VarStoreId: 0x1, VarOffset: 0xAE1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x779, VarStoreId: 0x1, VarOffset: 0xB11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x77A, VarStoreId: 0x1, VarOffset: 0xB29, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x77B, VarStoreId: 0x1, VarOffset: 0xB41, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x77C, VarStoreId: 0x1, VarOffset: 0xB59, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x77D, VarStoreId: 0x1, VarOffset: 0xB71, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x77E, VarStoreId: 0x1, VarOffset: 0xB89, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x77F, VarStoreId: 0x1, VarOffset: 0xBA1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x780, VarStoreId: 0x1, VarOffset: 0xBB9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x781, VarStoreId: 0x1, VarOffset: 0xFC8, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x782, VarStoreId: 0x1, VarOffset: 0xDD6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x783, VarStoreId: 0x1, VarOffset: 0xDF6, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x784, VarStoreId: 0x1, VarOffset: 0xE1E, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE9 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x785, VarStoreId: 0x1, VarOffset: 0xC9D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x785, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x786, VarStoreId: 0x1, VarOffset: 0xCCD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x786, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x787, VarStoreId: 0x1, VarOffset: 0xD35, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x788, VarStoreId: 0x1, VarOffset: 0xCE5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x789, VarStoreId: 0x1, VarOffset: 0xCFD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x789, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x78A, VarStoreId: 0x1, VarOffset: 0xD65, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x78B, VarStoreId: 0x1, VarOffset: 0xD15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x78C, VarStoreId: 0x1, VarOffset: 0xD8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE9 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x78D, VarStoreId: 0x1, VarOffset: 0xCB5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE9 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x78E, VarStoreId: 0x1, VarOffset: 0xDA5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0
				OneOfOption Option: "No CLKREQ" Value: 1, Default, MfgDefault
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x78E, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x78F, VarStoreId: 0x1, VarOffset: 0xDBD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x790, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27EB
		End 
	End 
	Form FormId: 0x2763, Title: "PCI Express Root Port 10"
		OneOf Prompt: "PCI Express Root Port 10", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x791, VarStoreId: 0x1, VarOffset: 0xA52, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x791, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x792, VarStoreId: 0x1, VarOffset: 0xC7A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x793, VarStoreId: 0x1, VarOffset: 0xA6A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x794, VarStoreId: 0x1, VarOffset: 0xBD2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x795, VarStoreId: 0x1, VarOffset: 0xC02, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x796, VarStoreId: 0x1, VarOffset: 0xC1A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x797, VarStoreId: 0x1, VarOffset: 0xC32, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x798, VarStoreId: 0x1, VarOffset: 0xBEA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x799, VarStoreId: 0x1, VarOffset: 0xA82, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x79A, VarStoreId: 0x1, VarOffset: 0xA9A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x79B, VarStoreId: 0x1, VarOffset: 0xAB2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x79C, VarStoreId: 0x1, VarOffset: 0xACA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x79D, VarStoreId: 0x1, VarOffset: 0xAE2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x79E, VarStoreId: 0x1, VarOffset: 0xB12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x79F, VarStoreId: 0x1, VarOffset: 0xB2A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7A0, VarStoreId: 0x1, VarOffset: 0xB42, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7A1, VarStoreId: 0x1, VarOffset: 0xB5A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7A2, VarStoreId: 0x1, VarOffset: 0xB72, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7A3, VarStoreId: 0x1, VarOffset: 0xB8A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x7A4, VarStoreId: 0x1, VarOffset: 0xBA2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7A5, VarStoreId: 0x1, VarOffset: 0xBBA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x7A6, VarStoreId: 0x1, VarOffset: 0xFCA, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x7A7, VarStoreId: 0x1, VarOffset: 0xDD7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x7A8, VarStoreId: 0x1, VarOffset: 0xDF8, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x7A9, VarStoreId: 0x1, VarOffset: 0xE1F, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE10 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x7AA, VarStoreId: 0x1, VarOffset: 0xC9E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x7AA, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x7AB, VarStoreId: 0x1, VarOffset: 0xCCE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x7AB, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x7AC, VarStoreId: 0x1, VarOffset: 0xD37, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x7AD, VarStoreId: 0x1, VarOffset: 0xCE6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x7AE, VarStoreId: 0x1, VarOffset: 0xCFE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x7AE, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x7AF, VarStoreId: 0x1, VarOffset: 0xD67, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x7B0, VarStoreId: 0x1, VarOffset: 0xD16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x7B1, VarStoreId: 0x1, VarOffset: 0xD8E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE10 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x7B2, VarStoreId: 0x1, VarOffset: 0xCB6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE10 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x7B3, VarStoreId: 0x1, VarOffset: 0xDA6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0
				OneOfOption Option: "No CLKREQ" Value: 1, Default, MfgDefault
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x7B3, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x7B4, VarStoreId: 0x1, VarOffset: 0xDBE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x7B5, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27EC
		End 
	End 
	Form FormId: 0x2764, Title: "PCI Express Root Port 11"
		OneOf Prompt: "PCI Express Root Port 11", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x7B6, VarStoreId: 0x1, VarOffset: 0xA53, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			OneOfOption Option: "Disabled" Value: 0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x7B6, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x7B7, VarStoreId: 0x1, VarOffset: 0xC7B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x7B8, VarStoreId: 0x1, VarOffset: 0xA6B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x7B9, VarStoreId: 0x1, VarOffset: 0xBD3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x7BA, VarStoreId: 0x1, VarOffset: 0xC03, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x7BB, VarStoreId: 0x1, VarOffset: 0xC1B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x7BC, VarStoreId: 0x1, VarOffset: 0xC33, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x7BD, VarStoreId: 0x1, VarOffset: 0xBEB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7BE, VarStoreId: 0x1, VarOffset: 0xA83, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7BF, VarStoreId: 0x1, VarOffset: 0xA9B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7C0, VarStoreId: 0x1, VarOffset: 0xAB3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7C1, VarStoreId: 0x1, VarOffset: 0xACB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7C2, VarStoreId: 0x1, VarOffset: 0xAE3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7C3, VarStoreId: 0x1, VarOffset: 0xB13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7C4, VarStoreId: 0x1, VarOffset: 0xB2B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7C5, VarStoreId: 0x1, VarOffset: 0xB43, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7C6, VarStoreId: 0x1, VarOffset: 0xB5B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7C7, VarStoreId: 0x1, VarOffset: 0xB73, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7C8, VarStoreId: 0x1, VarOffset: 0xB8B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x7C9, VarStoreId: 0x1, VarOffset: 0xBA3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7CA, VarStoreId: 0x1, VarOffset: 0xBBB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x7CB, VarStoreId: 0x1, VarOffset: 0xFCC, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x7CC, VarStoreId: 0x1, VarOffset: 0xDD8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x7CD, VarStoreId: 0x1, VarOffset: 0xDFA, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x7CE, VarStoreId: 0x1, VarOffset: 0xE20, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE11 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x7CF, VarStoreId: 0x1, VarOffset: 0xC9F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x7CF, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x7D0, VarStoreId: 0x1, VarOffset: 0xCCF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x7D0, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x7D1, VarStoreId: 0x1, VarOffset: 0xD39, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x7D2, VarStoreId: 0x1, VarOffset: 0xCE7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x7D3, VarStoreId: 0x1, VarOffset: 0xCFF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x7D3, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x7D4, VarStoreId: 0x1, VarOffset: 0xD69, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x7D5, VarStoreId: 0x1, VarOffset: 0xD17, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x7D6, VarStoreId: 0x1, VarOffset: 0xD8F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE11 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x7D7, VarStoreId: 0x1, VarOffset: 0xCB7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE11 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x7D8, VarStoreId: 0x1, VarOffset: 0xDA7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0
				OneOfOption Option: "No CLKREQ" Value: 1, Default, MfgDefault
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x7D8, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x7D9, VarStoreId: 0x1, VarOffset: 0xDBF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x7DA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27ED
		End 
	End 
	Form FormId: 0x2765, Title: "PCI Express Root Port 12"
		OneOf Prompt: "PCI Express Root Port 12", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x7DB, VarStoreId: 0x1, VarOffset: 0xA54, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x7DB, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x7DC, VarStoreId: 0x1, VarOffset: 0xC7C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x7DD, VarStoreId: 0x1, VarOffset: 0xA6C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x7DE, VarStoreId: 0x1, VarOffset: 0xBD4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x7DF, VarStoreId: 0x1, VarOffset: 0xC04, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x7E0, VarStoreId: 0x1, VarOffset: 0xC1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x7E1, VarStoreId: 0x1, VarOffset: 0xC34, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x7E2, VarStoreId: 0x1, VarOffset: 0xBEC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7E3, VarStoreId: 0x1, VarOffset: 0xA84, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7E4, VarStoreId: 0x1, VarOffset: 0xA9C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7E5, VarStoreId: 0x1, VarOffset: 0xAB4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7E6, VarStoreId: 0x1, VarOffset: 0xACC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7E7, VarStoreId: 0x1, VarOffset: 0xAE4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7E8, VarStoreId: 0x1, VarOffset: 0xB14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7E9, VarStoreId: 0x1, VarOffset: 0xB2C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7EA, VarStoreId: 0x1, VarOffset: 0xB44, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7EB, VarStoreId: 0x1, VarOffset: 0xB5C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7EC, VarStoreId: 0x1, VarOffset: 0xB74, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7ED, VarStoreId: 0x1, VarOffset: 0xB8C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x7EE, VarStoreId: 0x1, VarOffset: 0xBA4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x7EF, VarStoreId: 0x1, VarOffset: 0xBBC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x7F0, VarStoreId: 0x1, VarOffset: 0xFCE, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x7F1, VarStoreId: 0x1, VarOffset: 0xDD9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x7F2, VarStoreId: 0x1, VarOffset: 0xDFC, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x7F3, VarStoreId: 0x1, VarOffset: 0xE21, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE12 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x7F4, VarStoreId: 0x1, VarOffset: 0xCA0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x7F4, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x7F5, VarStoreId: 0x1, VarOffset: 0xCD0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x7F5, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x7F6, VarStoreId: 0x1, VarOffset: 0xD3B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x7F7, VarStoreId: 0x1, VarOffset: 0xCE8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x7F8, VarStoreId: 0x1, VarOffset: 0xD00, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x7F8, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x7F9, VarStoreId: 0x1, VarOffset: 0xD6B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x7FA, VarStoreId: 0x1, VarOffset: 0xD18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x7FB, VarStoreId: 0x1, VarOffset: 0xD90, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE12 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x7FC, VarStoreId: 0x1, VarOffset: 0xCB8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE12 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x7FD, VarStoreId: 0x1, VarOffset: 0xDA8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0
				OneOfOption Option: "No CLKREQ" Value: 1, Default, MfgDefault
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x7FD, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x7FE, VarStoreId: 0x1, VarOffset: 0xDC0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x7FF, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27EE
		End 
	End 
	Form FormId: 0x2766, Title: "PCI Express Root Port 13"
		OneOf Prompt: "PCI Express Root Port 13", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x800, VarStoreId: 0x1, VarOffset: 0xA55, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x800, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x801, VarStoreId: 0x1, VarOffset: 0xC7D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [72, 69, 68, 80, 74]
							Uint64 Value: 0x0
							Uint64 Value: 0x4
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x802, VarStoreId: 0x1, VarOffset: 0xA6D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x803, VarStoreId: 0x1, VarOffset: 0xBD5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x804, VarStoreId: 0x1, VarOffset: 0xC05, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x805, VarStoreId: 0x1, VarOffset: 0xC1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x806, VarStoreId: 0x1, VarOffset: 0xC35, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x807, VarStoreId: 0x1, VarOffset: 0xBED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x808, VarStoreId: 0x1, VarOffset: 0xA85, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x809, VarStoreId: 0x1, VarOffset: 0xA9D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x80A, VarStoreId: 0x1, VarOffset: 0xAB5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x80B, VarStoreId: 0x1, VarOffset: 0xACD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x80C, VarStoreId: 0x1, VarOffset: 0xAE5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x80D, VarStoreId: 0x1, VarOffset: 0xB15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x80E, VarStoreId: 0x1, VarOffset: 0xB2D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x80F, VarStoreId: 0x1, VarOffset: 0xB45, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x810, VarStoreId: 0x1, VarOffset: 0xB5D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x811, VarStoreId: 0x1, VarOffset: 0xB75, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x812, VarStoreId: 0x1, VarOffset: 0xB8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x813, VarStoreId: 0x1, VarOffset: 0xBA5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x814, VarStoreId: 0x1, VarOffset: 0xBBD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x815, VarStoreId: 0x1, VarOffset: 0xFD0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x816, VarStoreId: 0x1, VarOffset: 0xDDA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x817, VarStoreId: 0x1, VarOffset: 0xDFE, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x818, VarStoreId: 0x1, VarOffset: 0xE22, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE13 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x819, VarStoreId: 0x1, VarOffset: 0xCA1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x819, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x81A, VarStoreId: 0x1, VarOffset: 0xCD1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x81A, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x81B, VarStoreId: 0x1, VarOffset: 0xD3D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x81C, VarStoreId: 0x1, VarOffset: 0xCE9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x81D, VarStoreId: 0x1, VarOffset: 0xD01, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x81D, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x81E, VarStoreId: 0x1, VarOffset: 0xD6D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x81F, VarStoreId: 0x1, VarOffset: 0xD19, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x820, VarStoreId: 0x1, VarOffset: 0xD91, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE13 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x821, VarStoreId: 0x1, VarOffset: 0xCB9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE13 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x822, VarStoreId: 0x1, VarOffset: 0xDA9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0
				OneOfOption Option: "No CLKREQ" Value: 1, Default, MfgDefault
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x822, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x823, VarStoreId: 0x1, VarOffset: 0xDC1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x824, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27EF
		End 
	End 
	Form FormId: 0x2767, Title: "PCI Express Root Port 14"
		OneOf Prompt: "PCI Express Root Port 14", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x825, VarStoreId: 0x1, VarOffset: 0xA56, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x825, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x826, VarStoreId: 0x1, VarOffset: 0xC7E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x827, VarStoreId: 0x1, VarOffset: 0xA6E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x828, VarStoreId: 0x1, VarOffset: 0xBD6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x829, VarStoreId: 0x1, VarOffset: 0xC06, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x82A, VarStoreId: 0x1, VarOffset: 0xC1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x82B, VarStoreId: 0x1, VarOffset: 0xC36, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x82C, VarStoreId: 0x1, VarOffset: 0xBEE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x82D, VarStoreId: 0x1, VarOffset: 0xA86, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x82E, VarStoreId: 0x1, VarOffset: 0xA9E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x82F, VarStoreId: 0x1, VarOffset: 0xAB6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x830, VarStoreId: 0x1, VarOffset: 0xACE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x831, VarStoreId: 0x1, VarOffset: 0xAE6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x832, VarStoreId: 0x1, VarOffset: 0xB16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x833, VarStoreId: 0x1, VarOffset: 0xB2E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x834, VarStoreId: 0x1, VarOffset: 0xB46, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x835, VarStoreId: 0x1, VarOffset: 0xB5E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x836, VarStoreId: 0x1, VarOffset: 0xB76, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x837, VarStoreId: 0x1, VarOffset: 0xB8E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x838, VarStoreId: 0x1, VarOffset: 0xBA6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x839, VarStoreId: 0x1, VarOffset: 0xBBE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x83A, VarStoreId: 0x1, VarOffset: 0xFD2, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x83B, VarStoreId: 0x1, VarOffset: 0xDDB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x83C, VarStoreId: 0x1, VarOffset: 0xE00, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x83D, VarStoreId: 0x1, VarOffset: 0xE23, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE14 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x83E, VarStoreId: 0x1, VarOffset: 0xCA2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x83E, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x83F, VarStoreId: 0x1, VarOffset: 0xCD2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x83F, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x840, VarStoreId: 0x1, VarOffset: 0xD3F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x841, VarStoreId: 0x1, VarOffset: 0xCEA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x842, VarStoreId: 0x1, VarOffset: 0xD02, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x842, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x843, VarStoreId: 0x1, VarOffset: 0xD6F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x844, VarStoreId: 0x1, VarOffset: 0xD1A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x845, VarStoreId: 0x1, VarOffset: 0xD92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE14 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x846, VarStoreId: 0x1, VarOffset: 0xCBA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE14 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x847, VarStoreId: 0x1, VarOffset: 0xDAA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "No CLKREQ" Value: 1
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x847, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x848, VarStoreId: 0x1, VarOffset: 0xDC2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x849, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27F0
		End 
	End 
	Form FormId: 0x2768, Title: "PCI Express Root Port 15"
		OneOf Prompt: "PCI Express Root Port 15", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x84A, VarStoreId: 0x1, VarOffset: 0xA57, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x84A, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x84B, VarStoreId: 0x1, VarOffset: 0xC7F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x84C, VarStoreId: 0x1, VarOffset: 0xA6F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x84D, VarStoreId: 0x1, VarOffset: 0xBD7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x84E, VarStoreId: 0x1, VarOffset: 0xC07, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x84F, VarStoreId: 0x1, VarOffset: 0xC1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x850, VarStoreId: 0x1, VarOffset: 0xC37, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x851, VarStoreId: 0x1, VarOffset: 0xBEF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x852, VarStoreId: 0x1, VarOffset: 0xA87, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x853, VarStoreId: 0x1, VarOffset: 0xA9F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x854, VarStoreId: 0x1, VarOffset: 0xAB7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x855, VarStoreId: 0x1, VarOffset: 0xACF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x856, VarStoreId: 0x1, VarOffset: 0xAE7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x857, VarStoreId: 0x1, VarOffset: 0xB17, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x858, VarStoreId: 0x1, VarOffset: 0xB2F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x859, VarStoreId: 0x1, VarOffset: 0xB47, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x85A, VarStoreId: 0x1, VarOffset: 0xB5F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x85B, VarStoreId: 0x1, VarOffset: 0xB77, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x85C, VarStoreId: 0x1, VarOffset: 0xB8F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x85D, VarStoreId: 0x1, VarOffset: 0xBA7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x85E, VarStoreId: 0x1, VarOffset: 0xBBF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x85F, VarStoreId: 0x1, VarOffset: 0xFD4, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x860, VarStoreId: 0x1, VarOffset: 0xDDC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x861, VarStoreId: 0x1, VarOffset: 0xE02, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x862, VarStoreId: 0x1, VarOffset: 0xE24, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE15 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x863, VarStoreId: 0x1, VarOffset: 0xCA3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x863, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x864, VarStoreId: 0x1, VarOffset: 0xCD3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x864, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x865, VarStoreId: 0x1, VarOffset: 0xD41, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x866, VarStoreId: 0x1, VarOffset: 0xCEB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x867, VarStoreId: 0x1, VarOffset: 0xD03, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x867, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x868, VarStoreId: 0x1, VarOffset: 0xD71, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x869, VarStoreId: 0x1, VarOffset: 0xD1B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x86A, VarStoreId: 0x1, VarOffset: 0xD93, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE15 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x86B, VarStoreId: 0x1, VarOffset: 0xCBB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE15 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x86C, VarStoreId: 0x1, VarOffset: 0xDAB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "No CLKREQ" Value: 1
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x86C, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x86D, VarStoreId: 0x1, VarOffset: 0xDC3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x86E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27F1
		End 
	End 
	Form FormId: 0x2769, Title: "PCI Express Root Port 16"
		OneOf Prompt: "PCI Express Root Port 16", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x86F, VarStoreId: 0x1, VarOffset: 0xA58, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x86F, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x870, VarStoreId: 0x1, VarOffset: 0xC80, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x871, VarStoreId: 0x1, VarOffset: 0xA70, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x872, VarStoreId: 0x1, VarOffset: 0xBD8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x873, VarStoreId: 0x1, VarOffset: 0xC08, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x874, VarStoreId: 0x1, VarOffset: 0xC20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x875, VarStoreId: 0x1, VarOffset: 0xC38, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x876, VarStoreId: 0x1, VarOffset: 0xBF0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x877, VarStoreId: 0x1, VarOffset: 0xA88, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x878, VarStoreId: 0x1, VarOffset: 0xAA0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x879, VarStoreId: 0x1, VarOffset: 0xAB8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x87A, VarStoreId: 0x1, VarOffset: 0xAD0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x87B, VarStoreId: 0x1, VarOffset: 0xAE8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x87C, VarStoreId: 0x1, VarOffset: 0xB18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x87D, VarStoreId: 0x1, VarOffset: 0xB30, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x87E, VarStoreId: 0x1, VarOffset: 0xB48, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x87F, VarStoreId: 0x1, VarOffset: 0xB60, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x880, VarStoreId: 0x1, VarOffset: 0xB78, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x881, VarStoreId: 0x1, VarOffset: 0xB90, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x882, VarStoreId: 0x1, VarOffset: 0xBA8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x883, VarStoreId: 0x1, VarOffset: 0xBC0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x884, VarStoreId: 0x1, VarOffset: 0xFD6, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x885, VarStoreId: 0x1, VarOffset: 0xDDD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x886, VarStoreId: 0x1, VarOffset: 0xE04, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x887, VarStoreId: 0x1, VarOffset: 0xE25, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE16 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x888, VarStoreId: 0x1, VarOffset: 0xCA4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x888, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x889, VarStoreId: 0x1, VarOffset: 0xCD4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x889, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x88A, VarStoreId: 0x1, VarOffset: 0xD43, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x88B, VarStoreId: 0x1, VarOffset: 0xCEC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x88C, VarStoreId: 0x1, VarOffset: 0xD04, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x88C, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x88D, VarStoreId: 0x1, VarOffset: 0xD73, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x88E, VarStoreId: 0x1, VarOffset: 0xD1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x88F, VarStoreId: 0x1, VarOffset: 0xD94, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE16 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x890, VarStoreId: 0x1, VarOffset: 0xCBC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE16 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x891, VarStoreId: 0x1, VarOffset: 0xDAC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "No CLKREQ" Value: 1
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x891, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x892, VarStoreId: 0x1, VarOffset: 0xDC4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x893, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27F2
		End 
	End 
	Form FormId: 0x276A, Title: "PCI Express Root Port 17"
		OneOf Prompt: "PCI Express Root Port 17", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x894, VarStoreId: 0x1, VarOffset: 0xA59, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x894, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x895, VarStoreId: 0x1, VarOffset: 0xC81, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [72, 69, 68, 66, 65, 67, 70, 64, 74]
							Uint64 Value: 0x0
							Uint64 Value: 0x4
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x896, VarStoreId: 0x1, VarOffset: 0xA71, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x897, VarStoreId: 0x1, VarOffset: 0xBD9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x898, VarStoreId: 0x1, VarOffset: 0xC09, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x899, VarStoreId: 0x1, VarOffset: 0xC21, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x89A, VarStoreId: 0x1, VarOffset: 0xC39, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x89B, VarStoreId: 0x1, VarOffset: 0xBF1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x89C, VarStoreId: 0x1, VarOffset: 0xA89, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x89D, VarStoreId: 0x1, VarOffset: 0xAA1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x89E, VarStoreId: 0x1, VarOffset: 0xAB9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x89F, VarStoreId: 0x1, VarOffset: 0xAD1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8A0, VarStoreId: 0x1, VarOffset: 0xAE9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8A1, VarStoreId: 0x1, VarOffset: 0xB19, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8A2, VarStoreId: 0x1, VarOffset: 0xB31, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8A3, VarStoreId: 0x1, VarOffset: 0xB49, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8A4, VarStoreId: 0x1, VarOffset: 0xB61, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8A5, VarStoreId: 0x1, VarOffset: 0xB79, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8A6, VarStoreId: 0x1, VarOffset: 0xB91, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x8A7, VarStoreId: 0x1, VarOffset: 0xBA9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8A8, VarStoreId: 0x1, VarOffset: 0xBC1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x8A9, VarStoreId: 0x1, VarOffset: 0xFD8, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x8AA, VarStoreId: 0x1, VarOffset: 0xDDE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x8AB, VarStoreId: 0x1, VarOffset: 0xE06, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x8AC, VarStoreId: 0x1, VarOffset: 0xE26, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE17 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x8AD, VarStoreId: 0x1, VarOffset: 0xCA5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x8AD, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x8AE, VarStoreId: 0x1, VarOffset: 0xCD5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x8AE, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x8AF, VarStoreId: 0x1, VarOffset: 0xD45, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x8B0, VarStoreId: 0x1, VarOffset: 0xCED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x8B1, VarStoreId: 0x1, VarOffset: 0xD05, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x8B1, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x8B2, VarStoreId: 0x1, VarOffset: 0xD75, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x8B3, VarStoreId: 0x1, VarOffset: 0xD1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x8B4, VarStoreId: 0x1, VarOffset: 0xD95, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE17 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x8B5, VarStoreId: 0x1, VarOffset: 0xCBD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE17 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x8B6, VarStoreId: 0x1, VarOffset: 0xDAD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "No CLKREQ" Value: 1
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x8B6, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x8B7, VarStoreId: 0x1, VarOffset: 0xDC5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x8B8, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27F3
		End 
	End 
	Form FormId: 0x276B, Title: "PCI Express Root Port 18"
		OneOf Prompt: "PCI Express Root Port 18", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x8B9, VarStoreId: 0x1, VarOffset: 0xA5A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x8B9, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x8BA, VarStoreId: 0x1, VarOffset: 0xC82, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x8BB, VarStoreId: 0x1, VarOffset: 0xA72, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x8BC, VarStoreId: 0x1, VarOffset: 0xBDA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x8BD, VarStoreId: 0x1, VarOffset: 0xC0A, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x8BE, VarStoreId: 0x1, VarOffset: 0xC22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x8BF, VarStoreId: 0x1, VarOffset: 0xC3A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x8C0, VarStoreId: 0x1, VarOffset: 0xBF2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8C1, VarStoreId: 0x1, VarOffset: 0xA8A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8C2, VarStoreId: 0x1, VarOffset: 0xAA2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8C3, VarStoreId: 0x1, VarOffset: 0xABA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8C4, VarStoreId: 0x1, VarOffset: 0xAD2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8C5, VarStoreId: 0x1, VarOffset: 0xAEA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8C6, VarStoreId: 0x1, VarOffset: 0xB1A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8C7, VarStoreId: 0x1, VarOffset: 0xB32, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8C8, VarStoreId: 0x1, VarOffset: 0xB4A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8C9, VarStoreId: 0x1, VarOffset: 0xB62, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8CA, VarStoreId: 0x1, VarOffset: 0xB7A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8CB, VarStoreId: 0x1, VarOffset: 0xB92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x8CC, VarStoreId: 0x1, VarOffset: 0xBAA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8CD, VarStoreId: 0x1, VarOffset: 0xBC2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x8CE, VarStoreId: 0x1, VarOffset: 0xFDA, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x8CF, VarStoreId: 0x1, VarOffset: 0xDDF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x8D0, VarStoreId: 0x1, VarOffset: 0xE08, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x8D1, VarStoreId: 0x1, VarOffset: 0xE27, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE18 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x8D2, VarStoreId: 0x1, VarOffset: 0xCA6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x8D2, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x8D3, VarStoreId: 0x1, VarOffset: 0xCD6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x8D3, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x8D4, VarStoreId: 0x1, VarOffset: 0xD47, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x8D5, VarStoreId: 0x1, VarOffset: 0xCEE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x8D6, VarStoreId: 0x1, VarOffset: 0xD06, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x8D6, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x8D7, VarStoreId: 0x1, VarOffset: 0xD77, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x8D8, VarStoreId: 0x1, VarOffset: 0xD1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x8D9, VarStoreId: 0x1, VarOffset: 0xD96, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE18 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x8DA, VarStoreId: 0x1, VarOffset: 0xCBE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE18 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x8DB, VarStoreId: 0x1, VarOffset: 0xDAE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "No CLKREQ" Value: 1
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x8DB, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x8DC, VarStoreId: 0x1, VarOffset: 0xDC6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x8DD, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27F4
		End 
	End 
	Form FormId: 0x276C, Title: "PCI Express Root Port 19"
		OneOf Prompt: "PCI Express Root Port 19", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x8DE, VarStoreId: 0x1, VarOffset: 0xA5B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x8DE, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x8DF, VarStoreId: 0x1, VarOffset: 0xC83, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x8E0, VarStoreId: 0x1, VarOffset: 0xA73, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x8E1, VarStoreId: 0x1, VarOffset: 0xBDB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x8E2, VarStoreId: 0x1, VarOffset: 0xC0B, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x8E3, VarStoreId: 0x1, VarOffset: 0xC23, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x8E4, VarStoreId: 0x1, VarOffset: 0xC3B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x8E5, VarStoreId: 0x1, VarOffset: 0xBF3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8E6, VarStoreId: 0x1, VarOffset: 0xA8B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8E7, VarStoreId: 0x1, VarOffset: 0xAA3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8E8, VarStoreId: 0x1, VarOffset: 0xABB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8E9, VarStoreId: 0x1, VarOffset: 0xAD3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8EA, VarStoreId: 0x1, VarOffset: 0xAEB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8EB, VarStoreId: 0x1, VarOffset: 0xB1B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8EC, VarStoreId: 0x1, VarOffset: 0xB33, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8ED, VarStoreId: 0x1, VarOffset: 0xB4B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8EE, VarStoreId: 0x1, VarOffset: 0xB63, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8EF, VarStoreId: 0x1, VarOffset: 0xB7B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8F0, VarStoreId: 0x1, VarOffset: 0xB93, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x8F1, VarStoreId: 0x1, VarOffset: 0xBAB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x8F2, VarStoreId: 0x1, VarOffset: 0xBC3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x8F3, VarStoreId: 0x1, VarOffset: 0xFDC, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x8F4, VarStoreId: 0x1, VarOffset: 0xDE0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x8F5, VarStoreId: 0x1, VarOffset: 0xE0A, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x8F6, VarStoreId: 0x1, VarOffset: 0xE28, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE19 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x8F7, VarStoreId: 0x1, VarOffset: 0xCA7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x8F7, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x8F8, VarStoreId: 0x1, VarOffset: 0xCD7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x8F8, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x8F9, VarStoreId: 0x1, VarOffset: 0xD49, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x8FA, VarStoreId: 0x1, VarOffset: 0xCEF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x8FB, VarStoreId: 0x1, VarOffset: 0xD07, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x8FB, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x8FC, VarStoreId: 0x1, VarOffset: 0xD79, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x8FD, VarStoreId: 0x1, VarOffset: 0xD1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x8FE, VarStoreId: 0x1, VarOffset: 0xD97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE19 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x8FF, VarStoreId: 0x1, VarOffset: 0xCBF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE19 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x900, VarStoreId: 0x1, VarOffset: 0xDAF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "No CLKREQ" Value: 1
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x900, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x901, VarStoreId: 0x1, VarOffset: 0xDC7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x902, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27F5
		End 
	End 
	Form FormId: 0x276D, Title: "PCI Express Root Port 20"
		OneOf Prompt: "PCI Express Root Port 20", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x903, VarStoreId: 0x1, VarOffset: 0xA5C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x903, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x904, VarStoreId: 0x1, VarOffset: 0xC84, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x905, VarStoreId: 0x1, VarOffset: 0xA74, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x906, VarStoreId: 0x1, VarOffset: 0xBDC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x907, VarStoreId: 0x1, VarOffset: 0xC0C, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x908, VarStoreId: 0x1, VarOffset: 0xC24, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x909, VarStoreId: 0x1, VarOffset: 0xC3C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x90A, VarStoreId: 0x1, VarOffset: 0xBF4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x90B, VarStoreId: 0x1, VarOffset: 0xA8C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x90C, VarStoreId: 0x1, VarOffset: 0xAA4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x90D, VarStoreId: 0x1, VarOffset: 0xABC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x90E, VarStoreId: 0x1, VarOffset: 0xAD4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x90F, VarStoreId: 0x1, VarOffset: 0xAEC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x910, VarStoreId: 0x1, VarOffset: 0xB1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x911, VarStoreId: 0x1, VarOffset: 0xB34, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x912, VarStoreId: 0x1, VarOffset: 0xB4C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x913, VarStoreId: 0x1, VarOffset: 0xB64, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x914, VarStoreId: 0x1, VarOffset: 0xB7C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x915, VarStoreId: 0x1, VarOffset: 0xB94, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x916, VarStoreId: 0x1, VarOffset: 0xBAC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x917, VarStoreId: 0x1, VarOffset: 0xBC4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x918, VarStoreId: 0x1, VarOffset: 0xFDE, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x919, VarStoreId: 0x1, VarOffset: 0xDE1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x91A, VarStoreId: 0x1, VarOffset: 0xE0C, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x91B, VarStoreId: 0x1, VarOffset: 0xE29, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x14, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE20 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x91C, VarStoreId: 0x1, VarOffset: 0xCA8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x91C, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x91D, VarStoreId: 0x1, VarOffset: 0xCD8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x91D, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x91E, VarStoreId: 0x1, VarOffset: 0xD4B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x91F, VarStoreId: 0x1, VarOffset: 0xCF0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x920, VarStoreId: 0x1, VarOffset: 0xD08, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x920, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x921, VarStoreId: 0x1, VarOffset: 0xD7B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x922, VarStoreId: 0x1, VarOffset: 0xD20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x923, VarStoreId: 0x1, VarOffset: 0xD98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE20 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x924, VarStoreId: 0x1, VarOffset: 0xCC0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE20 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x925, VarStoreId: 0x1, VarOffset: 0xDB0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "No CLKREQ" Value: 1
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x925, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x926, VarStoreId: 0x1, VarOffset: 0xDC8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x927, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27F6
		End 
	End 
	Form FormId: 0x276E, Title: "PCI Express Root Port 21"
		OneOf Prompt: "PCI Express Root Port 21", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x928, VarStoreId: 0x1, VarOffset: 0xA5D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x928, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x929, VarStoreId: 0x1, VarOffset: 0xC85, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x92A, VarStoreId: 0x1, VarOffset: 0xA75, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x92B, VarStoreId: 0x1, VarOffset: 0xBDD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x92C, VarStoreId: 0x1, VarOffset: 0xC0D, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x92D, VarStoreId: 0x1, VarOffset: 0xC25, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x92E, VarStoreId: 0x1, VarOffset: 0xC3D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x92F, VarStoreId: 0x1, VarOffset: 0xBF5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x930, VarStoreId: 0x1, VarOffset: 0xA8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x931, VarStoreId: 0x1, VarOffset: 0xAA5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x932, VarStoreId: 0x1, VarOffset: 0xABD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x933, VarStoreId: 0x1, VarOffset: 0xAD5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x934, VarStoreId: 0x1, VarOffset: 0xAED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x935, VarStoreId: 0x1, VarOffset: 0xB1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x936, VarStoreId: 0x1, VarOffset: 0xB35, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x937, VarStoreId: 0x1, VarOffset: 0xB4D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x938, VarStoreId: 0x1, VarOffset: 0xB65, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x939, VarStoreId: 0x1, VarOffset: 0xB7D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x93A, VarStoreId: 0x1, VarOffset: 0xB95, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x93B, VarStoreId: 0x1, VarOffset: 0xBAD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x93C, VarStoreId: 0x1, VarOffset: 0xBC5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x93D, VarStoreId: 0x1, VarOffset: 0xFE0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x93E, VarStoreId: 0x1, VarOffset: 0xDE2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x93F, VarStoreId: 0x1, VarOffset: 0xE0E, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x15, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x940, VarStoreId: 0x1, VarOffset: 0xE2A, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x15, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE21 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x941, VarStoreId: 0x1, VarOffset: 0xCA9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x941, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x942, VarStoreId: 0x1, VarOffset: 0xCD9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x942, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x943, VarStoreId: 0x1, VarOffset: 0xD4D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x944, VarStoreId: 0x1, VarOffset: 0xCF1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x945, VarStoreId: 0x1, VarOffset: 0xD09, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x945, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x946, VarStoreId: 0x1, VarOffset: 0xD7D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x947, VarStoreId: 0x1, VarOffset: 0xD21, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x948, VarStoreId: 0x1, VarOffset: 0xD99, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE21 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x949, VarStoreId: 0x1, VarOffset: 0xCC1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE20 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x94A, VarStoreId: 0x1, VarOffset: 0xDB1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "No CLKREQ" Value: 1
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x94A, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x94B, VarStoreId: 0x1, VarOffset: 0xDC9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x94C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27F7
		End 
	End 
	Form FormId: 0x276F, Title: "PCI Express Root Port 22"
		OneOf Prompt: "PCI Express Root Port 22", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x94D, VarStoreId: 0x1, VarOffset: 0xA5E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x94D, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x94E, VarStoreId: 0x1, VarOffset: 0xC86, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x94F, VarStoreId: 0x1, VarOffset: 0xA76, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x950, VarStoreId: 0x1, VarOffset: 0xBDE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x951, VarStoreId: 0x1, VarOffset: 0xC0E, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x952, VarStoreId: 0x1, VarOffset: 0xC26, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x953, VarStoreId: 0x1, VarOffset: 0xC3E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x954, VarStoreId: 0x1, VarOffset: 0xBF6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x955, VarStoreId: 0x1, VarOffset: 0xA8E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x956, VarStoreId: 0x1, VarOffset: 0xAA6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x957, VarStoreId: 0x1, VarOffset: 0xABE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x958, VarStoreId: 0x1, VarOffset: 0xAD6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x959, VarStoreId: 0x1, VarOffset: 0xAEE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x95A, VarStoreId: 0x1, VarOffset: 0xB1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x95B, VarStoreId: 0x1, VarOffset: 0xB36, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x95C, VarStoreId: 0x1, VarOffset: 0xB4E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x95D, VarStoreId: 0x1, VarOffset: 0xB66, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x95E, VarStoreId: 0x1, VarOffset: 0xB7E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x95F, VarStoreId: 0x1, VarOffset: 0xB96, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x960, VarStoreId: 0x1, VarOffset: 0xBAE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x961, VarStoreId: 0x1, VarOffset: 0xBC6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x962, VarStoreId: 0x1, VarOffset: 0xFE2, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x963, VarStoreId: 0x1, VarOffset: 0xDE3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x964, VarStoreId: 0x1, VarOffset: 0xE10, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x16, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x965, VarStoreId: 0x1, VarOffset: 0xE2B, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x16, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE22 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x966, VarStoreId: 0x1, VarOffset: 0xCAA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x966, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x967, VarStoreId: 0x1, VarOffset: 0xCDA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x967, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x968, VarStoreId: 0x1, VarOffset: 0xD4F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x969, VarStoreId: 0x1, VarOffset: 0xCF2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x96A, VarStoreId: 0x1, VarOffset: 0xD0A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x96A, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x96B, VarStoreId: 0x1, VarOffset: 0xD7F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x96C, VarStoreId: 0x1, VarOffset: 0xD22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x96D, VarStoreId: 0x1, VarOffset: 0xD9A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE22 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x96E, VarStoreId: 0x1, VarOffset: 0xCC2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE20 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x96F, VarStoreId: 0x1, VarOffset: 0xDB2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "No CLKREQ" Value: 1
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x96F, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x970, VarStoreId: 0x1, VarOffset: 0xDCA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x971, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27F8
		End 
	End 
	Form FormId: 0x2770, Title: "PCI Express Root Port 23"
		OneOf Prompt: "PCI Express Root Port 23", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x972, VarStoreId: 0x1, VarOffset: 0xA5F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x972, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x973, VarStoreId: 0x1, VarOffset: 0xC87, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x974, VarStoreId: 0x1, VarOffset: 0xA77, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x975, VarStoreId: 0x1, VarOffset: 0xBDF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x976, VarStoreId: 0x1, VarOffset: 0xC0F, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x977, VarStoreId: 0x1, VarOffset: 0xC27, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x978, VarStoreId: 0x1, VarOffset: 0xC3F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x979, VarStoreId: 0x1, VarOffset: 0xBF7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x97A, VarStoreId: 0x1, VarOffset: 0xA8F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x97B, VarStoreId: 0x1, VarOffset: 0xAA7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x97C, VarStoreId: 0x1, VarOffset: 0xABF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x97D, VarStoreId: 0x1, VarOffset: 0xAD7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x97E, VarStoreId: 0x1, VarOffset: 0xAEF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x97F, VarStoreId: 0x1, VarOffset: 0xB1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x980, VarStoreId: 0x1, VarOffset: 0xB37, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x981, VarStoreId: 0x1, VarOffset: 0xB4F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x982, VarStoreId: 0x1, VarOffset: 0xB67, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x983, VarStoreId: 0x1, VarOffset: 0xB7F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x984, VarStoreId: 0x1, VarOffset: 0xB97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x985, VarStoreId: 0x1, VarOffset: 0xBAF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x986, VarStoreId: 0x1, VarOffset: 0xBC7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x987, VarStoreId: 0x1, VarOffset: 0xFE4, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x988, VarStoreId: 0x1, VarOffset: 0xDE4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x989, VarStoreId: 0x1, VarOffset: 0xE12, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x98A, VarStoreId: 0x1, VarOffset: 0xE2C, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x17, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE23 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x98B, VarStoreId: 0x1, VarOffset: 0xCAB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x98B, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x98C, VarStoreId: 0x1, VarOffset: 0xCDB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x98C, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x98D, VarStoreId: 0x1, VarOffset: 0xD51, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x98E, VarStoreId: 0x1, VarOffset: 0xCF3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x98F, VarStoreId: 0x1, VarOffset: 0xD0B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x98F, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x990, VarStoreId: 0x1, VarOffset: 0xD81, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x991, VarStoreId: 0x1, VarOffset: 0xD23, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x992, VarStoreId: 0x1, VarOffset: 0xD9B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE23 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x993, VarStoreId: 0x1, VarOffset: 0xCC3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE20 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x994, VarStoreId: 0x1, VarOffset: 0xDB3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "No CLKREQ" Value: 1
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x994, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x995, VarStoreId: 0x1, VarOffset: 0xDCB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x996, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27F9
		End 
	End 
	Form FormId: 0x2771, Title: "PCI Express Root Port 24"
		OneOf Prompt: "PCI Express Root Port 24", Help: "Control the PCI Express Root Port.", QuestionFlags: 0x10, QuestionId: 0x997, VarStoreId: 0x1, VarOffset: 0xA60, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x997, Value: 0x0
			OneOf Prompt: "  Topology", Help: "Identify the SATA Topology if it is Default or ISATA or Flex or DirectConnect or M2", QuestionFlags: 0x10, QuestionId: 0x998, VarStoreId: 0x1, VarOffset: 0xC88, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Unknown" Value: 0, Default, MfgDefault
				OneOfOption Option: "x1" Value: 1
				OneOfOption Option: "x4" Value: 2
				OneOfOption Option: "Sata Express" Value: 3
				OneOfOption Option: "M2" Value: 4
			End 
			OneOf Prompt: "ASPM", Help: "Set the ASPM Level:
Force L0s - Force all links to L0s State
AUTO - BIOS auto configure
DISABLE - Disables ASPM", QuestionFlags: 0x10, QuestionId: 0x999, VarStoreId: 0x1, VarOffset: 0xA78, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L0s" Value: 1
				OneOfOption Option: "L1" Value: 2
				OneOfOption Option: "L0sL1" Value: 3
				OneOfOption Option: "Auto" Value: 4, Default, MfgDefault
			End 
			OneOf Prompt: "L1 Substates", Help: "PCI Express L1 Substates settings.", QuestionFlags: 0x10, QuestionId: 0x99A, VarStoreId: 0x1, VarOffset: 0xBE0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "L1.1" Value: 1
				OneOfOption Option: "L1.2" Value: 2
				OneOfOption Option: "L1.1 & L1.2" Value: 3, Default, MfgDefault
			End 
			OneOf Prompt: "Gen3 Eq Phase3 Method", Help: "PCIe Gen3 Equalization Phase 3 Method", QuestionFlags: 0x10, QuestionId: 0x99B, VarStoreId: 0x1, VarOffset: 0xC10, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
				OneOfOption Option: "Hardware" Value: 1
				OneOfOption Option: "Static Coeff." Value: 4
				OneOfOption Option: "Software Search" Value: 2, Default
			End 
			Numeric Prompt: "UPTP", Help: "Upstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x99C, VarStoreId: 0x1, VarOffset: 0xC28, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 5
			End 
			Numeric Prompt: "DPTP", Help: "Downstream Port Transmitter Preset", QuestionFlags: 0x0, QuestionId: 0x99D, VarStoreId: 0x1, VarOffset: 0xC40, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x1
				Default DefaultId: 0x0 Value: 7
			End 
			OneOf Prompt: "ACS", Help: "Enable/Disable Access Control Services Extended Capability", QuestionFlags: 0x10, QuestionId: 0x99E, VarStoreId: 0x1, VarOffset: 0xBF8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  URR", Help: "PCI Express Unsupported Request Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x99F, VarStoreId: 0x1, VarOffset: 0xA90, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  FER", Help: "PCI Express Device Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9A0, VarStoreId: 0x1, VarOffset: 0xAA8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  NFER", Help: "PCI Express Device Non-Fatal Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9A1, VarStoreId: 0x1, VarOffset: 0xAC0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CER", Help: "PCI Express Device Correctable Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9A2, VarStoreId: 0x1, VarOffset: 0xAD8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  CTO", Help: "PCI Express Completion Timer TO Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9A3, VarStoreId: 0x1, VarOffset: 0xAF0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SEFE", Help: "Root PCI Express System Error on Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9A4, VarStoreId: 0x1, VarOffset: 0xB20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SENFE", Help: "Root PCI Express System Error on Non-Fatal Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9A5, VarStoreId: 0x1, VarOffset: 0xB38, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  SECE", Help: "Root PCI Express System Error on Correctable Error Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9A6, VarStoreId: 0x1, VarOffset: 0xB50, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  PME SCI", Help: "PCI Express PME SCI Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9A7, VarStoreId: 0x1, VarOffset: 0xB68, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "  Hot Plug", Help: "PCI Express Hot Plug Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9A8, VarStoreId: 0x1, VarOffset: 0xB80, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: "  Advanced Error Reporting", Help: "Advanced Error Reporting Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9A9, VarStoreId: 0x1, VarOffset: 0xB98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			OneOf Prompt: "PCIe Speed", Help: "Configure PCIe Speed", QuestionFlags: 0x10, QuestionId: 0x9AA, VarStoreId: 0x1, VarOffset: 0xBB0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "Gen1" Value: 1
				OneOfOption Option: "Gen2" Value: 2
				OneOfOption Option: "Gen3" Value: 3
			End 
			OneOf Prompt: "  Transmitter Half Swing", Help: "Transmitter Half Swing Enable/Disable.", QuestionFlags: 0x10, QuestionId: 0x9AB, VarStoreId: 0x1, VarOffset: 0xBC8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Detect Timeout", Help: "The number of milliseconds reference code will wait for link to exit Detect state for enabled ports before assuming there is no device and potentially disabling the port.", QuestionFlags: 0x0, QuestionId: 0x9AC, VarStoreId: 0x1, VarOffset: 0xFE6, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x27CB, Value: 0x1
					EqIdVal QuestionId: 0x338, Value: 0x1
					And 
				End 
				Numeric Prompt: "Extra Bus Reserved", Help: "Extra Bus Reserved (0-7) for bridges behind this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x9AD, VarStoreId: 0x1, VarOffset: 0xDE5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "Reserved Memory", Help: "Reserved Memory for this Root Bridge (1-20) MB", QuestionFlags: 0x0, QuestionId: 0x9AE, VarStoreId: 0x1, VarOffset: 0xE14, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x18, Step: 0x1
					Default DefaultId: 0x0 Value: 10
				End 
				Numeric Prompt: "Reserved I/O", Help: "Reserved I/O (4K/8K/12K/16K/20K) Range for this Root Bridge.", QuestionFlags: 0x0, QuestionId: 0x9AF, VarStoreId: 0x1, VarOffset: 0xE2D, Flags: 0x10, Size: 8, Min: 0x4, Max: 0x18, Step: 0x4
					Default DefaultId: 0x0 Value: 4
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe LTR Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCH PCIE24 LTR", Help: "PCH PCIE Latency Reporting Enable/Disable", QuestionFlags: 0x10, QuestionId: 0x9B0, VarStoreId: 0x1, VarOffset: 0xCAC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x9B0, Value: 0x0
				OneOf Prompt: "  Snoop Latency Override", Help: "Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x9B1, VarStoreId: 0x1, VarOffset: 0xCDC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x9B1, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Snoop Latency Value", Help: "LTR Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x9B2, VarStoreId: 0x1, VarOffset: 0xD53, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Snoop Latency Multiplier", Help: "LTR Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x9B3, VarStoreId: 0x1, VarOffset: 0xCF4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Non Snoop Latency Override", Help: "Non Snoop Latency Override for PCH PCIE.
Disabled: Disable override.
Manual: Manually enter override values.
Auto (default): Maintain default BIOS flow.", QuestionFlags: 0x10, QuestionId: 0x9B4, VarStoreId: 0x1, VarOffset: 0xD0C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Manual" Value: 1
					OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x9B4, Value: 0x1
						Not 
					End 
					Numeric Prompt: "    Non Snoop Latency Value", Help: "LTR Non Snoop Latency value of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x9B5, VarStoreId: 0x1, VarOffset: 0xD83, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x3FF, Step: 0x1
						Default DefaultId: 0x0 Value: 60
					End 
					OneOf Prompt: "    Non Snoop Latency Multiplier", Help: "LTR Non Snoop Latency Multiplier of PCH PCIE", QuestionFlags: 0x10, QuestionId: 0x9B6, VarStoreId: 0x1, VarOffset: 0xD24, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
						OneOfOption Option: "1 ns" Value: 0
						OneOfOption Option: "32 ns" Value: 1
						OneOfOption Option: "1024 ns" Value: 2, Default, MfgDefault
						OneOfOption Option: "32768 ns" Value: 3
						OneOfOption Option: "1048576 ns" Value: 4
						OneOfOption Option: "33554432 ns" Value: 5
					End 
				End 
				OneOf Prompt: "  Force LTR Override", Help: "Force LTR Override for PCH PCIE.
Disabled: LTR override values will not be forced.
Enable: LTR override values will be forced and LTR messages from the device will be ignored.", QuestionFlags: 0x10, QuestionId: 0x9B7, VarStoreId: 0x1, VarOffset: 0xD9C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE24 LTR Lock", Help: "PCIE LTR Configuration Lock", QuestionFlags: 0x10, QuestionId: 0x9B8, VarStoreId: 0x1, VarOffset: 0xCC4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Subtitle Prompt: "PCH PCIe CLKREQ# Configuration", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "PCIE20 CLKREQ Mapping Override", Help: "PCIE CLKREQ Override for default platform mapping.", QuestionFlags: 0x10, QuestionId: 0x9B9, VarStoreId: 0x1, VarOffset: 0xDB4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Default" Value: 0, Default, MfgDefault
				OneOfOption Option: "No CLKREQ" Value: 1
				OneOfOption Option: "Custom number" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x9B9, Value: 0x2
					Not 
				End 
				Numeric Prompt: "      CLKREQ Number", Help: "PCIE CLKREQ Number to be set (LP[0:5], H[0:15])", QuestionFlags: 0x10, QuestionId: 0x9BA, VarStoreId: 0x1, VarOffset: 0xDCC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xF, Step: 0x0
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Extra options ", Help: "PCI Express Root Port extra options.", QuestionFlags: 0x0, QuestionId: 0x9BB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27FA
		End 
	End 
	Form FormId: 0x2772, Title: "HD Audio Configuration"
		Subtitle Prompt: "HD Audio Subsystem Configuration Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "HD Audio", Help: "Control Detection of the HD-Audio device.

Disabled = HDA will be unconditionally disabled

Enabled = HDA will be unconditionally enabled

Auto = HDA will be enabled if present, disabled otherwise.", QuestionFlags: 0x10, QuestionId: 0x9BC, VarStoreId: 0x1, VarOffset: 0xE2E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			OneOfOption Option: "Auto" Value: 2
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x9BC, Value: 0x0
				OneOf Prompt: " Audio DSP", Help: "Enable/Disable Audio DSP.", QuestionFlags: 0x10, QuestionId: 0x9BD, VarStoreId: 0x1, VarOffset: 0xE2F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				SuppressIf 
					EqIdVal QuestionId: 0x9BD, Value: 0x0
					OneOf Prompt: " Audio DSP Compliance Mode", Help: "Specifies DSP enabled system compliance:
1. Non-UAA (IntelSST driver support only - CC_040100)
2. UAA (HD Audio Inbox or IntelSST driver support - CC_040380)

Note: NHLT (DMIC/BT/I2S configuration) is published for non-UAA only.", QuestionFlags: 0x10, QuestionId: 0x9BE, VarStoreId: 0x1, VarOffset: 0xE30, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
						OneOfOption Option: "Non-UAA (IntelSST)" Value: 0, Default, MfgDefault
						OneOfOption Option: "UAA (HDA Inbox/IntelSST)" Value: 1
					End 
				End 
				OneOf Prompt: " HDA-Link Codec Select", Help: "Selects whether Platform Onboard Codec (single Verb Table installed) or External Codec Kit (multiple Verb Tables installed) will be used.", QuestionFlags: 0x10, QuestionId: 0x9BF, VarStoreId: 0x1, VarOffset: 0xE38, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Platform Onboard" Value: 0, Default, MfgDefault
					OneOfOption Option: "External Kit" Value: 1
				End 
				OneOf Prompt: " iDisplay Audio Disconnect", Help: "Disconnects SDI2 signal to hide/disable iDisplay Audio Codec.", QuestionFlags: 0x10, QuestionId: 0x9C0, VarStoreId: 0x1, VarOffset: 0xE31, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
				OneOf Prompt: " PME Enable", Help: "Enables PME wake of HD Audio controller during POST.", QuestionFlags: 0x10, QuestionId: 0x9C1, VarStoreId: 0x1, VarOffset: 0xE32, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC42, Value: 0x0
					EqIdVal QuestionId: 0xC42, Value: 0x1
					Or 
				End 
				Ref Prompt: "HD Audio Advanced Configuration", Help: "HD Audio Subsystem Advanced Configuration Settings", QuestionFlags: 0x0, QuestionId: 0x9C2, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2773
			End 
			SuppressIf 
				EqIdVal QuestionId: 0x9BD, Value: 0x0
				Ref Prompt: "HD Audio DSP Features Configuration", Help: "HD Audio Subsystem Features Configuration (ACPI)", QuestionFlags: 0x0, QuestionId: 0x9C3, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2774
			End 
		End 
	End 
	Form FormId: 0x2773, Title: "HD Audio Advanced Configuration"
		Subtitle Prompt: "HD Audio Subsystem Advanced Configuration Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "I/O Buffer Control:", Help: "I/O buffer control based on the motherboard configuration.", Text: ""
		OneOf Prompt: " I/O Buffer Ownership", Help: "Selects the ownership of the I/O buffer between Intel HD Audio link vs I2S port (for bilingual codecs).", QuestionFlags: 0x10, QuestionId: 0x9C4, VarStoreId: 0x1, VarOffset: 0xE33, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
			OneOfOption Option: "HD-Audio Link" Value: 0, Default, MfgDefault
			OneOfOption Option: "HD-Audio Link / I2S Port" Value: 1
			OneOfOption Option: "I2S Port" Value: 3
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9C4, Value: 0x0
			OneOf Prompt: " I2S Configuration Select", Help: "Selects I2S Audio Codec support.", QuestionFlags: 0x10, QuestionId: 0x9C5, VarStoreId: 0x1, VarOffset: 0xE39, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Realtek ALC298" Value: 1
				OneOfOption Option: "Realtek ALC286S" Value: 2
				OneOfOption Option: "Analog Devices SSM4567" Value: 3
				OneOfOption Option: "24bit 48kHz Master" Value: 4
				OneOfOption Option: "24bit 48kHz Slave" Value: 5
				OneOfOption Option: "PCM 16bit 8kHz Master" Value: 6
				OneOfOption Option: "PCM 16bit 8kHz Slave" Value: 7
			End 
		End 
		OneOf Prompt: " I/O Buffer Voltage Select", Help: "Selects the voltage operation mode of the I/O buffer.", QuestionFlags: 0x10, QuestionId: 0x9C6, VarStoreId: 0x1, VarOffset: 0xE34, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "3.3V" Value: 0, Default, MfgDefault
			OneOfOption Option: "1.8V" Value: 1
		End 
		Text Prompt: "Statically Switchable BCLK Clock Frequency Configuration:", Help: "Statically Switchable BCLK Clock Frequency Configuration:", Text: ""
		OneOf Prompt: " HD Audio Link Frequency", Help: "Selects HD Audio Link frequency.
Applicable only if HDA codec supports selected frequency.", QuestionFlags: 0x10, QuestionId: 0x9C7, VarStoreId: 0x1, VarOffset: 0xE35, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "6 MHz" Value: 0
			OneOfOption Option: "12 MHz" Value: 1
			OneOfOption Option: "24 MHz" Value: 2, Default
		End 
		OneOf Prompt: " iDisplay Link Frequency", Help: "Selects iDisplay Link frequency.
Applicable only if iDisp codec supports selected frequency.", QuestionFlags: 0x10, QuestionId: 0x9C8, VarStoreId: 0x1, VarOffset: 0xE36, Flags: 0x10, Size: 8, Min: 0x3, Max: 0x4, Step: 0x0
			OneOfOption Option: "48 MHz" Value: 3
			OneOfOption Option: "96 MHz" Value: 4, Default
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9C8, Value: 0x4
			OneOf Prompt: "  iDisplay Link T-Mode", Help: "Selects iDisplay Link T-Mode for 48MHz:
2T - SDI data held for 2 BCLKs.
1T - SDI data held for 1 BCLK.", QuestionFlags: 0x10, QuestionId: 0x9C9, VarStoreId: 0x1, VarOffset: 0xE37, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "2T Mode" Value: 0, Default, MfgDefault
				OneOfOption Option: "1T Mode" Value: 1
			End 
		End 
	End 
	Form FormId: 0x2774, Title: "HD Audio DSP Features Configuration"
		Subtitle Prompt: "HD Audio Subsystem Features Configuration (ACPI)", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9BE, Value: 0x0
				Not 
			End 
			Text Prompt: "Audio DSP NHLT Endpoints Configuration:", Help: "Audio DSP NHLT Endpoints Configuration:", Text: ""
			OneOf Prompt: " DMIC", Help: "Selects DMIC to expose in NHLT ACPI table
", QuestionFlags: 0x10, QuestionId: 0x9CA, VarStoreId: 0x1, VarOffset: 0xE3A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "4 Mic Array" Value: 2, Default, MfgDefault
				OneOfOption Option: "2 Mic Array" Value: 1
				OneOfOption Option: "1 Mic Array" Value: 3
				OneOfOption Option: "Disabled" Value: 0
			End 
			OneOf Prompt: " Bluetooth", Help: "Enables/Disables Bluetooth Endpoint in NHLT ACPI table
", QuestionFlags: 0x10, QuestionId: 0x9CB, VarStoreId: 0x1, VarOffset: 0xE3B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default
				OneOfOption Option: "Enabled" Value: 1
			End 
			OneOf Prompt: " I2S", Help: "Enables/Disables I2S Endpoint in NHLT ACPI table.
Can be enabled only for I2S codec mode (HDA Advanced Configuration):
1. I/O Buffer Ownership <I2S Port>
2. I2S Codec Select", QuestionFlags: 0x10, QuestionId: 0x9CC, VarStoreId: 0x1, VarOffset: 0xE3C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default
				SuppressIf 
					EqIdVal QuestionId: 0x9C5, Value: 0x0
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "Audio DSP Feature Support:", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", Text: ""
		CheckBox Prompt: " WoV (Wake on Voice)", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0x9CD, VarStoreId: 0x1, VarOffset: 0xE3D, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			Default DefaultId: 0x0 Value: 0
		End 
		CheckBox Prompt: " Bluetooth Sideband", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0x9CE, VarStoreId: 0x1, VarOffset: 0xE3E, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9CE, Value: 0x0
			CheckBox Prompt: " BT Intel HFP", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0x9CF, VarStoreId: 0x1, VarOffset: 0xE42, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			CheckBox Prompt: " BT Intel A2DP", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0x9D0, VarStoreId: 0x1, VarOffset: 0xE43, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
		End 
		CheckBox Prompt: " Codec based VAD", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0x9D1, VarStoreId: 0x1, VarOffset: 0xE3F, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9D3, Value: 0x1
			CheckBox Prompt: " DSP based Speech
 Pre-Processing Disabled", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0x9D2, VarStoreId: 0x1, VarOffset: 0xE44, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		OneOf Prompt: " Voice Activity Detection", Help: "Enables/Disables DSP Feature.
Bitmask structure:
[BIT0] - WoV
[BIT1] - BT Sideband
[BIT2] - Codec based VAD
[BIT5] - BT Intel HFP
[BIT6] - BT Intel A2DP
[BIT7] - DSP based speech pre-processing disabled (for Intel WoV mode)
[BIT8] - WoV Mode: Intel WoV / Windows Voice Activation for Cortana", QuestionFlags: 0x10, QuestionId: 0x9D3, VarStoreId: 0x1, VarOffset: 0xE45, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Intel Wake on Voice" Value: 0, Default
			OneOfOption Option: "Windows 10 Voice Activation" Value: 1
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Text Prompt: "Audio DSP Pre/Post-Processing Module Support:", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", Text: ""
		CheckBox Prompt: " Waves Post-process", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9D4, VarStoreId: 0x1, VarOffset: 0xE46, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " DTS", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9D5, VarStoreId: 0x1, VarOffset: 0xE47, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " IntelSST Speech", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9D6, VarStoreId: 0x1, VarOffset: 0xE48, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			Default DefaultId: 0x0 Value: 0
		End 
		CheckBox Prompt: " Dolby", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9D7, VarStoreId: 0x1, VarOffset: 0xE49, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " Waves Pre-process", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9D8, VarStoreId: 0x1, VarOffset: 0xE4A, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " Audyssey", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9D9, VarStoreId: 0x1, VarOffset: 0xE4B, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " Maxim Smart AMP", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9DA, VarStoreId: 0x1, VarOffset: 0xE4C, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " ForteMedia SAMSoft", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9DB, VarStoreId: 0x1, VarOffset: 0xE4D, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9CD, Value: 0x0
			CheckBox Prompt: " Intel WoV", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9DC, VarStoreId: 0x1, VarOffset: 0xE4E, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		CheckBox Prompt: " Sound Research IP", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9DD, VarStoreId: 0x1, VarOffset: 0xE4F, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " Conexant Pre-Process", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9DE, VarStoreId: 0x1, VarOffset: 0xE50, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " Conexant Smart Amp", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9DF, VarStoreId: 0x1, VarOffset: 0xE51, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " Realtek Post-Process", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9E0, VarStoreId: 0x1, VarOffset: 0xE52, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " Realtek Smart Amp", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9E1, VarStoreId: 0x1, VarOffset: 0xE53, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " Icepower IP MFX sub module", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9E2, VarStoreId: 0x1, VarOffset: 0xE54, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " Icepower IP EFX sub module", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9E3, VarStoreId: 0x1, VarOffset: 0xE55, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " Icepower IP SFX sub module", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9E4, VarStoreId: 0x1, VarOffset: 0xE56, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		CheckBox Prompt: " Custom Module 'Alpha'", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9E5, VarStoreId: 0x1, VarOffset: 0xE63, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9E5, Value: 0x0
			String Prompt: " 'Alpha' GUID:", Help: "Input hex digit character in aabbccdd-eeff-gghh-iijj-kkllmmnnoopp format.", QuestionFlags: 0x10, QuestionId: 0x9E6, VarStoreId: 0x1, VarStoreInfo: 0xE66, MinSize: 0x24, MaxSize: 0x24, Flags: 0x0
			End 
		End 
		CheckBox Prompt: " Custom Module 'Beta'", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9E7, VarStoreId: 0x1, VarOffset: 0xE64, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9E7, Value: 0x0
			String Prompt: " 'Beta'  GUID:", Help: "Input hex digit character in aabbccdd-eeff-gghh-iijj-kkllmmnnoopp format.", QuestionFlags: 0x10, QuestionId: 0x9E8, VarStoreId: 0x1, VarStoreInfo: 0xEB0, MinSize: 0x24, MaxSize: 0x24, Flags: 0x0
			End 
		End 
		CheckBox Prompt: " Custom Module 'Gamma'", Help: "Enables/Disables 3rd Party Processing Module Support (identified by GUID).
WoV must be enabled as a feature first to select relevant WoV IP.", QuestionFlags: 0x10, QuestionId: 0x9E9, VarStoreId: 0x1, VarOffset: 0xE65, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9E9, Value: 0x0
			String Prompt: " 'Gamma' GUID:", Help: "Input hex digit character in aabbccdd-eeff-gghh-iijj-kkllmmnnoopp format.", QuestionFlags: 0x10, QuestionId: 0x9EA, VarStoreId: 0x1, VarStoreInfo: 0xEFA, MinSize: 0x24, MaxSize: 0x24, Flags: 0x0
			End 
		End 
	End 
	Form FormId: 0x2775, Title: "Security Configuration"
		Subtitle Prompt: "Security Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "RTC Lock", Help: "Enable will lock bytes 38h-3Fh in the lower/upper 128-byte bank of RTC RAM", QuestionFlags: 0x10, QuestionId: 0x9EB, VarStoreId: 0x1, VarOffset: 0x9A0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			Default DefaultId: 0x0 Value: 1
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, MfgDefault
		End 
		SuppressIf 
			EqIdValList QuestionId: 0x37B, Values: [1]
			OneOf Prompt: "BIOS Lock", Help: "Enable/Disable the PCH BIOS Lock Enable feature. Required to be enabled to ensure SMM protection of flash.", QuestionFlags: 0x10, QuestionId: 0x9EC, VarStoreId: 0x1, VarOffset: 0x9A1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x0 Value: 0
				OneOfOption Option: "Disabled" Value: 0, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
	End 
	Form FormId: 0x2776, Title: "SerialIo Configuration"
		Subtitle Prompt: "SerialIo Configuration", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC50, Value: 0x20
				Not 
			End 
			OneOf Prompt: "Touch Panel", Help: "Configure GPIO to select between Integrated (SPI) Touch or I2C Touch", QuestionFlags: 0x10, QuestionId: 0x9ED, VarStoreId: 0x1, VarOffset: 0x2AA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "SPI Touch" Value: 0, Default, MfgDefault
				OneOfOption Option: "I2C Touch" Value: 1
			End 
			OneOf Prompt: "BT/UART Mux Select", Help: "Configure GPIO to select between BT or UART signals to go to M.2 module", QuestionFlags: 0x10, QuestionId: 0x9EE, VarStoreId: 0x1, VarOffset: 0x2AB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "UART Signal" Value: 0, Default, MfgDefault
				OneOfOption Option: "BT Signal" Value: 1
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9F0, Value: 0x1
				EqIdVal QuestionId: 0x9F1, Value: 0x1
				Or 
				EqIdVal QuestionId: 0x9F2, Value: 0x1
				Or 
			End 
			OneOf Prompt: "I2C0 Controller", Help: "Enables/Disables SerialIo Controller
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5", QuestionFlags: 0x10, QuestionId: 0x9EF, VarStoreId: 0x1, VarOffset: 0xF5E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9EF, Value: 0x0
			OneOf Prompt: "I2C1 Controller", Help: "Enables/Disables SerialIo Controller
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5", QuestionFlags: 0x10, QuestionId: 0x9F0, VarStoreId: 0x1, VarOffset: 0xF5F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9EF, Value: 0x0
			OneOf Prompt: "I2C2 Controller", Help: "Enables/Disables SerialIo Controller
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5", QuestionFlags: 0x10, QuestionId: 0x9F1, VarStoreId: 0x1, VarOffset: 0xF60, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9EF, Value: 0x0
			OneOf Prompt: "I2C3 Controller", Help: "Enables/Disables SerialIo Controller
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5", QuestionFlags: 0x10, QuestionId: 0x9F2, VarStoreId: 0x1, VarOffset: 0xF61, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC50, Values: [4, 20, 10, 26, 8, 11, 7, 19, 3, 27, 12]
				EqIdVal QuestionId: 0xC51, Value: 0x2
				Not 
				Or 
			End 
			OneOf Prompt: "I2C4 Controller", Help: "Enables/Disables SerialIo Controller
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5", QuestionFlags: 0x10, QuestionId: 0x9F3, VarStoreId: 0x1, VarOffset: 0xF62, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				SuppressIf 
					EqIdVal QuestionId: 0x9F9, Value: 0x0
					OneOfOption Option: "Enabled in PCI Mode" Value: 1
				End 
				OneOfOption Option: "Enabled in ACPI Mode" Value: 2
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC50, Values: [4, 20, 10, 26, 8, 11, 7, 19, 3, 27, 12]
				Not 
			End 
			Text Prompt: "I2C4 Controller", Help: "", Text: "used for IoExpander"
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC51, Value: 0x2
				Not 
			End 
			OneOf Prompt: "I2C5 Controller", Help: "Enables/Disables SerialIo Controller
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5", QuestionFlags: 0x10, QuestionId: 0x9F4, VarStoreId: 0x1, VarOffset: 0xF63, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				SuppressIf 
					EqIdVal QuestionId: 0x9F9, Value: 0x0
					OneOfOption Option: "Enabled in PCI Mode" Value: 1
				End 
				OneOfOption Option: "Enabled in ACPI Mode" Value: 2
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9F7, Value: 0x0
			OneOf Prompt: "SPI0 Controller", Help: "Enables/Disables SerialIo Controller
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5", QuestionFlags: 0x10, QuestionId: 0x9F5, VarStoreId: 0x1, VarOffset: 0xF64, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9F7, Value: 0x0
			OneOf Prompt: "SPI1 Controller", Help: "Enables/Disables SerialIo Controller
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5", QuestionFlags: 0x10, QuestionId: 0x9F6, VarStoreId: 0x1, VarOffset: 0xF65, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9F8, Value: 0x1
				EqIdVal QuestionId: 0x9F5, Value: 0x1
				Or 
				EqIdVal QuestionId: 0x9F6, Value: 0x1
				Or 
				EqIdVal QuestionId: 0xC51, Value: 0x2
				EqIdVal QuestionId: 0xA62, Value: 0x1
				EqIdVal QuestionId: 0xA65, Value: 0x1
				Or 
				And 
				Or 
			End 
			OneOf Prompt: "UART0 Controller", Help: "Enables/Disables SerialIo Controller
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5", QuestionFlags: 0x10, QuestionId: 0x9F7, VarStoreId: 0x1, VarOffset: 0xF66, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9F7, Value: 0x0
				EqIdVal QuestionId: 0x542, Value: 0x1
				Or 
			End 
			OneOf Prompt: "UART1 Controller", Help: "Enables/Disables SerialIo Controller
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5", QuestionFlags: 0x10, QuestionId: 0x9F8, VarStoreId: 0x1, VarOffset: 0xF67, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x541, Value: 0x3
			GrayOutIf 
				EqIdVal QuestionId: 0x9F3, Value: 0x1
					EqIdVal QuestionId: 0x9F4, Value: 0x1
					Or 
				End 
				OneOf Prompt: "UART2 Controller", Help: "Enables/Disables SerialIo Controller
The following devices depend on each other:
I2C0 and I2C1,2,3
UART0 and UART1,SPI0,1
UART2 and I2C4,5", QuestionFlags: 0x10, QuestionId: 0x9F9, VarStoreId: 0x1, VarOffset: 0xF68, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "Enabled" Value: 1
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x541, Value: 0x3
				Not 
			End 
			Text Prompt: "UART2 Controller", Help: "", Text: "used as debug port"
		End 
		OneOf Prompt: "GPIO Controller", Help: "Enables/Disables the GPIO Controller", QuestionFlags: 0x10, QuestionId: 0x9FA, VarStoreId: 0x1, VarOffset: 0xF69, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9EF, Value: 0x0
			Ref Prompt: "Serial IO I2C0 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0x9FB, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2778
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9F0, Value: 0x0
			Ref Prompt: "Serial IO I2C1 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0x9FC, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2779
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9F1, Value: 0x0
			Ref Prompt: "Serial IO I2C2 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0x9FD, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x277A
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9F2, Value: 0x0
			Ref Prompt: "Serial IO I2C3 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0x9FE, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x277B
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC50, Values: [4, 20, 10, 26, 8, 11, 7, 19, 3, 27, 12]
				EqIdVal QuestionId: 0x9F3, Value: 0x0
				Or 
			End 
			Ref Prompt: "Serial IO I2C4 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0x9FF, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x277C
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9F4, Value: 0x0
			Ref Prompt: "Serial IO I2C5 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xA00, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x277D
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9F5, Value: 0x0
			Ref Prompt: "Serial IO SPI0 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xA01, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x277E
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9F6, Value: 0x0
			Ref Prompt: "Serial IO SPI1 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xA02, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x277F
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9F7, Value: 0x0
				EqIdVal QuestionId: 0x541, Value: 0x1
				Or 
			End 
			Ref Prompt: "Serial IO UART0 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xA03, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2780
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9F8, Value: 0x0
				EqIdVal QuestionId: 0x541, Value: 0x2
				Or 
			End 
			Ref Prompt: "Serial IO UART1 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xA04, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2781
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9F9, Value: 0x0
			Ref Prompt: "Serial IO UART2 Settings", Help: "Configure SerialIo Controller", QuestionFlags: 0x0, QuestionId: 0xA05, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2782
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x9FA, Value: 0x0
			Ref Prompt: "Serial IO GPIO Settings", Help: "Serial IO GPIO Settings", QuestionFlags: 0x0, QuestionId: 0xA06, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2783
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "WITT/MITT Test Device", Help: "Choose if WITT Device is used and with which controller", QuestionFlags: 0x10, QuestionId: 0xA07, VarStoreId: 0x1, VarOffset: 0x284, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x8, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled - I2C0" Value: 1
			OneOfOption Option: "Enabled - I2C1" Value: 2
			OneOfOption Option: "Enabled - I2C2" Value: 3
			OneOfOption Option: "Enabled - I2C3" Value: 4
			OneOfOption Option: "Enabled - I2C4" Value: 5
			OneOfOption Option: "Enabled - I2C5" Value: 6
			OneOfOption Option: "Enabled - SPI0" Value: 7
			OneOfOption Option: "Enabled - SPI1" Value: 8
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA07, Value: 0x0
			OneOf Prompt: "WITT/MITT Device selection", Help: "Change WITT Device version", QuestionFlags: 0x10, QuestionId: 0xA08, VarStoreId: 0x1, VarOffset: 0x285, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "WITT" Value: 0
				OneOfOption Option: "MITT" Value: 1, Default, MfgDefault
			End 
		End 
		OneOf Prompt: "UART Test Device", Help: "Choose if UART Test Device is used and with which controller", QuestionFlags: 0x10, QuestionId: 0xA09, VarStoreId: 0x1, VarOffset: 0x286, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled - UART0" Value: 1
			OneOfOption Option: "Enabled - UART1" Value: 2
			OneOfOption Option: "Enabled - UART2" Value: 3
		End 
		CheckBox Prompt: "Additional Serial IO devices", Help: "When enabled, ACPI will report additional devices connected to Serial IO.", QuestionFlags: 0x10, QuestionId: 0xA0A, VarStoreId: 0x1, VarOffset: 0xF6B, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		Ref Prompt: "SerialIO timing parameters", Help: "SerialIO timing parameters (test only)", QuestionFlags: 0x0, QuestionId: 0xA0B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2777
		OneOf Prompt: "UCSI/UCMC device", Help: "When enabled, ACPI will report UCSI/UCMC device", QuestionFlags: 0x10, QuestionId: 0xA0C, VarStoreId: 0x1, VarOffset: 0xFB7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
	End 
	Form FormId: 0x2777, Title: "SerialIO timing parameters"
		CheckBox Prompt: "SerialIO timing parameters", Help: "SerialIO timing parameters (test only)", QuestionFlags: 0x10, QuestionId: 0xA0D, VarStoreId: 0x1, VarOffset: 0x28A, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA0D, Value: 0x0
			Numeric Prompt: "StandardSpeed SCL High for I2C1", Help: "StandardSpeed SCL High for I2C1", QuestionFlags: 0x0, QuestionId: 0xA0E, VarStoreId: 0x1, VarOffset: 0x28B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
				Default DefaultId: 0x0 Value: 528
			End 
			Numeric Prompt: "StandardSpeed SCL Low for I2C1", Help: "StandardSpeed SCL Low for I2C1", QuestionFlags: 0x0, QuestionId: 0xA0F, VarStoreId: 0x1, VarOffset: 0x28D, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
				Default DefaultId: 0x0 Value: 640
			End 
			Numeric Prompt: "StandardSpeed SDA Hold for I2C1", Help: "StandardSpeed SDA Hold for I2C1", QuestionFlags: 0x0, QuestionId: 0xA10, VarStoreId: 0x1, VarOffset: 0x28F, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
				Default DefaultId: 0x0 Value: 30
			End 
			Numeric Prompt: "FastSpeed SCL High for I2C1", Help: "FastSpeed SCL High for I2C1", QuestionFlags: 0x0, QuestionId: 0xA11, VarStoreId: 0x1, VarOffset: 0x291, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
				Default DefaultId: 0x0 Value: 128
			End 
			Numeric Prompt: "FastSpeed SCL Low for I2C1", Help: "FastSpeed SCL Low for I2C1", QuestionFlags: 0x0, QuestionId: 0xA12, VarStoreId: 0x1, VarOffset: 0x293, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
				Default DefaultId: 0x0 Value: 160
			End 
			Numeric Prompt: "FastSpeed SDA Hold for I2C1", Help: "FastSpeed SDA Hold for I2C1", QuestionFlags: 0x0, QuestionId: 0xA13, VarStoreId: 0x1, VarOffset: 0x295, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
				Default DefaultId: 0x0 Value: 30
			End 
			Numeric Prompt: "FastSpeedPlus SCL High for I2C1", Help: "FastSpeedPlus SCL High for I2C1", QuestionFlags: 0x0, QuestionId: 0xA14, VarStoreId: 0x1, VarOffset: 0x297, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
				Default DefaultId: 0x0 Value: 48
			End 
			Numeric Prompt: "FastSpeedPlus SCL Low for I2C1", Help: "FastSpeedPlus SCL Low for I2C1", QuestionFlags: 0x0, QuestionId: 0xA15, VarStoreId: 0x1, VarOffset: 0x299, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
				Default DefaultId: 0x0 Value: 64
			End 
			Numeric Prompt: "FastSpeedPlus SDA Hold for I2C1", Help: "FastSpeedPlus SDA Hold for I2C1", QuestionFlags: 0x0, QuestionId: 0xA16, VarStoreId: 0x1, VarOffset: 0x29B, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
				Default DefaultId: 0x0 Value: 30
			End 
			Numeric Prompt: "D0->D3 idle timeout for I2C1 (screen off)", Help: "D0->D3 idle timeout (screen off)", QuestionFlags: 0x0, QuestionId: 0xA17, VarStoreId: 0x1, VarOffset: 0x29D, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0
				Default DefaultId: 0x0 Value: 200
			End 
			Numeric Prompt: "D0->D3 idle timeout for I2C1 (screen on)", Help: "D0->D3 idle timeout (screen on)", QuestionFlags: 0x0, QuestionId: 0xA18, VarStoreId: 0x1, VarOffset: 0x29F, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0
				Default DefaultId: 0x0 Value: 2000
			End 
			Numeric Prompt: "D0->D3 idle timeout for SPI1 (screen off)", Help: "D0->D3 idle timeout (screen off)", QuestionFlags: 0x0, QuestionId: 0xA19, VarStoreId: 0x1, VarOffset: 0x2A1, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0
				Default DefaultId: 0x0 Value: 200
			End 
			Numeric Prompt: "D0->D3 idle timeout for SPI1 (screen on)", Help: "D0->D3 idle timeout (screen on)", QuestionFlags: 0x0, QuestionId: 0xA1A, VarStoreId: 0x1, VarOffset: 0x2A3, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0
				Default DefaultId: 0x0 Value: 2000
			End 
			Numeric Prompt: "D0->D3 idle timeout for UART1 (screen off)", Help: "D0->D3 idle timeout (screen off)", QuestionFlags: 0x0, QuestionId: 0xA1B, VarStoreId: 0x1, VarOffset: 0x2A5, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0
				Default DefaultId: 0x0 Value: 200
			End 
			Numeric Prompt: "D0->D3 idle timeout for UART1 (screen on)", Help: "D0->D3 idle timeout (screen on)", QuestionFlags: 0x0, QuestionId: 0xA1C, VarStoreId: 0x1, VarOffset: 0x2A7, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x2710, Step: 0x0
				Default DefaultId: 0x0 Value: 200
			End 
		End 
	End 
	Form FormId: 0x2778, Title: "Serial IO I2C0 Settings"
		Subtitle Prompt: "Serial IO I2C0 Settings", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "I2C IO Voltage Select", Help: "Selects 1.8v or 3.3v for the controller.", QuestionFlags: 0x10, QuestionId: 0xA1D, VarStoreId: 0x1, VarOffset: 0xF6F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "3.3V" Value: 0, Default, MfgDefault
			OneOfOption Option: "1.8V" Value: 1
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Connected device", Help: "Indicates what type of device is connected to this SerialIo controller", QuestionFlags: 0x10, QuestionId: 0xA1E, VarStoreId: 0x1, VarOffset: 0x26D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Synaptics Precision Touchpad" Value: 1
			OneOfOption Option: "Synaptics Forcepad" Value: 2
			OneOfOption Option: "ALPS Precision Touchpad ClickPad" Value: 6
			SuppressIf 
				EqIdVal QuestionId: 0xC50, Value: 0x20
					Not 
				End 
				OneOfOption Option: "SAR SX9306 Sensor" Value: 3
				OneOfOption Option: "SAR SX9310 Sensor" Value: 4
			End 
			OneOfOption Option: "Custom device" Value: 5
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA1E, Value: 0x0
				EqIdVal QuestionId: 0xA1E, Value: 0x3
				Or 
				EqIdVal QuestionId: 0xA1E, Value: 0x4
				Or 
			End 
			OneOf Prompt: "Interrupt mode", Help: "Selects different routing for interrupts from external device", QuestionFlags: 0x10, QuestionId: 0xA1F, VarStoreId: 0x1, VarOffset: 0x272, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "GPIO Interrupt" Value: 0
				OneOfOption Option: "APIC Interrupt" Value: 1, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA1E, Value: 0x5
				Not 
			End 
			Numeric Prompt: "Device's bus address", Help: "Specify parameters of custom I2C device", QuestionFlags: 0x10, QuestionId: 0xA20, VarStoreId: 0x1, VarOffset: 0x26E, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "Device's HID address", Help: "Specify parameters of custom I2C device", QuestionFlags: 0x10, QuestionId: 0xA21, VarStoreId: 0x1, VarOffset: 0x26F, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "Device's bus speed", Help: "Specify parameters of custom I2C device", QuestionFlags: 0x10, QuestionId: 0xA22, VarStoreId: 0x1, VarOffset: 0x271, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "100kHz" Value: 0, Default, MfgDefault
				OneOfOption Option: "400kHz" Value: 1
				OneOfOption Option: "1MHz" Value: 2
			End 
		End 
	End 
	Form FormId: 0x2779, Title: "Serial IO I2C1 Settings"
		Subtitle Prompt: "Serial IO I2C1 Settings", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "I2C IO Voltage Select", Help: "Selects 1.8v or 3.3v for the controller.", QuestionFlags: 0x10, QuestionId: 0xA23, VarStoreId: 0x1, VarOffset: 0xF70, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "3.3V" Value: 0, Default, MfgDefault
			OneOfOption Option: "1.8V" Value: 1
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Connected device", Help: "Indicates what type of device is connected to this SerialIo controller", QuestionFlags: 0x10, QuestionId: 0xA24, VarStoreId: 0x1, VarOffset: 0x273, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Atmel3432 TouchPanel" Value: 1
			OneOfOption Option: "Atmel2952 TouchPanel" Value: 2
			OneOfOption Option: "Elan2097 TouchPanel" Value: 3
			OneOfOption Option: "N-Trig/Samsung 13.3"" Value: 4
			OneOfOption Option: "N-Trig/Sharp 12.5"" Value: 5
			OneOfOption Option: "WACOM9015 TouchPanel"" Value: 6
			OneOfOption Option: "Custom device" Value: 7
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA24, Value: 0x0
			OneOf Prompt: "Interrupt mode", Help: "Selects different routing for interrupts from external device", QuestionFlags: 0x10, QuestionId: 0xA25, VarStoreId: 0x1, VarOffset: 0x274, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "GPIO Interrupt" Value: 0
				OneOfOption Option: "APIC Interrupt" Value: 1, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA24, Value: 0x6
				Not 
			End 
			OneOf Prompt: "Device's bus speed", Help: "Specify parameters of custom I2C device", QuestionFlags: 0x10, QuestionId: 0xA26, VarStoreId: 0x1, VarOffset: 0x279, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "400kHz" Value: 0
				OneOfOption Option: "1MHz" Value: 1, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA24, Value: 0x7
				Not 
			End 
			Numeric Prompt: "Device's bus address", Help: "Specify parameters of custom I2C device", QuestionFlags: 0x10, QuestionId: 0xA27, VarStoreId: 0x1, VarOffset: 0x275, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "Device's HID address", Help: "Specify parameters of custom I2C device", QuestionFlags: 0x10, QuestionId: 0xA28, VarStoreId: 0x1, VarOffset: 0x276, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			OneOf Prompt: "Device's bus speed", Help: "Specify parameters of custom I2C device", QuestionFlags: 0x10, QuestionId: 0xA29, VarStoreId: 0x1, VarOffset: 0x278, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "100kHz" Value: 0, Default, MfgDefault
				OneOfOption Option: "400kHz" Value: 1
				OneOfOption Option: "1MHz" Value: 2
			End 
		End 
	End 
	Form FormId: 0x277A, Title: "Serial IO I2C2 Settings"
		Subtitle Prompt: "Serial IO I2C2 Settings", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "I2C IO Voltage Select", Help: "Selects 1.8v or 3.3v for the controller.", QuestionFlags: 0x10, QuestionId: 0xA2A, VarStoreId: 0x1, VarOffset: 0xF71, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "3.3V" Value: 0
			OneOfOption Option: "1.8V" Value: 1, Default, MfgDefault
		End 
	End 
	Form FormId: 0x277B, Title: "Serial IO I2C3 Settings"
		Subtitle Prompt: "Serial IO I2C3 Settings", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "I2C IO Voltage Select", Help: "Selects 1.8v or 3.3v for the controller.", QuestionFlags: 0x10, QuestionId: 0xA2B, VarStoreId: 0x1, VarOffset: 0xF72, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "3.3V" Value: 0
			OneOfOption Option: "1.8V" Value: 1, Default, MfgDefault
		End 
	End 
	Form FormId: 0x277C, Title: "Serial IO I2C4 Settings"
		Subtitle Prompt: "Serial IO I2C4 Settings", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "I2C IO Voltage Select", Help: "Selects 1.8v or 3.3v for the controller.", QuestionFlags: 0x10, QuestionId: 0xA2C, VarStoreId: 0x1, VarOffset: 0xF73, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "3.3V" Value: 0, Default, MfgDefault
			OneOfOption Option: "1.8V" Value: 1
		End 
	End 
	Form FormId: 0x277D, Title: "Serial IO I2C5 Settings"
		Subtitle Prompt: "Serial IO I2C5 Settings", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "I2C IO Voltage Select", Help: "Selects 1.8v or 3.3v for the controller.", QuestionFlags: 0x10, QuestionId: 0xA2D, VarStoreId: 0x1, VarOffset: 0xF74, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "3.3V" Value: 0, Default, MfgDefault
			OneOfOption Option: "1.8V" Value: 1
		End 
	End 
	Form FormId: 0x277E, Title: "Serial IO SPI0 Settings"
		Subtitle Prompt: "Serial IO SPI0 Settings", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "ChipSelect polarity", Help: "Sets initial polarity for ChipSelect signal", QuestionFlags: 0x10, QuestionId: 0xA2E, VarStoreId: 0x1, VarOffset: 0xF75, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Active Low" Value: 0
			OneOfOption Option: "Active High" Value: 1, Default, MfgDefault
		End 
	End 
	Form FormId: 0x277F, Title: "Serial IO SPI1 Settings"
		Subtitle Prompt: "Serial IO SPI1 Settings", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC50, Value: 0x20
				Not 
			End 
			OneOf Prompt: "Enable Finger Print Sensor", Help: "Auto - FPS will be set to FPC1021 if CSME FW Corporate SKU or DISABLE if CSME FW Consumer SKU; ENABLE - Allows the User to select Finger Print Sensor Device; DISABLE - Forces the FPS to be Disable regardless of the CSME FW SKU", QuestionFlags: 0x10, QuestionId: 0xA2F, VarStoreId: 0x1, VarOffset: 0x289, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Auto" Value: 2, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC50, Value: 0x20
				EqIdVal QuestionId: 0xA2F, Value: 0x1
				Not 
				And 
			End 
			OneOf Prompt: "Finger Print Sensor", Help: "Select the HID to enable Finger Print Sensor", QuestionFlags: 0x10, QuestionId: 0xA30, VarStoreId: 0x1, VarOffset: 0x27D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "FPC1011" Value: 1
				OneOfOption Option: "FPC1020" Value: 2
				OneOfOption Option: "VFSI6101" Value: 3
				OneOfOption Option: "Synaptics VFSI7500" Value: 4
				OneOfOption Option: "EGIS0300" Value: 5
				OneOfOption Option: "FPC1021" Value: 6
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA30, Value: 0x0
			OneOf Prompt: "Interrupt mode", Help: "Selects different routing for interrupts from external device", QuestionFlags: 0x10, QuestionId: 0xA31, VarStoreId: 0x1, VarOffset: 0x27E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x1 Value: Other
					Value 
						EqIdValList QuestionId: 0xC50, Values: [74]
							Uint64 Value: 0x1
							Uint64 Value: 0x0
							Conditional 
						End 
					End 
				End 
				OneOfOption Option: "GPIO Interrupt" Value: 0
				OneOfOption Option: "APIC Interrupt" Value: 1, MfgDefault
			End 
		End 
	End 
	Form FormId: 0x2780, Title: "Serial IO UART0 Settings"
		Subtitle Prompt: "Serial IO UART0 Settings", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Bluetooth Device", Help: "Enables/Disables the Vendor Sensor", QuestionFlags: 0x10, QuestionId: 0xA32, VarStoreId: 0x1, VarOffset: 0x27F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Intel Snowfield Peak" Value: 1
			OneOfOption Option: "Broadcom BRCM 43241" Value: 2
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA32, Value: 0x0
			OneOf Prompt: "BT Interrupt Mode", Help: "Selects different routing for interrupts from external device", QuestionFlags: 0x10, QuestionId: 0xA33, VarStoreId: 0x1, VarOffset: 0x280, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "GPIO Interrupt" Value: 0, Default, MfgDefault
				OneOfOption Option: "APIC Interrupt" Value: 1
			End 
		End 
		OneOf Prompt: "Wireless Charging Mode", Help: "Set The Wireless Charging Mode", QuestionFlags: 0x10, QuestionId: 0xA34, VarStoreId: 0x1, VarOffset: 0x2AC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "WC Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "WC Enabled" Value: 1
		End 
		OneOf Prompt: "Hardware Flow Control", Help: "When enabled configures additional 2 GPIO pads for use as RTS/CTS signals for UART", QuestionFlags: 0x10, QuestionId: 0xA35, VarStoreId: 0x1, VarOffset: 0xF77, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
	End 
	Form FormId: 0x2781, Title: "Serial IO UART1 Settings"
		Subtitle Prompt: "Serial IO UART1 Settings", Help: "", Flags: 0x0
		End 
		Text Prompt: "GNSS moved 2 menu levels up", Help: "", Text: ""
		OneOf Prompt: "Hardware Flow Control", Help: "When enabled configures additional 2 GPIO pads for use as RTS/CTS signals for UART", QuestionFlags: 0x10, QuestionId: 0xA36, VarStoreId: 0x1, VarOffset: 0xF78, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
	End 
	Form FormId: 0x2782, Title: "Serial IO UART2 Settings"
		Subtitle Prompt: "Serial IO UART2 Settings", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Hardware Flow Control", Help: "When enabled configures additional 2 GPIO pads for use as RTS/CTS signals for UART", QuestionFlags: 0x10, QuestionId: 0xA37, VarStoreId: 0x1, VarOffset: 0xF79, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
		End 
	End 
	Form FormId: 0x2783, Title: "GPIO Configuration"
		Subtitle Prompt: "GPIO Configuration", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "GPIO IRQ Route", Help: "Route all GPIOs to one of the IRQ.", QuestionFlags: 0x10, QuestionId: 0xA38, VarStoreId: 0x1, VarOffset: 0xF6A, Flags: 0x10, Size: 8, Min: 0xE, Max: 0xF, Step: 0x0
			OneOfOption Option: "IRQ14" Value: 14, Default, MfgDefault
			OneOfOption Option: "IRQ15" Value: 15
		End 
	End 
	Form FormId: 0x2784, Title: "SkyCam Configuration"
		OneOf Prompt: "SkyCam CIO2 Device", Help: "This option configures CIO2 Device as either Disabled, Enabled (as PCIe device) or Enabled as ACPI device", QuestionFlags: 0x10, QuestionId: 0xA39, VarStoreId: 0x1, VarOffset: 0xF46, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "Control Logic 0", Help: "Control Logic 0", QuestionFlags: 0x10, QuestionId: 0xA3A, VarStoreId: 0x1, VarOffset: 0x50, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA3A, Value: 0x0
			Ref Prompt: "Control Logic options", Help: "Control Logic options", QuestionFlags: 0x0, QuestionId: 0xA3B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x278D
		End 
		OneOf Prompt: "Control Logic 1", Help: "Control Logic 1", QuestionFlags: 0x10, QuestionId: 0xA3C, VarStoreId: 0x1, VarOffset: 0x51, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA3C, Value: 0x0
			Ref Prompt: "Control Logic options", Help: "Control Logic options", QuestionFlags: 0x0, QuestionId: 0xA3D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x278E
		End 
		OneOf Prompt: "Control Logic 2", Help: "Control Logic 2", QuestionFlags: 0x10, QuestionId: 0xA3E, VarStoreId: 0x1, VarOffset: 0x52, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA3E, Value: 0x0
			Ref Prompt: "Control Logic options", Help: "Control Logic options", QuestionFlags: 0x0, QuestionId: 0xA3F, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x278F
		End 
		OneOf Prompt: "Control Logic 3", Help: "Control Logic 3", QuestionFlags: 0x10, QuestionId: 0xA40, VarStoreId: 0x1, VarOffset: 0x53, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA40, Value: 0x0
			Ref Prompt: "Control Logic options", Help: "Control Logic options", QuestionFlags: 0x0, QuestionId: 0xA41, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2790
		End 
		OneOf Prompt: "Link0", Help: "Link0", QuestionFlags: 0x10, QuestionId: 0xA42, VarStoreId: 0x1, VarOffset: 0x54, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA42, Value: 0x0
			Ref Prompt: "Link options", Help: "Link options", QuestionFlags: 0x0, QuestionId: 0xA43, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2789
		End 
		OneOf Prompt: "Link1", Help: "Link1", QuestionFlags: 0x10, QuestionId: 0xA44, VarStoreId: 0x1, VarOffset: 0x55, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA44, Value: 0x0
			Ref Prompt: "Link options", Help: "Link options", QuestionFlags: 0x0, QuestionId: 0xA45, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x278A
		End 
		OneOf Prompt: "Link2", Help: "Link2", QuestionFlags: 0x10, QuestionId: 0xA46, VarStoreId: 0x1, VarOffset: 0x56, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA46, Value: 0x0
			Ref Prompt: "Link options", Help: "Link options", QuestionFlags: 0x0, QuestionId: 0xA47, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x278B
		End 
		OneOf Prompt: "Link3", Help: "Link3", QuestionFlags: 0x10, QuestionId: 0xA48, VarStoreId: 0x1, VarOffset: 0x57, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA48, Value: 0x0
			Ref Prompt: "Link options", Help: "Link options", QuestionFlags: 0x0, QuestionId: 0xA49, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x278C
		End 
		OneOf Prompt: "PORT-A HS-RXEN / TEM-EN Override", Help: "PORT-A HS-RXEN / TEM-EN Override", QuestionFlags: 0x10, QuestionId: 0xA4A, VarStoreId: 0x1, VarOffset: 0x35, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PORT-B HS-RXEN / TEM-EN Override", Help: "PORT-B HS-RXEN / TEM-EN Override", QuestionFlags: 0x10, QuestionId: 0xA4B, VarStoreId: 0x1, VarOffset: 0x36, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PORT-C HS-RXEN / TEM-EN Override", Help: "PORT-C HS-RXEN / TEM-EN Override", QuestionFlags: 0x10, QuestionId: 0xA4C, VarStoreId: 0x1, VarOffset: 0x37, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PORT-D HS-RXEN / TEM-EN Override", Help: "PORT-D HS-RXEN / TEM-EN Override", QuestionFlags: 0x10, QuestionId: 0xA4D, VarStoreId: 0x1, VarOffset: 0x38, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default
			OneOfOption Option: "Enabled" Value: 1
		End 
		OneOf Prompt: "PORT-A CTLE", Help: "PORT-A CTLE", QuestionFlags: 0x10, QuestionId: 0xA4E, VarStoreId: 0x1, VarOffset: 0x3D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default
		End 
		OneOf Prompt: "PORT-B CTLE", Help: "PORT-B CTLE", QuestionFlags: 0x10, QuestionId: 0xA4F, VarStoreId: 0x1, VarOffset: 0x3E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default
		End 
		OneOf Prompt: "PORT-C/D CTLE", Help: "PORT-C/D CTLE", QuestionFlags: 0x10, QuestionId: 0xA50, VarStoreId: 0x1, VarOffset: 0x3F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default
		End 
		Numeric Prompt: "PORT-A CTLE CAP Value", Help: "PORT-A CTLE CAP Value", QuestionFlags: 0x10, QuestionId: 0xA51, VarStoreId: 0x1, VarOffset: 0x46, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 14
		End 
		Numeric Prompt: "PORT-A CTLE RES Value", Help: "PORT-A CTLE RES Value", QuestionFlags: 0x10, QuestionId: 0xA52, VarStoreId: 0x1, VarOffset: 0x49, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
			Default DefaultId: 0x0 Value: 13
		End 
		Numeric Prompt: "PORT-B CTLE CAP Value", Help: "PORT-B CTLE CAP Value", QuestionFlags: 0x10, QuestionId: 0xA53, VarStoreId: 0x1, VarOffset: 0x47, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 14
		End 
		Numeric Prompt: "PORT-B CTLE RES Value", Help: "PORT-B CTLE RES Value", QuestionFlags: 0x10, QuestionId: 0xA54, VarStoreId: 0x1, VarOffset: 0x4A, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
			Default DefaultId: 0x0 Value: 13
		End 
		Numeric Prompt: "PORT-C/D CTLE CAP Value", Help: "PORT-C/D CTLE CAP Value", QuestionFlags: 0x10, QuestionId: 0xA55, VarStoreId: 0x1, VarOffset: 0x48, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 14
		End 
		Numeric Prompt: "PORT-C/D CTLE RES Value", Help: "PORT-C/D CTLE RES Value", QuestionFlags: 0x10, QuestionId: 0xA56, VarStoreId: 0x1, VarOffset: 0x4B, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
			Default DefaultId: 0x0 Value: 13
		End 
		OneOf Prompt: "PORT-A TRIM", Help: "PORT-A TRIM", QuestionFlags: 0x10, QuestionId: 0xA57, VarStoreId: 0x1, VarOffset: 0x39, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default
		End 
		OneOf Prompt: "PORT-B TRIM", Help: "PORT-B TRIM", QuestionFlags: 0x10, QuestionId: 0xA58, VarStoreId: 0x1, VarOffset: 0x3A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default
		End 
		OneOf Prompt: "PORT-C TRIM", Help: "PORT-C TRIM", QuestionFlags: 0x10, QuestionId: 0xA59, VarStoreId: 0x1, VarOffset: 0x3B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default
		End 
		OneOf Prompt: "PORT-D TRIM", Help: "PORT-D TRIM", QuestionFlags: 0x10, QuestionId: 0xA5A, VarStoreId: 0x1, VarOffset: 0x3C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, Default
		End 
		Numeric Prompt: "PORT-A Data Trim Value", Help: "PORT-A Data Trim Value", QuestionFlags: 0x10, QuestionId: 0xA5B, VarStoreId: 0x1, VarOffset: 0x40, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
			Default DefaultId: 0x0 Value: 48059
		End 
		Numeric Prompt: "PORT-B Data Trim Value", Help: "PORT-B Data Trim Value", QuestionFlags: 0x10, QuestionId: 0xA5C, VarStoreId: 0x1, VarOffset: 0x42, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
			Default DefaultId: 0x0 Value: 48059
		End 
		Numeric Prompt: "PORT-C/D Data Trim Value", Help: "PORT-C/D Data Trim Value", QuestionFlags: 0x10, QuestionId: 0xA5D, VarStoreId: 0x1, VarOffset: 0x44, Flags: 0x21, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
			Default DefaultId: 0x0 Value: 52428
		End 
		Numeric Prompt: "PORT-A Clk Trim Value", Help: "PORT-A Clk Trim Value", QuestionFlags: 0x10, QuestionId: 0xA5E, VarStoreId: 0x1, VarOffset: 0x4C, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 10
		End 
		Numeric Prompt: "PORT-B Clk Trim Value", Help: "PORT-B Clk Trim Value", QuestionFlags: 0x10, QuestionId: 0xA5F, VarStoreId: 0x1, VarOffset: 0x4D, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 10
		End 
		Numeric Prompt: "PORT-C Clk Trim Value", Help: "PORT-C Clk Trim Value", QuestionFlags: 0x10, QuestionId: 0xA60, VarStoreId: 0x1, VarOffset: 0x4E, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 9
		End 
		Numeric Prompt: "PORT-D Clk Trim Value", Help: "PORT-D Clk Trim Value", QuestionFlags: 0x10, QuestionId: 0xA61, VarStoreId: 0x1, VarOffset: 0x4F, Flags: 0x20, Size: 8, Min: 0x0, Max: 0xF, Step: 0x1
			Default DefaultId: 0x0 Value: 10
		End 
	End 
	Form FormId: 0x2785, Title: "SCS Configuration"
		GrayOutIf 
			EqIdVal QuestionId: 0x9F7, Value: 0x0
			OneOf Prompt: "eMMC 5.0 Controller", Help: "Enable or Disable SCS eMMC 5.0 Controller", QuestionFlags: 0x10, QuestionId: 0xA62, VarStoreId: 0x1, VarOffset: 0xF47, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA62, Value: 0x0
			OneOf Prompt: "eMMC 5.0 HS400 Mode", Help: "Enable or Disable SCS eMMC 5.0 HS400 Mode", QuestionFlags: 0x10, QuestionId: 0xA63, VarStoreId: 0x1, VarOffset: 0xF48, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, Default, MfgDefault
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0xA63, Value: 0x0
				OneOf Prompt: "Driver Strength", Help: "Sets I/O driver strength", QuestionFlags: 0x10, QuestionId: 0xA64, VarStoreId: 0x1, VarOffset: 0xF49, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					OneOfOption Option: "33 Ohm" Value: 0
					OneOfOption Option: "40 Ohm" Value: 1, Default, MfgDefault
					OneOfOption Option: "50 Ohm" Value: 2
				End 
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0x9F7, Value: 0x0
			OneOf Prompt: "SDCard 3.0 Controller", Help: "Enable or Disable SCS SDHC 3.0 Controller", QuestionFlags: 0x10, QuestionId: 0xA65, VarStoreId: 0x1, VarOffset: 0xF4A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Enabled" Value: 1
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA65, Value: 0x0
			OneOf Prompt: "  SDCard Sideband Events", Help: "Card detect support:
Disabled: Uses GPP_G5 in native mode (inband wake - not functional for SDHC in D3).
GPP_B17: sets GPP_B17 as GpioInt/GpioIo.
Warning:
1. Requires RVP rework.
2. Thunderbolt(TBT) must be disabled due to GPIO conflict.
GPP_D10: sets GPP_D10 as GpioInt/GpioIo
Warning:
1. Requires RVP rework.

Sideband card detect is not supported on Win 7.", QuestionFlags: 0x10, QuestionId: 0xA66, VarStoreId: 0x1, VarOffset: 0xF4B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Use GPP_B17" Value: 1
				OneOfOption Option: "Use GPP_D10" Value: 2
			End 
		End 
	End 
	Form FormId: 0x2786, Title: "ISH Configuration"
		GrayOutIf 
			EqIdVal QuestionId: 0x542, Value: 0x2
			OneOf Prompt: "ISH Controller", Help: "Enables/Disables Integrated Sensor Hub (ISH) Device", QuestionFlags: 0x10, QuestionId: 0xA67, VarStoreId: 0x1, VarOffset: 0xF4C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA67, Value: 0x0
			CheckBox Prompt: "PDT Unlock Message", Help: "Checked = Sends PDT Unlock Message to ISH.
After the message is sent the field is set back to unchecked automatically.", QuestionFlags: 0x10, QuestionId: 0xA68, VarStoreId: 0x1, VarOffset: 0xF5B, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			Text Prompt: "ISH GPIO Assignment Configuration", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", Text: ""
			CheckBox Prompt: " SPI", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA69, VarStoreId: 0x1, VarOffset: 0xF4D, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0x9F1, Value: 0x0
					Not 
					EqIdVal QuestionId: 0xC51, Value: 0x1
					And 
				End 
				CheckBox Prompt: " UART0", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA6A, VarStoreId: 0x1, VarOffset: 0xF4E, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
				End 
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0x9F8, Value: 0x1
				CheckBox Prompt: " UART1", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA6B, VarStoreId: 0x1, VarOffset: 0xF4F, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
				End 
			End 
			CheckBox Prompt: " I2C0", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA6C, VarStoreId: 0x1, VarOffset: 0xF50, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			CheckBox Prompt: " I2C1", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA6D, VarStoreId: 0x1, VarOffset: 0xF51, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			GrayOutIf 
				EqIdVal QuestionId: 0x9F4, Value: 0x0
					Not 
					EqIdVal QuestionId: 0xC51, Value: 0x2
					And 
					EqIdVal QuestionId: 0x9F2, Value: 0x0
					Not 
					EqIdVal QuestionId: 0xC51, Value: 0x1
					And 
					Or 
				End 
				CheckBox Prompt: " I2C2", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA6E, VarStoreId: 0x1, VarOffset: 0xF52, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
				End 
			End 
			CheckBox Prompt: " GP_0", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA6F, VarStoreId: 0x1, VarOffset: 0xF53, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			CheckBox Prompt: " GP_1", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA70, VarStoreId: 0x1, VarOffset: 0xF54, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			CheckBox Prompt: " GP_2", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA71, VarStoreId: 0x1, VarOffset: 0xF55, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			CheckBox Prompt: " GP_3", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA72, VarStoreId: 0x1, VarOffset: 0xF56, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			CheckBox Prompt: " GP_4", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA73, VarStoreId: 0x1, VarOffset: 0xF57, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			CheckBox Prompt: " GP_5", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA74, VarStoreId: 0x1, VarOffset: 0xF58, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			CheckBox Prompt: " GP_6", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA75, VarStoreId: 0x1, VarOffset: 0xF59, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			CheckBox Prompt: " GP_7", Help: "Checked = Pin set to ISH Native function.
Checkbox grayed out = disable conflicting SerialIo controller to set.
Shared pins:
1. ISH UART0 - LPSS I2C2(PCH-H)
2. ISH UART1 - LPSS UART1
3. ISH I2C2 - LPSS I2C5(PCH-LP) / I2C3(PCH-H)", QuestionFlags: 0x10, QuestionId: 0xA76, VarStoreId: 0x1, VarOffset: 0xF5A, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
		End 
	End 
	Form FormId: 0x2787, Title: "TraceHub Configuration Menu"
		OneOf Prompt: "TraceHub Enable Mode", Help: "Select Enable, Disable or Debugger", QuestionFlags: 0x10, QuestionId: 0xA77, VarStoreId: 0x1, VarOffset: 0xF7A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
			OneOfOption Option: "Disable" Value: 0, Default, MfgDefault
			OneOfOption Option: "Host Debugger" Value: 2
		End 
		OneOf Prompt: "MemRegion 0 Buffer Size", Help: "Select size of mem region 0 buffer", QuestionFlags: 0x10, QuestionId: 0xA78, VarStoreId: 0x1, VarOffset: 0xF7B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
			OneOfOption Option: "None" Value: 0
			OneOfOption Option: "1MB" Value: 1, Default, MfgDefault
			OneOfOption Option: "8MB" Value: 2
			OneOfOption Option: "64MB" Value: 3
			OneOfOption Option: "128MB" Value: 4
			OneOfOption Option: "256MB" Value: 5
			OneOfOption Option: "512MB" Value: 6
			OneOfOption Option: "1GB" Value: 7
		End 
		OneOf Prompt: "MemRegion 1 Buffer Size", Help: "Select size of mem region 1 buffer", QuestionFlags: 0x10, QuestionId: 0xA79, VarStoreId: 0x1, VarOffset: 0xF7C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
			OneOfOption Option: "None" Value: 0
			OneOfOption Option: "1MB" Value: 1, Default, MfgDefault
			OneOfOption Option: "8MB" Value: 2
			OneOfOption Option: "64MB" Value: 3
			OneOfOption Option: "128MB" Value: 4
			OneOfOption Option: "256MB" Value: 5
			OneOfOption Option: "512MB" Value: 6
			OneOfOption Option: "1GB" Value: 7
		End 
	End 
	Form FormId: 0x2788, Title: "Pch Thermal Throttling Control"
		OneOf Prompt: "Thermal Throttling Level", Help: "Determine if use Intel suggested setting", QuestionFlags: 0x10, QuestionId: 0xA7A, VarStoreId: 0x1, VarOffset: 0xF7D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Suggested Setting" Value: 1, Default
			OneOfOption Option: "Manual" Value: 0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA7A, Value: 0x1
			CheckBox Prompt: "Thermal Throttling", Help: "Enable/Disable the thermal throttling states control", QuestionFlags: 0x10, QuestionId: 0xA7B, VarStoreId: 0x1, VarOffset: 0xF84, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			CheckBox Prompt: "TT State 13", Help: "PMSync state 13 will force at least T2 state", QuestionFlags: 0x10, QuestionId: 0xA7C, VarStoreId: 0x1, VarOffset: 0xF85, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			CheckBox Prompt: "Thermal Throttling Lock", Help: "Lock the entire TL register", QuestionFlags: 0x10, QuestionId: 0xA7D, VarStoreId: 0x1, VarOffset: 0xF86, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			Numeric Prompt: "T0 Level", Help: "If Trip Point Temperature <= T0Level, the system is in T0 state", QuestionFlags: 0x10, QuestionId: 0xA7E, VarStoreId: 0x1, VarOffset: 0xF7E, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "T1 Level", Help: "If T1Level >= Trip Point Temperature > T0Level, the system is in T1 state", QuestionFlags: 0x10, QuestionId: 0xA7F, VarStoreId: 0x1, VarOffset: 0xF80, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
			Numeric Prompt: "T2 Level", Help: "If T2Level >= Trip Point Temperature > T1Level, the system is in T2 state", QuestionFlags: 0x10, QuestionId: 0xA80, VarStoreId: 0x1, VarOffset: 0xF82, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x1
				Default DefaultId: 0x0 Value: 0
			End 
		End 
		OneOf Prompt: "DMI Thermal Setting", Help: "Determine if use Intel suggested setting", QuestionFlags: 0x10, QuestionId: 0xA81, VarStoreId: 0x1, VarOffset: 0xF87, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Suggested Setting" Value: 1, Default
			OneOfOption Option: "Manual" Value: 0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA81, Value: 0x1
			CheckBox Prompt: "DMI Thermal Sensor Autonomous Width", Help: "Enable/Disable Thermal Sensor initiated Autonomous Width Negotiation", QuestionFlags: 0x10, QuestionId: 0xA82, VarStoreId: 0x1, VarOffset: 0xF8C, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
			OneOf Prompt: "Thermal Sensor 0 Width", Help: "Determine the DMI Link Width when the output from the Thermal Sensor is T0", QuestionFlags: 0x10, QuestionId: 0xA83, VarStoreId: 0x1, VarOffset: 0xF88, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "x 4" Value: 0, Default
				OneOfOption Option: "x 2" Value: 1
				OneOfOption Option: "x 1" Value: 2
			End 
			OneOf Prompt: "Thermal Sensor 1 Width", Help: "Determine the DMI Link Width when the output from the Thermal Sensor is T1", QuestionFlags: 0x10, QuestionId: 0xA84, VarStoreId: 0x1, VarOffset: 0xF89, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "x 4" Value: 0, Default
				OneOfOption Option: "x 2" Value: 1
				OneOfOption Option: "x 1" Value: 2
			End 
			OneOf Prompt: "Thermal Sensor 2 Width", Help: "Determine the DMI Link Width when the output from the Thermal Sensor is T2", QuestionFlags: 0x10, QuestionId: 0xA85, VarStoreId: 0x1, VarOffset: 0xF8A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "x 4" Value: 0, Default
				OneOfOption Option: "x 2" Value: 1
				OneOfOption Option: "x 1" Value: 2
			End 
			OneOf Prompt: "Thermal Sensor 3 Width", Help: "Determine the DMI Link Width when the output from the Thermal Sensor is T3", QuestionFlags: 0x10, QuestionId: 0xA86, VarStoreId: 0x1, VarOffset: 0xF8B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "x 4" Value: 0, Default
				OneOfOption Option: "x 2" Value: 1
				OneOfOption Option: "x 1" Value: 2
			End 
		End 
		OneOf Prompt: "SATA Thermal Setting", Help: "Determine if use Intel suggested setting", QuestionFlags: 0x10, QuestionId: 0xA87, VarStoreId: 0x1, VarOffset: 0xF8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Suggested Setting" Value: 1, Default
			OneOfOption Option: "Manual" Value: 0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA87, Value: 0x1
			Subtitle Prompt: "Port 0", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "T1 Multipler", Help: "Determine the value of SATA Port T1 Multipler", QuestionFlags: 0x10, QuestionId: 0xA88, VarStoreId: 0x1, VarOffset: 0xF8E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "x 1" Value: 1, Default
				OneOfOption Option: "x 2" Value: 2
				OneOfOption Option: "x 4" Value: 3
			End 
			OneOf Prompt: "T2 Multipler", Help: "Determine the value of SATA Port T2 Multipler", QuestionFlags: 0x10, QuestionId: 0xA89, VarStoreId: 0x1, VarOffset: 0xF8F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "x 1" Value: 1
				OneOfOption Option: "x 2" Value: 2, Default
				OneOfOption Option: "x 4" Value: 3
			End 
			OneOf Prompt: "T3 Multipler", Help: "Determine the value of SATA Port T3 Multipler", QuestionFlags: 0x10, QuestionId: 0xA8A, VarStoreId: 0x1, VarOffset: 0xF90, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "x 1" Value: 1
				OneOfOption Option: "x 2" Value: 2
				OneOfOption Option: "x 4" Value: 3, Default
			End 
			CheckBox Prompt: "Alternate Fast Init Tdispatch", Help: "Enable/Disable SATA Port Alternate Fast Init Tdispatch", QuestionFlags: 0x10, QuestionId: 0xA8B, VarStoreId: 0x1, VarOffset: 0xF93, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA8B, Value: 0x0
				EqIdVal QuestionId: 0xA87, Value: 0x1
				Or 
			End 
			OneOf Prompt: "Tdispatch", Help: "Determine the value of SATA Port Tdispatch", QuestionFlags: 0x10, QuestionId: 0xA8C, VarStoreId: 0x1, VarOffset: 0xF91, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "~32us" Value: 0, Default
				OneOfOption Option: "~128us" Value: 1
				OneOfOption Option: "~8us" Value: 3
			End 
			OneOf Prompt: "Tinactive", Help: "Determine the value of SATA Port Tinactive", QuestionFlags: 0x10, QuestionId: 0xA8D, VarStoreId: 0x1, VarOffset: 0xF92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "~32us" Value: 0, Default
				OneOfOption Option: "~128us" Value: 1
				OneOfOption Option: "~8us" Value: 3
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA8B, Value: 0x1
				EqIdVal QuestionId: 0xA87, Value: 0x1
				Or 
			End 
			OneOf Prompt: "Tdispatch", Help: "Determine the value of SATA Port Tdispatch", QuestionFlags: 0x10, QuestionId: 0xA8E, VarStoreId: 0x1, VarOffset: 0xF91, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "~32us" Value: 0, Default
				OneOfOption Option: "~128us" Value: 1
				OneOfOption Option: "~8us" Value: 3
			End 
			OneOf Prompt: "Tinactive", Help: "Determine the value of SATA Port Tinactive", QuestionFlags: 0x10, QuestionId: 0xA8F, VarStoreId: 0x1, VarOffset: 0xF92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "~32us" Value: 0, Default
				OneOfOption Option: "~128us" Value: 1
				OneOfOption Option: "~8us" Value: 3
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA87, Value: 0x1
			Subtitle Prompt: "Port 1", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "T1 Multipler", Help: "Determine the value of SATA Port T1 Multipler", QuestionFlags: 0x10, QuestionId: 0xA90, VarStoreId: 0x1, VarOffset: 0xF94, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "x 1" Value: 1, Default
				OneOfOption Option: "x 2" Value: 2
				OneOfOption Option: "x 4" Value: 3
			End 
			OneOf Prompt: "T2 Multipler", Help: "Determine the value of SATA Port T2 Multipler", QuestionFlags: 0x10, QuestionId: 0xA91, VarStoreId: 0x1, VarOffset: 0xF95, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "x 1" Value: 1
				OneOfOption Option: "x 2" Value: 2, Default
				OneOfOption Option: "x 4" Value: 3
			End 
			OneOf Prompt: "T3 Multipler", Help: "Determine the value of SATA Port T3 Multipler", QuestionFlags: 0x10, QuestionId: 0xA92, VarStoreId: 0x1, VarOffset: 0xF96, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "x 1" Value: 1
				OneOfOption Option: "x 2" Value: 2
				OneOfOption Option: "x 4" Value: 3, Default
			End 
			CheckBox Prompt: "Alternate Fast Init Tdispatch", Help: "Enable/Disable SATA Port Alternate Fast Init Tdispatch", QuestionFlags: 0x10, QuestionId: 0xA93, VarStoreId: 0x1, VarOffset: 0xF99, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA93, Value: 0x0
				EqIdVal QuestionId: 0xA87, Value: 0x1
				Or 
			End 
			OneOf Prompt: "Tdispatch", Help: "Determine the value of SATA Port Tdispatch", QuestionFlags: 0x10, QuestionId: 0xA94, VarStoreId: 0x1, VarOffset: 0xF97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "~32us" Value: 0, Default
				OneOfOption Option: "~128us" Value: 1
				OneOfOption Option: "~8us" Value: 3
			End 
			OneOf Prompt: "Tinactive", Help: "Determine the value of SATA Port Tinactive", QuestionFlags: 0x10, QuestionId: 0xA95, VarStoreId: 0x1, VarOffset: 0xF98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "~32us" Value: 0, Default
				OneOfOption Option: "~128us" Value: 1
				OneOfOption Option: "~8us" Value: 3
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA93, Value: 0x1
				EqIdVal QuestionId: 0xA87, Value: 0x1
				Or 
			End 
			OneOf Prompt: "Tdispatch", Help: "Determine the value of SATA Port Tdispatch", QuestionFlags: 0x10, QuestionId: 0xA96, VarStoreId: 0x1, VarOffset: 0xF97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "~32us" Value: 0, Default
				OneOfOption Option: "~128us" Value: 1
				OneOfOption Option: "~8us" Value: 3
			End 
			OneOf Prompt: "Tinactive", Help: "Determine the value of SATA Port Tinactive", QuestionFlags: 0x10, QuestionId: 0xA97, VarStoreId: 0x1, VarOffset: 0xF98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
				OneOfOption Option: "~32us" Value: 0, Default
				OneOfOption Option: "~128us" Value: 1
				OneOfOption Option: "~8us" Value: 3
			End 
		End 
	End 
	Form FormId: 0x2789, Title: "Link options"
		Subtitle Prompt: "Link0", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Sensor Model", Help: "Sensor Model", QuestionFlags: 0x10, QuestionId: 0xA98, VarStoreId: 0x1, VarOffset: 0xC5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			OneOfOption Option: "IMX135" Value: 0, Default
			OneOfOption Option: "OV5693" Value: 1
			OneOfOption Option: "IMX179" Value: 2
			OneOfOption Option: "OV8858" Value: 3
			OneOfOption Option: "OV2740-IVCAM" Value: 4
			OneOfOption Option: "OV9728" Value: 5
			OneOfOption Option: "IMX188" Value: 6
			OneOfOption Option: "IMX208" Value: 7
			OneOfOption Option: "OV5670" Value: 8
			OneOfOption Option: "OV8865" Value: 9
			OneOfOption Option: "HM2051" Value: 10
			OneOfOption Option: "OV2742" Value: 11
			OneOfOption Option: "OV9234" Value: 12
			OneOfOption Option: "OV8856" Value: 13
			OneOfOption Option: "OV16860" Value: 14
			OneOfOption Option: "User Custom" Value: 255
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA98, Value: 0xFF
				Not 
			End 
			String Prompt: "Custom HID", Help: "Custom HID", QuestionFlags: 0x0, QuestionId: 0xA99, VarStoreId: 0x1, VarStoreInfo: 0xC6, MinSize: 0x6, MaxSize: 0x8, Flags: 0x0
			End 
		End 
		OneOf Prompt: "Lanes Clock division", Help: "Lanes Clock division", QuestionFlags: 0x10, QuestionId: 0xA9A, VarStoreId: 0x1, VarOffset: 0x58, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
			OneOfOption Option: "4 4 2 2" Value: 0, Default
			OneOfOption Option: "4 4 3 1" Value: 2
			OneOfOption Option: "4 4 4 0" Value: 3
			OneOfOption Option: "8 0 2 2" Value: 4
			OneOfOption Option: "8 0 3 1" Value: 6
			OneOfOption Option: "8 0 4 0" Value: 7
		End 
		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0xA9B, VarStoreId: 0x1, VarOffset: 0x120, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0
			OneOfOption Option: "PTC" Value: 16
			OneOfOption Option: "CRD-D" Value: 32
			OneOfOption Option: "CRD-G" Value: 48, Default
			OneOfOption Option: "Kilshon-PPV" Value: 64
			OneOfOption Option: "CRD-G2" Value: 80
		End 
		OneOf Prompt: "GPIO control", Help: "GPIO control", QuestionFlags: 0x10, QuestionId: 0xA9C, VarStoreId: 0x1, VarOffset: 0x12C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			OneOfOption Option: "No Control Logic" Value: 255, Default, MfgDefault
			SuppressIf 
				EqIdVal QuestionId: 0xA3A, Value: 0x0
				OneOfOption Option: "Control Logic 0" Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xA3C, Value: 0x0
				OneOfOption Option: "Control Logic 1" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xA3E, Value: 0x0
				OneOfOption Option: "Control Logic 2" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xA40, Value: 0x0
				OneOfOption Option: "Control Logic 3" Value: 3
			End 
		End 
		OneOf Prompt: "Camera position", Help: "Camera position", QuestionFlags: 0x10, QuestionId: 0xA9D, VarStoreId: 0x1, VarOffset: 0xD8, Flags: 0x10, Size: 8, Min: 0x61, Max: 0x69, Step: 0x0
			OneOfOption Option: "Front" Value: 97
			OneOfOption Option: "Back" Value: 105, Default
		End 
		OneOf Prompt: "Flash Support", Help: "Flash Support", QuestionFlags: 0x10, QuestionId: 0xA9E, VarStoreId: 0x1, VarOffset: 0x12D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
			OneOfOption Option: "Driver default" Value: 0, Default
			OneOfOption Option: "Disabled" Value: 2
			OneOfOption Option: "Enabled" Value: 3
		End 
		OneOf Prompt: "Privacy LED", Help: "Privacy LED", QuestionFlags: 0x10, QuestionId: 0xA9F, VarStoreId: 0x1, VarOffset: 0x502, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
			OneOfOption Option: "Driver default" Value: 0, Default, MfgDefault
			OneOfOption Option: "ILEDA, 16mA" Value: 1
			OneOfOption Option: "ILEDB, 2mA" Value: 2
			OneOfOption Option: "ILEDB, 4mA" Value: 3
			OneOfOption Option: "ILEDB, 8mA" Value: 4
			OneOfOption Option: "ILEDB, 16mA" Value: 5
		End 
		OneOf Prompt: "Rotation", Help: "Rotation", QuestionFlags: 0x10, QuestionId: 0xAA0, VarStoreId: 0x1, VarOffset: 0x12E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
			OneOfOption Option: "0" Value: 0, Default, MfgDefault
			OneOfOption Option: "90" Value: 2
			OneOfOption Option: "180" Value: 4
			OneOfOption Option: "270" Value: 6
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xA9B, Value: 0x50
				Not 
			End 
			OneOf Prompt: "PMIC Position", Help: "PMIC Position
Position 1 indicates the current module is placed on the left side of the CRD-G2 card
Position 2 indicates the current module is placed on the right side of the CRD-G2 card", QuestionFlags: 0x10, QuestionId: 0xAA1, VarStoreId: 0x1, VarOffset: 0x503, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Position 1" Value: 0, Default, MfgDefault
				OneOfOption Option: "Position 2" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xAA1, Value: 0x1
				Not 
			End 
			OneOf Prompt: "Voltage Rail", Help: "Voltage Rail", QuestionFlags: 0x10, QuestionId: 0xAA2, VarStoreId: 0x1, VarOffset: 0x504, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "3 voltage rail" Value: 0, Default, MfgDefault
				OneOfOption Option: "2 voltage rail" Value: 1
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC50, Value: 0x20
			String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0xAA3, VarStoreId: 0x1, VarStoreInfo: 0xD9, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0
			End 
		End 
		OneOf Prompt: "LaneUsed", Help: "LaneUsed", QuestionFlags: 0x10, QuestionId: 0xAA4, VarStoreId: 0x1, VarOffset: 0x121, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x8, Step: 0x0
			OneOfOption Option: "x1" Value: 1
			OneOfOption Option: "x2" Value: 2
			OneOfOption Option: "x3" Value: 3
			OneOfOption Option: "x4" Value: 4, Default
			OneOfOption Option: "x8" Value: 8
		End 
		OneOf Prompt: "MCLK", Help: "MCLK", QuestionFlags: 0x10, QuestionId: 0xAA5, VarStoreId: 0x1, VarOffset: 0x128, Flags: 0x12, Size: 32, Min: 0x124F800, Max: 0x16E3600, Step: 0x0
			OneOfOption Option: "19.2 MHz" Value: 19200000
			OneOfOption Option: "24 MHz" Value: 24000000, Default
			OneOfOption Option: "20 MHz" Value: 20000000
		End 
		OneOf Prompt: "EEPROM Type", Help: "EEPROM Type", QuestionFlags: 0x10, QuestionId: 0xAA6, VarStoreId: 0x1, VarOffset: 0x122, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x0
			OneOfOption Option: "ROM_NONE" Value: 0
			OneOfOption Option: "ROM_OTP" Value: 1
			OneOfOption Option: "ROM_EEPROM_16K_64" Value: 2
			OneOfOption Option: "ROM_EEPROM_16K_16" Value: 3
			OneOfOption Option: "ROM_OTP_ACPI_ACPI" Value: 4
			OneOfOption Option: "ROM_ACPI" Value: 5
			OneOfOption Option: "ROM_EEPROM_BRCA016GWZ" Value: 6
			OneOfOption Option: "ROM_EEPROM_24AA32" Value: 7
			OneOfOption Option: "ROM_EEPROM_CAT24C08" Value: 8, Default
			OneOfOption Option: "ROM_RESERVED1" Value: 9
			OneOfOption Option: "ROM_RESERVED2" Value: 10
		End 
		OneOf Prompt: "VCM Type", Help: "VCM Type", QuestionFlags: 0x10, QuestionId: 0xAA7, VarStoreId: 0x1, VarOffset: 0x123, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
			OneOfOption Option: "VCM_NONE" Value: 0
			OneOfOption Option: "VCM_AD5823" Value: 1
			OneOfOption Option: "VCM_DW9714" Value: 2
			OneOfOption Option: "VCM_AD5816" Value: 3, Default
			OneOfOption Option: "VCM_DW9719" Value: 4
			OneOfOption Option: "VCM_DW9718" Value: 5
			OneOfOption Option: "VCM_RESERVED1" Value: 6
			OneOfOption Option: "VCM_RESERVED2" Value: 7
		End 
		Numeric Prompt: "Number of I2C Components", Help: "Number of I2C Components", QuestionFlags: 0x10, QuestionId: 0xAA8, VarStoreId: 0x1, VarOffset: 0xF9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xAA8, Value: 0x0
			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0xAA9, VarStoreId: 0x1, VarOffset: 0xFA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "I2C0" Value: 0
				OneOfOption Option: "I2C1" Value: 1
				OneOfOption Option: "I2C2" Value: 2, Default
				OneOfOption Option: "I2C3" Value: 3
				OneOfOption Option: "I2C4" Value: 4
				OneOfOption Option: "I2C5" Value: 5
			End 
			Subtitle Prompt: "  Device 0", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAAA, VarStoreId: 0x1, VarOffset: 0xFB, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 16
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAAB, VarStoreId: 0x1, VarOffset: 0x113, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0, Default
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAA8, Values: [0, 1]
			Subtitle Prompt: "  Device 1", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAAC, VarStoreId: 0x1, VarOffset: 0xFD, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 14
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAAD, VarStoreId: 0x1, VarOffset: 0x114, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1, Default
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAA8, Values: [0, 1, 2]
			Subtitle Prompt: "  Device 2", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAAE, VarStoreId: 0x1, VarOffset: 0xFF, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 80
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAAF, VarStoreId: 0x1, VarOffset: 0x115, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2, Default
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAA8, Values: [0, 1, 2, 3]
			Subtitle Prompt: "  Device 3", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAB0, VarStoreId: 0x1, VarOffset: 0x101, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 81
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAB1, VarStoreId: 0x1, VarOffset: 0x116, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3, Default
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAA8, Values: [0, 1, 2, 3, 4]
			Subtitle Prompt: "  Device 4", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAB2, VarStoreId: 0x1, VarOffset: 0x103, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 82
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAB3, VarStoreId: 0x1, VarOffset: 0x117, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4, Default
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAA8, Values: [0, 1, 2, 3, 4, 5]
			Subtitle Prompt: "  Device 5", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAB4, VarStoreId: 0x1, VarOffset: 0x105, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 83
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAB5, VarStoreId: 0x1, VarOffset: 0x118, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5, Default
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAA8, Values: [0, 1, 2, 3, 4, 5, 6]
			Subtitle Prompt: "  Device 6", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAB6, VarStoreId: 0x1, VarOffset: 0x107, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 84
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAB7, VarStoreId: 0x1, VarOffset: 0x119, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6, Default
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAA8, Values: [0, 1, 2, 3, 4, 5, 6, 7]
			Subtitle Prompt: "  Device 7", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAB8, VarStoreId: 0x1, VarOffset: 0x109, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 85
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAB9, VarStoreId: 0x1, VarOffset: 0x11A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7, Default
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAA8, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8]
			Subtitle Prompt: "  Device 8", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xABA, VarStoreId: 0x1, VarOffset: 0x10B, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 86
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xABB, VarStoreId: 0x1, VarOffset: 0x11B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8, Default
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAA8, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9]
			Subtitle Prompt: "  Device 9", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xABC, VarStoreId: 0x1, VarOffset: 0x10D, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 87
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xABD, VarStoreId: 0x1, VarOffset: 0x11C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9, Default
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAA8, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10]
			Subtitle Prompt: "  Device 10", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xABE, VarStoreId: 0x1, VarOffset: 0x10F, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 88
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xABF, VarStoreId: 0x1, VarOffset: 0x11D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10, Default
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAA8, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11]
			Subtitle Prompt: "  Device 11", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAC0, VarStoreId: 0x1, VarOffset: 0x111, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 89
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAC1, VarStoreId: 0x1, VarOffset: 0x11E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0, Default
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
	End 
	Form FormId: 0x278A, Title: "Link options"
		Subtitle Prompt: "Link1", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Sensor Model", Help: "Sensor Model", QuestionFlags: 0x10, QuestionId: 0xAC2, VarStoreId: 0x1, VarOffset: 0x12F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			OneOfOption Option: "IMX135" Value: 0
			OneOfOption Option: "OV5693" Value: 1, Default
			OneOfOption Option: "IMX179" Value: 2
			OneOfOption Option: "OV8858" Value: 3
			OneOfOption Option: "OV2740-IVCAM" Value: 4
			OneOfOption Option: "OV9728" Value: 5
			OneOfOption Option: "IMX188" Value: 6
			OneOfOption Option: "IMX208" Value: 7
			OneOfOption Option: "OV5670" Value: 8
			OneOfOption Option: "OV8865" Value: 9
			OneOfOption Option: "HM2051" Value: 10
			OneOfOption Option: "OV2742" Value: 11
			OneOfOption Option: "OV9234" Value: 12
			OneOfOption Option: "OV8856" Value: 13
			OneOfOption Option: "OV16860" Value: 14
			OneOfOption Option: "User Custom" Value: 255
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xAC2, Value: 0xFF
				Not 
			End 
			String Prompt: "Custom HID", Help: "Custom HID", QuestionFlags: 0x0, QuestionId: 0xAC3, VarStoreId: 0x1, VarStoreInfo: 0x130, MinSize: 0x6, MaxSize: 0x8, Flags: 0x0
			End 
		End 
		OneOf Prompt: "Lanes Clock division", Help: "Lanes Clock division", QuestionFlags: 0x10, QuestionId: 0xAC4, VarStoreId: 0x1, VarOffset: 0x58, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
			OneOfOption Option: "4 4 2 2" Value: 0, Default
			OneOfOption Option: "4 4 3 1" Value: 2
			OneOfOption Option: "4 4 4 0" Value: 3
			OneOfOption Option: "8 0 2 2" Value: 4
			OneOfOption Option: "8 0 3 1" Value: 6
			OneOfOption Option: "8 0 4 0" Value: 7
		End 
		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0xAC5, VarStoreId: 0x1, VarOffset: 0x18A, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0
			OneOfOption Option: "PTC" Value: 16
			OneOfOption Option: "CRD-D" Value: 32
			OneOfOption Option: "CRD-G" Value: 48, Default
			OneOfOption Option: "Kilshon-PPV" Value: 64
			OneOfOption Option: "CRD-G2" Value: 80
		End 
		OneOf Prompt: "GPIO control", Help: "GPIO control", QuestionFlags: 0x10, QuestionId: 0xAC6, VarStoreId: 0x1, VarOffset: 0x196, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			OneOfOption Option: "No Control Logic" Value: 255, Default
			SuppressIf 
				EqIdVal QuestionId: 0xA3A, Value: 0x0
				OneOfOption Option: "Control Logic 0" Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xA3C, Value: 0x0
				OneOfOption Option: "Control Logic 1" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xA3E, Value: 0x0
				OneOfOption Option: "Control Logic 2" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xA40, Value: 0x0
				OneOfOption Option: "Control Logic 3" Value: 3
			End 
		End 
		OneOf Prompt: "Camera position", Help: "Camera position", QuestionFlags: 0x10, QuestionId: 0xAC7, VarStoreId: 0x1, VarOffset: 0x142, Flags: 0x10, Size: 8, Min: 0x61, Max: 0x69, Step: 0x0
			OneOfOption Option: "Front" Value: 97, Default
			OneOfOption Option: "Back" Value: 105
		End 
		OneOf Prompt: "Flash Support", Help: "Flash Support", QuestionFlags: 0x10, QuestionId: 0xAC8, VarStoreId: 0x1, VarOffset: 0x197, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
			OneOfOption Option: "Driver default" Value: 0, Default
			OneOfOption Option: "Disabled" Value: 2
			OneOfOption Option: "Enabled" Value: 3
		End 
		OneOf Prompt: "Privacy LED", Help: "Privacy LED", QuestionFlags: 0x10, QuestionId: 0xAC9, VarStoreId: 0x1, VarOffset: 0x505, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
			OneOfOption Option: "Driver default" Value: 0, Default, MfgDefault
			OneOfOption Option: "ILEDA, 16mA" Value: 1
			OneOfOption Option: "ILEDB, 2mA" Value: 2
			OneOfOption Option: "ILEDB, 4mA" Value: 3
			OneOfOption Option: "ILEDB, 8mA" Value: 4
			OneOfOption Option: "ILEDB, 16mA" Value: 5
		End 
		OneOf Prompt: "Rotation", Help: "Rotation", QuestionFlags: 0x10, QuestionId: 0xACA, VarStoreId: 0x1, VarOffset: 0x198, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
			OneOfOption Option: "0" Value: 0, Default, MfgDefault
			OneOfOption Option: "90" Value: 2
			OneOfOption Option: "180" Value: 4
			OneOfOption Option: "270" Value: 6
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xAC5, Value: 0x50
				Not 
			End 
			OneOf Prompt: "PMIC Position", Help: "PMIC Position
Position 1 indicates the current module is placed on the left side of the CRD-G2 card
Position 2 indicates the current module is placed on the right side of the CRD-G2 card", QuestionFlags: 0x10, QuestionId: 0xACB, VarStoreId: 0x1, VarOffset: 0x506, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Position 1" Value: 0, Default, MfgDefault
				OneOfOption Option: "Position 2" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xACB, Value: 0x1
				Not 
			End 
			OneOf Prompt: "Voltage Rail", Help: "Voltage Rail", QuestionFlags: 0x10, QuestionId: 0xACC, VarStoreId: 0x1, VarOffset: 0x507, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "3 voltage rail" Value: 0, Default, MfgDefault
				OneOfOption Option: "2 voltage rail" Value: 1
			End 
		End 
		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0xACD, VarStoreId: 0x1, VarStoreInfo: 0x143, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0
		End 
		OneOf Prompt: "LaneUsed", Help: "LaneUsed", QuestionFlags: 0x10, QuestionId: 0xACE, VarStoreId: 0x1, VarOffset: 0x18B, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
			OneOfOption Option: "x1" Value: 1
			OneOfOption Option: "x2" Value: 2, Default
			OneOfOption Option: "x3" Value: 3
			OneOfOption Option: "x4" Value: 4
		End 
		OneOf Prompt: "MCLK", Help: "MCLK", QuestionFlags: 0x10, QuestionId: 0xACF, VarStoreId: 0x1, VarOffset: 0x192, Flags: 0x12, Size: 32, Min: 0x124F800, Max: 0x16E3600, Step: 0x0
			OneOfOption Option: "19.2 MHz" Value: 19200000, Default
			OneOfOption Option: "24 MHz" Value: 24000000
			OneOfOption Option: "20 MHz" Value: 20000000
		End 
		OneOf Prompt: "EEPROM Type", Help: "EEPROM Type", QuestionFlags: 0x10, QuestionId: 0xAD0, VarStoreId: 0x1, VarOffset: 0x18C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x0
			OneOfOption Option: "ROM_NONE" Value: 0
			OneOfOption Option: "ROM_OTP" Value: 1
			OneOfOption Option: "ROM_EEPROM_16K_64" Value: 2
			OneOfOption Option: "ROM_EEPROM_16K_16" Value: 3
			OneOfOption Option: "ROM_OTP_ACPI_ACPI" Value: 4
			OneOfOption Option: "ROM_ACPI" Value: 5
			OneOfOption Option: "ROM_EEPROM_BRCA016GWZ" Value: 6
			OneOfOption Option: "ROM_EEPROM_24AA32" Value: 7
			OneOfOption Option: "ROM_EEPROM_CAT24C08" Value: 8, Default
			OneOfOption Option: "ROM_RESERVED1" Value: 9
			OneOfOption Option: "ROM_RESERVED2" Value: 10
		End 
		OneOf Prompt: "VCM Type", Help: "VCM Type", QuestionFlags: 0x10, QuestionId: 0xAD1, VarStoreId: 0x1, VarOffset: 0x18D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
			OneOfOption Option: "VCM_NONE" Value: 0
			OneOfOption Option: "VCM_AD5823" Value: 1, Default
			OneOfOption Option: "VCM_DW9714" Value: 2
			OneOfOption Option: "VCM_AD5816" Value: 3
			OneOfOption Option: "VCM_DW9719" Value: 4
			OneOfOption Option: "VCM_DW9718" Value: 5
			OneOfOption Option: "VCM_RESERVED1" Value: 6
			OneOfOption Option: "VCM_RESERVED2" Value: 7
		End 
		Numeric Prompt: "Number of I2C Components", Help: "Number of I2C Components", QuestionFlags: 0x10, QuestionId: 0xAD2, VarStoreId: 0x1, VarOffset: 0x163, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xAD2, Value: 0x0
			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0xAD3, VarStoreId: 0x1, VarOffset: 0x164, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "I2C0" Value: 0
				OneOfOption Option: "I2C1" Value: 1
				OneOfOption Option: "I2C2" Value: 2
				OneOfOption Option: "I2C3" Value: 3, Default
				OneOfOption Option: "I2C4" Value: 4
				OneOfOption Option: "I2C5" Value: 5
			End 
			Subtitle Prompt: "  Device 0", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAD4, VarStoreId: 0x1, VarOffset: 0x165, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 16
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAD5, VarStoreId: 0x1, VarOffset: 0x17D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0, Default
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAD2, Values: [0, 1]
			Subtitle Prompt: "  Device 1", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAD6, VarStoreId: 0x1, VarOffset: 0x167, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 12
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAD7, VarStoreId: 0x1, VarOffset: 0x17E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1, Default
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAD2, Values: [0, 1, 2]
			Subtitle Prompt: "  Device 2", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAD8, VarStoreId: 0x1, VarOffset: 0x169, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 80
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAD9, VarStoreId: 0x1, VarOffset: 0x17F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2, Default
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAD2, Values: [0, 1, 2, 3]
			Subtitle Prompt: "  Device 3", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xADA, VarStoreId: 0x1, VarOffset: 0x16B, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 81
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xADB, VarStoreId: 0x1, VarOffset: 0x180, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3, Default
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAD2, Values: [0, 1, 2, 3, 4]
			Subtitle Prompt: "  Device 4", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xADC, VarStoreId: 0x1, VarOffset: 0x16D, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 82
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xADD, VarStoreId: 0x1, VarOffset: 0x181, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4, Default
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAD2, Values: [0, 1, 2, 3, 4, 5]
			Subtitle Prompt: "  Device 5", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xADE, VarStoreId: 0x1, VarOffset: 0x16F, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 83
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xADF, VarStoreId: 0x1, VarOffset: 0x182, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5, Default
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAD2, Values: [0, 1, 2, 3, 4, 5, 6]
			Subtitle Prompt: "  Device 6", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAE0, VarStoreId: 0x1, VarOffset: 0x171, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 84
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAE1, VarStoreId: 0x1, VarOffset: 0x183, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6, Default
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAD2, Values: [0, 1, 2, 3, 4, 5, 6, 7]
			Subtitle Prompt: "  Device 7", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAE2, VarStoreId: 0x1, VarOffset: 0x173, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 85
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAE3, VarStoreId: 0x1, VarOffset: 0x184, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7, Default
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAD2, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8]
			Subtitle Prompt: "  Device 8", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAE4, VarStoreId: 0x1, VarOffset: 0x175, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 86
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAE5, VarStoreId: 0x1, VarOffset: 0x185, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8, Default
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAD2, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9]
			Subtitle Prompt: "  Device 9", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAE6, VarStoreId: 0x1, VarOffset: 0x177, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 87
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAE7, VarStoreId: 0x1, VarOffset: 0x186, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9, Default
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAD2, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10]
			Subtitle Prompt: "  Device 10", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAE8, VarStoreId: 0x1, VarOffset: 0x179, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 88
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAE9, VarStoreId: 0x1, VarOffset: 0x187, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10, Default
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAD2, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11]
			Subtitle Prompt: "  Device 11", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAEA, VarStoreId: 0x1, VarOffset: 0x17B, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 89
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAEB, VarStoreId: 0x1, VarOffset: 0x188, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12, Default
			End 
		End 
	End 
	Form FormId: 0x278B, Title: "Link options"
		Subtitle Prompt: "Link2", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Sensor Model", Help: "Sensor Model", QuestionFlags: 0x10, QuestionId: 0xAEC, VarStoreId: 0x1, VarOffset: 0x199, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			OneOfOption Option: "IMX135" Value: 0, Default
			OneOfOption Option: "OV5693" Value: 1
			OneOfOption Option: "IMX179" Value: 2
			OneOfOption Option: "OV8858" Value: 3
			OneOfOption Option: "OV2740-IVCAM" Value: 4
			OneOfOption Option: "OV9728" Value: 5
			OneOfOption Option: "IMX188" Value: 6
			OneOfOption Option: "IMX208" Value: 7
			OneOfOption Option: "OV5670" Value: 8
			OneOfOption Option: "OV8865" Value: 9
			OneOfOption Option: "HM2051" Value: 10
			OneOfOption Option: "OV2742" Value: 11
			OneOfOption Option: "OV9234" Value: 12
			OneOfOption Option: "OV8856" Value: 13
			OneOfOption Option: "OV16860" Value: 14
			OneOfOption Option: "User Custom" Value: 255
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xAEC, Value: 0xFF
				Not 
			End 
			String Prompt: "Custom HID", Help: "Custom HID", QuestionFlags: 0x0, QuestionId: 0xAED, VarStoreId: 0x1, VarStoreInfo: 0x19A, MinSize: 0x6, MaxSize: 0x8, Flags: 0x0
			End 
		End 
		OneOf Prompt: "Lanes Clock division", Help: "Lanes Clock division", QuestionFlags: 0x10, QuestionId: 0xAEE, VarStoreId: 0x1, VarOffset: 0x58, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
			OneOfOption Option: "4 4 2 2" Value: 0, Default
			OneOfOption Option: "4 4 3 1" Value: 2
			OneOfOption Option: "4 4 4 0" Value: 3
			OneOfOption Option: "8 0 2 2" Value: 4
			OneOfOption Option: "8 0 3 1" Value: 6
			OneOfOption Option: "8 0 4 0" Value: 7
		End 
		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0xAEF, VarStoreId: 0x1, VarOffset: 0x1F4, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0
			OneOfOption Option: "PTC" Value: 16
			OneOfOption Option: "CRD-D" Value: 32
			OneOfOption Option: "CRD-G" Value: 48, Default
			OneOfOption Option: "Kilshon-PPV" Value: 64
			OneOfOption Option: "CRD-G2" Value: 80
		End 
		OneOf Prompt: "GPIO control", Help: "GPIO control", QuestionFlags: 0x10, QuestionId: 0xAF0, VarStoreId: 0x1, VarOffset: 0x200, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			OneOfOption Option: "No Control Logic" Value: 255, Default
			SuppressIf 
				EqIdVal QuestionId: 0xA3A, Value: 0x0
				OneOfOption Option: "Control Logic 0" Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xA3C, Value: 0x0
				OneOfOption Option: "Control Logic 1" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xA3E, Value: 0x0
				OneOfOption Option: "Control Logic 2" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xA40, Value: 0x0
				OneOfOption Option: "Control Logic 3" Value: 3
			End 
		End 
		OneOf Prompt: "Camera position", Help: "Camera position", QuestionFlags: 0x10, QuestionId: 0xAF1, VarStoreId: 0x1, VarOffset: 0x1AC, Flags: 0x10, Size: 8, Min: 0x61, Max: 0x69, Step: 0x0
			OneOfOption Option: "Front" Value: 97
			OneOfOption Option: "Back" Value: 105, Default
		End 
		OneOf Prompt: "Flash Support", Help: "Flash Support", QuestionFlags: 0x10, QuestionId: 0xAF2, VarStoreId: 0x1, VarOffset: 0x201, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
			OneOfOption Option: "Driver default" Value: 0, Default
			OneOfOption Option: "Disabled" Value: 2
			OneOfOption Option: "Enabled" Value: 3
		End 
		OneOf Prompt: "Privacy LED", Help: "Privacy LED", QuestionFlags: 0x10, QuestionId: 0xAF3, VarStoreId: 0x1, VarOffset: 0x508, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
			OneOfOption Option: "Driver default" Value: 0, Default, MfgDefault
			OneOfOption Option: "ILEDA, 16mA" Value: 1
			OneOfOption Option: "ILEDB, 2mA" Value: 2
			OneOfOption Option: "ILEDB, 4mA" Value: 3
			OneOfOption Option: "ILEDB, 8mA" Value: 4
			OneOfOption Option: "ILEDB, 16mA" Value: 5
		End 
		OneOf Prompt: "Rotation", Help: "Rotation", QuestionFlags: 0x10, QuestionId: 0xAF4, VarStoreId: 0x1, VarOffset: 0x202, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
			OneOfOption Option: "0" Value: 0, Default, MfgDefault
			OneOfOption Option: "90" Value: 2
			OneOfOption Option: "180" Value: 4
			OneOfOption Option: "270" Value: 6
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xAEF, Value: 0x50
				Not 
			End 
			OneOf Prompt: "PMIC Position", Help: "PMIC Position
Position 1 indicates the current module is placed on the left side of the CRD-G2 card
Position 2 indicates the current module is placed on the right side of the CRD-G2 card", QuestionFlags: 0x10, QuestionId: 0xAF5, VarStoreId: 0x1, VarOffset: 0x509, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Position 1" Value: 0, Default, MfgDefault
				OneOfOption Option: "Position 2" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xAF5, Value: 0x1
				Not 
			End 
			OneOf Prompt: "Voltage Rail", Help: "Voltage Rail", QuestionFlags: 0x10, QuestionId: 0xAF6, VarStoreId: 0x1, VarOffset: 0x50A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "3 voltage rail" Value: 0, Default, MfgDefault
				OneOfOption Option: "2 voltage rail" Value: 1
			End 
		End 
		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0xAF7, VarStoreId: 0x1, VarStoreInfo: 0x1AD, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0
		End 
		OneOf Prompt: "LaneUsed", Help: "LaneUsed", QuestionFlags: 0x10, QuestionId: 0xAF8, VarStoreId: 0x1, VarOffset: 0x1F5, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
			OneOfOption Option: "x1" Value: 1
			OneOfOption Option: "x2" Value: 2
			OneOfOption Option: "x3" Value: 3
			OneOfOption Option: "x4" Value: 4, Default
		End 
		OneOf Prompt: "MCLK", Help: "MCLK", QuestionFlags: 0x10, QuestionId: 0xAF9, VarStoreId: 0x1, VarOffset: 0x1FC, Flags: 0x12, Size: 32, Min: 0x124F800, Max: 0x16E3600, Step: 0x0
			OneOfOption Option: "19.2 MHz" Value: 19200000
			OneOfOption Option: "24 MHz" Value: 24000000, Default
			OneOfOption Option: "20 MHz" Value: 20000000
		End 
		OneOf Prompt: "EEPROM Type", Help: "EEPROM Type", QuestionFlags: 0x10, QuestionId: 0xAFA, VarStoreId: 0x1, VarOffset: 0x1F6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x0
			OneOfOption Option: "ROM_NONE" Value: 0
			OneOfOption Option: "ROM_OTP" Value: 1
			OneOfOption Option: "ROM_EEPROM_16K_64" Value: 2
			OneOfOption Option: "ROM_EEPROM_16K_16" Value: 3
			OneOfOption Option: "ROM_OTP_ACPI_ACPI" Value: 4
			OneOfOption Option: "ROM_ACPI" Value: 5
			OneOfOption Option: "ROM_EEPROM_BRCA016GWZ" Value: 6
			OneOfOption Option: "ROM_EEPROM_24AA32" Value: 7
			OneOfOption Option: "ROM_EEPROM_CAT24C08" Value: 8, Default
			OneOfOption Option: "ROM_RESERVED1" Value: 9
			OneOfOption Option: "ROM_RESERVED2" Value: 10
		End 
		OneOf Prompt: "VCM Type", Help: "VCM Type", QuestionFlags: 0x10, QuestionId: 0xAFB, VarStoreId: 0x1, VarOffset: 0x1F7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
			OneOfOption Option: "VCM_NONE" Value: 0
			OneOfOption Option: "VCM_AD5823" Value: 1
			OneOfOption Option: "VCM_DW9714" Value: 2
			OneOfOption Option: "VCM_AD5816" Value: 3, Default
			OneOfOption Option: "VCM_DW9719" Value: 4
			OneOfOption Option: "VCM_DW9718" Value: 5
			OneOfOption Option: "VCM_RESERVED1" Value: 6
			OneOfOption Option: "VCM_RESERVED2" Value: 7
		End 
		Numeric Prompt: "Number of I2C Components", Help: "Number of I2C Components", QuestionFlags: 0x10, QuestionId: 0xAFC, VarStoreId: 0x1, VarOffset: 0x1CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xAFC, Value: 0x0
			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0xAFD, VarStoreId: 0x1, VarOffset: 0x1CE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "I2C0" Value: 0
				OneOfOption Option: "I2C1" Value: 1
				OneOfOption Option: "I2C2" Value: 2, Default
				OneOfOption Option: "I2C3" Value: 3
				OneOfOption Option: "I2C4" Value: 4
				OneOfOption Option: "I2C5" Value: 5
			End 
			Subtitle Prompt: "  Device 0", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xAFE, VarStoreId: 0x1, VarOffset: 0x1CF, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 16
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xAFF, VarStoreId: 0x1, VarOffset: 0x1E7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0, Default
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAFC, Values: [0, 1]
			Subtitle Prompt: "  Device 1", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB00, VarStoreId: 0x1, VarOffset: 0x1D1, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 14
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB01, VarStoreId: 0x1, VarOffset: 0x1E8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1, Default
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAFC, Values: [0, 1, 2]
			Subtitle Prompt: "  Device 2", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB02, VarStoreId: 0x1, VarOffset: 0x1D3, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 80
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB03, VarStoreId: 0x1, VarOffset: 0x1E9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2, Default
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAFC, Values: [0, 1, 2, 3]
			Subtitle Prompt: "  Device 3", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB04, VarStoreId: 0x1, VarOffset: 0x1D5, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 81
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB05, VarStoreId: 0x1, VarOffset: 0x1EA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3, Default
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAFC, Values: [0, 1, 2, 3, 4]
			Subtitle Prompt: "  Device 4", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB06, VarStoreId: 0x1, VarOffset: 0x1D7, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 82
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB07, VarStoreId: 0x1, VarOffset: 0x1EB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4, Default
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAFC, Values: [0, 1, 2, 3, 4, 5]
			Subtitle Prompt: "  Device 5", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB08, VarStoreId: 0x1, VarOffset: 0x1D9, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 83
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB09, VarStoreId: 0x1, VarOffset: 0x1EC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5, Default
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAFC, Values: [0, 1, 2, 3, 4, 5, 6]
			Subtitle Prompt: "  Device 6", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB0A, VarStoreId: 0x1, VarOffset: 0x1DB, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 84
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB0B, VarStoreId: 0x1, VarOffset: 0x1ED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6, Default
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAFC, Values: [0, 1, 2, 3, 4, 5, 6, 7]
			Subtitle Prompt: "  Device 7", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB0C, VarStoreId: 0x1, VarOffset: 0x1DD, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 85
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB0D, VarStoreId: 0x1, VarOffset: 0x1EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7, Default
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAFC, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8]
			Subtitle Prompt: "  Device 8", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB0E, VarStoreId: 0x1, VarOffset: 0x1DF, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 86
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB0F, VarStoreId: 0x1, VarOffset: 0x1EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0, Default
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAFC, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9]
			Subtitle Prompt: "  Device 9", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB10, VarStoreId: 0x1, VarOffset: 0x1E1, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 87
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB11, VarStoreId: 0x1, VarOffset: 0x1F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0, Default
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAFC, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10]
			Subtitle Prompt: "  Device 10", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB12, VarStoreId: 0x1, VarOffset: 0x1E3, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 88
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB13, VarStoreId: 0x1, VarOffset: 0x1F1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0, Default
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xAFC, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11]
			Subtitle Prompt: "  Device 11", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB14, VarStoreId: 0x1, VarOffset: 0x1E5, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 89
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB15, VarStoreId: 0x1, VarOffset: 0x1F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0, Default
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
	End 
	Form FormId: 0x278C, Title: "Link options"
		Subtitle Prompt: "Link3", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Sensor Model", Help: "Sensor Model", QuestionFlags: 0x10, QuestionId: 0xB16, VarStoreId: 0x1, VarOffset: 0x203, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			OneOfOption Option: "IMX135" Value: 0
			OneOfOption Option: "OV5693" Value: 1, Default
			OneOfOption Option: "IMX179" Value: 2
			OneOfOption Option: "OV8858" Value: 3
			OneOfOption Option: "OV2740-IVCAM" Value: 4
			OneOfOption Option: "OV9728" Value: 5
			OneOfOption Option: "IMX188" Value: 6
			OneOfOption Option: "IMX208" Value: 7
			OneOfOption Option: "OV5670" Value: 8
			OneOfOption Option: "OV8865" Value: 9
			OneOfOption Option: "HM2051" Value: 10
			OneOfOption Option: "OV2742" Value: 11
			OneOfOption Option: "OV9234" Value: 12
			OneOfOption Option: "OV8856" Value: 13
			OneOfOption Option: "OV16860" Value: 14
			OneOfOption Option: "User Custom" Value: 255
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xB16, Value: 0xFF
				Not 
			End 
			String Prompt: "Custom HID", Help: "Custom HID", QuestionFlags: 0x0, QuestionId: 0xB17, VarStoreId: 0x1, VarStoreInfo: 0x204, MinSize: 0x6, MaxSize: 0x8, Flags: 0x0
			End 
		End 
		OneOf Prompt: "Lanes Clock division", Help: "Lanes Clock division", QuestionFlags: 0x10, QuestionId: 0xB18, VarStoreId: 0x1, VarOffset: 0x58, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
			OneOfOption Option: "4 4 2 2" Value: 0, Default
			OneOfOption Option: "4 4 3 1" Value: 2
			OneOfOption Option: "4 4 4 0" Value: 3
			OneOfOption Option: "8 0 2 2" Value: 4
			OneOfOption Option: "8 0 3 1" Value: 6
			OneOfOption Option: "8 0 4 0" Value: 7
		End 
		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0xB19, VarStoreId: 0x1, VarOffset: 0x25E, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0
			OneOfOption Option: "PTC" Value: 16
			OneOfOption Option: "CRD-D" Value: 32
			OneOfOption Option: "CRD-G" Value: 48, Default
			OneOfOption Option: "Kilshon-PPV" Value: 64
			OneOfOption Option: "CRD-G2" Value: 80
		End 
		OneOf Prompt: "GPIO control", Help: "GPIO control", QuestionFlags: 0x10, QuestionId: 0xB1A, VarStoreId: 0x1, VarOffset: 0x26A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			OneOfOption Option: "No Control Logic" Value: 255, Default
			SuppressIf 
				EqIdVal QuestionId: 0xA3A, Value: 0x0
				OneOfOption Option: "Control Logic 0" Value: 0
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xA3C, Value: 0x0
				OneOfOption Option: "Control Logic 1" Value: 1
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xA3E, Value: 0x0
				OneOfOption Option: "Control Logic 2" Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xA40, Value: 0x0
				OneOfOption Option: "Control Logic 3" Value: 3
			End 
		End 
		OneOf Prompt: "Camera position", Help: "Camera position", QuestionFlags: 0x10, QuestionId: 0xB1B, VarStoreId: 0x1, VarOffset: 0x216, Flags: 0x10, Size: 8, Min: 0x61, Max: 0x69, Step: 0x0
			OneOfOption Option: "Front" Value: 97
			OneOfOption Option: "Back" Value: 105, Default
		End 
		OneOf Prompt: "Flash Support", Help: "Flash Support", QuestionFlags: 0x10, QuestionId: 0xB1C, VarStoreId: 0x1, VarOffset: 0x26B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x3, Step: 0x0
			OneOfOption Option: "Driver default" Value: 0, Default
			OneOfOption Option: "Disabled" Value: 2
			OneOfOption Option: "Enabled" Value: 3
		End 
		OneOf Prompt: "Privacy LED", Help: "Privacy LED", QuestionFlags: 0x10, QuestionId: 0xB1D, VarStoreId: 0x1, VarOffset: 0x50B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
			OneOfOption Option: "Driver default" Value: 0, Default, MfgDefault
			OneOfOption Option: "ILEDA, 16mA" Value: 1
			OneOfOption Option: "ILEDB, 2mA" Value: 2
			OneOfOption Option: "ILEDB, 4mA" Value: 3
			OneOfOption Option: "ILEDB, 8mA" Value: 4
			OneOfOption Option: "ILEDB, 16mA" Value: 5
		End 
		OneOf Prompt: "Rotation", Help: "Rotation", QuestionFlags: 0x10, QuestionId: 0xB1E, VarStoreId: 0x1, VarOffset: 0x26C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
			OneOfOption Option: "0" Value: 0, Default, MfgDefault
			OneOfOption Option: "90" Value: 2
			OneOfOption Option: "180" Value: 4
			OneOfOption Option: "270" Value: 6
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xB19, Value: 0x50
				Not 
			End 
			OneOf Prompt: "PMIC Position", Help: "PMIC Position
Position 1 indicates the current module is placed on the left side of the CRD-G2 card
Position 2 indicates the current module is placed on the right side of the CRD-G2 card", QuestionFlags: 0x10, QuestionId: 0xB1F, VarStoreId: 0x1, VarOffset: 0x50C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Position 1" Value: 0, Default, MfgDefault
				OneOfOption Option: "Position 2" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xB1F, Value: 0x1
				Not 
			End 
			OneOf Prompt: "Voltage Rail", Help: "Voltage Rail", QuestionFlags: 0x10, QuestionId: 0xB20, VarStoreId: 0x1, VarOffset: 0x50D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "3 voltage rail" Value: 0, Default, MfgDefault
				OneOfOption Option: "2 voltage rail" Value: 1
			End 
		End 
		String Prompt: "Camera module name", Help: "Camera module name", QuestionFlags: 0x0, QuestionId: 0xB21, VarStoreId: 0x1, VarStoreInfo: 0x217, MinSize: 0x1, MaxSize: 0xF, Flags: 0x0
		End 
		OneOf Prompt: "LaneUsed", Help: "LaneUsed", QuestionFlags: 0x10, QuestionId: 0xB22, VarStoreId: 0x1, VarOffset: 0x25F, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x4, Step: 0x0
			OneOfOption Option: "x1" Value: 1
			OneOfOption Option: "x2" Value: 2
			OneOfOption Option: "x3" Value: 3
			OneOfOption Option: "x4" Value: 4, Default
		End 
		OneOf Prompt: "MCLK", Help: "MCLK", QuestionFlags: 0x10, QuestionId: 0xB23, VarStoreId: 0x1, VarOffset: 0x266, Flags: 0x12, Size: 32, Min: 0x124F800, Max: 0x16E3600, Step: 0x0
			OneOfOption Option: "19.2 MHz" Value: 19200000
			OneOfOption Option: "24 MHz" Value: 24000000, Default
			OneOfOption Option: "20 MHz" Value: 20000000
		End 
		OneOf Prompt: "EEPROM Type", Help: "EEPROM Type", QuestionFlags: 0x10, QuestionId: 0xB24, VarStoreId: 0x1, VarOffset: 0x260, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xA, Step: 0x0
			OneOfOption Option: "ROM_NONE" Value: 0
			OneOfOption Option: "ROM_OTP" Value: 1
			OneOfOption Option: "ROM_EEPROM_16K_64" Value: 2
			OneOfOption Option: "ROM_EEPROM_16K_16" Value: 3
			OneOfOption Option: "ROM_OTP_ACPI_ACPI" Value: 4
			OneOfOption Option: "ROM_ACPI" Value: 5
			OneOfOption Option: "ROM_EEPROM_BRCA016GWZ" Value: 6
			OneOfOption Option: "ROM_EEPROM_24AA32" Value: 7
			OneOfOption Option: "ROM_EEPROM_CAT24C08" Value: 8, Default
			OneOfOption Option: "ROM_RESERVED1" Value: 9
			OneOfOption Option: "ROM_RESERVED2" Value: 10
		End 
		OneOf Prompt: "VCM Type", Help: "VCM Type", QuestionFlags: 0x10, QuestionId: 0xB25, VarStoreId: 0x1, VarOffset: 0x261, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x7, Step: 0x0
			OneOfOption Option: "VCM_NONE" Value: 0
			OneOfOption Option: "VCM_AD5823" Value: 1
			OneOfOption Option: "VCM_DW9714" Value: 2
			OneOfOption Option: "VCM_AD5816" Value: 3, Default
			OneOfOption Option: "VCM_DW9719" Value: 4
			OneOfOption Option: "VCM_DW9718" Value: 5
			OneOfOption Option: "VCM_RESERVED1" Value: 6
			OneOfOption Option: "VCM_RESERVED2" Value: 7
		End 
		Numeric Prompt: "Number of I2C Components", Help: "Number of I2C Components", QuestionFlags: 0x10, QuestionId: 0xB26, VarStoreId: 0x1, VarOffset: 0x237, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x1
			Default DefaultId: 0x0 Value: 6
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xB26, Value: 0x0
			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0xB27, VarStoreId: 0x1, VarOffset: 0x238, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "I2C0" Value: 0
				OneOfOption Option: "I2C1" Value: 1
				OneOfOption Option: "I2C2" Value: 2
				OneOfOption Option: "I2C3" Value: 3, Default
				OneOfOption Option: "I2C4" Value: 4
				OneOfOption Option: "I2C5" Value: 5
			End 
			Subtitle Prompt: "  Device 0", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB28, VarStoreId: 0x1, VarOffset: 0x239, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 16
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB29, VarStoreId: 0x1, VarOffset: 0x251, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0, Default
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB26, Values: [0, 1]
			Subtitle Prompt: "  Device 1", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB2A, VarStoreId: 0x1, VarOffset: 0x23B, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 12
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB2B, VarStoreId: 0x1, VarOffset: 0x252, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1, Default
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB26, Values: [0, 1, 2]
			Subtitle Prompt: "  Device 2", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB2C, VarStoreId: 0x1, VarOffset: 0x23D, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 80
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB2D, VarStoreId: 0x1, VarOffset: 0x253, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2, Default
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB26, Values: [0, 1, 2, 3]
			Subtitle Prompt: "  Device 3", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB2E, VarStoreId: 0x1, VarOffset: 0x23F, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 81
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB2F, VarStoreId: 0x1, VarOffset: 0x254, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3, Default
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB26, Values: [0, 1, 2, 3, 4]
			Subtitle Prompt: "  Device 4", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB30, VarStoreId: 0x1, VarOffset: 0x241, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 82
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB31, VarStoreId: 0x1, VarOffset: 0x255, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4, Default
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB26, Values: [0, 1, 2, 3, 4, 5]
			Subtitle Prompt: "  Device 5", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB32, VarStoreId: 0x1, VarOffset: 0x243, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 83
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB33, VarStoreId: 0x1, VarOffset: 0x256, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5, Default
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB26, Values: [0, 1, 2, 3, 4, 5, 6]
			Subtitle Prompt: "  Device 6", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB34, VarStoreId: 0x1, VarOffset: 0x245, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 84
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB35, VarStoreId: 0x1, VarOffset: 0x257, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6, Default
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB26, Values: [0, 1, 2, 3, 4, 5, 6, 7]
			Subtitle Prompt: "  Device 7", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB36, VarStoreId: 0x1, VarOffset: 0x247, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 85
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB37, VarStoreId: 0x1, VarOffset: 0x258, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7, Default
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB26, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8]
			Subtitle Prompt: "  Device 8", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB38, VarStoreId: 0x1, VarOffset: 0x249, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 86
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB39, VarStoreId: 0x1, VarOffset: 0x259, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8, Default
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB26, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9]
			Subtitle Prompt: "  Device 9", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB3A, VarStoreId: 0x1, VarOffset: 0x24B, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 87
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB3B, VarStoreId: 0x1, VarOffset: 0x25A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9, Default
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB26, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10]
			Subtitle Prompt: "  Device 10", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB3C, VarStoreId: 0x1, VarOffset: 0x24D, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 88
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB3D, VarStoreId: 0x1, VarOffset: 0x25B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10, Default
				OneOfOption Option: "Flash" Value: 12
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB26, Values: [0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11]
			Subtitle Prompt: "  Device 11", Help: "", Flags: 0x0
			End 
			Numeric Prompt: "  I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB3E, VarStoreId: 0x1, VarOffset: 0x24F, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 89
			End 
			OneOf Prompt: "  Device Type", Help: "  Device Type", QuestionFlags: 0x10, QuestionId: 0xB3F, VarStoreId: 0x1, VarOffset: 0x25C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xC, Step: 0x0
				OneOfOption Option: "Sensor" Value: 0
				OneOfOption Option: "VCM" Value: 1
				OneOfOption Option: "EEPROM" Value: 2
				OneOfOption Option: "EEPROM_EXT1" Value: 3
				OneOfOption Option: "EEPROM_EXT2" Value: 4
				OneOfOption Option: "EEPROM_EXT3" Value: 5
				OneOfOption Option: "EEPROM_EXT4" Value: 6
				OneOfOption Option: "EEPROM_EXT5" Value: 7
				OneOfOption Option: "EEPROM_EXT6" Value: 8
				OneOfOption Option: "EEPROM_EXT7" Value: 9
				OneOfOption Option: "IO Expander" Value: 10
				OneOfOption Option: "Flash" Value: 12, Default
			End 
		End 
	End 
	Form FormId: 0x278D, Title: "Control Logic options"
		Subtitle Prompt: "Control Logic options", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Control Logic Type", Help: "Control Logic Type", QuestionFlags: 0x10, QuestionId: 0xB40, VarStoreId: 0x1, VarOffset: 0x59, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFE, Step: 0x0
			OneOfOption Option: "Discrete" Value: 1
			OneOfOption Option: "PMIC_TPS68470" Value: 2, Default
			OneOfOption Option: "PMIC_UP6641" Value: 3
			OneOfOption Option: "PMIC_USER0" Value: 253
			OneOfOption Option: "PMIC_USER1" Value: 254
		End 
		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0xB41, VarStoreId: 0x1, VarOffset: 0x5A, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0
			OneOfOption Option: "PTC" Value: 16
			OneOfOption Option: "CRD-D" Value: 32
			OneOfOption Option: "CRD-G" Value: 48, Default
			OneOfOption Option: "Kilshon-PPV" Value: 64
			OneOfOption Option: "CRD-G2" Value: 80
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB41, Values: [48, 80]
				Not 
			End 
			OneOf Prompt: "PMIC Flash Panel", Help: "PMIC Flash Panel", QuestionFlags: 0x10, QuestionId: 0xB42, VarStoreId: 0x1, VarOffset: 0x5F, Flags: 0x10, Size: 8, Min: 0x21, Max: 0x29, Step: 0x0
				Default DefaultId: 0x0 Value: Other
					Value 
						Uint64 Value: 0x21
					End 
				End 
				OneOfOption Option: "Front" Value: 33, Default
				OneOfOption Option: "Back" Value: 41
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xB40, Value: 0x1
			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0xB43, VarStoreId: 0x1, VarOffset: 0x5C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "I2C0" Value: 0
				OneOfOption Option: "I2C1" Value: 1
				OneOfOption Option: "I2C2" Value: 2, Default
				OneOfOption Option: "I2C3" Value: 3
				OneOfOption Option: "I2C4" Value: 4
				OneOfOption Option: "I2C5" Value: 5
			End 
			Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB44, VarStoreId: 0x1, VarOffset: 0x5D, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: Other
					Value 
						Uint64 Value: 0x4D
					End 
				End 
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xB40, Values: [2, 3]
					Not 
				End 
				OneOf Prompt: "WLED1 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0xB45, VarStoreId: 0x1, VarOffset: 0x4EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "White Led" Value: 1
					OneOfOption Option: "Warm Led" Value: 2
					OneOfOption Option: "IR Led" Value: 3
					OneOfOption Option: "Xeon Led" Value: 4
				End 
				Numeric Prompt: "WLED1 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xB46, VarStoreId: 0x1, VarOffset: 0x4EA, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "WLED1 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xB47, VarStoreId: 0x1, VarOffset: 0x4EB, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				OneOf Prompt: "WLED2 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0xB48, VarStoreId: 0x1, VarOffset: 0x4EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "White Led" Value: 1
					OneOfOption Option: "Warm Led" Value: 2
					OneOfOption Option: "IR Led" Value: 3
					OneOfOption Option: "Xeon Led" Value: 4
				End 
				Numeric Prompt: "WLED2 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xB49, VarStoreId: 0x1, VarOffset: 0x4EC, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "WLED2 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xB4A, VarStoreId: 0x1, VarOffset: 0x4ED, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB40, Values: [2, 3, 4]
			Numeric Prompt: "Number of GPIO Pins", Help: "Number of GPIO Pins", QuestionFlags: 0x10, QuestionId: 0xB4B, VarStoreId: 0x1, VarOffset: 0x5B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x1
				Default DefaultId: 0x0 Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xB4B, Value: 0x0
				Subtitle Prompt: "GPIO 0", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xB4C, VarStoreId: 0x1, VarOffset: 0x60, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 22
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xB4D, VarStoreId: 0x1, VarOffset: 0x64, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xB4E, VarStoreId: 0x1, VarOffset: 0x68, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xB4F, VarStoreId: 0x1, VarOffset: 0x6C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xB50, VarStoreId: 0x1, VarOffset: 0x70, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xB4B, Values: [0, 1]
				Subtitle Prompt: "GPIO 1", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xB51, VarStoreId: 0x1, VarOffset: 0x61, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 11
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xB52, VarStoreId: 0x1, VarOffset: 0x65, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xB53, VarStoreId: 0x1, VarOffset: 0x69, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xB54, VarStoreId: 0x1, VarOffset: 0x6D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xB55, VarStoreId: 0x1, VarOffset: 0x71, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xB4B, Values: [0, 1, 2]
				Subtitle Prompt: "GPIO 2", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xB56, VarStoreId: 0x1, VarOffset: 0x62, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 11
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xB57, VarStoreId: 0x1, VarOffset: 0x66, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xB58, VarStoreId: 0x1, VarOffset: 0x6A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12, Default
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xB59, VarStoreId: 0x1, VarOffset: 0x6E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xB5A, VarStoreId: 0x1, VarOffset: 0x72, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xB4B, Values: [0, 1, 2, 3]
				Subtitle Prompt: "GPIO 3", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xB5B, VarStoreId: 0x1, VarOffset: 0x63, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 11
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xB5C, VarStoreId: 0x1, VarOffset: 0x67, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xB5D, VarStoreId: 0x1, VarOffset: 0x6B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xB5E, VarStoreId: 0x1, VarOffset: 0x6F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xB5F, VarStoreId: 0x1, VarOffset: 0x73, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
		End 
	End 
	Form FormId: 0x278E, Title: "Control Logic options"
		Subtitle Prompt: "Control Logic options", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Control Logic Type", Help: "Control Logic Type", QuestionFlags: 0x10, QuestionId: 0xB60, VarStoreId: 0x1, VarOffset: 0x74, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFE, Step: 0x0
			OneOfOption Option: "Discrete" Value: 1
			OneOfOption Option: "PMIC_TPS68470" Value: 2, Default
			OneOfOption Option: "PMIC_UP6641" Value: 3
			OneOfOption Option: "PMIC_USER0" Value: 253
			OneOfOption Option: "PMIC_USER1" Value: 254
		End 
		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0xB61, VarStoreId: 0x1, VarOffset: 0x75, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0
			OneOfOption Option: "PTC" Value: 16
			OneOfOption Option: "CRD-D" Value: 32
			OneOfOption Option: "CRD-G" Value: 48, Default
			OneOfOption Option: "Kilshon-PPV" Value: 64
			OneOfOption Option: "CRD-G2" Value: 80
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB61, Values: [48, 80]
				Not 
			End 
			OneOf Prompt: "PMIC Flash Panel", Help: "PMIC Flash Panel", QuestionFlags: 0x10, QuestionId: 0xB62, VarStoreId: 0x1, VarOffset: 0x7A, Flags: 0x10, Size: 8, Min: 0x21, Max: 0x29, Step: 0x0
				OneOfOption Option: "Front" Value: 33
				OneOfOption Option: "Back" Value: 41, Default
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xB60, Value: 0x1
			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0xB63, VarStoreId: 0x1, VarOffset: 0x77, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "I2C0" Value: 0
				OneOfOption Option: "I2C1" Value: 1
				OneOfOption Option: "I2C2" Value: 2
				OneOfOption Option: "I2C3" Value: 3, Default
				OneOfOption Option: "I2C4" Value: 4
				OneOfOption Option: "I2C5" Value: 5
			End 
			Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB64, VarStoreId: 0x1, VarOffset: 0x78, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 73
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xB60, Values: [2, 3]
					Not 
				End 
				OneOf Prompt: "WLED1 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0xB65, VarStoreId: 0x1, VarOffset: 0x4F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "White Led" Value: 1
					OneOfOption Option: "Warm Led" Value: 2
					OneOfOption Option: "IR Led" Value: 3
					OneOfOption Option: "Xeon Led" Value: 4
				End 
				Numeric Prompt: "WLED1 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xB66, VarStoreId: 0x1, VarOffset: 0x4F0, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "WLED1 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xB67, VarStoreId: 0x1, VarOffset: 0x4F1, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				OneOf Prompt: "WLED2 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0xB68, VarStoreId: 0x1, VarOffset: 0x4F5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "White Led" Value: 1
					OneOfOption Option: "Warm Led" Value: 2
					OneOfOption Option: "IR Led" Value: 3
					OneOfOption Option: "Xeon Led" Value: 4
				End 
				Numeric Prompt: "WLED2 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xB69, VarStoreId: 0x1, VarOffset: 0x4F2, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "WLED2 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xB6A, VarStoreId: 0x1, VarOffset: 0x4F3, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB60, Values: [2, 3, 4]
			Numeric Prompt: "Number of GPIO Pins", Help: "Number of GPIO Pins", QuestionFlags: 0x10, QuestionId: 0xB6B, VarStoreId: 0x1, VarOffset: 0x76, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x1
				Default DefaultId: 0x0 Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xB6B, Value: 0x0
				Subtitle Prompt: "GPIO 0", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xB6C, VarStoreId: 0x1, VarOffset: 0x7B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 22
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xB6D, VarStoreId: 0x1, VarOffset: 0x7F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xB6E, VarStoreId: 0x1, VarOffset: 0x83, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xB6F, VarStoreId: 0x1, VarOffset: 0x87, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xB70, VarStoreId: 0x1, VarOffset: 0x8B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xB6B, Values: [0, 1]
				Subtitle Prompt: "GPIO 1", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xB71, VarStoreId: 0x1, VarOffset: 0x7C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 11
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xB72, VarStoreId: 0x1, VarOffset: 0x80, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xB73, VarStoreId: 0x1, VarOffset: 0x84, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xB74, VarStoreId: 0x1, VarOffset: 0x88, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xB75, VarStoreId: 0x1, VarOffset: 0x8C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xB6B, Values: [0, 1, 2]
				Subtitle Prompt: "GPIO 2", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xB76, VarStoreId: 0x1, VarOffset: 0x7D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 11
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xB77, VarStoreId: 0x1, VarOffset: 0x81, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xB78, VarStoreId: 0x1, VarOffset: 0x85, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xB79, VarStoreId: 0x1, VarOffset: 0x89, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xB7A, VarStoreId: 0x1, VarOffset: 0x8D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xB6B, Values: [0, 1, 2, 3]
				Subtitle Prompt: "GPIO 3", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xB7B, VarStoreId: 0x1, VarOffset: 0x7E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 11
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xB7C, VarStoreId: 0x1, VarOffset: 0x82, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xB7D, VarStoreId: 0x1, VarOffset: 0x86, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xB7E, VarStoreId: 0x1, VarOffset: 0x8A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xB7F, VarStoreId: 0x1, VarOffset: 0x8E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
		End 
	End 
	Form FormId: 0x278F, Title: "Control Logic options"
		Subtitle Prompt: "Control Logic options", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Control Logic Type", Help: "Control Logic Type", QuestionFlags: 0x10, QuestionId: 0xB80, VarStoreId: 0x1, VarOffset: 0x8F, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFE, Step: 0x0
			OneOfOption Option: "Discrete" Value: 1
			OneOfOption Option: "PMIC_TPS68470" Value: 2, Default
			OneOfOption Option: "PMIC_UP6641" Value: 3
			OneOfOption Option: "PMIC_USER0" Value: 253
			OneOfOption Option: "PMIC_USER1" Value: 254
		End 
		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0xB81, VarStoreId: 0x1, VarOffset: 0x90, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0
			OneOfOption Option: "PTC" Value: 16
			OneOfOption Option: "CRD-D" Value: 32
			OneOfOption Option: "CRD-G" Value: 48, Default
			OneOfOption Option: "Kilshon-PPV" Value: 64
			OneOfOption Option: "CRD-G2" Value: 80
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB81, Values: [48, 80]
				Not 
			End 
			OneOf Prompt: "PMIC Flash Panel", Help: "PMIC Flash Panel", QuestionFlags: 0x10, QuestionId: 0xB82, VarStoreId: 0x1, VarOffset: 0x95, Flags: 0x10, Size: 8, Min: 0x21, Max: 0x29, Step: 0x0
				OneOfOption Option: "Front" Value: 33
				OneOfOption Option: "Back" Value: 41, Default
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xB80, Value: 0x1
			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0xB83, VarStoreId: 0x1, VarOffset: 0x92, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "I2C0" Value: 0
				OneOfOption Option: "I2C1" Value: 1
				OneOfOption Option: "I2C2" Value: 2
				OneOfOption Option: "I2C3" Value: 3, Default
				OneOfOption Option: "I2C4" Value: 4
				OneOfOption Option: "I2C5" Value: 5
			End 
			Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xB84, VarStoreId: 0x1, VarOffset: 0x93, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 73
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xB80, Values: [2, 3]
					Not 
				End 
				OneOf Prompt: "WLED1 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0xB85, VarStoreId: 0x1, VarOffset: 0x4FA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "White Led" Value: 1
					OneOfOption Option: "Warm Led" Value: 2
					OneOfOption Option: "IR Led" Value: 3
					OneOfOption Option: "Xeon Led" Value: 4
				End 
				Numeric Prompt: "WLED1 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xB86, VarStoreId: 0x1, VarOffset: 0x4F6, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "WLED1 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xB87, VarStoreId: 0x1, VarOffset: 0x4F7, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				OneOf Prompt: "WLED2 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0xB88, VarStoreId: 0x1, VarOffset: 0x4FB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "White Led" Value: 1
					OneOfOption Option: "Warm Led" Value: 2
					OneOfOption Option: "IR Led" Value: 3
					OneOfOption Option: "Xeon Led" Value: 4
				End 
				Numeric Prompt: "WLED2 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xB89, VarStoreId: 0x1, VarOffset: 0x4F8, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "WLED2 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xB8A, VarStoreId: 0x1, VarOffset: 0x4F9, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xB80, Values: [2, 3, 4]
			Numeric Prompt: "Number of GPIO Pins", Help: "Number of GPIO Pins", QuestionFlags: 0x10, QuestionId: 0xB8B, VarStoreId: 0x1, VarOffset: 0x91, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x1
				Default DefaultId: 0x0 Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xB8B, Value: 0x0
				Subtitle Prompt: "GPIO 0", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xB8C, VarStoreId: 0x1, VarOffset: 0x96, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 22
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xB8D, VarStoreId: 0x1, VarOffset: 0x9A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xB8E, VarStoreId: 0x1, VarOffset: 0x9E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xB8F, VarStoreId: 0x1, VarOffset: 0xA2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xB90, VarStoreId: 0x1, VarOffset: 0xA6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xB8B, Values: [0, 1]
				Subtitle Prompt: "GPIO 1", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xB91, VarStoreId: 0x1, VarOffset: 0x97, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 11
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xB92, VarStoreId: 0x1, VarOffset: 0x9B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xB93, VarStoreId: 0x1, VarOffset: 0x9F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xB94, VarStoreId: 0x1, VarOffset: 0xA3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xB95, VarStoreId: 0x1, VarOffset: 0xA7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xB8B, Values: [0, 1, 2]
				Subtitle Prompt: "GPIO 2", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xB96, VarStoreId: 0x1, VarOffset: 0x98, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 11
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xB97, VarStoreId: 0x1, VarOffset: 0x9C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xB98, VarStoreId: 0x1, VarOffset: 0xA0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xB99, VarStoreId: 0x1, VarOffset: 0xA4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xB9A, VarStoreId: 0x1, VarOffset: 0xA8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xB8B, Values: [0, 1, 2, 3]
				Subtitle Prompt: "GPIO 3", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xB9B, VarStoreId: 0x1, VarOffset: 0x99, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 11
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xB9C, VarStoreId: 0x1, VarOffset: 0x9D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xB9D, VarStoreId: 0x1, VarOffset: 0xA1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xB9E, VarStoreId: 0x1, VarOffset: 0xA5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xB9F, VarStoreId: 0x1, VarOffset: 0xA9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
		End 
	End 
	Form FormId: 0x2790, Title: "Control Logic options"
		Subtitle Prompt: "Control Logic options", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Control Logic Type", Help: "Control Logic Type", QuestionFlags: 0x10, QuestionId: 0xBA0, VarStoreId: 0x1, VarOffset: 0xAA, Flags: 0x10, Size: 8, Min: 0x1, Max: 0xFE, Step: 0x0
			OneOfOption Option: "Discrete" Value: 1
			OneOfOption Option: "PMIC_TPS68470" Value: 2, Default
			OneOfOption Option: "PMIC_UP6641" Value: 3
			OneOfOption Option: "PMIC_USER0" Value: 253
			OneOfOption Option: "PMIC_USER1" Value: 254
		End 
		OneOf Prompt: "CRD Version", Help: "CRD Version", QuestionFlags: 0x10, QuestionId: 0xBA1, VarStoreId: 0x1, VarOffset: 0xAB, Flags: 0x10, Size: 8, Min: 0x10, Max: 0x50, Step: 0x0
			OneOfOption Option: "PTC" Value: 16
			OneOfOption Option: "CRD-D" Value: 32
			OneOfOption Option: "CRD-G" Value: 48, Default
			OneOfOption Option: "Kilshon-PPV" Value: 64
			OneOfOption Option: "CRD-G2" Value: 80
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xBA1, Values: [48, 80]
				Not 
			End 
			OneOf Prompt: "PMIC Flash Panel", Help: "PMIC Flash Panel", QuestionFlags: 0x10, QuestionId: 0xBA2, VarStoreId: 0x1, VarOffset: 0xB0, Flags: 0x10, Size: 8, Min: 0x21, Max: 0x29, Step: 0x0
				OneOfOption Option: "Front" Value: 33
				OneOfOption Option: "Back" Value: 41, Default
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xBA0, Value: 0x1
			OneOf Prompt: "I2C Channel", Help: "I2C Channel", QuestionFlags: 0x10, QuestionId: 0xBA3, VarStoreId: 0x1, VarOffset: 0xAD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x5, Step: 0x0
				OneOfOption Option: "I2C0" Value: 0
				OneOfOption Option: "I2C1" Value: 1
				OneOfOption Option: "I2C2" Value: 2
				OneOfOption Option: "I2C3" Value: 3, Default
				OneOfOption Option: "I2C4" Value: 4
				OneOfOption Option: "I2C5" Value: 5
			End 
			Numeric Prompt: "I2C Address", Help: "I2C Address", QuestionFlags: 0x10, QuestionId: 0xBA4, VarStoreId: 0x1, VarOffset: 0xAE, Flags: 0x21, Size: 16, Min: 0x0, Max: 0x7F, Step: 0x1
				Default DefaultId: 0x0 Value: 73
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xBA0, Values: [2, 3]
					Not 
				End 
				OneOf Prompt: "WLED1 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0xBA5, VarStoreId: 0x1, VarOffset: 0x500, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "White Led" Value: 1
					OneOfOption Option: "Warm Led" Value: 2
					OneOfOption Option: "IR Led" Value: 3
					OneOfOption Option: "Xeon Led" Value: 4
				End 
				Numeric Prompt: "WLED1 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xBA6, VarStoreId: 0x1, VarOffset: 0x4FC, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "WLED1 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xBA7, VarStoreId: 0x1, VarOffset: 0x4FD, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				OneOf Prompt: "WLED2 Type", Help: "WLED Type", QuestionFlags: 0x10, QuestionId: 0xBA8, VarStoreId: 0x1, VarOffset: 0x501, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x0
					OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
					OneOfOption Option: "White Led" Value: 1
					OneOfOption Option: "Warm Led" Value: 2
					OneOfOption Option: "IR Led" Value: 3
					OneOfOption Option: "Xeon Led" Value: 4
				End 
				Numeric Prompt: "WLED2 Flash Max Current", Help: "WLED Flash Max Current
Valid range is 0x00-0x1F
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xBA9, VarStoreId: 0x1, VarOffset: 0x4FE, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x1F, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
				Numeric Prompt: "WLED2 Torch Max Current", Help: "WLED Torch Max Current
Valid range is 0x00-0x07
0x00 for HW default max current", QuestionFlags: 0x10, QuestionId: 0xBAA, VarStoreId: 0x1, VarOffset: 0x4FF, Flags: 0x20, Size: 8, Min: 0x0, Max: 0x7, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xBA0, Values: [2, 3, 4]
			Numeric Prompt: "Number of GPIO Pins", Help: "Number of GPIO Pins", QuestionFlags: 0x10, QuestionId: 0xBAB, VarStoreId: 0x1, VarOffset: 0xAC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x4, Step: 0x1
				Default DefaultId: 0x0 Value: 2
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xBAB, Value: 0x0
				Subtitle Prompt: "GPIO 0", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xBAC, VarStoreId: 0x1, VarOffset: 0xB1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 22
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xBAD, VarStoreId: 0x1, VarOffset: 0xB5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xBAE, VarStoreId: 0x1, VarOffset: 0xB9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xBAF, VarStoreId: 0x1, VarOffset: 0xBD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xBB0, VarStoreId: 0x1, VarOffset: 0xC1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xBAB, Values: [0, 1]
				Subtitle Prompt: "GPIO 1", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xBB1, VarStoreId: 0x1, VarOffset: 0xB2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 11
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xBB2, VarStoreId: 0x1, VarOffset: 0xB6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xBB3, VarStoreId: 0x1, VarOffset: 0xBA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xBB4, VarStoreId: 0x1, VarOffset: 0xBE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xBB5, VarStoreId: 0x1, VarOffset: 0xC2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xBAB, Values: [0, 1, 2]
				Subtitle Prompt: "GPIO 2", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xBB6, VarStoreId: 0x1, VarOffset: 0xB3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 11
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xBB7, VarStoreId: 0x1, VarOffset: 0xB7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xBB8, VarStoreId: 0x1, VarOffset: 0xBB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xBB9, VarStoreId: 0x1, VarOffset: 0xBF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xBBA, VarStoreId: 0x1, VarOffset: 0xC3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
			SuppressIf 
				EqIdValList QuestionId: 0xBAB, Values: [0, 1, 2, 3]
				Subtitle Prompt: "GPIO 3", Help: "", Flags: 0x0
				End 
				Numeric Prompt: "  Group Pad Number", Help: "  Group Pad Number", QuestionFlags: 0x10, QuestionId: 0xBBB, VarStoreId: 0x1, VarOffset: 0xB4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x17, Step: 0x1
					Default DefaultId: 0x0 Value: 11
				End 
				OneOf Prompt: "  Group Number", Help: "  Group Number", QuestionFlags: 0x10, QuestionId: 0xBBC, VarStoreId: 0x1, VarOffset: 0xB8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x6, Step: 0x0
					OneOfOption Option: "A" Value: 0
					OneOfOption Option: "B" Value: 1
					OneOfOption Option: "C" Value: 2
					OneOfOption Option: "D" Value: 3, Default
					OneOfOption Option: "E" Value: 4
					OneOfOption Option: "F" Value: 5
					OneOfOption Option: "G" Value: 6
				End 
				OneOf Prompt: "  Function", Help: "  Function", QuestionFlags: 0x10, QuestionId: 0xBBD, VarStoreId: 0x1, VarOffset: 0xBC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xD, Step: 0x0
					OneOfOption Option: "Reset" Value: 0, Default
					OneOfOption Option: "Power_En" Value: 11
					OneOfOption Option: "Clock_En" Value: 12
					OneOfOption Option: "pLED_En" Value: 13
				End 
				Numeric Prompt: "  Active Value", Help: "  Active Value", QuestionFlags: 0x10, QuestionId: 0xBBE, VarStoreId: 0x1, VarOffset: 0xC0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 1
				End 
				Numeric Prompt: "  Initial Value", Help: "  Initial Value", QuestionFlags: 0x10, QuestionId: 0xBBF, VarStoreId: 0x1, VarOffset: 0xC4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x1
					Default DefaultId: 0x0 Value: 0
				End 
			End 
		End 
	End 
	Form FormId: 0x27E2, Title: "SB Porting Configuration"
		Subtitle Prompt: "SB Porting Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
	End 
	Form FormId: 0x27E3, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBC0, VarStoreId: 0x1, VarOffset: 0xFFC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBC1, VarStoreId: 0x1, VarOffset: 0x1014, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBC2, VarStoreId: 0x1, VarOffset: 0x1044, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBC3, VarStoreId: 0x1, VarOffset: 0x105C, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27E4, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBC4, VarStoreId: 0x1, VarOffset: 0xFFD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBC5, VarStoreId: 0x1, VarOffset: 0x1016, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBC6, VarStoreId: 0x1, VarOffset: 0x1045, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBC7, VarStoreId: 0x1, VarOffset: 0x105D, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27E5, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBC8, VarStoreId: 0x1, VarOffset: 0xFFE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBC9, VarStoreId: 0x1, VarOffset: 0x1018, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBCA, VarStoreId: 0x1, VarOffset: 0x1046, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBCB, VarStoreId: 0x1, VarOffset: 0x105E, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27E6, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBCC, VarStoreId: 0x1, VarOffset: 0xFFF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBCD, VarStoreId: 0x1, VarOffset: 0x101A, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBCE, VarStoreId: 0x1, VarOffset: 0x1047, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBCF, VarStoreId: 0x1, VarOffset: 0x105F, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27E7, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBD0, VarStoreId: 0x1, VarOffset: 0x1000, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBD1, VarStoreId: 0x1, VarOffset: 0x101C, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBD2, VarStoreId: 0x1, VarOffset: 0x1048, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBD3, VarStoreId: 0x1, VarOffset: 0x1060, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27E8, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBD4, VarStoreId: 0x1, VarOffset: 0x1001, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBD5, VarStoreId: 0x1, VarOffset: 0x101E, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBD6, VarStoreId: 0x1, VarOffset: 0x1049, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBD7, VarStoreId: 0x1, VarOffset: 0x1061, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27E9, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBD8, VarStoreId: 0x1, VarOffset: 0x1002, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBD9, VarStoreId: 0x1, VarOffset: 0x1020, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBDA, VarStoreId: 0x1, VarOffset: 0x104A, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBDB, VarStoreId: 0x1, VarOffset: 0x1062, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27EA, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBDC, VarStoreId: 0x1, VarOffset: 0x1003, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBDD, VarStoreId: 0x1, VarOffset: 0x1022, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBDE, VarStoreId: 0x1, VarOffset: 0x104B, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBDF, VarStoreId: 0x1, VarOffset: 0x1063, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27EB, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBE0, VarStoreId: 0x1, VarOffset: 0x1004, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBE1, VarStoreId: 0x1, VarOffset: 0x1024, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBE2, VarStoreId: 0x1, VarOffset: 0x104C, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBE3, VarStoreId: 0x1, VarOffset: 0x1064, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27EC, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBE4, VarStoreId: 0x1, VarOffset: 0x1005, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBE5, VarStoreId: 0x1, VarOffset: 0x1026, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBE6, VarStoreId: 0x1, VarOffset: 0x104D, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBE7, VarStoreId: 0x1, VarOffset: 0x1065, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27ED, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBE8, VarStoreId: 0x1, VarOffset: 0x1006, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBE9, VarStoreId: 0x1, VarOffset: 0x1028, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBEA, VarStoreId: 0x1, VarOffset: 0x104E, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBEB, VarStoreId: 0x1, VarOffset: 0x1066, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27EE, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBEC, VarStoreId: 0x1, VarOffset: 0x1007, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBED, VarStoreId: 0x1, VarOffset: 0x102A, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBEE, VarStoreId: 0x1, VarOffset: 0x104F, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBEF, VarStoreId: 0x1, VarOffset: 0x1067, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27EF, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBF0, VarStoreId: 0x1, VarOffset: 0x1008, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBF1, VarStoreId: 0x1, VarOffset: 0x102C, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBF2, VarStoreId: 0x1, VarOffset: 0x1050, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBF3, VarStoreId: 0x1, VarOffset: 0x1068, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27F0, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBF4, VarStoreId: 0x1, VarOffset: 0x1009, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBF5, VarStoreId: 0x1, VarOffset: 0x102E, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBF6, VarStoreId: 0x1, VarOffset: 0x1051, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBF7, VarStoreId: 0x1, VarOffset: 0x1069, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27F1, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBF8, VarStoreId: 0x1, VarOffset: 0x100A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBF9, VarStoreId: 0x1, VarOffset: 0x1030, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBFA, VarStoreId: 0x1, VarOffset: 0x1052, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBFB, VarStoreId: 0x1, VarOffset: 0x106A, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27F2, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xBFC, VarStoreId: 0x1, VarOffset: 0x100B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xBFD, VarStoreId: 0x1, VarOffset: 0x1032, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBFE, VarStoreId: 0x1, VarOffset: 0x1053, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xBFF, VarStoreId: 0x1, VarOffset: 0x106B, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27F3, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xC00, VarStoreId: 0x1, VarOffset: 0x100C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xC01, VarStoreId: 0x1, VarOffset: 0x1034, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC02, VarStoreId: 0x1, VarOffset: 0x1054, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC03, VarStoreId: 0x1, VarOffset: 0x106C, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27F4, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xC04, VarStoreId: 0x1, VarOffset: 0x100D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xC05, VarStoreId: 0x1, VarOffset: 0x1036, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC06, VarStoreId: 0x1, VarOffset: 0x1055, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC07, VarStoreId: 0x1, VarOffset: 0x106D, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27F5, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xC08, VarStoreId: 0x1, VarOffset: 0x100E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xC09, VarStoreId: 0x1, VarOffset: 0x1038, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC0A, VarStoreId: 0x1, VarOffset: 0x1056, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC0B, VarStoreId: 0x1, VarOffset: 0x106E, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27F6, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xC0C, VarStoreId: 0x1, VarOffset: 0x100F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xC0D, VarStoreId: 0x1, VarOffset: 0x103A, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC0E, VarStoreId: 0x1, VarOffset: 0x1057, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC0F, VarStoreId: 0x1, VarOffset: 0x106F, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27F7, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xC10, VarStoreId: 0x1, VarOffset: 0x1010, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xC11, VarStoreId: 0x1, VarOffset: 0x103C, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC12, VarStoreId: 0x1, VarOffset: 0x1058, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC13, VarStoreId: 0x1, VarOffset: 0x1070, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27F8, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xC14, VarStoreId: 0x1, VarOffset: 0x1011, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xC15, VarStoreId: 0x1, VarOffset: 0x103E, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC16, VarStoreId: 0x1, VarOffset: 0x1059, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC17, VarStoreId: 0x1, VarOffset: 0x1071, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27F9, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xC18, VarStoreId: 0x1, VarOffset: 0x1012, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xC19, VarStoreId: 0x1, VarOffset: 0x1040, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC1A, VarStoreId: 0x1, VarOffset: 0x105A, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC1B, VarStoreId: 0x1, VarOffset: 0x1072, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x27FA, Title: "Extra options "
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device. If enable, it will take more time at POST time.", QuestionFlags: 0x10, QuestionId: 0xC1C, VarStoreId: 0x1, VarOffset: 0x1013, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory", Help: "Prefetchable Memory Range for this Root Bridge.", QuestionFlags: 0x10, QuestionId: 0xC1D, VarStoreId: 0x1, VarOffset: 0x1042, Flags: 0x11, Size: 16, Min: 0x1, Max: 0x14, Step: 0x1
				Default DefaultId: 0x0 Value: 10
				Default DefaultId: 0x1 Value: 10
			End 
			Numeric Prompt: "Reseved Memory Alignment", Help: "Reseved Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC1E, VarStoreId: 0x1, VarOffset: 0x105B, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
			Numeric Prompt: "Prefetchable Memory Alignment", Help: "Prefetchable Memory Alignment (0 - 31 bits)", QuestionFlags: 0x10, QuestionId: 0xC1F, VarStoreId: 0x1, VarOffset: 0x1073, Flags: 0x10, Size: 8, Min: 0x1, Max: 0x1F, Step: 0x1
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
	End 
	Form FormId: 0x280E, Title: "PEG Port Feature Configuration"
		Subtitle Prompt: "PEG Port Feature Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		OneOf Prompt: "Detect Non-Compliance Device", Help: "Detect Non-Compliance PCI Express Device in PEG", QuestionFlags: 0x10, QuestionId: 0xC20, VarStoreId: 0x1, VarOffset: 0x109C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			OneOfOption Option: "Disabled" Value: 0, Default, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
	End 
	Form FormId: 0x280F, Title: "External Gfx Card Primary Display Configuration"
		Subtitle Prompt: "External Gfx Card Primary Display Configuration", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x3FA, Value: 0x0
				EqIdVal QuestionId: 0x3AC, Value: 0x1
				Or 
				EqIdVal QuestionId: 0x2829, Value: 0x0
				Or 
				EqIdVal QuestionId: 0x3FA, Value: 0x4
				Or 
			End 
			OneOf Prompt: " Primary PEG", Help: "Select PEG0/PEG1/PEG2/PEG3 Graphics device should be Primary PEG.", QuestionFlags: 0x10, QuestionId: 0xC21, VarStoreId: 0x1, VarOffset: 0x109A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "PEG11" Value: 1
				OneOfOption Option: "PEG12" Value: 2
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0x3FA, Value: 0x0
				EqIdVal QuestionId: 0x3AC, Value: 0x1
				Or 
				EqIdVal QuestionId: 0x2829, Value: 0x0
				Or 
				EqIdVal QuestionId: 0x3FA, Value: 0x4
				Or 
			End 
			OneOf Prompt: " Primary PCIE", Help: "Select Auto/PCIE1/PCIE2/PCIE3/PCIE4/PCIE5/PCIE6/PCIE7 of D28:F0/F1/F2/F3/F4/F5/F6/F7, PCIE8/PCIE9/PCIE10/PCIE11/PCIE12/PCIE13/PCIE14/PCIE15 of D29:F0/F1/F2/F3/F4/F5/F6/F7, PCIE16/PCIE17/PCIE18/PCIE19 of D27:F0/F1/F2/F3, Graphics device should be Primary PCIE.", QuestionFlags: 0x10, QuestionId: 0xC22, VarStoreId: 0x1, VarOffset: 0x109B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x13, Step: 0x0
				OneOfOption Option: "Auto" Value: 0, Default, MfgDefault
				OneOfOption Option: "PCIE1" Value: 1
				OneOfOption Option: "PCIE2" Value: 2
				OneOfOption Option: "PCIE3" Value: 3
				OneOfOption Option: "PCIE4" Value: 4
				OneOfOption Option: "PCIE5" Value: 5
				OneOfOption Option: "PCIE6" Value: 6
				OneOfOption Option: "PCIE7" Value: 7
				OneOfOption Option: "PCIE8" Value: 8
				OneOfOption Option: "PCIE9" Value: 9
				OneOfOption Option: "PCIE10" Value: 10
				OneOfOption Option: "PCIE11" Value: 11
				OneOfOption Option: "PCIE12" Value: 12
				OneOfOption Option: "PCIE13" Value: 13
				OneOfOption Option: "PCIE14" Value: 14
				OneOfOption Option: "PCIE15" Value: 15
				OneOfOption Option: "PCIE16" Value: 16
				OneOfOption Option: "PCIE17" Value: 17
				OneOfOption Option: "PCIE18" Value: 18
				OneOfOption Option: "PCIE19" Value: 19
			End 
		End 
	End 
	Form FormId: 0x2714, Title: "Security"
		Subtitle Prompt: "Password Description", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "If ONLY the Administrator's password is set,", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "then this only limits access to Setup and is", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "only asked for when entering Setup.", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "If ONLY the User's password is set, then this", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "is a power on password and must be entered to", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "boot or enter Setup. In Setup the User will", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "have Administrator rights.", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "The password length must be", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "in the following range:", Help: "", Flags: 0x0
		End 
		Text Prompt: "Minimum length", Help: "", Text: "N/A"
		Text Prompt: "Maximum length", Help: "", Text: "N/A"
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			Password Prompt: "Administrator Password", Help: "Set Administrator Password", QuestionFlags: 0x0, QuestionId: 0xC23, VarStoreId: 0x6, VarStoreInfo: 0x28, MinSize: 0x3, MaxSize: 0x14
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC23, Value: 0x0
			Password Prompt: "User Password", Help: "Set User Password", QuestionFlags: 0x0, QuestionId: 0xC24, VarStoreId: 0x6, VarStoreInfo: 0x0, MinSize: 0x3, MaxSize: 0x14
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Secure Boot", Help: "Customizable Secure Boot settings", QuestionFlags: 0x4, QuestionId: 0x28F5, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28F6
		End 
	End 
	Form FormId: 0x28F6, Title: "Secure Boot"
		SuppressIf 
			EqIdVal QuestionId: 0xC4F, Value: 0x0
			Text Prompt: "System Mode", Help: "", Text: "Setup"
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC4F, Value: 0x1
			Text Prompt: "System Mode", Help: "", Text: "User"
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC4E, Value: 0x1
				Not 
			End 
			Text Prompt: "Vendor Keys", Help: "", Text: "Not Modified"
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC4E, Value: 0x0
				Not 
			End 
			Text Prompt: "Vendor Keys", Help: "", Text: "Modified"
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
			OneOf Prompt: "Secure Boot", Help: "Secure Boot activated when:
 Secure Boot is enabled
 Platform Key(PK) is enrolled,
 System mode is User/Deployed,
 and CSM is disabled", QuestionFlags: 0x14, QuestionId: 0x28F7, VarStoreId: 0x2F, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x0 Value: 0
				OneOfOption Option: "Disabled" Value: 0
				OneOfOption Option: "Enabled" Value: 1, MfgDefault
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC4D, Value: 0x0
					Not 
				End 
				Text Prompt: "", Help: "", Text: "Not Active"
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC4D, Value: 0x1
					Not 
				End 
				Text Prompt: "", Help: "", Text: "Active"
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			OneOf Prompt: "Secure Boot Customization", Help: "Customizable Secure Boot mode:
In Custom mode Secure Boot Policy variables can be configured by a physically present user without full authentication", QuestionFlags: 0x14, QuestionId: 0x28F8, VarStoreId: 0x2F, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x0 Value: 1
				OneOfOption Option: "Standard" Value: 0, MfgDefault
				OneOfOption Option: "Custom" Value: 1
			End 
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC42, Value: 0x1
				EqIdVal QuestionId: 0x28F8, Value: 0x0
				Or 
			End 
			Ref Prompt: "Restore Factory Keys", Help: "Force System to User Mode.
Configure NVRAM to contain OEM-defined factory default Secure Boot keys", QuestionFlags: 0x14, QuestionId: 0x28F9, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28F6
			GrayOutIf 
				EqIdVal QuestionId: 0xC4C, Value: 0x0
				Ref Prompt: "Reset To Setup Mode", Help: "Delete NVRAM content of all UEFI Secure Boot key databases", QuestionFlags: 0x14, QuestionId: 0x28FA, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28F6
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
			Ref Prompt: "Key Management", Help: "Enables expert users to modify
Secure Boot Policy variables
without full authentication", QuestionFlags: 0x4, QuestionId: 0x28FE, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF
		End 
	End 
	Form FormId: 0x28FF, Title: "Key Management"
		OneOf Prompt: "Factory Key Provision", Help: "Provision factory default keys on next re-boot only when System in Setup Mode", QuestionFlags: 0x14, QuestionId: 0x2900, VarStoreId: 0x2F, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			Default DefaultId: 0x0 Value: 0
			OneOfOption Option: "Disabled" Value: 0
			OneOfOption Option: "Enabled" Value: 1, MfgDefault
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Ref Prompt: "Restore Factory Keys", Help: "Force System to User Mode.
Configure NVRAM to contain OEM-defined factory default Secure Boot keys", QuestionFlags: 0x14, QuestionId: 0x2901, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF
		GrayOutIf 
			EqIdVal QuestionId: 0xC4C, Value: 0x0
			Ref Prompt: "Reset To Setup Mode", Help: "Delete NVRAM content of all UEFI Secure Boot key databases", QuestionFlags: 0x14, QuestionId: 0x2902, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC4C, Value: 0x0
				EqIdVal QuestionId: 0xC4B, Value: 0x0
				And 
				EqIdVal QuestionId: 0xC47, Value: 0x0
				And 
				EqIdVal QuestionId: 0xC4A, Value: 0x0
				And 
				EqIdVal QuestionId: 0xC49, Value: 0x0
				And 
				EqIdVal QuestionId: 0xC48, Value: 0x0
				And 
			End 
			Ref Prompt: "Export Secure Boot variables", Help: "Copy NVRAM content of Secure Boot variables to files in a root folder on a file system device", QuestionFlags: 0x4, QuestionId: 0x2903, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF
		End 
		Ref Prompt: "Enroll Efi Image", Help: "Allow the image to run in Secure Boot mode.
Enroll SHA256 Hash certificate of a PE image into Authorized Signature Database (db)", QuestionFlags: 0x4, QuestionId: 0x2904, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "Device Guard Ready", Help: "", Flags: 0x0
		End 
		GrayOutIf 
			EqIdVal QuestionId: 0xC47, Value: 0x0
			Ref Prompt: "Remove 'UEFI CA' from DB", Help: "Device Guard ready system must not list 'Microsoft UEFI CA' Certificate in Authorized Signature database (db)", QuestionFlags: 0x4, QuestionId: 0x2905, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF
		End 
		Ref Prompt: "Restore DB defaults", Help: "Restore DB variable to factory defaults", QuestionFlags: 0x4, QuestionId: 0x2906, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "Secure Boot variable | Size| Keys| Key Source", Help: "", Flags: 0x0
		End 
		Ref Prompt: " ", Help: "Enroll Factory Defaults or load certificates from a file:
 1.Public Key Certificate in:
  a)EFI_SIGNATURE_LIST
  b)EFI_CERT_X509 (DER encoded)
  c)EFI_CERT_RSA2048 (bin)
  d)EFI_CERT_SHA256,384,512
 2.Authenticated UEFI Variable
 3.EFI PE/COFF Image(SHA256)
Key Source:
 Factory,External,Mixed", QuestionFlags: 0x14, QuestionId: 0x2907, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF
		Ref Prompt: " ", Help: "Enroll Factory Defaults or load certificates from a file:
 1.Public Key Certificate in:
  a)EFI_SIGNATURE_LIST
  b)EFI_CERT_X509 (DER encoded)
  c)EFI_CERT_RSA2048 (bin)
  d)EFI_CERT_SHA256,384,512
 2.Authenticated UEFI Variable
 3.EFI PE/COFF Image(SHA256)
Key Source:
 Factory,External,Mixed", QuestionFlags: 0x4, QuestionId: 0x2908, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF
		Ref Prompt: " ", Help: "Enroll Factory Defaults or load certificates from a file:
 1.Public Key Certificate in:
  a)EFI_SIGNATURE_LIST
  b)EFI_CERT_X509 (DER encoded)
  c)EFI_CERT_RSA2048 (bin)
  d)EFI_CERT_SHA256,384,512
 2.Authenticated UEFI Variable
 3.EFI PE/COFF Image(SHA256)
Key Source:
 Factory,External,Mixed", QuestionFlags: 0x4, QuestionId: 0x2909, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF
		Ref Prompt: " ", Help: "Enroll Factory Defaults or load certificates from a file:
 1.Public Key Certificate in:
  a)EFI_SIGNATURE_LIST
  b)EFI_CERT_X509 (DER encoded)
  c)EFI_CERT_RSA2048 (bin)
  d)EFI_CERT_SHA256,384,512
 2.Authenticated UEFI Variable
 3.EFI PE/COFF Image(SHA256)
Key Source:
 Factory,External,Mixed", QuestionFlags: 0x4, QuestionId: 0x290A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF
		Ref Prompt: " ", Help: "Enroll Factory Defaults or load certificates from a file:
 1.Public Key Certificate in:
  a)EFI_SIGNATURE_LIST
  b)EFI_CERT_X509 (DER encoded)
  c)EFI_CERT_RSA2048 (bin)
  d)EFI_CERT_SHA256,384,512
 2.Authenticated UEFI Variable
 3.EFI PE/COFF Image(SHA256)
Key Source:
 Factory,External,Mixed", QuestionFlags: 0x4, QuestionId: 0x290B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF
		Ref Prompt: " ", Help: "Enroll Factory Defaults or load certificates from a file:
 1.Public Key Certificate in:
  a)EFI_SIGNATURE_LIST
  b)EFI_CERT_X509 (DER encoded)
  c)EFI_CERT_RSA2048 (bin)
  d)EFI_CERT_SHA256,384,512
 2.Authenticated UEFI Variable
 3.EFI PE/COFF Image(SHA256)
Key Source:
 Factory,External,Mixed", QuestionFlags: 0x4, QuestionId: 0x290C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x28FF
	End 
	Form FormId: 0x2715, Title: "Boot"
		Subtitle Prompt: "Boot Configuration", Help: "", Flags: 0x0
		End 
		Numeric Prompt: "Setup Prompt Timeout", Help: "Number of seconds to wait for setup activation key. 65535(0xFFFF) means indefinite waiting.", QuestionFlags: 0x0, QuestionId: 0xC25, VarStoreId: 0x8, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x1, Max: 0xFFFF, Step: 0x1
			Default DefaultId: 0x0 Value: 1
			Default DefaultId: 0x1 Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			OneOf Prompt: "Bootup NumLock State", Help: "Select the keyboard NumLock state", QuestionFlags: 0x10, QuestionId: 0xC26, VarStoreId: 0x1, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "On" Value: 1
				OneOfOption Option: "Off" Value: 0
				Default DefaultId: 0x0 Value: 1
				Default DefaultId: 0x1 Value: 1
			End 
		End 
		CheckBox Prompt: "Quiet Boot", Help: "Enables or disables Quiet Boot option", QuestionFlags: 0x0, QuestionId: 0xC27, VarStoreId: 0x6, VarOffset: 0x50, Flags: 0x0, Default: Disabled, MfgDefault: Disabled
			Default DefaultId: 0x0 Value: 0
			Default DefaultId: 0x1 Value: 0
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "Boot Option Priorities", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC46, Values: [65535]
			OneOf Prompt: "Boot Option #%d", Help: "Sets the system boot order", QuestionFlags: 0x0, QuestionId: 0xC28, VarStoreId: 0x9, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "" Value: 0
				OneOfOption Option: "" Value: 1
				Default DefaultId: 0x0 Value: 0
				Default DefaultId: 0x1 Value: 0
			End 
		End 
		OneOf Prompt: "Fast Boot", Help: "Enables or disables boot with initialization of a minimal set of devices required to launch active boot option. Has no effect for BBS boot options.", QuestionFlags: 0x10, QuestionId: 0xC29, VarStoreId: 0x1, VarOffset: 0xFEE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
			Default DefaultId: 0x0 Value: 0
			OneOfOption Option: "Disabled" Value: 0, MfgDefault
			OneOfOption Option: "Enabled" Value: 1
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC29, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC29, Value: 0x0
				OneOf Prompt: " SATA Support", Help: "If Last Boot HDD Only, Only last boot HDD device will be available in Post. If All Sata Devices, all SATA devices will be available in OS and Post.", QuestionFlags: 0x10, QuestionId: 0xC2A, VarStoreId: 0x1, VarOffset: 0xFEF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 1
					OneOfOption Option: "Last Boot HDD Only" Value: 0
					OneOfOption Option: "All Sata Devices" Value: 1, MfgDefault
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC29, Value: 0x0
			OneOf Prompt: " VGA Support", Help: "If Auto, only install Legacy OpRom with Legacy OS and logo would NOT be shown during post. Efi driver will still be installed with EFI OS.", QuestionFlags: 0x10, QuestionId: 0xC2B, VarStoreId: 0x1, VarOffset: 0xFF0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x0 Value: 1
				OneOfOption Option: "Auto" Value: 0
				OneOfOption Option: "EFI Driver" Value: 1, MfgDefault
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC29, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC29, Value: 0x0
				OneOf Prompt: " USB Support", Help: "If Disabled, all USB devices will NOT be available until after OS boot. If Partial Initial, USB Mass Storage and specific USB port/device will NOT be available before OS boot. If Enabled, all USB devices will be available in OS and Post.", QuestionFlags: 0x10, QuestionId: 0xC2C, VarStoreId: 0x1, VarOffset: 0xFF1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
					Default DefaultId: 0x0 Value: 2
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Full Initial" Value: 1, MfgDefault
					OneOfOption Option: "Partial Initial" Value: 2
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC29, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC29, Value: 0x0
				OneOf Prompt: " PS2 Devices Support", Help: "If Disabled, PS2 devices will be skipped.", QuestionFlags: 0x10, QuestionId: 0xC2D, VarStoreId: 0x1, VarOffset: 0xFF2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 1
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, MfgDefault
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC29, Value: 0x0
			GrayOutIf 
				EqIdVal QuestionId: 0xC29, Value: 0x0
				OneOf Prompt: " NetWork Stack Driver Support", Help: "If Disabled, NetWork Stack Driver will be skipped.", QuestionFlags: 0x10, QuestionId: 0xC2E, VarStoreId: 0x1, VarOffset: 0xFF4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
					Default DefaultId: 0x0 Value: 0
					OneOfOption Option: "Disabled" Value: 0
					OneOfOption Option: "Enabled" Value: 1, MfgDefault
				End 
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC29, Value: 0x0
			OneOf Prompt: "Redirection Support", Help: "If disable, Redirection function will be disabled.", QuestionFlags: 0x10, QuestionId: 0xC2F, VarStoreId: 0x1, VarOffset: 0xFF3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x1, Step: 0x0
				Default DefaultId: 0x0 Value: 0
				OneOfOption Option: "Disabled" Value: 0, MfgDefault
				OneOfOption Option: "Enabled" Value: 1
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC45, Values: [0]
			Subtitle Prompt: "Driver Option Priorities", Help: "", Flags: 0x0
			End 
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC45, Values: [65535]
			OneOf Prompt: "Driver Option #%d", Help: "Sets the system driver order", QuestionFlags: 0x0, QuestionId: 0xC30, VarStoreId: 0x26, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "" Value: 0, Default, MfgDefault
				OneOfOption Option: "" Value: 1
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			OneOf Prompt: "New Boot Option Policy", Help: "Controls the placement of newly detected UEFI boot options", QuestionFlags: 0x10, QuestionId: 0xC31, VarStoreId: 0x29, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0x2, Step: 0x0
				Default DefaultId: 0x0 Value: 0
				OneOfOption Option: "Default" Value: 0
				OneOfOption Option: "Place First" Value: 1
				OneOfOption Option: "Place Last" Value: 2
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC44, Values: [65535]
			Ref Prompt: "", Help: "Set the order of the legacy devices in this group", QuestionFlags: 0x0, QuestionId: 0xC32, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x27DF
		End 
	End 
	Form FormId: 0x27DF, Title: "Boot"
		SuppressIf 
			EqIdValList QuestionId: 0xC43, Values: [65535]
			OneOf Prompt: "Boot Option #%d", Help: "Sets the system boot order", QuestionFlags: 0x0, QuestionId: 0xC33, VarStoreId: 0xE, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0x1, Step: 0x0
				OneOfOption Option: "" Value: 0
				OneOfOption Option: "" Value: 1
				Default DefaultId: 0x0 Value: 0
				Default DefaultId: 0x1 Value: 0
			End 
		End 
	End 
	Form FormId: 0x2716, Title: "Save & Exit"
		Subtitle Prompt: "Save Options", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC41, Value: 0x1
				Ref Prompt: "Save Changes and Exit", Help: "Exit system setup after saving the changes.", QuestionFlags: 0x0, QuestionId: 0xC34, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC41, Value: 0x2
				Ref Prompt: "Discard Changes and Exit", Help: "Exit system setup without saving any changes.", QuestionFlags: 0x0, QuestionId: 0xC35, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC41, Value: 0x9
			Ref Prompt: "Save Changes and Reset", Help: "Reset the system after saving the changes.", QuestionFlags: 0x0, QuestionId: 0xC36, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC41, Value: 0xA
			Ref Prompt: "Discard Changes and Reset", Help: "Reset system setup without saving any changes.", QuestionFlags: 0x0, QuestionId: 0xC37, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC41, Value: 0x3
				Ref Prompt: "Save Changes", Help: "Save Changes done so far to any of the setup options.", QuestionFlags: 0x0, QuestionId: 0xC38, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC41, Value: 0x4
				Ref Prompt: "Discard Changes", Help: "Discard Changes done so far to any of the setup options.", QuestionFlags: 0x0, QuestionId: 0xC39, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716
			End 
			Subtitle Prompt: "", Help: "", Flags: 0x0
			End 
		End 
		Subtitle Prompt: "Default Options", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC41, Value: 0x5
			Ref Prompt: "Restore Defaults", Help: "Restore/Load Default values for all the setup options.", QuestionFlags: 0x0, QuestionId: 0xC3A, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716
		End 
		SuppressIf 
			EqIdVal QuestionId: 0xC42, Value: 0x0
				EqIdVal QuestionId: 0xC42, Value: 0x1
				Or 
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC41, Value: 0x6
				Ref Prompt: "Save as User Defaults", Help: "Save the changes done so far as User Defaults.", QuestionFlags: 0x0, QuestionId: 0xC3B, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716
			End 
			SuppressIf 
				EqIdVal QuestionId: 0xC41, Value: 0x7
				Ref Prompt: "Restore User Defaults", Help: "Restore the User Defaults to all the setup options.", QuestionFlags: 0x0, QuestionId: 0xC3C, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716
			End 
		End 
		Subtitle Prompt: "", Help: "", Flags: 0x0
		End 
		Subtitle Prompt: "Boot Override", Help: "", Flags: 0x0
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC40, Values: [65535]
			Ref Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC3D, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716
		End 
		SuppressIf 
			EqIdValList QuestionId: 0xC3F, Values: [1]
			Ref Prompt: "Launch EFI Shell from filesystem device", Help: "Attempts to Launch EFI Shell application (Shell.efi) from one of the available filesystem devices", QuestionFlags: 0x0, QuestionId: 0xC3E, VarStoreId: 0x0, VarStoreInfo: 0xFFFF, FormId: 0x2716
		End 
		DisableIf 
			True 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC3F, VarStoreId: 0x10, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC40, VarStoreId: 0xF, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC41, VarStoreId: 0x5, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC42, VarStoreId: 0x4, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC43, VarStoreId: 0xD, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC44, VarStoreId: 0xC, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC45, VarStoreId: 0x25, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC46, VarStoreId: 0x7, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC47, VarStoreId: 0x30, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC48, VarStoreId: 0x30, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC49, VarStoreId: 0x30, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC4A, VarStoreId: 0x30, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC4B, VarStoreId: 0x30, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC4C, VarStoreId: 0x30, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC4D, VarStoreId: 0x33, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC4E, VarStoreId: 0x31, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC4F, VarStoreId: 0x32, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC50, VarStoreId: 0x36, VarOffset: 0x2, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC51, VarStoreId: 0x36, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC52, VarStoreId: 0x36, VarOffset: 0x2A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC53, VarStoreId: 0x1, VarOffset: 0x9F4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC54, VarStoreId: 0x36, VarOffset: 0x29, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC55, VarStoreId: 0x1, VarOffset: 0x9F3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC56, VarStoreId: 0x36, VarOffset: 0x28, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC57, VarStoreId: 0x1, VarOffset: 0x9F2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC58, VarStoreId: 0x36, VarOffset: 0x27, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC59, VarStoreId: 0x1, VarOffset: 0x9F1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC5A, VarStoreId: 0x36, VarOffset: 0x26, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC5B, VarStoreId: 0x1, VarOffset: 0x9F0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC5C, VarStoreId: 0x36, VarOffset: 0x25, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC5D, VarStoreId: 0x1, VarOffset: 0x9EF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC5E, VarStoreId: 0x36, VarOffset: 0x24, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC5F, VarStoreId: 0x1, VarOffset: 0x9EE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC60, VarStoreId: 0x36, VarOffset: 0x23, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC61, VarStoreId: 0x1, VarOffset: 0x9ED, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC62, VarStoreId: 0x36, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC63, VarStoreId: 0x36, VarOffset: 0x5D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC64, VarStoreId: 0x36, VarOffset: 0x45, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC65, VarStoreId: 0x36, VarOffset: 0x5B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC66, VarStoreId: 0x36, VarOffset: 0x43, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC67, VarStoreId: 0x36, VarOffset: 0x64, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC68, VarStoreId: 0x36, VarOffset: 0x59, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC69, VarStoreId: 0x36, VarOffset: 0x41, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC6A, VarStoreId: 0x36, VarOffset: 0x57, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC6B, VarStoreId: 0x36, VarOffset: 0x3F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC6C, VarStoreId: 0x36, VarOffset: 0x63, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC6D, VarStoreId: 0x36, VarOffset: 0x55, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC6E, VarStoreId: 0x36, VarOffset: 0x3D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC6F, VarStoreId: 0x36, VarOffset: 0x53, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC70, VarStoreId: 0x36, VarOffset: 0x3B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC71, VarStoreId: 0x36, VarOffset: 0x62, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC72, VarStoreId: 0x36, VarOffset: 0x51, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC73, VarStoreId: 0x36, VarOffset: 0x39, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC74, VarStoreId: 0x36, VarOffset: 0x4F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC75, VarStoreId: 0x36, VarOffset: 0x37, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC76, VarStoreId: 0x36, VarOffset: 0x61, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC77, VarStoreId: 0x36, VarOffset: 0x4D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC78, VarStoreId: 0x36, VarOffset: 0x35, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC79, VarStoreId: 0x36, VarOffset: 0x4B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC7A, VarStoreId: 0x36, VarOffset: 0x33, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC7B, VarStoreId: 0x36, VarOffset: 0x60, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC7C, VarStoreId: 0x36, VarOffset: 0x49, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC7D, VarStoreId: 0x36, VarOffset: 0x31, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC7E, VarStoreId: 0x36, VarOffset: 0x47, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC7F, VarStoreId: 0x36, VarOffset: 0x2F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC80, VarStoreId: 0x36, VarOffset: 0x5F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC81, VarStoreId: 0x36, VarOffset: 0x22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC82, VarStoreId: 0x36, VarOffset: 0x4, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC83, VarStoreId: 0x36, VarOffset: 0x2D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC84, VarStoreId: 0x36, VarOffset: 0x2C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC85, VarStoreId: 0x36, VarOffset: 0x18, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC86, VarStoreId: 0x36, VarOffset: 0x17, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC87, VarStoreId: 0x36, VarOffset: 0x16, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC88, VarStoreId: 0x36, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC89, VarStoreId: 0x36, VarOffset: 0x15, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC8A, VarStoreId: 0x36, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC8B, VarStoreId: 0x36, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC8C, VarStoreId: 0x36, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC8D, VarStoreId: 0x36, VarOffset: 0xD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC8E, VarStoreId: 0x36, VarOffset: 0x21, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC8F, VarStoreId: 0x36, VarOffset: 0x20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC90, VarStoreId: 0x36, VarOffset: 0x1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC91, VarStoreId: 0x12, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC92, VarStoreId: 0x36, VarOffset: 0x79, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC93, VarStoreId: 0x11, VarOffset: 0x17, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC94, VarStoreId: 0x36, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC95, VarStoreId: 0x36, VarOffset: 0x7C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC96, VarStoreId: 0x12, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC97, VarStoreId: 0x12, VarOffset: 0x2, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC98, VarStoreId: 0x12, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC99, VarStoreId: 0x36, VarOffset: 0x12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC9A, VarStoreId: 0x36, VarOffset: 0x11, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC9B, VarStoreId: 0x36, VarOffset: 0x10, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC9C, VarStoreId: 0x36, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC9D, VarStoreId: 0x1, VarOffset: 0x10DC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC9E, VarStoreId: 0x2E, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xC9F, VarStoreId: 0x2B, VarOffset: 0xF, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCA0, VarStoreId: 0x2B, VarOffset: 0xE, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCA1, VarStoreId: 0x2B, VarOffset: 0xD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCA2, VarStoreId: 0x2B, VarOffset: 0xC, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCA3, VarStoreId: 0x2B, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCA4, VarStoreId: 0x2B, VarOffset: 0xA, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCA5, VarStoreId: 0x2B, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCA6, VarStoreId: 0x2B, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCA7, VarStoreId: 0x2B, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCA8, VarStoreId: 0x2B, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCA9, VarStoreId: 0x2B, VarOffset: 0x5, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCAA, VarStoreId: 0x2B, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCAB, VarStoreId: 0x2B, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCAC, VarStoreId: 0x2B, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCAD, VarStoreId: 0x2B, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCAE, VarStoreId: 0x2B, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCAF, VarStoreId: 0x2A, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCB0, VarStoreId: 0x2C, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCB1, VarStoreId: 0x2C, VarOffset: 0x2, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCB2, VarStoreId: 0x2C, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCB3, VarStoreId: 0x2C, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCB4, VarStoreId: 0x28, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCB5, VarStoreId: 0x28, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCB6, VarStoreId: 0x27, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCB7, VarStoreId: 0x22, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCB8, VarStoreId: 0x20, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCB9, VarStoreId: 0x1A, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCBA, VarStoreId: 0x19, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCBB, VarStoreId: 0x36, VarOffset: 0x7B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCBC, VarStoreId: 0x1, VarOffset: 0x796, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCBD, VarStoreId: 0x1, VarOffset: 0x6E6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCBE, VarStoreId: 0x1, VarOffset: 0x6C9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCBF, VarStoreId: 0x36, VarOffset: 0x77, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCC0, VarStoreId: 0x11, VarOffset: 0x1D, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCC1, VarStoreId: 0x11, VarOffset: 0x1C, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCC2, VarStoreId: 0x14, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCC3, VarStoreId: 0x1, VarOffset: 0x757, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCC4, VarStoreId: 0x14, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCC5, VarStoreId: 0x14, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCC6, VarStoreId: 0x1, VarOffset: 0x75A, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCC7, VarStoreId: 0x1, VarOffset: 0x768, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCC8, VarStoreId: 0x14, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCC9, VarStoreId: 0x1, VarOffset: 0x756, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCCA, VarStoreId: 0x11, VarOffset: 0x28, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCCB, VarStoreId: 0x11, VarOffset: 0x27, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCCC, VarStoreId: 0x12, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCCD, VarStoreId: 0x12, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCCE, VarStoreId: 0x12, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCCF, VarStoreId: 0x12, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCD0, VarStoreId: 0x11, VarOffset: 0x14, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCD1, VarStoreId: 0x11, VarOffset: 0x3, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCD2, VarStoreId: 0x11, VarOffset: 0x1E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCD3, VarStoreId: 0x11, VarOffset: 0x9, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCD4, VarStoreId: 0x11, VarOffset: 0xB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCD5, VarStoreId: 0x11, VarOffset: 0x1, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCD6, VarStoreId: 0x11, VarOffset: 0x13, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCD7, VarStoreId: 0x11, VarOffset: 0x12, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCD8, VarStoreId: 0x11, VarOffset: 0x22, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCD9, VarStoreId: 0x11, VarOffset: 0x25, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCDA, VarStoreId: 0x11, VarOffset: 0x24, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCDB, VarStoreId: 0x11, VarOffset: 0x23, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCDC, VarStoreId: 0x11, VarOffset: 0x21, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCDD, VarStoreId: 0x11, VarOffset: 0x20, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCDE, VarStoreId: 0x11, VarOffset: 0x1F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCDF, VarStoreId: 0x11, VarOffset: 0x4, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCE0, VarStoreId: 0x1, VarOffset: 0x61E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCE1, VarStoreId: 0x11, VarOffset: 0x8, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCE2, VarStoreId: 0x11, VarOffset: 0x7, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCE3, VarStoreId: 0x11, VarOffset: 0x6, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCE4, VarStoreId: 0x1, VarOffset: 0x63B, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCE5, VarStoreId: 0x11, VarOffset: 0x19, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCE6, VarStoreId: 0x1, VarOffset: 0xF65, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCE7, VarStoreId: 0x1, VarOffset: 0xF64, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCE8, VarStoreId: 0x1, VarOffset: 0xF63, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCE9, VarStoreId: 0x1, VarOffset: 0xF62, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCEA, VarStoreId: 0x1, VarOffset: 0xF61, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCEB, VarStoreId: 0x1, VarOffset: 0xF60, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCEC, VarStoreId: 0x1, VarOffset: 0xF5F, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCED, VarStoreId: 0x1, VarOffset: 0xF68, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCEE, VarStoreId: 0x1, VarOffset: 0xF67, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCEF, VarStoreId: 0x1, VarOffset: 0xF66, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCF0, VarStoreId: 0x1, VarOffset: 0x3CD, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCF1, VarStoreId: 0x27, VarOffset: 0x0, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCF2, VarStoreId: 0x18, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCF3, VarStoreId: 0x17, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCF4, VarStoreId: 0x3, VarOffset: 0x0, Flags: 0x11, Size: 16, Min: 0x0, Max: 0xFFFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCF5, VarStoreId: 0x36, VarOffset: 0x2E, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
			Numeric Prompt: "", Help: "", QuestionFlags: 0x0, QuestionId: 0xCF6, VarStoreId: 0x1, VarOffset: 0x2BB, Flags: 0x10, Size: 8, Min: 0x0, Max: 0xFF, Step: 0x0
			End 
		End 
	End 
End 
